(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 20)
    (zones 0)
    (modules 13)
    (nets 12)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 GND)
  (net 6 "Net-(J4-Pad1)")
  (net 7 "Net-(J6-Pad1)")
  (net 8 "Net-(J7-Pad1)")
  (net 9 "Net-(J8-Pad1)")
  (net 10 "Net-(RV1-Pad3)")
  (net 11 "Net-(RV2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(RV2-Pad3)")
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BBFE)
    (at 67.31 66.04)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J8 (at 0 -2.54) (layer F.Fab))
    (fp_text value "Y out" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 9 "Net-(J8-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BBDE)
    (at 67.31 40.64)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J5 (at 0 -2.54) (layer F.Fab))
    (fp_text value GND (at 3.81 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 5 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BBBD)
    (at 67.31 60.96)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J7 (at 0 -2.54) (layer F.Fab))
    (fp_text value "Pb out" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 8 "Net-(J7-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BB9A)
    (at 114.3 66.04)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J4 (at 0 -2.54) (layer F.Fab))
    (fp_text value "Y in" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 6 "Net-(J4-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BB70)
    (at 67.31 55.88)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J6 (at 0 -2.54) (layer F.Fab))
    (fp_text value "Pr out" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 7 "Net-(J6-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BB52)
    (at 114.3 60.96)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J3 (at 0 -2.54) (layer F.Fab))
    (fp_text value "Pb in" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BB2A)
    (at 114.3 55.88)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J2 (at 0 -2.54) (layer F.Fab))
    (fp_text value "Pr in" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2BB04)
    (at 114.3 40.64)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J1 (at 0 -2.54) (layer F.Fab))
    (fp_text value GND (at -3.81 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 5 GND))
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3386P_Vertical (layer Top) (tedit 5AA07388)
    (at 85.09 62.23)
    (descr "Potentiometer, vertical, Bourns 3386P, https://www.bourns.com/pdfs/3386.pdf")
    (tags "Potentiometer vertical Bourns 3386P")
    (fp_text reference RV2 (at -0.015 -8.555) (layer F.SilkS))
    (fp_text value "100 ohm" (at -0.015 3.475) (layer F.Fab))
    (fp_text user %R (at -3.78 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J7-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(RV2-Pad3)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3386P_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3386P_Vertical (layer Top) (tedit 5AA07388)
    (at 85.09 48.356)
    (descr "Potentiometer, vertical, Bourns 3386P, https://www.bourns.com/pdfs/3386.pdf")
    (tags "Potentiometer vertical Bourns 3386P")
    (fp_text reference RV1 (at -0.015 -8.555) (layer F.SilkS))
    (fp_text value "100 ohm" (at -0.015 3.475) (layer F.Fab))
    (fp_text user %R (at -3.78 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J6-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(RV1-Pad3)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3386P_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer Top) (tedit 5AE5139B)
    (at 101.6 66.04 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 2.54) (layer F.SilkS))
    (fp_text value "10 ohm" (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 100.33 57.15 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.27 4.445) (layer F.SilkS))
    (fp_text value "220 uF" (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 100.33 46.99 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.27 4.445) (layer F.SilkS))
    (fp_text value "220 uF" (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 118.11 38.1) (end 118.11 68.58) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.5 38.1) (end 118.11 38.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.5 68.58) (end 63.5 38.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.11 68.58) (end 63.5 68.58) (layer Edge.Cuts) (width 0.1))
  (gr_text "KPackLabs\n2023-03" (at 72.39 50.8) (layer F.SilkS))
  (gr_text "S-ENC-YUV\nMini-B v1.1" (at 72.39 45.72) (layer F.SilkS))
  (gr_text INPUT (at 107.95 60.96 90) (layer F.SilkS))
  (gr_text OUTPUT (at 73.66 60.96 90) (layer F.SilkS))
  (gr_text Y (at 71.12 66.04 90) (layer F.SilkS))
  (gr_text Pb (at 71.12 60.96 90) (layer F.SilkS))
  (gr_text Pr (at 71.12 55.88 90) (layer F.SilkS))
  (gr_text Y (at 110.49 66.04 90) (layer F.SilkS))
  (gr_text Pb (at 110.49 60.96 90) (layer F.SilkS))
  (gr_text Pr (at 110.49 55.88 90) (layer F.SilkS))
)
