(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 129)
    (no_connects 0)
    (area 61.457999 54.2976 241.530915 150.020001)
    (thickness 1.6)
    (drawings 16)
    (tracks 446)
    (zones 0)
    (modules 51)
    (nets 64)
  )
  (page A4)
  (title_block
    (title "IBX ][ HV Board")
    (rev 1)
    (company "Princeton University")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory rev2/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BUS101-Pad2)")
  (net 3 "Net-(BUS101-Pad3)")
  (net 4 "Net-(BUS101-Pad4)")
  (net 5 "Net-(BUS101-Pad18)")
  (net 6 "Net-(BUS101-Pad25)")
  (net 7 +12V)
  (net 8 /D0)
  (net 9 /D1)
  (net 10 /D2)
  (net 11 /D3)
  (net 12 /D4)
  (net 13 /D5)
  (net 14 /D6)
  (net 15 /D7)
  (net 16 "Net-(BUS101-Pad41)")
  (net 17 "Net-(BUS101-Pad38)")
  (net 18 "Net-(D101-Pad1)")
  (net 19 "Net-(D101-Pad2)")
  (net 20 +5V)
  (net 21 "Net-(J101-Pad1)")
  (net 22 "Net-(J102-Pad1)")
  (net 23 "Net-(R101-Pad1)")
  (net 24 "Net-(R101-Pad2)")
  (net 25 "Net-(R103-Pad2)")
  (net 26 "Net-(R104-Pad2)")
  (net 27 "Net-(R105-Pad2)")
  (net 28 "Net-(R106-Pad2)")
  (net 29 "Net-(R107-Pad2)")
  (net 30 "Net-(R108-Pad2)")
  (net 31 "Net-(R109-Pad2)")
  (net 32 "Net-(R110-Pad2)")
  (net 33 "Net-(R111-Pad2)")
  (net 34 "Net-(R112-Pad2)")
  (net 35 "Net-(R113-Pad2)")
  (net 36 "Net-(R114-Pad2)")
  (net 37 "Net-(R117-Pad2)")
  (net 38 "Net-(R120-Pad1)")
  (net 39 "Net-(R121-Pad1)")
  (net 40 "Net-(U104-Pad12)")
  (net 41 "Net-(U104-Pad10)")
  (net 42 "Net-(U104-Pad11)")
  (net 43 "Net-(U105-Pad1)")
  (net 44 "Net-(U104-Pad6)")
  (net 45 "Net-(U105-Pad11)")
  (net 46 "Net-(BUS101-Pad50)")
  (net 47 "Net-(C101-Pad1)")
  (net 48 "Net-(C101-Pad2)")
  (net 49 "Net-(R128-Pad1)")
  (net 50 "Net-(R128-Pad2)")
  (net 51 "Net-(C104-Pad1)")
  (net 52 "Net-(J103-Pad2)")
  (net 53 "Net-(J103-Pad3)")
  (net 54 "Net-(J103-Pad4)")
  (net 55 "Net-(C108-Pad1)")
  (net 56 "Net-(C110-Pad1)")
  (net 57 "Net-(U102-Pad2)")
  (net 58 "Net-(U102-Pad4)")
  (net 59 "Net-(U102-Pad5)")
  (net 60 "Net-(U102-Pad6)")
  (net 61 "Net-(U103-Pad4)")
  (net 62 "Net-(U105-Pad9)")
  (net 63 "Net-(R125-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net GND)
    (add_net "Net-(BUS101-Pad18)")
    (add_net "Net-(BUS101-Pad2)")
    (add_net "Net-(BUS101-Pad3)")
    (add_net "Net-(BUS101-Pad38)")
    (add_net "Net-(BUS101-Pad4)")
    (add_net "Net-(BUS101-Pad41)")
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C101-Pad2)")
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(C108-Pad1)")
    (add_net "Net-(C110-Pad1)")
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D101-Pad2)")
    (add_net "Net-(J101-Pad1)")
    (add_net "Net-(J103-Pad2)")
    (add_net "Net-(J103-Pad3)")
    (add_net "Net-(J103-Pad4)")
    (add_net "Net-(R101-Pad1)")
    (add_net "Net-(R101-Pad2)")
    (add_net "Net-(R103-Pad2)")
    (add_net "Net-(R104-Pad2)")
    (add_net "Net-(R105-Pad2)")
    (add_net "Net-(R106-Pad2)")
    (add_net "Net-(R107-Pad2)")
    (add_net "Net-(R108-Pad2)")
    (add_net "Net-(R109-Pad2)")
    (add_net "Net-(R110-Pad2)")
    (add_net "Net-(R111-Pad2)")
    (add_net "Net-(R112-Pad2)")
    (add_net "Net-(R113-Pad2)")
    (add_net "Net-(R114-Pad2)")
    (add_net "Net-(R117-Pad2)")
    (add_net "Net-(R120-Pad1)")
    (add_net "Net-(R121-Pad1)")
    (add_net "Net-(R125-Pad2)")
    (add_net "Net-(R128-Pad1)")
    (add_net "Net-(R128-Pad2)")
    (add_net "Net-(U102-Pad2)")
    (add_net "Net-(U102-Pad4)")
    (add_net "Net-(U102-Pad5)")
    (add_net "Net-(U102-Pad6)")
    (add_net "Net-(U103-Pad4)")
    (add_net "Net-(U104-Pad10)")
    (add_net "Net-(U104-Pad11)")
    (add_net "Net-(U104-Pad12)")
    (add_net "Net-(U104-Pad6)")
    (add_net "Net-(U105-Pad1)")
    (add_net "Net-(U105-Pad11)")
    (add_net "Net-(U105-Pad9)")
  )
  (net_class HV ""
    (clearance 5.08)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J102-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 1)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net "Net-(BUS101-Pad25)")
    (add_net "Net-(BUS101-Pad50)")
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A279F37)
    (at 190.627 86.614 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U105 (at 3.937 0.635 90) (layer F.SilkS))
    (fp_text value 7400 (at 3.683 12.7 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U105-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(U102-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U105-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(U105-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(R128-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(U102-Pad4)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U105-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U104-Pad11)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(R128-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27927F)
    (at 145.034 110.998)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R105 (at 5.207 -0.508) (layer F.SilkS))
    (fp_text value 10k (at 5.334 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R103-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R105-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 140.3604 74.676 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D101 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(D101-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(D101-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_TE5_Littlefuse-395Series (layer F.Cu) (tedit 5A373E46)
    (at 198.3105 117.856 270)
    (descr "Fuse, TE5, Littlefuse/Wickmann, No. 460, No560,")
    (tags "Fuse TE5 Littlefuse/Wickmann No. 460 No560 ")
    (fp_text reference F101 (at 8.0772 -0.2667 360) (layer F.SilkS))
    (fp_text value Polyfuse_Small (at 2.35 3.1 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole circle (at 5.08 0.01 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(BUS101-Pad25)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27921E)
    (at 145.034 100.838)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R101 (at 5.08 -0.635) (layer F.SilkS))
    (fp_text value 20k (at 5.08 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R101-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R101-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27920B)
    (at 145.034 97.409)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R102 (at 5.08 -0.635) (layer F.SilkS))
    (fp_text value 20k (at 5.207 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R101-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27923A)
    (at 145.034 104.14)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R103 (at 5.08 -0.635) (layer F.SilkS))
    (fp_text value 10k (at 5.207 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R101-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R103-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27926E)
    (at 145.034 107.569)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R104 (at 5.207 -0.635) (layer F.SilkS))
    (fp_text value 20k (at 5.334 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R103-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R104-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279EA8)
    (at 145.034 114.427)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R106 (at 5.207 -0.635) (layer F.SilkS))
    (fp_text value 20k (at 5.207 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R105-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R106-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279E93)
    (at 145.034 117.856)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R107 (at 5.334 -0.635) (layer F.SilkS))
    (fp_text value 10k (at 5.334 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R105-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R107-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279E9A)
    (at 145.034 121.285)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R108 (at 5.207 -0.635) (layer F.SilkS))
    (fp_text value 20k (at 5.334 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R107-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R108-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27F7EA)
    (at 168.021 121.158)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R109 (at 4.953 -0.508) (layer F.SilkS))
    (fp_text value 10k (at 5.08 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R107-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R109-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27F816)
    (at 178.181 117.856 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R110 (at 5.08 0.508 180) (layer F.SilkS))
    (fp_text value 20k (at 5.08 -0.635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R109-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R110-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27F833)
    (at 168.021 114.554)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R111 (at 5.334 -0.508) (layer F.SilkS))
    (fp_text value 10k (at 5.207 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R109-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R111-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27F843)
    (at 178.181 111.252 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R112 (at 5.08 0.508 180) (layer F.SilkS))
    (fp_text value 20k (at 4.953 -0.635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R111-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R112-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A281099)
    (at 168.021 107.95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R113 (at 5.207 -0.508) (layer F.SilkS))
    (fp_text value 10k (at 5.334 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R111-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R113-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A2810A0)
    (at 178.181 104.648 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R114 (at 4.953 0.508 180) (layer F.SilkS))
    (fp_text value 20k (at 4.953 -0.635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R113-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R114-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A2810A3)
    (at 168.021 101.346)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R115 (at 5.08 -0.508) (layer F.SilkS))
    (fp_text value 10k (at 5.207 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R113-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J101-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27F6E4)
    (at 155.2448 80.3656 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R116 (at 5.08 0.508 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 -0.635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(J103-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27A04E)
    (at 178.181 98.044 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R117 (at 4.953 0.508 180) (layer F.SilkS))
    (fp_text value 20k (at 5.08 -0.635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J101-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R117-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279EC3)
    (at 145.034 83.9724)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R118 (at 5.207 0.635) (layer F.SilkS))
    (fp_text value 10k (at 5.207 -0.508) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(J103-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27F790)
    (at 144.9324 74.676)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R119 (at 4.953 0.635) (layer F.SilkS))
    (fp_text value 470 (at 5.207 -0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D101-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279EFB)
    (at 205.867 115.062 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R120 (at 5.207 0.508 270) (layer F.SilkS))
    (fp_text value 4k7 (at 5.207 -0.635 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R120-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279F0C)
    (at 202.438 115.062 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R121 (at 4.953 -0.635 270) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 0.635 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R121-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ibxlib:CHV-rev2 (layer F.Cu) (tedit 56DC34F4)
    (at 132.08 90.678)
    (descr "HV source from CAEN")
    (tags hv)
    (fp_text reference U107 (at -39.5986 -0.635) (layer F.SilkS))
    (fp_text value CHV (at -0.6 6.6) (layer F.Fab))
    (fp_text user "HV Pin" (at -34.9758 18.3134) (layer B.SilkS))
    (fp_text user "HV Pin" (at -35.0774 18.3134) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at -2.54 0 180) (size 1.727 1.727) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C108-Pad1)"))
    (pad 6 thru_hole circle (at -5.08 0 180) (size 1.727 1.727) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(J103-Pad4)"))
    (pad 8 thru_hole circle (at -7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.54 180) (size 1.727 1.727) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D101-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 2.54 180) (size 1.727 1.727) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(J103-Pad2)"))
    (pad 5 thru_hole circle (at -5.08 2.54 180) (size 1.727 1.727) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J103-Pad3)"))
    (pad 7 thru_hole circle (at -7.62 2.54 180) (size 1.727 1.727) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 +12V))
    (pad 9 thru_hole circle (at -34.99 15.94 180) (size 1.727 1.727) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J102-Pad1)"))
    (pad S4 thru_hole trapezoid (at -22.1 -2.9 180) (size 3.5 2.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad S3 thru_hole trapezoid (at -22.1 24.1 180) (size 3.5 2.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad S2 thru_hole rect (at 3.9 10.6 180) (size 2.2 3.5) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad S1 thru_hole rect (at -48.1 10.6 180) (size 2.2 3.5) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A27F9C1)
    (at 169.1005 88.7095 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C101 (at -2.032 0.254 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.56 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C101-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C101-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_TE5_Littlefuse-395Series (layer F.Cu) (tedit 5880C2E0)
    (at 137.033 119.634 270)
    (descr "Fuse, TE5, Littlefuse/Wickmann, No. 460, No560,")
    (tags "Fuse TE5 Littlefuse/Wickmann No. 460 No560 ")
    (fp_text reference F103 (at 2.65 -2.95 270) (layer F.SilkS))
    (fp_text value Polyfuse_Small (at 2.35 3.1 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 +12V))
    (pad 2 thru_hole circle (at 5.08 0.01 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(BUS101-Pad50)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27A004)
    (at 155.1432 90.7796 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R122 (at 5.207 -0.635 180) (layer F.SilkS))
    (fp_text value 8k2 (at 5.207 0.508 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J101-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C108-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279FD6)
    (at 182.372 64.262 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R123 (at 5.08 0.635 270) (layer F.SilkS))
    (fp_text value 1M (at 5.08 -0.635 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C110-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A27F7B5)
    (at 144.9832 87.4268)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R124 (at 5.207 0.635) (layer F.SilkS))
    (fp_text value 10k (at 5.207 -0.508) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C108-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A279F7A)
    (at 182.4355 76.962 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R128 (at 5.08 0.508 270) (layer F.SilkS))
    (fp_text value 0 (at 5.08 -0.635 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(R128-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(R128-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A279FEE)
    (at 157.9245 86.1695)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U101 (at 3.937 0.635) (layer F.SilkS))
    (fp_text value AD584 (at 3.81 7.366) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C104-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C104-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(C101-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(C101-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +12V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A279FA9)
    (at 163.0045 77.724 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U103 (at 3.81 0.635 90) (layer F.SilkS))
    (fp_text value 74HC74 (at 3.81 12.446 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(U102-Pad6)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(U103-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(D101-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A279F8E)
    (at 190.6905 99.5045 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U104 (at 3.937 0.381 90) (layer F.SilkS))
    (fp_text value 7400 (at 4.064 12.827 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(BUS101-Pad18)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U104-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(BUS101-Pad18)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U104-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U104-Pad10)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U104-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(BUS101-Pad38)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U104-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(BUS101-Pad38)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U104-Pad12)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U104-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U104-Pad12)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A27A023)
    (at 157.861 98.044)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U106 (at 3.81 0.635) (layer F.SilkS))
    (fp_text value 74LS374 (at 3.937 19.939 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R125-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U105-Pad11)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R101-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R110-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D0))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /D4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D1))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /D5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R104-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R112-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R106-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R114-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /D2))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /D6))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /D3))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /D7))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R108-Pad2)"))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R117-Pad2)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C104-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A279F1E)
    (at 188.214 112.014 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U108 (at 3.937 0.889 90) (layer F.SilkS))
    (fp_text value 74LS138 (at 3.937 14.605 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(BUS101-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(BUS101-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(BUS101-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(BUS101-Pad41)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R121-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(U105-Pad9)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R120-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(U103-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U105-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Apple2_bus:BUS_A2 (layer F.Cu) (tedit 5A37C94F)
    (at 159.5882 135.8392)
    (descr "Connector Apple ][ Slot")
    (tags "CONN BUS APPLE ][")
    (fp_text reference BUS101 (at -22.86 -7.62) (layer F.SilkS) hide)
    (fp_text value A2_BUS (at 0 -7.62) (layer F.Fab))
    (pad 2 connect rect (at -20.32 0 180) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 2 "Net-(BUS101-Pad2)"))
    (pad 3 connect rect (at -17.78 0 180) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 3 "Net-(BUS101-Pad3)"))
    (pad 4 connect rect (at -15.24 0 180) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 4 "Net-(BUS101-Pad4)"))
    (pad 18 connect rect (at 20.32 0 180) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 5 "Net-(BUS101-Pad18)"))
    (pad 25 connect rect (at 38.1 0 180) (size 1.778 7.62) (layers F.Cu F.Mask)
      (net 6 "Net-(BUS101-Pad25)"))
    (pad 50 connect rect (at -22.86 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 46 "Net-(BUS101-Pad50)"))
    (pad 49 connect rect (at -20.32 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 8 /D0))
    (pad 48 connect rect (at -17.78 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 9 /D1))
    (pad 47 connect rect (at -15.24 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 10 /D2))
    (pad 46 connect rect (at -12.7 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 11 /D3))
    (pad 45 connect rect (at -10.16 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 12 /D4))
    (pad 44 connect rect (at -7.62 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 13 /D5))
    (pad 43 connect rect (at -5.08 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 14 /D6))
    (pad 42 connect rect (at -2.54 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 15 /D7))
    (pad 41 connect rect (at 0 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 16 "Net-(BUS101-Pad41)"))
    (pad 38 connect rect (at 7.62 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 17 "Net-(BUS101-Pad38)"))
    (pad 26 connect rect (at 38.1 0 180) (size 1.778 7.62) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A27A039)
    (at 177.1904 92.1512 270)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J101 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Debug-1 (at 0.127 -2.54 270) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J101-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module ibxlib:HVConnector3D (layer F.Cu) (tedit 5A2815DB)
    (at 78.613 73.533)
    (fp_text reference J102 (at 6 6) (layer F.SilkS))
    (fp_text value HV (at 0 -0.5) (layer F.Fab))
    (fp_text user "HV GND" (at 0 19.304) (layer F.SilkS))
    (pad 1 thru_hole circle (at 30 0) (size 3.302 3.302) (drill 1.6764) (layers *.Cu *.Mask)
      (net 22 "Net-(J102-Pad1)"))
    (pad "" np_thru_hole circle (at 0 -6) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 6) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 16) (size 3.302 3.302) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A373DF8)
    (at 187.1345 66.167 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C103 (at 1.1938 2.3241 270) (layer F.SilkS))
    (fp_text value 0.1µF (at -2.0066 -0.0127 360) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A373E6C)
    (at 157.9245 82.7405)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C104 (at 1.25 -2.56) (layer F.SilkS))
    (fp_text value 2.2µF (at 6.0071 -0.1905) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C104-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A373E76)
    (at 159.7025 70.4215 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C105 (at 1.5621 2.6289 270) (layer F.SilkS))
    (fp_text value 0.1µF (at -2.2479 0.1397 360) (layer F.Fab))
    (fp_text user %R (at 1.25 0 450) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A373E1A)
    (at 187.071 91.948 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C106 (at 1.3716 2.3114 270) (layer F.SilkS))
    (fp_text value 0.1µF (at -2.032 0.0762 360) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A373E1E)
    (at 187.071 79.0575 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C107 (at 1.3589 2.2606 270) (layer F.SilkS))
    (fp_text value 0.1µF (at -1.8923 -0.0254 360) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 142.1892 90.0176 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C108 (at 1.25 -2.56 90) (layer F.SilkS))
    (fp_text value 2.2µF (at 1.25 2.56 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C108-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A373E30)
    (at 184.023 106.8705 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C109 (at 1.25 -2.56 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 4.8641 0.3302 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A373DE5)
    (at 178.943 64.262 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C110 (at 1.27 2.3114 270) (layer F.SilkS))
    (fp_text value 0.47µF (at -1.9304 1.3462 360) (layer F.Fab))
    (fp_text user %R (at 1.25 0 450) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C110-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5A373E88)
    (at 125.857 121.539 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J103 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Debug-2 (at 2.8194 4.5974 360) (layer F.SilkS))
    (fp_text user %R (at 0 5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(C108-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J103-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J103-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J103-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A373E09)
    (at 190.627 73.7235 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U102 (at 3.9243 0.6858 90) (layer F.SilkS))
    (fp_text value 74LS14 (at 4.0259 13.1318 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C110-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(U102-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(U102-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(U102-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(U102-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(U102-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A373E3C)
    (at 192.024 119.253 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C102 (at -3.429 0.2032 360) (layer F.SilkS))
    (fp_text value 47µF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 173.2788 84.4296 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R125 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value 0 (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R125-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 80.01 (width 0.3) (layer Cmts.User)
    (gr_text "3.1500 in" (at 235.9952 100.965 90) (layer Cmts.User))
    (feature1 (pts (xy 198.9836 60.96) (xy 237.3452 60.96)))
    (feature2 (pts (xy 198.9836 140.97) (xy 237.3452 140.97)))
    (crossbar (pts (xy 234.6452 140.97) (xy 234.6452 60.96)))
    (arrow1a (pts (xy 234.6452 60.96) (xy 235.231621 62.086504)))
    (arrow1b (pts (xy 234.6452 60.96) (xy 234.058779 62.086504)))
    (arrow2a (pts (xy 234.6452 140.97) (xy 235.231621 139.843496)))
    (arrow2b (pts (xy 234.6452 140.97) (xy 234.058779 139.843496)))
  )
  (dimension 145.034 (width 0.3) (layer Cmts.User)
    (gr_text "5.7100 in" (at 137.287 55.6476) (layer Cmts.User))
    (feature1 (pts (xy 64.77 60.96) (xy 64.77 54.2976)))
    (feature2 (pts (xy 209.804 60.96) (xy 209.804 54.2976)))
    (crossbar (pts (xy 209.804 56.9976) (xy 64.77 56.9976)))
    (arrow1a (pts (xy 64.77 56.9976) (xy 65.896504 56.411179)))
    (arrow1b (pts (xy 64.77 56.9976) (xy 65.896504 57.584021)))
    (arrow2a (pts (xy 209.804 56.9976) (xy 208.677496 56.411179)))
    (arrow2b (pts (xy 209.804 56.9976) (xy 208.677496 57.584021)))
  )
  (gr_text "IBX ][ HV Board Rev. 2\nMade up in J207" (at 97.663 121.92) (layer F.SilkS))
  (gr_line (start 64.77 130.81) (end 110.109 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.77 60.96) (end 64.77 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.804 60.96) (end 64.77 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.109 130.81) (end 134.239 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.804 130.81) (end 209.804 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.279 130.81) (end 209.804 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.279 139.7) (end 200.279 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.009 140.97) (end 200.279 139.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.509 140.97) (end 199.009 140.97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.239 139.7) (end 135.509 140.97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.239 130.81) (end 134.239 139.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 69.85 (width 0.3) (layer Cmts.User)
    (gr_text "2.7500 in" (at 228.299 95.885 270) (layer Cmts.User))
    (feature1 (pts (xy 200.279 130.81) (xy 229.649 130.81)))
    (feature2 (pts (xy 200.279 60.96) (xy 229.649 60.96)))
    (crossbar (pts (xy 226.949 60.96) (xy 226.949 130.81)))
    (arrow1a (pts (xy 226.949 130.81) (xy 226.362579 129.683496)))
    (arrow1b (pts (xy 226.949 130.81) (xy 227.535421 129.683496)))
    (arrow2a (pts (xy 226.949 60.96) (xy 226.362579 62.086504)))
    (arrow2b (pts (xy 226.949 60.96) (xy 227.535421 62.086504)))
  )
  (dimension 9.525 (width 0.3) (layer Cmts.User)
    (gr_text "0.3750 in" (at 205.0415 148.67) (layer Cmts.User))
    (feature1 (pts (xy 209.804 130.81) (xy 209.804 150.02)))
    (feature2 (pts (xy 200.279 130.81) (xy 200.279 150.02)))
    (crossbar (pts (xy 200.279 147.32) (xy 209.804 147.32)))
    (arrow1a (pts (xy 209.804 147.32) (xy 208.677496 147.906421)))
    (arrow1b (pts (xy 209.804 147.32) (xy 208.677496 146.733579)))
    (arrow2a (pts (xy 200.279 147.32) (xy 201.405504 147.906421)))
    (arrow2b (pts (xy 200.279 147.32) (xy 201.405504 146.733579)))
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.423 130.556) (xy 200.025 130.556) (xy 200.025 138.938) (xy 196.723 138.938) (xy 196.723 130.556)
        (xy 72.39 130.556) (xy 72.39 85.979) (xy 84.582 85.979) (xy 84.582 119.126) (xy 108.204 119.126)
        (xy 108.204 84.455) (xy 129.794 84.455) (xy 129.794 61.341) (xy 209.423 61.341)
      )
    )
  )
)
