(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J0-Pad1)")
  (net 2 "Net-(J0-Pad2)")
  (net 3 "Net-(J0-Pad3)")
  (net 4 "Net-(J0-Pad4)")
  (net 5 "Net-(J0-Pad5)")
  (net 6 "Net-(J0-Pad6)")
  (net 7 "Net-(J0-Pad7)")
  (net 8 "Net-(J0-Pad8)")
  (net 9 "Net-(J0-Pad9)")
  (net 10 "Net-(J0-Pad10)")
  (net 11 "Net-(J0-Pad11)")
  (net 12 "Net-(J0-Pad12)")
  (footprint "Millmax_PinConnectors:12Pin_Recepticle" (layer "F.Cu")
    (tedit 0)
    (at 135.636 73.152 -90)
    (property "Sheetfile" "PST_Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 2.54 -2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x12" (at 2.54 2.54 -90 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 5.08 -90 unlocked) (layer "F.Fab") hide)
    (fp_circle (center 2.54 -5.08) (end 5.08 -7.62) (layer "Edge.Cuts") (width 0.12) (fill none))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.5 2) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.2)
      (chamfer_ratio 0.2) (chamfer top_left)
      (net 1 "Net-(J0-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 2.54 0 270) (size 2 2.5) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(J0-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 5.08 0 270) (size 2 2.5) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(J0-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole roundrect (at 7.62 -2.54 180) (size 2 2.5) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.2)
      (net 4 "Net-(J0-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole roundrect (at 7.62 -5.08 180) (size 2 2.5) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.2)
      (net 5 "Net-(J0-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole roundrect (at 7.62 -7.62 270) (size 2.5 2) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.25)
      (net 6 "Net-(J0-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole roundrect (at 5.08 -10.16 270) (size 2 2.5) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.2)
      (net 7 "Net-(J0-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole roundrect (at 2.54 -10.16 270) (size 2 2.5) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.2)
      (net 8 "Net-(J0-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole roundrect (at 0 -10.16) (size 2.5 2) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J0-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole roundrect (at -2.54 -7.62 270) (size 2.5 2) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.25)
      (net 10 "Net-(J0-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole roundrect (at -2.54 -5.08 180) (size 2 2.5) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.2)
      (net 11 "Net-(J0-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole roundrect (at -2.54 -2.54 180) (size 2 2.5) (drill 1.7) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu") (roundrect_rratio 0.2)
      (net 12 "Net-(J0-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (model "C:/Users/dan.jones/Documents/KiCad/6.0/3dmodels/0666-0-15_pinX12.STEP"
      (offset (xyz 0 0 -3.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Imports:MOLEX_530471210" (layer "B.Cu")
    (tedit 63881166)
    (at 134.095 85.402 180)
    (property "Sheetfile" "PST_Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J0" (at -13.075 3.635) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x12" (at -6.725 -4.365) (layer "B.Fab") hide)
    (fp_text user "PTH D0.5 +/- 0.05" (at -16.25 -7) (layer "B.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 1 "Net-(J0-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -1.25 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 2 "Net-(J0-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -2.5 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 3 "Net-(J0-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -3.75 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 4 "Net-(J0-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at -5 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 5 "Net-(J0-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at -6.25 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 6 "Net-(J0-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at -7.5 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 7 "Net-(J0-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at -8.75 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 8 "Net-(J0-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at -10 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 9 "Net-(J0-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at -11.25 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 10 "Net-(J0-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle locked (at -12.5 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 11 "Net-(J0-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle locked (at -13.75 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu)
      (net 12 "Net-(J0-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (model "C:/Users/dan.jones/Documents/KiCad/6.0/3dmodels/530471210--3DModel-STEP-231308.STEP"
      (offset (xyz -6.87 -0.45 3.25))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_arc (start 130.041418 75.81) (mid 140.595 65.256418) (end 151.148582 75.81) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 130.048 87.884) (end 130.041418 75.81) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 151.13 87.884) (mid 150.906815 88.422815) (end 150.368 88.646) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150.368 88.646) (end 130.81 88.646) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 151.148582 75.81) (end 151.13 87.884) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 130.81 88.646) (mid 130.271185 88.422815) (end 130.048 87.884) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Moxtek\nPST Connector" (at 140.462 67.564) (layer "B.SilkS"))
  (gr_text "V0.1" (at 140.716 83.312) (layer "B.SilkS"))
  (zone (net 8) (net_name "Net-(J0-Pad8)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 3))
    (polygon
      (pts
        (xy 151.13 88.646)
        (xy 130.048 88.646)
        (xy 130.048 65.024)
        (xy 151.13 65.024)
      )
    )
  )
)
