(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.5318)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1999)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.9906)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1999)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(IC2-RF-IN)")
	(net 2 "Net-(U1-LO)")
	(net 3 "Net-(IC2-RF-OUT_&_DC)")
	(net 4 "/RF_IN")
	(net 5 "Net-(IC3-OUT)")
	(net 6 "/RF_OUT")
	(net 7 "/ESP")
	(net 8 "GND")
	(net 9 "/5V")
	(net 10 "Net-(IC1-D4{slash}LE0)")
	(net 11 "/LE")
	(net 12 "/SI")
	(net 13 "/CLK")
	(net 14 "Net-(IC2-BIAS)")
	(net 15 "unconnected-(IC2-NC_5-Pad8)")
	(net 16 "unconnected-(IC2-NC_3-Pad4)")
	(net 17 "unconnected-(IC2-NC_1-Pad2)")
	(net 18 "unconnected-(IC2-NC_2-Pad3)")
	(net 19 "unconnected-(IC2-NC_4-Pad5)")
	(net 20 "/Tune")
	(net 21 "unconnected-(IC3-N.C.-Pad1)")
	(net 22 "Net-(J2-In)")
	(net 23 "Net-(C10-Pad1)")
	(net 24 "Net-(U1-IF)")
	(net 25 "unconnected-(IC5-OUT_2-Pad2)")
	(net 26 "Net-(IC1-S{slash}~{P})")
	(net 27 "/FLL")
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 115.09 93.13 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 3.61 1.66 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 3.45 -0.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 142.6 73.07 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0.29 -2.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0.15 1.88 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.05x1.20mm_HandSolder"
		(layer "F.Cu")
		(at 124.41 72.1985 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L1"
			(at 0.1085 -1.74 180)
			(layer "F.SilkS")
		)
		(property "Value" "390n"
			(at 3.6685 0.259 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0 90)
			(size 1.05 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 1 "Net-(IC2-RF-IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.15 0 90)
			(size 1.05 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.238095)
			(net 14 "Net-(IC2-BIAS)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 146.52 61.66)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.15 -2.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.23p"
			(at 1.92 2.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/FLL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 129.731 64.7685 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -0.9385 3.311 180)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at -2.9785 3.101 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(U1-LO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(IC2-RF-OUT_&_DC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 138.01 87.02)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 1.1 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x08_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 146.56 68.51 -90)
		(descr "Through hole straight pin header, 1x08, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x08 1.00mm single row")
		(property "Reference" "J3"
			(at 0 -1.61 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 5.93 -3.05 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/FLL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Tune")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 4 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/LE")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 5 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/CLK")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 6 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SI")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 7 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/ESP")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x08_P1.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 118.28 55.31)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 3.34 -0.58 0)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 3.59 1.12 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 116.62 77.085)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0.82 -2.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.69k"
			(at -0.14 2.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ADP3338AKCZ-5-R7:SOT230P700X180-4N"
		(layer "F.Cu")
		(at 140.35 80.24 180)
		(descr "SOT230P700X180-4N")
		(tags "Integrated Circuit")
		(property "Reference" "IC5"
			(at 3.91 4.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADP3338AKCZ-5-R7"
			(at -4.8006 -3.556 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Analog Devices ADP3338AKCZ-5-R7, LDO Voltage Regulator, 1A, 5 V +/-1.6%, 2.7  8 Vin, 3-Pin SOT-223"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "584-ADP3338AKCZ-5-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/ADP3338AKCZ-5-R7?qs=WIvQP4zGangs6Tv%252BSE3hsA%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ADP3338AKCZ-5-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 3.9 4.17 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.2004 -2.3114 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.2004 0 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(IC5-OUT_2-Pad2)")
			(pinfunction "OUT_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.2004 2.3114 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/5V")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 3.2004 0 180)
			(size 1.6256 3.175)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 115.09 83.09 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 3.43 1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10p"
			(at 3.35 -0.54 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 145.57 54.1 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 2.97 -0.03 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.69k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "/FLL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(U1-IF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 130.7575 101.65)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at -0.205 1.865 0)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at -0.0875 3.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "/RF_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(IC3-OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 139.54 54.11 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 2.94 0.12 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.69k"
			(at -2.47 2.04 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 7 "/ESP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(U1-IF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "QFN50P500X500X90:QFN50P500X500X90-33N-D"
		(layer "F.Cu")
		(at 128.47 92 90)
		(descr "32-lead 5 × 5 × 0.85 mm QFN")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0.090715 4.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "PE44820B-X"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.psemi.com/pdf/datasheets/pe44820ds.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Phase Detectors/Shifters 8-bit 1.7-2.2 GHz RF Digital Phase Shifter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "81-PE44820B-X"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/pSemi/PE44820B-X?qs=Cb2nCFKsA8prCrkfl5FDIQ%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Peregrine Semiconductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PE44820B-X"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.005 4.27 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 -1.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "OPT")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.45 -1.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.45 -0.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pinfunction "S/~{P}")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.45 -0.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.45 0.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.45 0.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_3")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -2.45 1.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/RF_IN")
			(pinfunction "RF1")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -2.45 1.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.75 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_5")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -1.25 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_6")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -0.75 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_7")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -0.25 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_8")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.25 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_9")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.75 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_10")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 1.25 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_11")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 1.75 2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_12")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2.45 1.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_13")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 2.45 1.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/RF_OUT")
			(pinfunction "RF2")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 2.45 0.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_14")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 2.45 0.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "VSS_EXT")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 2.45 -0.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_15")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 2.45 -0.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LE")
			(pinfunction "LE")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 2.45 -1.25 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/CLK")
			(pinfunction "CLK")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 2.45 -1.75 180)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/SI")
			(pinfunction "SI")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 1.75 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC1-D4{slash}LE0)")
			(pinfunction "D7/SDO2")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 1.25 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC1-D4{slash}LE0)")
			(pinfunction "D6/SDO1")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 0.75 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC1-D4{slash}LE0)")
			(pinfunction "D5/CLK0")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 0.25 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC1-D4{slash}LE0)")
			(pinfunction "D4/LE0")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -0.25 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "D3/A3")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -0.75 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "D2/A2")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -1.25 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "D1/A1")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at -1.75 -2.45 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "D0/A0")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 0 0 90)
			(size 3.65 3.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_16")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "PE44820B-X.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 118.28 60.45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 3.45 -1.06 0)
			(layer "F.SilkS")
		)
		(property "Value" "10p"
			(at 3.59 0.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 129.74 40.63 -90)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J2"
			(at -1.5 7 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial_Small"
			(at -5.89 -9.14 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0 270)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(J2-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 270)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 270)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 270)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 270)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 270)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 270)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 270)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 270)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 270)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 270)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 113.02 50.4 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 4.17 0.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 4.09 -0.58 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 113.03 55.33 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 3.84 1.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 4.18 -0.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 118.29 50.39)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 3.46 -0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 3.4 1.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 125.835 77.13)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L2"
			(at -0.746 -2.0985 0)
			(layer "F.SilkS")
		)
		(property "Value" "18n"
			(at 0.034 1.8515 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 23 "Net-(C10-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "Net-(IC2-RF-IN)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 140.49 61.67)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -3.4 -0.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.5u"
			(at -3.34 0.91 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/ESP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MAX2623EUA:SOP65P490X110-9N"
		(layer "F.Cu")
		(at 145.805 93.062 -90)
		(descr "8 µMAX 1")
		(tags "Integrated Circuit")
		(property "Reference" "IC3"
			(at 0.008 -3.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "MAX2623EUA+"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX2622-MAX2624.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Voltage Controlled Oscillator 950MHz, 8-Pin uMAX"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "700-MAX2623EUA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices-Maxim-Integrated/MAX2623EUA%2b?qs=1THa7WoU59G3eRvnxYOLFg%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "MAX2623EUA+"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.935 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.212 -0.975)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(IC3-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -2.212 -0.325)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "/Tune")
			(pinfunction "TUNE")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.212 0.325)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.212 0.975)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pinfunction "~{SHDN}")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.212 0.975)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pinfunction "VCC_1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.212 0.325)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pinfunction "VCC_2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.212 -0.325)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(IC3-OUT)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.212 -0.975)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 1.88 2.515)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "MAX2623EUA+.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LNA_PLL:QFN66P300X300X89-9N"
		(layer "F.Cu")
		(at 130.041 71.3485 90)
		(descr "DQ849")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at 0 3.719 90)
			(layer "F.SilkS")
		)
		(property "Value" "PMA-5456+"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PMA-5456+.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RF Amplifier SMT Low Noise Amplifier, 50 - 6000 MHz, 50 ohms"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.894"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "139-PMA-5456"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mini-Circuits/PMA-5456%2b?qs=xZ%2FP%252Ba9zWqZjLgmszR6SXg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Mini-Circuits"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PMA-5456+"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 3.719 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.45 -0.33 180)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(IC2-RF-IN)")
			(pinfunction "RF-IN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.45 0.33 180)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(IC2-NC_1-Pad2)")
			(pinfunction "NC_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.33 1.45 90)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(IC2-NC_2-Pad3)")
			(pinfunction "NC_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.33 1.45 90)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(IC2-NC_3-Pad4)")
			(pinfunction "NC_3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.45 0.33 180)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(IC2-NC_4-Pad5)")
			(pinfunction "NC_4")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.45 -0.33 180)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(IC2-RF-OUT_&_DC)")
			(pinfunction "RF-OUT_&_DC")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.33 -1.45 90)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(IC2-BIAS)")
			(pinfunction "BIAS")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.33 -1.45 90)
			(size 0.35 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(IC2-NC_5-Pad8)")
			(pinfunction "NC_5")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 1.702 1.702)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "PMA-5456+.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 129.72 82.5275 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "/RF_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "Net-(IC2-RF-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 113.03 60.4 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 3.82 1.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "10p"
			(at 3.79 -0.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.23 93.13)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 3.23 -1.19 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 3.24 0.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 115.08 88.03 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 3.64 1.78 0)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 3.72 -0.13 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints_mix:TTT166_MNC"
		(layer "F.Cu")
		(at 129.6775 53.0979 90)
		(tags "SYM-63LH+ ")
		(property "Reference" "U1"
			(at 0 0.0762 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SYM-63LH+"
			(at 0 0.0762 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SYM-63LH+"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TTT166_MNC")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0762 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 5.969 0.0762 90)
			(size 1.778 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(J2-In)")
			(pinfunction "F")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -5.969 0.0762 90)
			(size 1.778 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(U1-LO)")
			(pinfunction "LO")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 4.445 90)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U1-IF)")
			(pinfunction "IF")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 -4.318 90)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(pad "5" smd rect
			(at -4.445 4.445 90)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(pad "6" smd rect
			(at 4.445 4.445 90)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.23 88.03)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 3.06 -1.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at 3.52 0.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.25 83.1)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 3.37 -1.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "10p"
			(at 3.46 0.59 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 116.645 65.695)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L4"
			(at 1.825 -1.775 0)
			(layer "F.SilkS")
		)
		(property "Value" "18n"
			(at 1.135 2.075 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "PLL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 26 "Net-(IC1-S{slash}~{P})")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "Net-(IC2-RF-OUT_&_DC)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 120.475534 106.074466)
		(end 148.004466 106.074466)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148.004466 35.425534)
		(mid 151.54 36.89)
		(end 153.004466 40.425534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.004466 101.0745)
		(end 153.004466 40.425534)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 108.905534 106.074466)
		(mid 105.37 104.61)
		(end 103.905534 101.074466)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 153.004466 101.074466)
		(mid 151.54 104.61)
		(end 148.004466 106.074466)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.905535 101.074466)
		(end 103.905535 40.43)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.004466 35.425535)
		(end 120.48 35.425535)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.48 35.43)
		(end 108.91 35.43)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.91 40.43)
		(mid 105.374466 36.894466)
		(end 108.91 35.43)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120.475534 106.074466)
		(end 108.905534 106.074466)
		(layer "Edge.Cuts")
	)
	(zone
		(net 8)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.75)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 155.33 33.63) (xy 155.46 33.76) (xy 155.46 109.36) (xy 102.16 109.36) (xy 101.25 108.45) (xy 101.25 33.63)
			)
		)
	)
	(embedded_fonts no)
)
