(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(J101-Pad3)")
  (net 3 "Net-(J101-Pad4)")
  (net 4 "Net-(J101-Pad5)")
  (net 5 "Net-(J101-Pad6)")
  (net 6 "unconnected-(J102-Pad1)")
  (net 7 "unconnected-(J102-Pad4)")
  (net 8 "unconnected-(J102-Pad6)")
  (net 9 "unconnected-(J102-Pad8)")
  (footprint "Connector_PCBEdge:DB9F_CI_REV" locked (layer "F.Cu")
    (tedit 0)
    (at 149.19 98.8565 -90)
    (descr "Connecteur DB9 femelle encarte")
    (tags "CONN DB9")
    (property "Sheetfile" "FTDI_Adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J102" (at 0 -9.144 90) (layer "F.SilkS"))
    (fp_text value "DB9_Male" (at 0 -3.048 90) (layer "F.Fab"))
    (pad "1" connect rect locked (at 5.588 2.54 270) (size 1.778 5.08) (layers "F.Cu" "F.Mask")
      (net 6 "unconnected-(J102-Pad1)") (pinfunction "1") (pintype "passive+no_connect"))
    (pad "2" connect rect locked (at 2.794 2.54 270) (size 1.778 5.08) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(J101-Pad4)") (pinfunction "2") (pintype "passive"))
    (pad "3" connect rect locked (at 0 2.54 270) (size 1.778 5.08) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(J101-Pad5)") (pinfunction "3") (pintype "passive"))
    (pad "4" connect rect locked (at -2.794 2.54 270) (size 1.778 5.08) (layers "F.Cu" "F.Mask")
      (net 7 "unconnected-(J102-Pad4)") (pinfunction "4") (pintype "passive+no_connect"))
    (pad "5" connect rect locked (at -5.588 2.54 270) (size 1.778 5.08) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" connect rect locked (at 4.191 2.54 270) (size 1.778 5.08) (layers "B.Cu" "B.Mask")
      (net 8 "unconnected-(J102-Pad6)") (pinfunction "6") (pintype "passive+no_connect"))
    (pad "7" connect rect locked (at 1.397 2.54 270) (size 1.778 5.08) (layers "B.Cu" "B.Mask")
      (net 5 "Net-(J101-Pad6)") (pinfunction "7") (pintype "passive"))
    (pad "8" connect rect locked (at -1.397 2.54 270) (size 1.778 5.08) (layers "B.Cu" "B.Mask")
      (net 9 "unconnected-(J102-Pad8)") (pinfunction "8") (pintype "passive+no_connect"))
    (pad "9" connect rect locked (at -4.191 2.54 270) (size 1.778 5.08) (layers "B.Cu" "B.Mask")
      (net 2 "Net-(J101-Pad3)") (pinfunction "9") (pintype "passive"))
    (model "Connect.3dshapes/DB9F_CI.wrl"
      (offset (xyz 0 0 -0.8381999874))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal" locked (layer "B.Cu")
    (tedit 59FED5CB)
    (at 141.75 92.48 180)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "FTDI_Adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J101" (at 4.385 2.27) (layer "B.SilkS"))
    (fp_text value "Conn_01x06" (at 4.385 -14.97) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -6.35 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 -2.54 180) (size 2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -5.08 180) (size 2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J101-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 -7.62 180) (size 2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J101-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -10.16 180) (size 2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J101-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 -12.7 180) (size 2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J101-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line locked (start 139.91 107.68) (end 149.51 107.68) (layer "Edge.Cuts") (width 0.15))
  (gr_line locked (start 149.51 90.18) (end 149.51 107.68) (layer "Edge.Cuts") (width 0.15))
  (gr_line locked (start 139.91 90.18) (end 149.51 90.18) (layer "Edge.Cuts") (width 0.15))
  (gr_line locked (start 139.91 107.68) (end 139.91 90.18) (layer "Edge.Cuts") (width 0.15))
  (gr_text "FTDI Adapter" (at 143.45 98.83 90) (layer "B.SilkS"))
  (gr_text "Rev 3.0" (at 145.71 106.66) (layer "B.SilkS"))
  (gr_text "GND" (at 144.48 90.93) (layer "B.SilkS"))
  (gr_text "Rev 3.0" (at 145.37 106.61) (layer "F.SilkS"))
  (gr_text "FTDI Adapter" (at 143.42 99.3 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 144.46 90.98) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (name "Plane") (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149 107.3)
        (xy 140.28 107.3)
        (xy 140.28 90.42)
        (xy 149 90.42)
      )
    )
  )
)
