<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15" y2="0" width="0" layer="20"/>
<wire x1="15" y1="0" x2="15" y2="15" width="0" layer="20"/>
<wire x1="15" y1="15" x2="0" y2="15" width="0" layer="20"/>
<wire x1="0" y1="15" x2="0" y2="0" width="0" layer="20"/>
<text>T</text>
<text>COM</text>
<text>COM</text>
</plain>
<libraries>
<library name="dword1511-optoelectronics">
<description>LEDs, PDs, etc.</description>
<packages>
<package name="XPE-TIGHT">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="dword1511-optoelectronics" package="XPE-TIGHT" value="XPEBWT-TIGHT"/>
<element name="D2" library="dword1511-optoelectronics" package="XPE-TIGHT" value="XPEBWT-TIGHT"/>
<element name="D3" library="dword1511-optoelectronics" package="XPE-TIGHT" value="XPEBWT-TIGHT"/>
<element name="D4" library="dword1511-optoelectronics" package="XPE-TIGHT" value="XPEBWT-TIGHT"/>
<element name="TP4" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="COM">
<contactref element="D1" pad="K"/>
<contactref element="TP4" pad="TP"/>
<contactref element="TP5" pad="TP"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="D4" pad="K"/>
</signal>
<signal name="T">
<contactref element="D1" pad="T"/>
<contactref element="D4" pad="T"/>
<contactref element="D3" pad="T"/>
<contactref element="D2" pad="T"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="A"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="N$7">
<contactref element="D2" pad="A"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="N$8">
<contactref element="D3" pad="A"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$9">
<contactref element="D4" pad="A"/>
<contactref element="TP2" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
