(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 124)
    (zones 0)
    (modules 5)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /UP)
  (net 2 /LEFT)
  (net 3 /1P)
  (net 4 /3P)
  (net 5 /START)
  (net 6 /2K)
  (net 7 "Net-(CN1-Pad9)")
  (net 8 /VCC)
  (net 9 /2P)
  (net 10 /RIGHT)
  (net 11 /1K)
  (net 12 /SELECT)
  (net 13 /3K)
  (net 14 /GND)
  (net 15 /4K)
  (net 16 /4P)
  (net 17 /HOME)
  (net 18 /DOWN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /1K)
    (add_net /1P)
    (add_net /2K)
    (add_net /2P)
    (add_net /3K)
    (add_net /3P)
    (add_net /4K)
    (add_net /4P)
    (add_net /DOWN)
    (add_net /GND)
    (add_net /HOME)
    (add_net /LEFT)
    (add_net /RIGHT)
    (add_net /SELECT)
    (add_net /START)
    (add_net /UP)
    (add_net /VCC)
    (add_net "Net-(CN1-Pad9)")
  )
  (module neoextend:ngface (layer F.Cu) (tedit 0)
    (at 157.48 91.44 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module neoextend:ngface (layer F.Cu) (tedit 0)
    (at 123.19 91.44 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 152.4 83.82 270)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference CN3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value "Out 2x10" (at 1.27 25.19 90) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VCC))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VCC))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /4K))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /3K))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /2K))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /1K))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /4P))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3P))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /2P))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /1P))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /START))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /HOME))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SELECT))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /LEFT))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /RIGHT))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DOWN))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /UP))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 152.4 96.52 270)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference CN2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value "In 2x10" (at 1.27 25.19 90) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VCC))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VCC))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /4K))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /3K))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /2K))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /1K))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /4P))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3P))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /2P))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /1P))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /START))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /HOME))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SELECT))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /LEFT))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /RIGHT))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DOWN))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /UP))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Dsub:DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm (layer F.Cu) (tedit 59FEDEE2)
    (at 130.81 71.12 180)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm")
    (fp_text reference CN1 (at -9.695 -3.7) (layer F.SilkS))
    (fp_text value DB15_Female (at -9.695 15.85) (layer F.Fab))
    (fp_text user %R (at -9.695 11.265) (layer F.Fab))
    (pad 0 thru_hole circle (at 6.955 0.3 180) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at -26.345 0.3 180) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -18.005 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 /UP))
    (pad 14 thru_hole circle (at -15.235 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 /LEFT))
    (pad 13 thru_hole circle (at -12.465 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 /1P))
    (pad 12 thru_hole circle (at -9.695 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3P))
    (pad 11 thru_hole circle (at -6.925 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 /START))
    (pad 10 thru_hole circle (at -4.155 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 /2K))
    (pad 9 thru_hole circle (at -1.385 2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(CN1-Pad9)"))
    (pad 8 thru_hole circle (at -19.39 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VCC))
    (pad 7 thru_hole circle (at -16.62 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DOWN))
    (pad 6 thru_hole circle (at -13.85 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 /RIGHT))
    (pad 5 thru_hole circle (at -11.08 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 /2P))
    (pad 4 thru_hole circle (at -8.31 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 /1K))
    (pad 3 thru_hole circle (at -5.54 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SELECT))
    (pad 2 thru_hole circle (at -2.77 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 /3K))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text H (at 147.32 88.265 90) (layer B.SilkS))
  (gr_text D (at 152.4 88.265 90) (layer B.SilkS))
  (gr_text L (at 149.86 88.265 90) (layer B.SilkS))
  (gr_text 1P (at 144.78 88.265 90) (layer B.SilkS))
  (gr_text 3P (at 142.24 88.265 90) (layer B.SilkS))
  (gr_text GND (at 139.7 88.265 90) (layer B.SilkS))
  (gr_text 2K (at 137.16 88.265 90) (layer B.SilkS))
  (gr_text 4K (at 134.62 88.265 90) (layer B.SilkS))
  (gr_text GND (at 132.08 88.265 90) (layer B.SilkS))
  (gr_text VCC (at 129.54 88.265 90) (layer B.SilkS))
  (gr_text VCC (at 129.54 81.915 90) (layer B.SilkS))
  (gr_text GND (at 132.08 81.915 90) (layer B.SilkS))
  (gr_text 3K (at 134.62 81.915 90) (layer B.SilkS))
  (gr_text 1K (at 137.16 81.915 90) (layer B.SilkS))
  (gr_text 4P (at 139.7 81.915 90) (layer B.SilkS))
  (gr_text 2P (at 142.24 81.915 90) (layer B.SilkS))
  (gr_text Start (at 144.78 80.01 90) (layer B.SilkS))
  (gr_text Select (at 147.32 79.375 90) (layer B.SilkS))
  (gr_text R (at 149.86 81.28 90) (layer B.SilkS))
  (gr_text U (at 152.4 81.28 90) (layer B.SilkS))
  (gr_text "↓↘→ ↓↘→ K" (at 155.575 102.87) (layer F.SilkS))
  (gr_text "BRP NEOExtend DB15" (at 129.54 76.2) (layer F.SilkS))
  (gr_line (start 161.29 63.5) (end 161.29 104.14) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 63.5) (end 161.29 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 104.14) (end 119.38 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.29 104.14) (end 119.38 104.14) (layer Edge.Cuts) (width 0.1))
  (zone (net 8) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 104.14) (xy 119.38 104.14) (xy 119.38 63.5) (xy 161.29 63.5)
      )
    )
  )
  (zone (net 14) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 104.14) (xy 119.38 104.14) (xy 119.38 63.5) (xy 161.29 63.5)
      )
    )
  )
)
