(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 49)
    (zones 0)
    (modules 8)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.5)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 11 11)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 68 90.55)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 /DC+IN)
  (net 2 /DC-)
  (net 3 /DC+PRO)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 1.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DC+IN)
    (add_net /DC+PRO)
    (add_net /DC-)
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5E0098B7)
    (at 59.5 98)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.498) (layer F.SilkS) hide)
    (fp_text value 105-1102-001 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 /DC-))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5E0098C2)
    (at 77 84)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference J4 (at 0 -2.498) (layer F.SilkS) hide)
    (fp_text value 105-1102-001 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 /DC-))
  )
  (module my-footprints:6mmFpad-SMD (layer F.Cu) (tedit 5F38567B)
    (at 68 90.5)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 105-1102-001 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 11 11) (layers F.Cu F.Paste F.Mask)
      (net 1 /DC+IN))
  )
  (module my-footprints:6mmBpad-SMD (layer F.Cu) (tedit 5F38569C)
    (at 68 90.5)
    (fp_text reference J3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 105-1102-001 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 11 11) (layers B.Cu B.Paste B.Mask)
      (net 3 /DC+PRO))
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 78 90.55 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SSM3J355R,LF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC-))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /DC+PRO))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /DC+IN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 67.95 100 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value SSM3J355R,LF (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /DC+IN))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /DC+PRO))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC-))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 58.5 90.55)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SSM3J355R,LF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC-))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /DC+PRO))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /DC+IN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 68 81 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value SSM3J355R,LF (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /DC+IN))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /DC+PRO))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC-))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text DC- (at 73.5 84.5) (layer F.SilkS))
  (gr_text DC- (at 63 98.5) (layer F.SilkS))
  (gr_circle (center 68 90.5) (end 83.5 90.5) (layer Edge.Cuts) (width 0.15))
  (gr_text +IN (at 73 95) (layer F.SilkS))
  (gr_text +OUT (at 62 86.5) (layer B.SilkS))
  (zone (net 2) (net_name /DC-) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.5 76) (xy 81 80.5) (xy 83.5 86) (xy 84 97.5) (xy 76.5 105)
        (xy 66.5 107) (xy 60.5 105) (xy 56 101.5) (xy 52 93.5) (xy 52 88.5)
        (xy 54 83) (xy 58 78.5) (xy 62.5 76) (xy 67.5 74.5)
      )
    )
  )
  (zone (net 2) (net_name /DC-) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 75.5) (xy 79.5 79) (xy 84 88) (xy 82.5 97) (xy 78.5 102.5)
        (xy 71.5 106) (xy 64 106) (xy 57.5 102.5) (xy 53 95.5) (xy 52.5 87.5)
        (xy 54.5 82.5) (xy 59 77.5) (xy 67.5 74.5)
      )
    )
  )
)
