(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 129)
    (no_connects 0)
    (area 167.564999 54.534999 212.165001 119.455001)
    (thickness 1.6)
    (drawings 10)
    (tracks 113)
    (zones 0)
    (modules 97)
    (nets 43)
  )
  (page A4)
  (title_block
    (date 2018-03-17)
    (rev A)
    (company GeRoGo)
  )
  (layers
    (0 F.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory drill/))
  )
  (net 0 "")
  (net 1 /LIVE_+15V_Washer)
  (net 2 /LIVE_0V_Washer)
  (net 3 /+5V_Instr)
  (net 4 /0V_Instr)
  (net 5 /SDA_Washer)
  (net 6 /SDA_Instr_Rx)
  (net 7 /SDA_Instr_Tx)
  (net 8 /SCL_Instr_Rx)
  (net 9 /SCL_Instr_Tx)
  (net 10 "Net-(Q1-Pad2)")
  (net 11 "Net-(Q1-Pad1)")
  (net 12 "Net-(Q2-Pad2)")
  (net 13 "Net-(Q2-Pad1)")
  (net 14 "Net-(Q3-Pad2)")
  (net 15 "Net-(Q3-Pad1)")
  (net 16 "Net-(Q4-Pad2)")
  (net 17 "Net-(Q4-Pad1)")
  (net 18 "Net-(R5-Pad1)")
  (net 19 "Net-(R6-Pad1)")
  (net 20 "Net-(R7-Pad2)")
  (net 21 "Net-(R8-Pad2)")
  (net 22 "Net-(U1-Pad1)")
  (net 23 "Net-(U1-Pad7)")
  (net 24 "Net-(U1-Pad4)")
  (net 25 "Net-(U2-Pad1)")
  (net 26 "Net-(U2-Pad7)")
  (net 27 "Net-(U2-Pad4)")
  (net 28 "Net-(U3-Pad1)")
  (net 29 "Net-(U3-Pad7)")
  (net 30 "Net-(U3-Pad4)")
  (net 31 "Net-(U4-Pad1)")
  (net 32 "Net-(U4-Pad7)")
  (net 33 "Net-(U4-Pad4)")
  (net 34 "Net-(J1-Pad3)")
  (net 35 "Net-(J3-Pad1)")
  (net 36 "Net-(J3-Pad3)")
  (net 37 "Net-(J4-Pad1)")
  (net 38 "Net-(J4-Pad3)")
  (net 39 "Net-(J5-Pad1)")
  (net 40 "Net-(J6-Pad1)")
  (net 41 "Net-(J9-Pad1)")
  (net 42 "Net-(J10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V_Instr)
    (add_net /0V_Instr)
    (add_net /LIVE_+15V_Washer)
    (add_net /LIVE_0V_Washer)
    (add_net /SCL_Instr_Rx)
    (add_net /SCL_Instr_Tx)
    (add_net /SDA_Instr_Rx)
    (add_net /SDA_Instr_Tx)
    (add_net /SDA_Washer)
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad7)")
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 179.07 105.41)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 203.2 96.52)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 207.01 93.98)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 179.07 71.12)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 83.82)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 88.9)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 93.98)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 99.06)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 105.41)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 111.76)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 80.01)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 73.66)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 67.31)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 60.96)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 205.74 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 200.66 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 208.28 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 198.12 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 200.66 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 204.47 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 208.28 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 109.22)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 111.76)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 105.41)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 101.6)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 88.9)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 85.09)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 72.39)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 68.58)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 195.58 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 180.34 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 175.26 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 171.45 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 111.76)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 105.41)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 99.06)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 92.71)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 86.36)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 80.01)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 73.66)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 67.31)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 60.96)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB39909)
    (at 171.45 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 175.26 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 180.34 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 184.15 114.3)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 105.41)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 101.6)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 88.9)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 85.09)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 72.39)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 68.58)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 118.11)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 185.42 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38E9F)
    (at 210.82 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 4 /0V_Instr) (zone_connect 2))
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 182.88 57.15 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C1 (at 2.5 -3.06 180) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 182.88 90.17 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C2 (at 2.5 -3.06 180) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 181.61 82.55 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C3 (at 2.5 -3.06 90) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 181.61 115.57 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C4 (at 2.5 -3.06 90) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 199.39 58.42 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C5 (at 2.5 -3.06 270) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 199.39 91.44 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C6 (at 2.5 -3.06 270) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 198.12 83.82)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C7 (at 2.5 -3.06) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 198.12 116.84)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (fp_text reference C8 (at 2.5 -3.06) (layer F.SilkS))
    (fp_text value C (at 2.5 3.06) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AABBC87)
    (at 171.45 86.36)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 16.51 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SDA_Washer))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5AABBC70)
    (at 209.55 82.55)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 -8.89 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SDA_Instr_Rx))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SDA_Instr_Tx))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SCL_Instr_Rx))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SCL_Instr_Tx))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5AB21CF9)
    (at 177.8 63.5 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56 180) (layer F.SilkS))
    (fp_text value BC547 (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 177.8 96.52 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 180) (layer F.SilkS))
    (fp_text value BC547 (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 12 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 201.93 77.47)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value BC547 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 203.2 110.49)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value BC547 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 "Net-(Q4-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 177.8 82.55 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 1.27 -2.66 90) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 177.8 115.57 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 1.27 -2.66 90) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 173.99 67.31)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R3 (at 1.27 -2.66) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 173.99 100.33)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R4 (at 1.27 -2.66) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 181.61 63.5 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R5 (at 1.27 -2.66 90) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 181.61 96.52 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R6 (at 1.27 -2.66 90) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 198.12 80.01 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R7 (at 1.27 -2.66 90) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 199.39 113.03 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R8 (at 1.27 -2.66 90) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Q4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 203.2 72.39 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R9 (at 1.27 -2.66 180) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /SDA_Instr_Tx))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Q3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 204.47 105.41 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R10 (at 1.27 -2.66 180) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /SCL_Instr_Tx))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 204.47 58.42 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R11 (at 1.27 -2.66 270) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 204.47 91.44 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R12 (at 1.27 -2.66 270) (layer F.SilkS))
    (fp_text value R (at 1.27 2.66 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 186.69 58.42)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 6N135 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /SDA_Instr_Rx))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R5-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 194.31 82.55 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value 6N135 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R7-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U2-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 186.69 91.44)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 6N135 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U3-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /0V_Instr))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /SCL_Instr_Rx))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R6-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U3-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U3-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 194.31 115.57 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value 6N135 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U4-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /LIVE_0V_Washer))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /+5V_Instr))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J3-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R8-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U4-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U4-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /LIVE_+15V_Washer))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 181.61 106.68 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 181.61 73.66 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SDA_Washer))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 173.99 82.55 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 173.99 115.57 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 176.53 104.14)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 176.53 71.12)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 204.47 64.77)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SDA_Instr_Rx))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 204.47 99.06)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SCL_Instr_Rx))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module via:stitch_0.6mm (layer F.Cu) (tedit 5AB38C59)
    (at 168.91 55.88)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value stitch_0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 /LIVE_0V_Washer) (zone_connect 2))
  )
  (gr_text "All Rights Reserved" (at 209.55 67.31 90) (layer F.SilkS))
  (gr_text "Copyright (C) 2018" (at 170.18 67.31 90) (layer F.SilkS))
  (gr_line (start 167.64 119.38) (end 212.09 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 54.61) (end 212.09 54.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "I2C Isolator" (at 170.18 110.49 90) (layer F.SilkS))
  (gr_line (start 212.09 54.61) (end 212.09 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Robar Systems" (at 209.55 100.33 90) (layer F.SilkS))
  (gr_line (start 167.64 54.61) (end 167.64 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (target plus (at 208.28 115.57) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 196.85 69.85) (size 5) (width 0.15) (layer Edge.Cuts))
  (zone (net 2) (net_name /LIVE_0V_Washer) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.69 119.38) (xy 167.64 119.38) (xy 167.64 54.61) (xy 186.69 54.61)
      )
    )
  )
  (zone (net 4) (net_name /0V_Instr) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.09 119.38) (xy 194.31 119.38) (xy 194.31 54.61) (xy 212.09 54.61)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 119.38) (xy 186.69 119.38) (xy 186.69 54.61) (xy 194.31 54.61)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.69 54.61) (xy 194.31 54.61) (xy 194.31 119.38) (xy 186.69 119.38)
      )
    )
  )
  (zone (net 2) (net_name /LIVE_0V_Washer) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 54.61) (xy 186.69 54.61) (xy 186.69 119.38) (xy 167.64 119.38)
      )
    )
  )
  (zone (net 4) (net_name /0V_Instr) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 54.61) (xy 212.09 54.61) (xy 212.09 119.38) (xy 194.31 119.38)
      )
    )
  )
)
