(kicad_pcb (version 3) (host pcbnew "(22-Jun-2014 BZR 4027)-stable")
  (general
    (links 18)
    (no_connects 0)
    (area 189.012612 139.6965 237.707388 157.4835)
    (thickness 1.6)
    (drawings 5)
    (tracks 81)
    (zones 0)
    (modules 14)
    (nets 19)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.0635)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 3178497)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /LED_P1_A)
  (net 2 /LED_P1_B)
  (net 3 /LED_P2_A)
  (net 4 /LED_P2_B)
  (net 5 /LED_P3_A)
  (net 6 /LED_P3_B)
  (net 7 /LED_P4_A)
  (net 8 /LED_P4_B)
  (net 9 /LED_P5_A)
  (net 10 /LED_P5_B)
  (net 11 /LED_P6_A)
  (net 12 /LED_P6_B)
  (net 13 /LED_P7_A)
  (net 14 /LED_P7_B)
  (net 15 /LED_P8_A)
  (net 16 /LED_P8_B)
  (net 17 /LED_PWR_A)
  (net 18 /LED_PWR_B)
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.0635)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net /LED_P1_A)
    (add_net /LED_P1_B)
    (add_net /LED_P2_A)
    (add_net /LED_P2_B)
    (add_net /LED_P3_A)
    (add_net /LED_P3_B)
    (add_net /LED_P4_A)
    (add_net /LED_P4_B)
    (add_net /LED_P5_A)
    (add_net /LED_P5_B)
    (add_net /LED_P6_A)
    (add_net /LED_P6_B)
    (add_net /LED_P7_A)
    (add_net /LED_P7_B)
    (add_net /LED_P8_A)
    (add_net /LED_P8_B)
    (add_net /LED_PWR_A)
    (add_net /LED_PWR_B)
  )
  (module pin_array_9x2 (layer F.Cu) (tedit 5781E6CB)
    (at 213.36 144.78)
    (descr "Double rangee de contacts 2 x 8 pins")
    (tags CONN)
    (fp_text reference X1 (at 0 -3.21) (layer F.SilkS) hide)
    (fp_text value PINHEAD9X2 (at 0 3.202) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -10.16 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 18 /LED_PWR_B)
    )
    (pad 3 thru_hole circle (at -7.62 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 /LED_P1_A)
    )
    (pad 4 thru_hole circle (at -7.62 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 /LED_P1_B)
    )
    (pad 5 thru_hole circle (at -5.08 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 /LED_P2_A)
    )
    (pad 6 thru_hole circle (at -5.08 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 /LED_P2_B)
    )
    (pad 7 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 /LED_P3_A)
    )
    (pad 8 thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /LED_P3_B)
    )
    (pad 9 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /LED_P4_A)
    )
    (pad 10 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 /LED_P4_B)
    )
    (pad 11 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 /LED_P5_A)
    )
    (pad 12 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 /LED_P5_B)
    )
    (pad 13 thru_hole circle (at 5.08 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 /LED_P6_A)
    )
    (pad 14 thru_hole circle (at 5.08 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 12 /LED_P6_B)
    )
    (pad 15 thru_hole circle (at 7.62 1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 /LED_P7_A)
    )
    (pad 16 thru_hole circle (at 7.62 -1.27) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 /LED_P7_B)
    )
    (pad 1 thru_hole circle (at -10.16 1.27) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 17 /LED_PWR_A)
    )
    (pad 17 thru_hole circle (at 10.16 1.27) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 /LED_P8_A)
    )
    (pad 18 thru_hole circle (at 10.16 -1.27) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 /LED_P8_B)
    )
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hole_3mm (layer F.Cu) (tedit 5781EA0F)
    (at 233.68 143.51)
    (fp_text reference Hole3mm (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 3.175) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module hole_3mm (layer F.Cu) (tedit 5781EA0F)
    (at 233.68 153.67)
    (fp_text reference Hole3mm (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 3.175) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module hole_3mm (layer F.Cu) (tedit 5781EA0F)
    (at 193.04 153.67)
    (fp_text reference Hole3mm (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 3.175) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module hole_3mm (layer F.Cu) (tedit 5781EA0F)
    (at 193.04 143.51)
    (fp_text reference Hole3mm (at 0 -3.175) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 3.175) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 198.12 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 17 /LED_PWR_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 18 /LED_PWR_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 201.93 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /LED_P1_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /LED_P1_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 205.74 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D3 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /LED_P2_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /LED_P2_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 209.55 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /LED_P3_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /LED_P3_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 213.36 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D5 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /LED_P4_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_P4_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 217.17 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D6 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 9 /LED_P5_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /LED_P5_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 220.98 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D7 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /LED_P6_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /LED_P6_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 224.79 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D8 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /LED_P7_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /LED_P7_B)
    )
  )
  (module LED-1206 (layer F.Cu) (tedit 5781EC29)
    (at 228.6 152.4 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D9 (at -2.032 -1.524 90) (layer F.SilkS))
    (fp_text value LED (at 1.778 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /LED_P8_A)
    )
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086)
      (layers F.Cu F.Paste F.Mask)
      (net 16 /LED_P8_B)
    )
  )
  (gr_line (start 189.865 156.845) (end 189.865 140.335) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.855 156.845) (end 189.865 156.845) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.855 140.335) (end 236.855 156.845) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.865 140.335) (end 236.855 140.335) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Network Switch LED bar v0.1\n07/2016 by Kai Lauterbach\nme@klaute.net\n@kailauterbach\nhttps://www.klaute.de" (at 229.87 151.13) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.865 140.335) (xy 236.855 140.335) (xy 236.855 156.845) (xy 189.865 156.845)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 236.855 156.845) (xy 189.865 156.845) (xy 189.865 140.335) (xy 236.855 140.335)
      )
    )
  )
)
