(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 62)
    (tracks 334)
    (zones 0)
    (modules 15)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.4)
    (via_drill 0.2)
    (via_min_size 0.4)
    (via_min_drill 0.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.09)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFE3F)
    (pcbplotparams
      (layerselection 0x010f8_80000007)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "prod"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /ID_SD_EEPROM)
  (net 3 /ID_SC_EEPROM)
  (net 4 "Net-(J1-Pad2)")
  (net 5 +3V3)
  (net 6 +5V)
  (net 7 /GPIO2)
  (net 8 /GPIO3)
  (net 9 /GPIO4)
  (net 10 "Net-(J2-Pad8)")
  (net 11 "Net-(J2-Pad10)")
  (net 12 /GPIO17)
  (net 13 /GPIO18)
  (net 14 "Net-(J2-Pad13)")
  (net 15 /GPIO22)
  (net 16 /GPIO23)
  (net 17 "Net-(J2-Pad17)")
  (net 18 /GPIO24)
  (net 19 /GPIO10)
  (net 20 /GPIO9)
  (net 21 /GPIO25)
  (net 22 /GPIO11)
  (net 23 /GPIO8)
  (net 24 "Net-(J2-Pad26)")
  (net 25 "Net-(J2-Pad29)")
  (net 26 /GPIO6)
  (net 27 "Net-(J2-Pad32)")
  (net 28 /GPIO13)
  (net 29 /GPIO19)
  (net 30 "Net-(J2-Pad36)")
  (net 31 /GPIO26)
  (net 32 /GPIO20)
  (net 33 /GPIO21)
  (net 34 /CONTROL0)
  (net 35 /CONTROL1)
  (net 36 /DATA0)
  (net 37 /STATUS3)
  (net 38 /DATA1)
  (net 39 /CONTROL2)
  (net 40 /DATA2)
  (net 41 /CONTROL3)
  (net 42 /DATA3)
  (net 43 /DATA4)
  (net 44 /DATA5)
  (net 45 /DATA6)
  (net 46 /DATA7)
  (net 47 /STATUS6)
  (net 48 /STATUS7)
  (net 49 /STATUS5)
  (net 50 /STATUS4)
  (net 51 "Net-(U2-Pad30)")
  (net 52 "Net-(U2-Pad43)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.4)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /CONTROL0)
    (add_net /CONTROL1)
    (add_net /CONTROL2)
    (add_net /CONTROL3)
    (add_net /DATA0)
    (add_net /DATA1)
    (add_net /DATA2)
    (add_net /DATA3)
    (add_net /DATA4)
    (add_net /DATA5)
    (add_net /DATA6)
    (add_net /DATA7)
    (add_net /GPIO10)
    (add_net /GPIO11)
    (add_net /GPIO13)
    (add_net /GPIO17)
    (add_net /GPIO18)
    (add_net /GPIO19)
    (add_net /GPIO2)
    (add_net /GPIO20)
    (add_net /GPIO21)
    (add_net /GPIO22)
    (add_net /GPIO23)
    (add_net /GPIO24)
    (add_net /GPIO25)
    (add_net /GPIO26)
    (add_net /GPIO3)
    (add_net /GPIO4)
    (add_net /GPIO6)
    (add_net /GPIO8)
    (add_net /GPIO9)
    (add_net /ID_SC_EEPROM)
    (add_net /ID_SD_EEPROM)
    (add_net /STATUS3)
    (add_net /STATUS4)
    (add_net /STATUS5)
    (add_net /STATUS6)
    (add_net /STATUS7)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad43)")
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 102.1588 112.268)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder (layer F.Cu) (tedit 59FE48B8)
    (at 123.3905 111.252 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.65 0.05) (layer F.SilkS))
    (fp_text value 3.9K (at 2.7405 0.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.9625 0 180) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /ID_SC_EEPROM))
    (pad 1 smd rect (at -0.9625 0 180) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder (layer F.Cu) (tedit 59FE48B8)
    (at 114.3535 115.316 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.7405 0) (layer F.SilkS))
    (fp_text value DNP (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.9625 0 180) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9625 0 180) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SOIC:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 114.554 111.252)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -5.08 0.254 180) (layer F.SilkS))
    (fp_text value CAT24C32 (at -2.65 0.1 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /ID_SD_EEPROM))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /ID_SC_EEPROM))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SSOP-48_7.5x15.9mm_P0.635mm (layer F.Cu) (tedit 5A02F25C)
    (at 118.872 86.868 270)
    (descr "SSOP48: plastic shrink small outline package; 48 leads; body width 7.5 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot370-1_po.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U2 (at 0 -9.652 180) (layer F.SilkS))
    (fp_text value SN74LVC161284DLR (at 0 9 90) (layer F.Fab))
    (fp_text user %R (at -3.556 -1.524 90) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -7.3025 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 /GPIO20))
    (pad 2 smd rect (at -4.7 -6.6675 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 /GPIO26))
    (pad 3 smd rect (at -4.7 -6.0325 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /GPIO19))
    (pad 4 smd rect (at -4.7 -5.3975 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 /GPIO6))
    (pad 5 smd rect (at -4.7 -4.7625 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 /GPIO13))
    (pad 6 smd rect (at -4.7 -4.1275 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -4.7 -3.4925 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 8 smd rect (at -4.7 -2.8575 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 /GPIO11))
    (pad 9 smd rect (at -4.7 -2.2225 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 /GPIO8))
    (pad 10 smd rect (at -4.7 -1.5875 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -4.7 -0.9525 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /GPIO9))
    (pad 12 smd rect (at -4.7 -0.3175 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /GPIO25))
    (pad 13 smd rect (at -4.7 0.3175 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /GPIO10))
    (pad 14 smd rect (at -4.7 0.9525 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO24))
    (pad 15 smd rect (at -4.7 1.5875 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -4.7 2.2225 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 /GPIO23))
    (pad 17 smd rect (at -4.7 2.8575 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /GPIO22))
    (pad 18 smd rect (at -4.7 3.4925 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 19 smd rect (at -4.7 4.1275 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -4.7 4.7625 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /GPIO17))
    (pad 21 smd rect (at -4.7 5.3975 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /GPIO18))
    (pad 22 smd rect (at -4.7 6.0325 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /GPIO4))
    (pad 23 smd rect (at -4.7 6.6675 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /GPIO3))
    (pad 24 smd rect (at -4.7 7.3025 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /GPIO2))
    (pad 25 smd rect (at 4.7 7.3025 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 /STATUS3))
    (pad 26 smd rect (at 4.7 6.6675 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 50 /STATUS4))
    (pad 27 smd rect (at 4.7 6.0325 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 /STATUS5))
    (pad 28 smd rect (at 4.7 5.3975 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 /STATUS7))
    (pad 29 smd rect (at 4.7 4.7625 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 /STATUS6))
    (pad 30 smd rect (at 4.7 4.1275 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad30)"))
    (pad 31 smd rect (at 4.7 3.4925 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 32 smd rect (at 4.7 2.8575 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 /DATA7))
    (pad 33 smd rect (at 4.7 2.2225 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 /DATA6))
    (pad 34 smd rect (at 4.7 1.5875 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at 4.7 0.9525 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 /DATA5))
    (pad 36 smd rect (at 4.7 0.3175 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 /DATA4))
    (pad 37 smd rect (at 4.7 -0.3175 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 /DATA3))
    (pad 38 smd rect (at 4.7 -0.9525 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 /DATA2))
    (pad 39 smd rect (at 4.7 -1.5875 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 4.7 -2.2225 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 /DATA1))
    (pad 41 smd rect (at 4.7 -2.8575 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 /DATA0))
    (pad 42 smd rect (at 4.7 -3.4925 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 43 smd rect (at 4.7 -4.1275 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U2-Pad43)"))
    (pad 44 smd rect (at 4.7 -4.7625 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 /CONTROL0))
    (pad 45 smd rect (at 4.7 -5.3975 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /CONTROL1))
    (pad 46 smd rect (at 4.7 -6.0325 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 /CONTROL2))
    (pad 47 smd rect (at 4.7 -6.6675 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 /CONTROL3))
    (pad 48 smd rect (at 4.7 -7.3025 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /GPIO21))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-48_7.5x15.9mm_P0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder (layer F.Cu) (tedit 59FE48B8)
    (at 123.3905 109.474)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.5935 0) (layer F.SilkS))
    (fp_text value 10K (at -2.4865 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.9625 0) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 0.9625 0) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x13_P2.54mm_Horizontal locked (layer F.Cu) (tedit 59FED5CB)
    (at 91.44 104.14 180)
    (descr "Through hole angled pin header, 2x13, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x13 2.54mm double row")
    (fp_text reference J3 (at 5.655 -2.27) (layer F.SilkS))
    (fp_text value Conn_02x13_Odd_Even (at 5.655 32.75) (layer F.Fab))
    (fp_text user %R (at 5.31 15.24 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /CONTROL0))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /CONTROL1))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /DATA0))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /STATUS3))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /DATA1))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /CONTROL2))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /DATA2))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /CONTROL3))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /DATA3))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /DATA4))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /DATA5))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /DATA6))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /DATA7))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /STATUS6))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /STATUS7))
    (pad 22 thru_hole oval (at 2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /STATUS5))
    (pad 24 thru_hole oval (at 2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /STATUS4))
    (pad 26 thru_hole oval (at 2.54 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x13_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical locked (layer B.Cu) (tedit 5A19A433)
    (at 86.92 65.59 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J2 (at -1.27 2.77 270) (layer B.SilkS))
    (fp_text value 40HAT (at -1.27 -51.03 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO2))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO3))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO4))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO17))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO18))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIO22))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO23))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIO24))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /GPIO10))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /GPIO9))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /GPIO25))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /GPIO11))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /GPIO8))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /ID_SD_EEPROM))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /ID_SC_EEPROM))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad29)"))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /GPIO6))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad32)"))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /GPIO13))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /GPIO19))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad36)"))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /GPIO26))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /GPIO20))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /GPIO21))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 113.03 105.918 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at -0.254 5.334 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at -1.9 1.3 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.84x1.00mm_HandSolder (layer F.Cu) (tedit 59FE48B8)
    (at 123.444 113.03 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.65 -0.1) (layer F.SilkS))
    (fp_text value 3.9K (at 2.794 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.9625 0 180) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.9625 0 180) (size 0.845 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /ID_SD_EEPROM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 5A6D0885)
    (at 82.04 64.31)
    (fp_text reference H1 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 5A6D088A)
    (at 140.04 64.33)
    (fp_text reference H3 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 5A6D0898)
    (at 82.04 113.32)
    (fp_text reference H2 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module project_footprints:NPTH_3mm_ID locked (layer F.Cu) (tedit 5A6D0891)
    (at 140.03 113.31)
    (fp_text reference H4 (at 0.06 0.09) (layer F.SilkS))
    (fp_text value 3mm_Mounting_Hole (at 0 -2.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 1.6))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 107.442 88.891 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.785 0 180) (layer F.SilkS))
    (fp_text value 1.4K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 /STATUS3))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 87.122 68.834) (layer F.SilkS))
  (gr_text 1 (at 108.712 109.474) (layer F.SilkS))
  (gr_text 1 (at 94.488 104.14) (layer F.SilkS))
  (gr_text 1 (at 128.7 81.875) (layer F.SilkS))
  (gr_text "WorlickWerx (c) 2019" (at 92.5068 112.8268) (layer F.SilkS))
  (gr_text "pi-parport v3" (at 92.8624 110.8964) (layer F.SilkS))
  (gr_line (start 78.546356 63.817611) (end 78.546356 113.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 81.546356 63.817611) (end 81.546356 60.817611) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.546356 60.817611) (end 81.546356 60.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 140.546356 63.817611) (end 143.546356 63.817611) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.546356 113.817611) (end 143.546356 63.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 81.546356 113.817611) (end 78.546356 113.817611) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 81.546356 116.817611) (end 140.546356 116.817611) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 140.546356 113.817611) (end 140.546356 116.817611) (angle -89.9) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.78 118.11) (xy 75.946 118.11) (xy 75.946 60.198) (xy 144.78 60.198)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.4564 118.872) (xy 75.2348 118.872) (xy 75.0824 58.7756) (xy 146.4564 58.7756)
      )
    )
  )
)
