(kicad_pcb (version 20171130) (host pcbnew 5.1.10)
  (general
    (thickness 1.6)
    (drawings 72)
    (tracks 157)
    (zones 0)
    (modules 18)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.889)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.016 0.762)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 CPU_5V)
  (net 3 CPU_12V)
  (net 4 DISPLAY_15V)
  (net 5 CPU_MINUS_12V)
  (net 6 DISPLAY_VSYNC)
  (net 7 DISPLAY_VIDEO)
  (net 8 DISPLAY_HSYNC)
  (net 9 SPK_GND)
  (net 10 SPK_AUDIO)
  (net 11 ATX_POK)
  (net 12 "Net-(J2-Pad8)")
  (net 13 CONV_12V)
  (net 14 CONV_15V)
  (net 15 "Net-(J5-Pad1)")
  (net 16 +5V)
  (net 17 "Net-(J5-Pad9)")
  (net 18 +12V)
  (net 19 -12V)
  (net 20 ATX_PSON)
  (net 21 "Net-(J5-Pad20)")
  (net 22 +15V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +15V)
    (add_net +5V)
    (add_net -12V)
    (add_net ATX_POK)
    (add_net ATX_PSON)
    (add_net CONV_12V)
    (add_net CONV_15V)
    (add_net CPU_12V)
    (add_net CPU_5V)
    (add_net CPU_MINUS_12V)
    (add_net DISPLAY_15V)
    (add_net DISPLAY_HSYNC)
    (add_net DISPLAY_VIDEO)
    (add_net DISPLAY_VSYNC)
    (add_net GND)
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad20)")
    (add_net "Net-(J5-Pad9)")
    (add_net SPK_AUDIO)
    (add_net SPK_GND)
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_5-G-5,08_1x05_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047)
    (at 96.8375 98.8695 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/5-G-5,08; number of pins: 05; pin pitch: 5.08mm; Vertical || order number: 1755765 12A || order number: 1924334 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x05_G_5.08mm")
    (fp_text reference J1 (at 10.16 -6 90) (layer F.SilkS))
    (fp_text value VIDEO (at 10.16 5 90) (layer F.Fab))
    (fp_text user %R (at 10.16 -4.1 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 6 DISPLAY_VSYNC))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 DISPLAY_15V))
    (pad 4 thru_hole oval (at 15.24 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 DISPLAY_VIDEO))
    (pad 5 thru_hole oval (at 20.32 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 DISPLAY_HSYNC))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_5-G-5,08_1x05_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_12-G-5,08_1x12_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047)
    (at 79.502 81.661 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/12-G-5,08; number of pins: 12; pin pitch: 5.08mm; Vertical || order number: 1755833 12A || order number: 1924402 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x12_G_5.08mm")
    (fp_text reference J2 (at 27.94 -6 90) (layer F.SilkS))
    (fp_text value CPU (at 27.94 5 90) (layer F.Fab))
    (fp_text user %R (at 27.94 -4.1 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 8 DISPLAY_HSYNC))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 DISPLAY_VSYNC))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 DISPLAY_VIDEO))
    (pad 4 thru_hole oval (at 15.24 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 SPK_GND))
    (pad 5 thru_hole oval (at 20.32 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 10 SPK_AUDIO))
    (pad 6 thru_hole oval (at 25.4 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 ATX_POK))
    (pad 7 thru_hole oval (at 30.48 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 CPU_5V))
    (pad 8 thru_hole oval (at 35.56 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 40.64 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 45.72 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 50.8 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 CPU_12V))
    (pad 12 thru_hole oval (at 55.88 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 CPU_MINUS_12V))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_12-G-5,08_1x12_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_8-G-5,08_1x08_P5.08mm_Vertical (layer F.Cu) (tedit 5B785047)
    (at 96.647 64.8335 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBVA_2,5/8-G-5,08; number of pins: 08; pin pitch: 5.08mm; Vertical || order number: 1755794 12A || order number: 1924363 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x08_G_5.08mm")
    (fp_text reference J3 (at 17.78 -6 90) (layer F.SilkS))
    (fp_text value DRIVES (at 17.78 5 90) (layer F.Fab))
    (fp_text user %R (at 17.78 -4.1 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 3 CPU_12V))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 15.24 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 CPU_5V))
    (pad 5 thru_hole oval (at 20.32 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 CPU_12V))
    (pad 6 thru_hole oval (at 25.4 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 30.48 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 35.56 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 CPU_5V))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBVA_2,5_8-G-5,08_1x08_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 57.2135 111.633 90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value 15V_CONV (at 4.385 9.89 90) (layer F.Fab))
    (fp_text user %R (at 2.77 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 CONV_12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 CONV_15V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mini-Fit_Jr_5566-24A2_2x12_P4.20mm_Vertical (layer F.Cu) (tedit 5B781992)
    (at 25.273 70.2945 90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-24A2, example for new mpn: 39-28-924x, 12 Pins per row, Mounting: Snap-in Plastic Peg PCB Lock (http://www.molex.com/pdm_docs/sd/039289068_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr side entryplastic_peg")
    (fp_text reference J5 (at 23.1 -3.45 90) (layer F.SilkS))
    (fp_text value ATX-24 (at 23.1 9.95 90) (layer F.Fab))
    (fp_text user %R (at 23.1 -1.55 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.09259299999999999)
      (net 15 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 4.2 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (pad 3 thru_hole oval (at 8.4 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 12.6 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 5 thru_hole oval (at 16.8 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 21 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 7 thru_hole oval (at 25.2 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 29.4 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 ATX_POK))
    (pad 9 thru_hole oval (at 33.6 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad9)"))
    (pad 10 thru_hole oval (at 37.8 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 +12V))
    (pad 11 thru_hole oval (at 42 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 +12V))
    (pad 12 thru_hole oval (at 46.2 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (pad 13 thru_hole oval (at 0 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (pad 14 thru_hole oval (at 4.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 -12V))
    (pad 15 thru_hole oval (at 8.4 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 12.6 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 20 ATX_PSON))
    (pad 17 thru_hole oval (at 16.8 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 21 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 25.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 29.4 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 21 "Net-(J5-Pad20)"))
    (pad 21 thru_hole oval (at 33.6 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 22 thru_hole oval (at 37.8 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 23 thru_hole oval (at 42 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 24 thru_hole oval (at 46.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at -4.7 5.04 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 50.9 5.04 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-24A2_2x12_P4.20mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 46.6725 111.76 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value PWR (at 4.385 4.81 90) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 ATX_PSON))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 36.195 111.76 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value FAN (at 4.385 4.81 90) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 60.579 59.69 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.25 90) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 6.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 CPU_5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 60.7695 41.656 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 2.5 -6.25 90) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 6.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 CPU_12V))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 79.4385 95.25 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C3 (at 2.5 -6.25 90) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 6.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 DISPLAY_15V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 60.7695 29.0195 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C4 (at 2.5 -6.25 90) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 6.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 CPU_MINUS_12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC (layer F.Cu) (tedit 5AE59B05)
    (at 69.6595 92.3925 180)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4.5mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4.5mm Fastron MECC")
    (fp_text reference L1 (at 7.62 -3.37) (layer F.SilkS))
    (fp_text value 100uH (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 DISPLAY_15V))
    (pad 2 thru_hole oval (at 15.24 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 +15V))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC (layer F.Cu) (tedit 5AE59B05)
    (at 47.5615 62.992 270)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4.5mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4.5mm Fastron MECC")
    (fp_text reference L2 (at 7.62 -3.37 90) (layer F.SilkS))
    (fp_text value 100uH (at 7.62 3.37 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 CPU_5V))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC (layer F.Cu) (tedit 5AE59B05)
    (at 47.5615 42.1005 270)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4.5mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4.5mm Fastron MECC")
    (fp_text reference L3 (at 7.62 -3.37 90) (layer F.SilkS))
    (fp_text value 100uH (at 7.62 3.37 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 CPU_12V))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 +12V))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC (layer F.Cu) (tedit 5AE59B05)
    (at 47.5615 21.2725 270)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4.5mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4.5mm Fastron MECC")
    (fp_text reference L4 (at 7.62 -3.37 90) (layer F.SilkS))
    (fp_text value 100uH (at 7.62 3.37 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 -12V))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 CPU_MINUS_12V))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC (layer F.Cu) (tedit 5AE59B05)
    (at 69.723 75.2475 180)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4.5mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4.5mm Fastron MECC")
    (fp_text reference L5 (at 7.62 -3.37) (layer F.SilkS))
    (fp_text value 100uH (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 CONV_12V))
    (pad 2 thru_hole oval (at 15.24 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 +12V))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC (layer F.Cu) (tedit 5AE59B05)
    (at 69.723 83.6295 180)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4.5mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4.5mm Fastron MECC")
    (fp_text reference L6 (at 7.62 -3.37) (layer F.SilkS))
    (fp_text value 100uH (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 +15V))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 CONV_15V))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 73.025 109.22)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 4.385 -2.27) (layer F.SilkS))
    (fp_text value AUDIO (at 4.385 4.81) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SPK_GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SPK_AUDIO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text <adrian@freebsd.org> (at 28.829 95.25) (layer F.SilkS))
  (gr_text "Adrian Chadd" (at 28.829 92.2655) (layer F.SilkS))
  (gr_text "v0.1, May 2022" (at 28.9941 88.9508) (layer F.SilkS))
  (gr_text "Otrona Attache PSU" (at 28.2575 85.5345) (layer F.SilkS))
  (gr_text POK (at 20.3835 41.021) (layer F.SilkS))
  (gr_text +5v (at 20.574 49.276) (layer F.SilkS))
  (gr_text +5v (at 20.2565 57.7215) (layer F.SilkS))
  (gr_text -12v (at 37.2745 66.2305) (layer F.SilkS))
  (gr_text PSON (at 37.2745 57.9755) (layer F.SilkS))
  (gr_text +5v (at 36.6395 36.576) (layer F.SilkS))
  (gr_text +5v (at 36.5125 32.639) (layer F.SilkS))
  (gr_text +5v (at 36.3855 28.194) (layer F.SilkS))
  (gr_text +12v (at 20.066 32.4485) (layer F.SilkS))
  (gr_text +12v (at 20.3835 28.0035) (layer F.SilkS))
  (gr_text 100uF (at 66.929 26.416 90) (layer F.SilkS))
  (gr_text 100uF (at 73.2155 97.7265 90) (layer F.SilkS))
  (gr_text 100uF (at 54.5465 44.1325 90) (layer F.SilkS))
  (gr_text 100uF (at 54.356 62.1665 90) (layer F.SilkS))
  (gr_text 100uH (at 62.0395 89.027) (layer F.SilkS))
  (gr_text 100uH (at 62.0395 80.264) (layer F.SilkS))
  (gr_text 100uH (at 62.103 71.882) (layer F.SilkS))
  (gr_text 100uH (at 42.037 49.5935 90) (layer F.SilkS))
  (gr_text 100uH (at 41.8465 28.8925 90) (layer F.SilkS))
  (gr_text 100uH (at 42.4815 70.5485 90) (layer F.SilkS))
  (gr_text CPU (at 84.582 53.721 90) (layer F.SilkS))
  (gr_text HS (at 72.3265 81.788) (layer F.SilkS))
  (gr_text VS (at 72.771 76.581) (layer F.SilkS))
  (gr_text Video (at 71.8185 71.4375) (layer F.SilkS))
  (gr_text SG (at 72.0725 66.3575) (layer F.SilkS))
  (gr_text SA (at 72.009 61.341) (layer F.SilkS))
  (gr_text PwrOk (at 71.3105 56.134) (layer F.SilkS))
  (gr_text +5v (at 71.247 51.1175) (layer F.SilkS))
  (gr_text GND (at 71.3105 40.767) (layer F.SilkS))
  (gr_text GND (at 71.374 35.7505) (layer F.SilkS))
  (gr_text +12v (at 71.374 30.607) (layer F.SilkS))
  (gr_text -12v (at 71.6915 25.8445) (layer F.SilkS))
  (gr_text VIDEO (at 101.9175 83.7565 90) (layer F.SilkS))
  (gr_text "DRIVES\n" (at 101.981 41.0845 90) (layer F.SilkS))
  (gr_text 5v (at 88.138 29.5275) (layer F.SilkS))
  (gr_text GND (at 88.3285 34.417) (layer F.SilkS))
  (gr_text GND (at 88.3285 39.37) (layer F.SilkS))
  (gr_text 12v (at 88.2015 44.577) (layer F.SilkS))
  (gr_text 5v (at 88.3285 49.53) (layer F.SilkS))
  (gr_text GND (at 88.3285 54.737) (layer F.SilkS))
  (gr_text GND (at 88.392 59.69) (layer F.SilkS))
  (gr_text 12v (at 88.011 64.9605) (layer F.SilkS))
  (gr_text VSYNC (at 88.646 100.1395) (layer F.SilkS))
  (gr_text "GND\n" (at 88.265 93.726) (layer F.SilkS))
  (gr_text 15v (at 88.138 88.5825) (layer F.SilkS))
  (gr_text "VIDEO\n" (at 88.5825 83.7565) (layer F.SilkS))
  (gr_text "HSYNC\n" (at 88.646 78.359) (layer F.SilkS))
  (gr_text SA (at 69.977 111.6965) (layer F.SilkS))
  (gr_text SG (at 69.9135 109.22) (layer F.SilkS))
  (gr_text SPKR (at 77.343 114.554) (layer F.SilkS))
  (gr_text G (at 65.2145 114.681) (layer F.SilkS))
  (gr_text 15v (at 62.4205 114.6175) (layer F.SilkS))
  (gr_text G (at 59.817 114.7445) (layer F.SilkS))
  (gr_text 12v (at 56.769 114.681) (layer F.SilkS))
  (gr_text G (at 49.0855 114.681) (layer F.SilkS))
  (gr_text G (at 38.7985 114.681) (layer F.SilkS))
  (gr_text "ATX_ON\n" (at 44.7675 114.681) (layer F.SilkS))
  (gr_text +5v (at 35.4965 114.681) (layer F.SilkS))
  (gr_text "12/15v converter\n" (at 61.1505 98.806) (layer F.SilkS))
  (gr_text PowerButton (at 47.752 99.06) (layer F.SilkS))
  (gr_text FAN (at 37.338 99.187) (layer F.SilkS))
  (gr_line (start 14.9225 14.986) (end 14.9225 117.9195) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 14.9225 117.983) (end 14.9225 117.9195) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.7115 117.983) (end 14.9225 117.983) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.711 14.986) (end 14.9225 14.986) (layer Edge.Cuts) (width 0.05))
  (dimension 89.9795 (width 0.15) (layer Dwgs.User)
    (gr_text "89.980 mm" (at 59.72175 120.0485) (layer Dwgs.User))
    (feature1 (pts (xy 14.732 121.3485) (xy 14.732 120.762079)))
    (feature2 (pts (xy 104.7115 121.3485) (xy 104.7115 120.762079)))
    (crossbar (pts (xy 104.7115 121.3485) (xy 14.732 121.3485)))
    (arrow1a (pts (xy 14.732 121.3485) (xy 15.858504 120.762079)))
    (arrow1b (pts (xy 14.732 121.3485) (xy 15.858504 121.934921)))
    (arrow2a (pts (xy 104.7115 121.3485) (xy 103.584996 120.762079)))
    (arrow2b (pts (xy 104.7115 121.3485) (xy 103.584996 121.934921)))
  )
  (dimension 100.0125 (width 0.15) (layer Dwgs.User)
    (gr_text "100.013 mm" (at 54.51475 118.461) (layer Dwgs.User))
    (feature1 (pts (xy 4.5085 119.761) (xy 4.5085 119.174579)))
    (feature2 (pts (xy 104.521 119.761) (xy 104.521 119.174579)))
    (crossbar (pts (xy 104.521 119.761) (xy 4.5085 119.761)))
    (arrow1a (pts (xy 4.5085 119.761) (xy 5.635004 119.174579)))
    (arrow1b (pts (xy 4.5085 119.761) (xy 5.635004 120.347421)))
    (arrow2a (pts (xy 104.521 119.761) (xy 103.394496 119.174579)))
    (arrow2b (pts (xy 104.521 119.761) (xy 103.394496 120.347421)))
  )
  (gr_line (start 104.711 14.986) (end 104.711 117.986) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.7115 117.983) (xy 14.9225 117.983) (xy 14.9225 14.986) (xy 104.7115 14.986)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.7115 117.983) (xy 14.9225 117.983) (xy 14.9225 14.986) (xy 104.7115 14.986)
      )
    )
  )
)
