<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="9.535" y1="14.859" x2="9.535" y2="-1.0768" width="0.1524" layer="20"/>
<wire x1="9.535" y1="-1.0768" x2="10.5156" y2="-2.032" width="0.1524" layer="20" curve="90"/>
<wire x1="10.5156" y1="-2.032" x2="32.9184" y2="-2.032" width="0.1524" layer="20"/>
<wire x1="32.9184" y1="-2.032" x2="33.909" y2="-1.0668" width="0.1524" layer="20" curve="90"/>
<wire x1="33.909" y1="-1.0668" x2="33.909" y2="14.732" width="0.1524" layer="20"/>
<wire x1="33.909" y1="14.732" x2="32.588" y2="15.9768" width="0.1524" layer="20" curve="90"/>
<wire x1="32.588" y1="15.9768" x2="10.729" y2="15.9768" width="0.1524" layer="20"/>
<wire x1="10.729" y1="15.9768" x2="9.535" y2="14.859" width="0.1524" layer="20" curve="90"/>
</plain>
<libraries>
<library name="jacks">
<packages>
<package name="2PADS">
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="3PDT.TOGGLE">
<description>&lt;b&gt;Toogle Switch, Solder Lug&lt;/b&gt;
&lt;br&gt;&lt;a href="http://smallbear-electronics.mybigcommerce.com/3pdt-on-on-short-lever-solder-terminal/"&gt;http://smallbear-electronics.mybigcommerce.com/3pdt-on-on-short-lever-solder-terminal/&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FX2-IN" library="jacks" package="2PADS" value="FX1-IN"/>
<element name="FX2-OUT" library="jacks" package="2PADS" value=""/>
<element name="FX1-IN" library="jacks" package="2PADS" value=""/>
<element name="FX1-OUT" library="jacks" package="2PADS" value=""/>
<element name="INPUT" library="jacks" package="2PADS" value=""/>
<element name="OUTPUT" library="jacks" package="2PADS" value=""/>
<element name="FX-ORDER-SWITCH" library="switches" package="3PDT.TOGGLE" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="RTN2">
<contactref element="FX-ORDER-SWITCH" pad="C2"/>
<contactref element="FX1-OUT" pad="T"/>
</signal>
<signal name="SEND2">
<contactref element="FX-ORDER-SWITCH" pad="A1"/>
<contactref element="FX-ORDER-SWITCH" pad="B3"/>
<contactref element="FX1-IN" pad="T"/>
</signal>
<signal name="SEND1">
<contactref element="FX-ORDER-SWITCH" pad="C1"/>
<contactref element="FX-ORDER-SWITCH" pad="A3"/>
<contactref element="FX2-IN" pad="T"/>
</signal>
<signal name="INPUT">
<contactref element="FX-ORDER-SWITCH" pad="A2"/>
<contactref element="INPUT" pad="T"/>
</signal>
<signal name="OUTPUT">
<contactref element="FX-ORDER-SWITCH" pad="C3"/>
<contactref element="FX-ORDER-SWITCH" pad="B1"/>
<contactref element="OUTPUT" pad="T"/>
</signal>
<signal name="RTN1">
<contactref element="FX2-OUT" pad="T"/>
<contactref element="FX-ORDER-SWITCH" pad="B2"/>
</signal>
<signal name="GND">
<contactref element="FX2-OUT" pad="S"/>
<contactref element="OUTPUT" pad="S"/>
<contactref element="FX1-IN" pad="S"/>
<contactref element="FX1-OUT" pad="S"/>
<contactref element="INPUT" pad="S"/>
<contactref element="FX2-IN" pad="S"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
