<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<text>MakeCode Arcade
Shield for RPi0</text>
<text>v1.1</text>
<text>G L R D U</text>
<wire x1="0" y1="3.175" x2="0" y2="40.64" width="0.1524" layer="20"/>
<wire x1="0" y1="40.64" x2="3.175" y2="43.815" width="0.1524" layer="20" curve="-90"/>
<wire x1="3.175" y1="43.815" x2="62.23" y2="43.815" width="0.1524" layer="20"/>
<wire x1="62.23" y1="43.815" x2="64.77" y2="41.275" width="0.1524" layer="20" curve="-90"/>
<wire x1="64.77" y1="41.275" x2="64.77" y2="3.175" width="0.1524" layer="20"/>
<wire x1="64.77" y1="3.175" x2="61.595" y2="0" width="0.1524" layer="20" curve="-90"/>
<wire x1="61.595" y1="0" x2="3.175" y2="0" width="0.1524" layer="20"/>
<wire x1="3.175" y1="0" x2="0" y2="3.175" width="0.1524" layer="20" curve="-90"/>
</plain>
<libraries>
<library name="arcade-shield">
<description>Generated from &lt;b&gt;Adafruit Arcade Bonnet.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="JST-PH-2.5-SMT">
</package>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REV" value="B"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RPI1" library="arcade-shield" package="2X20" value="RASPBERRYPI_BPLUS_IDC"/>
<element name="L1" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="U1" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="R1" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="D1" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="A1" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="B1" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="L2" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="U2" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="R2" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="D2" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="A2" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="B2" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="EXIT" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="MENU" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="RST" library="arcade-shield" package="JST-PH-2.5-SMT" value=""/>
<element name="PLAYER1" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="PLAYER2" library="SparkFun-Connectors" package="1X05" value=""/>
</elements>
<signals>
<signal name="MENU">
<contactref element="RPI1" pad="3"/>
<contactref element="MENU" pad="1"/>
</signal>
<signal name="EXIT">
<contactref element="RPI1" pad="5"/>
<contactref element="EXIT" pad="1"/>
</signal>
<signal name="RST">
<contactref element="RPI1" pad="7"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="D2">
<contactref element="RPI1" pad="11"/>
<contactref element="D2" pad="1"/>
<contactref element="PLAYER2" pad="4"/>
</signal>
<signal name="R2">
<contactref element="RPI1" pad="13"/>
<contactref element="R2" pad="1"/>
<contactref element="PLAYER2" pad="3"/>
</signal>
<signal name="U2">
<contactref element="RPI1" pad="15"/>
<contactref element="U2" pad="1"/>
<contactref element="PLAYER2" pad="5"/>
</signal>
<signal name="B2">
<contactref element="RPI1" pad="21"/>
<contactref element="B2" pad="1"/>
</signal>
<signal name="R1">
<contactref element="RPI1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="PLAYER1" pad="3"/>
</signal>
<signal name="U1">
<contactref element="RPI1" pad="31"/>
<contactref element="U1" pad="1"/>
<contactref element="PLAYER1" pad="5"/>
</signal>
<signal name="L1">
<contactref element="RPI1" pad="33"/>
<contactref element="L1" pad="1"/>
<contactref element="PLAYER1" pad="2"/>
</signal>
<signal name="A1">
<contactref element="RPI1" pad="37"/>
<contactref element="A1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="RPI1" pad="17"/>
<contactref element="RPI1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="RPI1" pad="25"/>
<contactref element="RPI1" pad="9"/>
<contactref element="RPI1" pad="39"/>
<contactref element="RPI1" pad="6"/>
<contactref element="RPI1" pad="34"/>
<contactref element="RPI1" pad="30"/>
<contactref element="RPI1" pad="20"/>
<contactref element="RPI1" pad="14"/>
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="B1" pad="2"/>
<contactref element="A1" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="B2" pad="2"/>
<contactref element="A2" pad="2"/>
<contactref element="EXIT" pad="2"/>
<contactref element="MENU" pad="2"/>
<contactref element="RST" pad="2"/>
<contactref element="PLAYER1" pad="1"/>
<contactref element="PLAYER2" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="RPI1" pad="8"/>
</signal>
<signal name="RXD">
<contactref element="RPI1" pad="10"/>
</signal>
<signal name="GPIO24">
<contactref element="RPI1" pad="18"/>
</signal>
<signal name="GPIO25">
<contactref element="RPI1" pad="22"/>
</signal>
<signal name="SPI_CE0">
<contactref element="RPI1" pad="24"/>
</signal>
<signal name="SPI_CE1">
<contactref element="RPI1" pad="26"/>
</signal>
<signal name="EECLK">
<contactref element="RPI1" pad="28"/>
</signal>
<signal name="GPIO16">
<contactref element="RPI1" pad="36"/>
</signal>
<signal name="GPIO20">
<contactref element="RPI1" pad="38"/>
</signal>
<signal name="GPIO23">
<contactref element="RPI1" pad="16"/>
</signal>
<signal name="D1">
<contactref element="RPI1" pad="27"/>
<contactref element="D1" pad="1"/>
<contactref element="PLAYER1" pad="4"/>
</signal>
<signal name="GPIO12">
<contactref element="RPI1" pad="32"/>
</signal>
<signal name="+5V">
<contactref element="RPI1" pad="2"/>
<contactref element="RPI1" pad="4"/>
</signal>
<signal name="BCLK">
<contactref element="RPI1" pad="12"/>
</signal>
<signal name="B1">
<contactref element="RPI1" pad="35"/>
<contactref element="B1" pad="1"/>
</signal>
<signal name="DIN">
<contactref element="RPI1" pad="40"/>
</signal>
<signal name="L2">
<contactref element="RPI1" pad="19"/>
<contactref element="L2" pad="1"/>
<contactref element="PLAYER2" pad="2"/>
</signal>
<signal name="A2">
<contactref element="RPI1" pad="23"/>
<contactref element="A2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
