<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="42.2275" y1="89.535" x2="22.86" y2="89.535" width="0" layer="20"/>
<wire x1="22.86" y1="89.535" x2="21.59" y2="88.265" width="0" layer="20"/>
<wire x1="21.59" y1="88.265" x2="21.59" y2="74.93" width="0" layer="20"/>
<wire x1="20.32" y1="73.66" x2="8.255" y2="73.66" width="0" layer="20"/>
<wire x1="8.255" y1="73.66" x2="6.985" y2="72.39" width="0" layer="20"/>
<wire x1="6.985" y1="72.39" x2="6.985" y2="18.0975" width="0" layer="20"/>
<wire x1="6.985" y1="18.0975" x2="6.35" y2="17.4625" width="0" layer="20"/>
<wire x1="6.35" y1="17.4625" x2="-3.175" y2="17.4625" width="0" layer="20"/>
<wire x1="-3.175" y1="17.4625" x2="-3.81" y2="16.8275" width="0" layer="20"/>
<wire x1="-3.81" y1="16.8275" x2="-3.81" y2="-1.397" width="0" layer="20"/>
<wire x1="-3.81" y1="-1.397" x2="-3.175" y2="-2.032" width="0" layer="20"/>
<wire x1="-3.175" y1="-2.032" x2="14.605" y2="-2.032" width="0" layer="20"/>
<wire x1="14.605" y1="-2.032" x2="15.24" y2="-1.397" width="0" layer="20"/>
<wire x1="15.24" y1="-1.397" x2="15.24" y2="16.8275" width="0" layer="20"/>
<wire x1="15.24" y1="16.8275" x2="14.605" y2="17.4625" width="0" layer="20"/>
<wire x1="14.605" y1="17.4625" x2="10.795" y2="17.4625" width="0" layer="20"/>
<wire x1="10.795" y1="17.4625" x2="10.16" y2="18.0975" width="0" layer="20"/>
<wire x1="10.16" y1="18.0975" x2="10.16" y2="68.58" width="0" layer="20"/>
<wire x1="10.16" y1="68.58" x2="11.43" y2="69.85" width="0" layer="20"/>
<wire x1="11.43" y1="69.85" x2="24.13" y2="69.85" width="0" layer="20"/>
<wire x1="25.4" y1="71.12" x2="25.4" y2="85.09" width="0" layer="20"/>
<wire x1="25.4" y1="85.09" x2="26.67" y2="86.36" width="0" layer="20"/>
<wire x1="26.67" y1="86.36" x2="30.1625" y2="86.36" width="0" layer="20"/>
<wire x1="30.1625" y1="86.36" x2="30.1625" y2="77.47" width="0" layer="20"/>
<wire x1="30.1625" y1="77.47" x2="42.2275" y2="77.47" width="0" layer="20"/>
<wire x1="42.2275" y1="77.47" x2="42.2275" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="21.59" y1="74.93" x2="20.32" y2="73.66" width="0" layer="20"/>
<wire x1="24.13" y1="69.85" x2="25.4" y2="71.12" width="0" layer="20"/>
<wire x1="18.6055" y1="89.535" x2="-0.762" y2="89.535" width="0" layer="20"/>
<wire x1="-0.762" y1="89.535" x2="-2.032" y2="88.265" width="0" layer="20"/>
<wire x1="-2.032" y1="88.265" x2="-2.032" y2="74.93" width="0" layer="20"/>
<wire x1="-3.302" y1="73.66" x2="-15.367" y2="73.66" width="0" layer="20"/>
<wire x1="-15.367" y1="73.66" x2="-16.637" y2="72.39" width="0" layer="20"/>
<wire x1="-16.637" y1="72.39" x2="-16.637" y2="18.0975" width="0" layer="20"/>
<wire x1="-16.637" y1="18.0975" x2="-17.272" y2="17.4625" width="0" layer="20"/>
<wire x1="-17.272" y1="17.4625" x2="-26.797" y2="17.4625" width="0" layer="20"/>
<wire x1="-26.797" y1="17.4625" x2="-27.432" y2="16.8275" width="0" layer="20"/>
<wire x1="-27.432" y1="16.8275" x2="-27.432" y2="-1.397" width="0" layer="20"/>
<wire x1="-27.432" y1="-1.397" x2="-26.797" y2="-2.032" width="0" layer="20"/>
<wire x1="-26.797" y1="-2.032" x2="-9.017" y2="-2.032" width="0" layer="20"/>
<wire x1="-9.017" y1="-2.032" x2="-8.382" y2="-1.397" width="0" layer="20"/>
<wire x1="-8.382" y1="-1.397" x2="-8.382" y2="16.8275" width="0" layer="20"/>
<wire x1="-8.382" y1="16.8275" x2="-9.017" y2="17.4625" width="0" layer="20"/>
<wire x1="-9.017" y1="17.4625" x2="-12.827" y2="17.4625" width="0" layer="20"/>
<wire x1="-12.827" y1="17.4625" x2="-13.462" y2="18.0975" width="0" layer="20"/>
<wire x1="-13.462" y1="18.0975" x2="-13.462" y2="68.58" width="0" layer="20"/>
<wire x1="-13.462" y1="68.58" x2="-12.192" y2="69.85" width="0" layer="20"/>
<wire x1="-12.192" y1="69.85" x2="0.508" y2="69.85" width="0" layer="20"/>
<wire x1="1.778" y1="71.12" x2="1.778" y2="85.09" width="0" layer="20"/>
<wire x1="1.778" y1="85.09" x2="3.048" y2="86.36" width="0" layer="20"/>
<wire x1="3.048" y1="86.36" x2="6.5405" y2="86.36" width="0" layer="20"/>
<wire x1="6.5405" y1="86.36" x2="6.5405" y2="77.47" width="0" layer="20"/>
<wire x1="6.5405" y1="77.47" x2="18.6055" y2="77.47" width="0" layer="20"/>
<wire x1="18.6055" y1="77.47" x2="18.6055" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-2.032" y1="74.93" x2="-3.302" y2="73.66" width="0" layer="20"/>
<wire x1="0.508" y1="69.85" x2="1.778" y2="71.12" width="0" layer="20"/>
<wire x1="-5.0165" y1="89.535" x2="-24.384" y2="89.535" width="0" layer="20"/>
<wire x1="-24.384" y1="89.535" x2="-25.654" y2="88.265" width="0" layer="20"/>
<wire x1="-25.654" y1="88.265" x2="-25.654" y2="74.93" width="0" layer="20"/>
<wire x1="-26.924" y1="73.66" x2="-38.989" y2="73.66" width="0" layer="20"/>
<wire x1="-38.989" y1="73.66" x2="-40.259" y2="72.39" width="0" layer="20"/>
<wire x1="-40.259" y1="72.39" x2="-40.259" y2="18.0975" width="0" layer="20"/>
<wire x1="-40.259" y1="18.0975" x2="-40.894" y2="17.4625" width="0" layer="20"/>
<wire x1="-40.894" y1="17.4625" x2="-50.419" y2="17.4625" width="0" layer="20"/>
<wire x1="-50.419" y1="17.4625" x2="-51.054" y2="16.8275" width="0" layer="20"/>
<wire x1="-51.054" y1="16.8275" x2="-51.054" y2="-1.397" width="0" layer="20"/>
<wire x1="-51.054" y1="-1.397" x2="-50.419" y2="-2.032" width="0" layer="20"/>
<wire x1="-50.419" y1="-2.032" x2="-32.639" y2="-2.032" width="0" layer="20"/>
<wire x1="-32.639" y1="-2.032" x2="-32.004" y2="-1.397" width="0" layer="20"/>
<wire x1="-32.004" y1="-1.397" x2="-32.004" y2="16.8275" width="0" layer="20"/>
<wire x1="-32.004" y1="16.8275" x2="-32.639" y2="17.4625" width="0" layer="20"/>
<wire x1="-32.639" y1="17.4625" x2="-36.449" y2="17.4625" width="0" layer="20"/>
<wire x1="-36.449" y1="17.4625" x2="-37.084" y2="18.0975" width="0" layer="20"/>
<wire x1="-37.084" y1="18.0975" x2="-37.084" y2="68.58" width="0" layer="20"/>
<wire x1="-37.084" y1="68.58" x2="-35.814" y2="69.85" width="0" layer="20"/>
<wire x1="-35.814" y1="69.85" x2="-23.114" y2="69.85" width="0" layer="20"/>
<wire x1="-21.844" y1="71.12" x2="-21.844" y2="85.09" width="0" layer="20"/>
<wire x1="-21.844" y1="85.09" x2="-20.574" y2="86.36" width="0" layer="20"/>
<wire x1="-20.574" y1="86.36" x2="-17.0815" y2="86.36" width="0" layer="20"/>
<wire x1="-17.0815" y1="86.36" x2="-17.0815" y2="77.47" width="0" layer="20"/>
<wire x1="-17.0815" y1="77.47" x2="-5.0165" y2="77.47" width="0" layer="20"/>
<wire x1="-5.0165" y1="77.47" x2="-5.0165" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-25.654" y1="74.93" x2="-26.924" y2="73.66" width="0" layer="20"/>
<wire x1="-23.114" y1="69.85" x2="-21.844" y2="71.12" width="0" layer="20"/>
<wire x1="-28.6385" y1="89.535" x2="-48.006" y2="89.535" width="0" layer="20"/>
<wire x1="-48.006" y1="89.535" x2="-49.276" y2="88.265" width="0" layer="20"/>
<wire x1="-49.276" y1="88.265" x2="-49.276" y2="74.93" width="0" layer="20"/>
<wire x1="-50.546" y1="73.66" x2="-62.611" y2="73.66" width="0" layer="20"/>
<wire x1="-62.611" y1="73.66" x2="-63.881" y2="72.39" width="0" layer="20"/>
<wire x1="-63.881" y1="72.39" x2="-63.881" y2="18.0975" width="0" layer="20"/>
<wire x1="-63.881" y1="18.0975" x2="-64.516" y2="17.4625" width="0" layer="20"/>
<wire x1="-64.516" y1="17.4625" x2="-74.041" y2="17.4625" width="0" layer="20"/>
<wire x1="-74.041" y1="17.4625" x2="-74.676" y2="16.8275" width="0" layer="20"/>
<wire x1="-74.676" y1="16.8275" x2="-74.676" y2="-1.397" width="0" layer="20"/>
<wire x1="-74.676" y1="-1.397" x2="-74.041" y2="-2.032" width="0" layer="20"/>
<wire x1="-74.041" y1="-2.032" x2="-56.261" y2="-2.032" width="0" layer="20"/>
<wire x1="-56.261" y1="-2.032" x2="-55.626" y2="-1.397" width="0" layer="20"/>
<wire x1="-55.626" y1="-1.397" x2="-55.626" y2="16.8275" width="0" layer="20"/>
<wire x1="-55.626" y1="16.8275" x2="-56.261" y2="17.4625" width="0" layer="20"/>
<wire x1="-56.261" y1="17.4625" x2="-60.071" y2="17.4625" width="0" layer="20"/>
<wire x1="-60.071" y1="17.4625" x2="-60.706" y2="18.0975" width="0" layer="20"/>
<wire x1="-60.706" y1="18.0975" x2="-60.706" y2="68.58" width="0" layer="20"/>
<wire x1="-60.706" y1="68.58" x2="-59.436" y2="69.85" width="0" layer="20"/>
<wire x1="-59.436" y1="69.85" x2="-46.736" y2="69.85" width="0" layer="20"/>
<wire x1="-45.466" y1="71.12" x2="-45.466" y2="85.09" width="0" layer="20"/>
<wire x1="-45.466" y1="85.09" x2="-44.196" y2="86.36" width="0" layer="20"/>
<wire x1="-44.196" y1="86.36" x2="-40.7035" y2="86.36" width="0" layer="20"/>
<wire x1="-40.7035" y1="86.36" x2="-40.7035" y2="77.47" width="0" layer="20"/>
<wire x1="-40.7035" y1="77.47" x2="-28.6385" y2="77.47" width="0" layer="20"/>
<wire x1="-28.6385" y1="77.47" x2="-28.6385" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-49.276" y1="74.93" x2="-50.546" y2="73.66" width="0" layer="20"/>
<wire x1="-46.736" y1="69.85" x2="-45.466" y2="71.12" width="0" layer="20"/>
<wire x1="-52.2605" y1="89.535" x2="-71.628" y2="89.535" width="0" layer="20"/>
<wire x1="-71.628" y1="89.535" x2="-72.898" y2="88.265" width="0" layer="20"/>
<wire x1="-72.898" y1="88.265" x2="-72.898" y2="74.93" width="0" layer="20"/>
<wire x1="-74.168" y1="73.66" x2="-86.233" y2="73.66" width="0" layer="20"/>
<wire x1="-86.233" y1="73.66" x2="-87.503" y2="72.39" width="0" layer="20"/>
<wire x1="-87.503" y1="72.39" x2="-87.503" y2="18.0975" width="0" layer="20"/>
<wire x1="-87.503" y1="18.0975" x2="-88.138" y2="17.4625" width="0" layer="20"/>
<wire x1="-88.138" y1="17.4625" x2="-97.663" y2="17.4625" width="0" layer="20"/>
<wire x1="-97.663" y1="17.4625" x2="-98.298" y2="16.8275" width="0" layer="20"/>
<wire x1="-98.298" y1="16.8275" x2="-98.298" y2="-1.397" width="0" layer="20"/>
<wire x1="-98.298" y1="-1.397" x2="-97.663" y2="-2.032" width="0" layer="20"/>
<wire x1="-97.663" y1="-2.032" x2="-79.883" y2="-2.032" width="0" layer="20"/>
<wire x1="-79.883" y1="-2.032" x2="-79.248" y2="-1.397" width="0" layer="20"/>
<wire x1="-79.248" y1="-1.397" x2="-79.248" y2="16.8275" width="0" layer="20"/>
<wire x1="-79.248" y1="16.8275" x2="-79.883" y2="17.4625" width="0" layer="20"/>
<wire x1="-79.883" y1="17.4625" x2="-83.693" y2="17.4625" width="0" layer="20"/>
<wire x1="-83.693" y1="17.4625" x2="-84.328" y2="18.0975" width="0" layer="20"/>
<wire x1="-84.328" y1="18.0975" x2="-84.328" y2="68.58" width="0" layer="20"/>
<wire x1="-84.328" y1="68.58" x2="-83.058" y2="69.85" width="0" layer="20"/>
<wire x1="-83.058" y1="69.85" x2="-70.358" y2="69.85" width="0" layer="20"/>
<wire x1="-69.088" y1="71.12" x2="-69.088" y2="85.09" width="0" layer="20"/>
<wire x1="-69.088" y1="85.09" x2="-67.818" y2="86.36" width="0" layer="20"/>
<wire x1="-67.818" y1="86.36" x2="-64.3255" y2="86.36" width="0" layer="20"/>
<wire x1="-64.3255" y1="86.36" x2="-64.3255" y2="77.47" width="0" layer="20"/>
<wire x1="-64.3255" y1="77.47" x2="-52.2605" y2="77.47" width="0" layer="20"/>
<wire x1="-52.2605" y1="77.47" x2="-52.2605" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-72.898" y1="74.93" x2="-74.168" y2="73.66" width="0" layer="20"/>
<wire x1="-70.358" y1="69.85" x2="-69.088" y2="71.12" width="0" layer="20"/>
<wire x1="-75.8825" y1="89.535" x2="-95.25" y2="89.535" width="0" layer="20"/>
<wire x1="-95.25" y1="89.535" x2="-96.52" y2="88.265" width="0" layer="20"/>
<wire x1="-96.52" y1="88.265" x2="-96.52" y2="74.93" width="0" layer="20"/>
<wire x1="-97.79" y1="73.66" x2="-109.855" y2="73.66" width="0" layer="20"/>
<wire x1="-109.855" y1="73.66" x2="-111.125" y2="72.39" width="0" layer="20"/>
<wire x1="-111.125" y1="72.39" x2="-111.125" y2="18.0975" width="0" layer="20"/>
<wire x1="-111.125" y1="18.0975" x2="-111.76" y2="17.4625" width="0" layer="20"/>
<wire x1="-111.76" y1="17.4625" x2="-121.285" y2="17.4625" width="0" layer="20"/>
<wire x1="-121.285" y1="17.4625" x2="-121.92" y2="16.8275" width="0" layer="20"/>
<wire x1="-121.92" y1="16.8275" x2="-121.92" y2="-1.397" width="0" layer="20"/>
<wire x1="-121.92" y1="-1.397" x2="-121.285" y2="-2.032" width="0" layer="20"/>
<wire x1="-121.285" y1="-2.032" x2="-103.505" y2="-2.032" width="0" layer="20"/>
<wire x1="-103.505" y1="-2.032" x2="-102.87" y2="-1.397" width="0" layer="20"/>
<wire x1="-102.87" y1="-1.397" x2="-102.87" y2="16.8275" width="0" layer="20"/>
<wire x1="-102.87" y1="16.8275" x2="-103.505" y2="17.4625" width="0" layer="20"/>
<wire x1="-103.505" y1="17.4625" x2="-107.315" y2="17.4625" width="0" layer="20"/>
<wire x1="-107.315" y1="17.4625" x2="-107.95" y2="18.0975" width="0" layer="20"/>
<wire x1="-107.95" y1="18.0975" x2="-107.95" y2="68.58" width="0" layer="20"/>
<wire x1="-107.95" y1="68.58" x2="-106.68" y2="69.85" width="0" layer="20"/>
<wire x1="-106.68" y1="69.85" x2="-93.98" y2="69.85" width="0" layer="20"/>
<wire x1="-92.71" y1="71.12" x2="-92.71" y2="85.09" width="0" layer="20"/>
<wire x1="-92.71" y1="85.09" x2="-91.44" y2="86.36" width="0" layer="20"/>
<wire x1="-91.44" y1="86.36" x2="-87.9475" y2="86.36" width="0" layer="20"/>
<wire x1="-87.9475" y1="86.36" x2="-87.9475" y2="77.47" width="0" layer="20"/>
<wire x1="-87.9475" y1="77.47" x2="-75.8825" y2="77.47" width="0" layer="20"/>
<wire x1="-75.8825" y1="77.47" x2="-75.8825" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-96.52" y1="74.93" x2="-97.79" y2="73.66" width="0" layer="20"/>
<wire x1="-93.98" y1="69.85" x2="-92.71" y2="71.12" width="0" layer="20"/>
<wire x1="-99.5045" y1="89.535" x2="-118.872" y2="89.535" width="0" layer="20"/>
<wire x1="-118.872" y1="89.535" x2="-120.142" y2="88.265" width="0" layer="20"/>
<wire x1="-120.142" y1="88.265" x2="-120.142" y2="74.93" width="0" layer="20"/>
<wire x1="-121.412" y1="73.66" x2="-133.477" y2="73.66" width="0" layer="20"/>
<wire x1="-133.477" y1="73.66" x2="-134.747" y2="72.39" width="0" layer="20"/>
<wire x1="-134.747" y1="72.39" x2="-134.747" y2="18.0975" width="0" layer="20"/>
<wire x1="-134.747" y1="18.0975" x2="-135.382" y2="17.4625" width="0" layer="20"/>
<wire x1="-135.382" y1="17.4625" x2="-144.907" y2="17.4625" width="0" layer="20"/>
<wire x1="-144.907" y1="17.4625" x2="-145.542" y2="16.8275" width="0" layer="20"/>
<wire x1="-145.542" y1="16.8275" x2="-145.542" y2="-1.397" width="0" layer="20"/>
<wire x1="-145.542" y1="-1.397" x2="-144.907" y2="-2.032" width="0" layer="20"/>
<wire x1="-144.907" y1="-2.032" x2="-127.127" y2="-2.032" width="0" layer="20"/>
<wire x1="-127.127" y1="-2.032" x2="-126.492" y2="-1.397" width="0" layer="20"/>
<wire x1="-126.492" y1="-1.397" x2="-126.492" y2="16.8275" width="0" layer="20"/>
<wire x1="-126.492" y1="16.8275" x2="-127.127" y2="17.4625" width="0" layer="20"/>
<wire x1="-127.127" y1="17.4625" x2="-130.937" y2="17.4625" width="0" layer="20"/>
<wire x1="-130.937" y1="17.4625" x2="-131.572" y2="18.0975" width="0" layer="20"/>
<wire x1="-131.572" y1="18.0975" x2="-131.572" y2="68.58" width="0" layer="20"/>
<wire x1="-131.572" y1="68.58" x2="-130.302" y2="69.85" width="0" layer="20"/>
<wire x1="-130.302" y1="69.85" x2="-117.602" y2="69.85" width="0" layer="20"/>
<wire x1="-116.332" y1="71.12" x2="-116.332" y2="85.09" width="0" layer="20"/>
<wire x1="-116.332" y1="85.09" x2="-115.062" y2="86.36" width="0" layer="20"/>
<wire x1="-115.062" y1="86.36" x2="-111.5695" y2="86.36" width="0" layer="20"/>
<wire x1="-111.5695" y1="86.36" x2="-111.5695" y2="77.47" width="0" layer="20"/>
<wire x1="-111.5695" y1="77.47" x2="-99.5045" y2="77.47" width="0" layer="20"/>
<wire x1="-99.5045" y1="77.47" x2="-99.5045" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-120.142" y1="74.93" x2="-121.412" y2="73.66" width="0" layer="20"/>
<wire x1="-117.602" y1="69.85" x2="-116.332" y2="71.12" width="0" layer="20"/>
<wire x1="-123.1265" y1="89.535" x2="-142.494" y2="89.535" width="0" layer="20"/>
<wire x1="-142.494" y1="89.535" x2="-143.764" y2="88.265" width="0" layer="20"/>
<wire x1="-143.764" y1="88.265" x2="-143.764" y2="74.93" width="0" layer="20"/>
<wire x1="-145.034" y1="73.66" x2="-157.099" y2="73.66" width="0" layer="20"/>
<wire x1="-157.099" y1="73.66" x2="-158.369" y2="72.39" width="0" layer="20"/>
<wire x1="-158.369" y1="72.39" x2="-158.369" y2="18.0975" width="0" layer="20"/>
<wire x1="-158.369" y1="18.0975" x2="-159.004" y2="17.4625" width="0" layer="20"/>
<wire x1="-159.004" y1="17.4625" x2="-168.529" y2="17.4625" width="0" layer="20"/>
<wire x1="-168.529" y1="17.4625" x2="-169.164" y2="16.8275" width="0" layer="20"/>
<wire x1="-169.164" y1="16.8275" x2="-169.164" y2="-1.397" width="0" layer="20"/>
<wire x1="-169.164" y1="-1.397" x2="-168.529" y2="-2.032" width="0" layer="20"/>
<wire x1="-168.529" y1="-2.032" x2="-150.749" y2="-2.032" width="0" layer="20"/>
<wire x1="-150.749" y1="-2.032" x2="-150.114" y2="-1.397" width="0" layer="20"/>
<wire x1="-150.114" y1="-1.397" x2="-150.114" y2="16.8275" width="0" layer="20"/>
<wire x1="-150.114" y1="16.8275" x2="-150.749" y2="17.4625" width="0" layer="20"/>
<wire x1="-150.749" y1="17.4625" x2="-154.559" y2="17.4625" width="0" layer="20"/>
<wire x1="-154.559" y1="17.4625" x2="-155.194" y2="18.0975" width="0" layer="20"/>
<wire x1="-155.194" y1="18.0975" x2="-155.194" y2="68.58" width="0" layer="20"/>
<wire x1="-155.194" y1="68.58" x2="-153.924" y2="69.85" width="0" layer="20"/>
<wire x1="-153.924" y1="69.85" x2="-141.224" y2="69.85" width="0" layer="20"/>
<wire x1="-139.954" y1="71.12" x2="-139.954" y2="85.09" width="0" layer="20"/>
<wire x1="-139.954" y1="85.09" x2="-138.684" y2="86.36" width="0" layer="20"/>
<wire x1="-138.684" y1="86.36" x2="-135.1915" y2="86.36" width="0" layer="20"/>
<wire x1="-135.1915" y1="86.36" x2="-135.1915" y2="77.47" width="0" layer="20"/>
<wire x1="-135.1915" y1="77.47" x2="-123.1265" y2="77.47" width="0" layer="20"/>
<wire x1="-123.1265" y1="77.47" x2="-123.1265" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-143.764" y1="74.93" x2="-145.034" y2="73.66" width="0" layer="20"/>
<wire x1="-141.224" y1="69.85" x2="-139.954" y2="71.12" width="0" layer="20"/>
<wire x1="-146.7485" y1="89.535" x2="-166.116" y2="89.535" width="0" layer="20"/>
<wire x1="-166.116" y1="89.535" x2="-167.386" y2="88.265" width="0" layer="20"/>
<wire x1="-167.386" y1="88.265" x2="-167.386" y2="74.93" width="0" layer="20"/>
<wire x1="-168.656" y1="73.66" x2="-180.721" y2="73.66" width="0" layer="20"/>
<wire x1="-180.721" y1="73.66" x2="-181.991" y2="72.39" width="0" layer="20"/>
<wire x1="-181.991" y1="72.39" x2="-181.991" y2="18.0975" width="0" layer="20"/>
<wire x1="-181.991" y1="18.0975" x2="-182.626" y2="17.4625" width="0" layer="20"/>
<wire x1="-182.626" y1="17.4625" x2="-192.151" y2="17.4625" width="0" layer="20"/>
<wire x1="-192.151" y1="17.4625" x2="-192.786" y2="16.8275" width="0" layer="20"/>
<wire x1="-192.786" y1="16.8275" x2="-192.786" y2="-1.397" width="0" layer="20"/>
<wire x1="-192.786" y1="-1.397" x2="-192.151" y2="-2.032" width="0" layer="20"/>
<wire x1="-192.151" y1="-2.032" x2="-174.371" y2="-2.032" width="0" layer="20"/>
<wire x1="-174.371" y1="-2.032" x2="-173.736" y2="-1.397" width="0" layer="20"/>
<wire x1="-173.736" y1="-1.397" x2="-173.736" y2="16.8275" width="0" layer="20"/>
<wire x1="-173.736" y1="16.8275" x2="-174.371" y2="17.4625" width="0" layer="20"/>
<wire x1="-174.371" y1="17.4625" x2="-178.181" y2="17.4625" width="0" layer="20"/>
<wire x1="-178.181" y1="17.4625" x2="-178.816" y2="18.0975" width="0" layer="20"/>
<wire x1="-178.816" y1="18.0975" x2="-178.816" y2="68.58" width="0" layer="20"/>
<wire x1="-178.816" y1="68.58" x2="-177.546" y2="69.85" width="0" layer="20"/>
<wire x1="-177.546" y1="69.85" x2="-164.846" y2="69.85" width="0" layer="20"/>
<wire x1="-163.576" y1="71.12" x2="-163.576" y2="85.09" width="0" layer="20"/>
<wire x1="-163.576" y1="85.09" x2="-162.306" y2="86.36" width="0" layer="20"/>
<wire x1="-162.306" y1="86.36" x2="-158.8135" y2="86.36" width="0" layer="20"/>
<wire x1="-158.8135" y1="86.36" x2="-158.8135" y2="77.47" width="0" layer="20"/>
<wire x1="-158.8135" y1="77.47" x2="-146.7485" y2="77.47" width="0" layer="20"/>
<wire x1="-146.7485" y1="77.47" x2="-146.7485" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-167.386" y1="74.93" x2="-168.656" y2="73.66" width="0" layer="20"/>
<wire x1="-164.846" y1="69.85" x2="-163.576" y2="71.12" width="0" layer="20"/>
<wire x1="-170.3705" y1="89.535" x2="-189.738" y2="89.535" width="0" layer="20"/>
<wire x1="-189.738" y1="89.535" x2="-191.008" y2="88.265" width="0" layer="20"/>
<wire x1="-191.008" y1="88.265" x2="-191.008" y2="74.93" width="0" layer="20"/>
<wire x1="-192.278" y1="73.66" x2="-204.343" y2="73.66" width="0" layer="20"/>
<wire x1="-204.343" y1="73.66" x2="-205.613" y2="72.39" width="0" layer="20"/>
<wire x1="-205.613" y1="72.39" x2="-205.613" y2="18.0975" width="0" layer="20"/>
<wire x1="-205.613" y1="18.0975" x2="-206.248" y2="17.4625" width="0" layer="20"/>
<wire x1="-206.248" y1="17.4625" x2="-215.773" y2="17.4625" width="0" layer="20"/>
<wire x1="-215.773" y1="17.4625" x2="-216.408" y2="16.8275" width="0" layer="20"/>
<wire x1="-216.408" y1="16.8275" x2="-216.408" y2="-1.397" width="0" layer="20"/>
<wire x1="-216.408" y1="-1.397" x2="-215.773" y2="-2.032" width="0" layer="20"/>
<wire x1="-215.773" y1="-2.032" x2="-197.993" y2="-2.032" width="0" layer="20"/>
<wire x1="-197.993" y1="-2.032" x2="-197.358" y2="-1.397" width="0" layer="20"/>
<wire x1="-197.358" y1="-1.397" x2="-197.358" y2="16.8275" width="0" layer="20"/>
<wire x1="-197.358" y1="16.8275" x2="-197.993" y2="17.4625" width="0" layer="20"/>
<wire x1="-197.993" y1="17.4625" x2="-201.803" y2="17.4625" width="0" layer="20"/>
<wire x1="-201.803" y1="17.4625" x2="-202.438" y2="18.0975" width="0" layer="20"/>
<wire x1="-202.438" y1="18.0975" x2="-202.438" y2="68.58" width="0" layer="20"/>
<wire x1="-202.438" y1="68.58" x2="-201.168" y2="69.85" width="0" layer="20"/>
<wire x1="-201.168" y1="69.85" x2="-188.468" y2="69.85" width="0" layer="20"/>
<wire x1="-187.198" y1="71.12" x2="-187.198" y2="85.09" width="0" layer="20"/>
<wire x1="-187.198" y1="85.09" x2="-185.928" y2="86.36" width="0" layer="20"/>
<wire x1="-185.928" y1="86.36" x2="-182.4355" y2="86.36" width="0" layer="20"/>
<wire x1="-182.4355" y1="86.36" x2="-182.4355" y2="77.47" width="0" layer="20"/>
<wire x1="-182.4355" y1="77.47" x2="-170.3705" y2="77.47" width="0" layer="20"/>
<wire x1="-170.3705" y1="77.47" x2="-170.3705" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-191.008" y1="74.93" x2="-192.278" y2="73.66" width="0" layer="20"/>
<wire x1="-188.468" y1="69.85" x2="-187.198" y2="71.12" width="0" layer="20"/>
<wire x1="-193.9925" y1="89.535" x2="-213.36" y2="89.535" width="0" layer="20"/>
<wire x1="-213.36" y1="89.535" x2="-214.63" y2="88.265" width="0" layer="20"/>
<wire x1="-214.63" y1="88.265" x2="-214.63" y2="74.93" width="0" layer="20"/>
<wire x1="-215.9" y1="73.66" x2="-227.965" y2="73.66" width="0" layer="20"/>
<wire x1="-227.965" y1="73.66" x2="-229.235" y2="72.39" width="0" layer="20"/>
<wire x1="-229.235" y1="72.39" x2="-229.235" y2="18.0975" width="0" layer="20"/>
<wire x1="-229.235" y1="18.0975" x2="-229.87" y2="17.4625" width="0" layer="20"/>
<wire x1="-229.87" y1="17.4625" x2="-239.395" y2="17.4625" width="0" layer="20"/>
<wire x1="-239.395" y1="17.4625" x2="-240.03" y2="16.8275" width="0" layer="20"/>
<wire x1="-240.03" y1="16.8275" x2="-240.03" y2="-1.397" width="0" layer="20"/>
<wire x1="-240.03" y1="-1.397" x2="-239.395" y2="-2.032" width="0" layer="20"/>
<wire x1="-239.395" y1="-2.032" x2="-221.615" y2="-2.032" width="0" layer="20"/>
<wire x1="-221.615" y1="-2.032" x2="-220.98" y2="-1.397" width="0" layer="20"/>
<wire x1="-220.98" y1="-1.397" x2="-220.98" y2="16.8275" width="0" layer="20"/>
<wire x1="-220.98" y1="16.8275" x2="-221.615" y2="17.4625" width="0" layer="20"/>
<wire x1="-221.615" y1="17.4625" x2="-225.425" y2="17.4625" width="0" layer="20"/>
<wire x1="-225.425" y1="17.4625" x2="-226.06" y2="18.0975" width="0" layer="20"/>
<wire x1="-226.06" y1="18.0975" x2="-226.06" y2="68.58" width="0" layer="20"/>
<wire x1="-226.06" y1="68.58" x2="-224.79" y2="69.85" width="0" layer="20"/>
<wire x1="-224.79" y1="69.85" x2="-212.09" y2="69.85" width="0" layer="20"/>
<wire x1="-210.82" y1="71.12" x2="-210.82" y2="85.09" width="0" layer="20"/>
<wire x1="-210.82" y1="85.09" x2="-209.55" y2="86.36" width="0" layer="20"/>
<wire x1="-209.55" y1="86.36" x2="-206.0575" y2="86.36" width="0" layer="20"/>
<wire x1="-206.0575" y1="86.36" x2="-206.0575" y2="77.47" width="0" layer="20"/>
<wire x1="-206.0575" y1="77.47" x2="-193.9925" y2="77.47" width="0" layer="20"/>
<wire x1="-193.9925" y1="77.47" x2="-193.9925" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-214.63" y1="74.93" x2="-215.9" y2="73.66" width="0" layer="20"/>
<wire x1="-212.09" y1="69.85" x2="-210.82" y2="71.12" width="0" layer="20"/>
<wire x1="-217.6145" y1="89.535" x2="-236.982" y2="89.535" width="0" layer="20"/>
<wire x1="-236.982" y1="89.535" x2="-238.252" y2="88.265" width="0" layer="20"/>
<wire x1="-238.252" y1="88.265" x2="-238.252" y2="74.93" width="0" layer="20"/>
<wire x1="-239.522" y1="73.66" x2="-251.587" y2="73.66" width="0" layer="20"/>
<wire x1="-251.587" y1="73.66" x2="-252.857" y2="72.39" width="0" layer="20"/>
<wire x1="-252.857" y1="72.39" x2="-252.857" y2="18.0975" width="0" layer="20"/>
<wire x1="-252.857" y1="18.0975" x2="-253.492" y2="17.4625" width="0" layer="20"/>
<wire x1="-253.492" y1="17.4625" x2="-263.017" y2="17.4625" width="0" layer="20"/>
<wire x1="-263.017" y1="17.4625" x2="-263.652" y2="16.8275" width="0" layer="20"/>
<wire x1="-263.652" y1="16.8275" x2="-263.652" y2="-1.397" width="0" layer="20"/>
<wire x1="-263.652" y1="-1.397" x2="-263.017" y2="-2.032" width="0" layer="20"/>
<wire x1="-263.017" y1="-2.032" x2="-245.237" y2="-2.032" width="0" layer="20"/>
<wire x1="-245.237" y1="-2.032" x2="-244.602" y2="-1.397" width="0" layer="20"/>
<wire x1="-244.602" y1="-1.397" x2="-244.602" y2="16.8275" width="0" layer="20"/>
<wire x1="-244.602" y1="16.8275" x2="-245.237" y2="17.4625" width="0" layer="20"/>
<wire x1="-245.237" y1="17.4625" x2="-249.047" y2="17.4625" width="0" layer="20"/>
<wire x1="-249.047" y1="17.4625" x2="-249.682" y2="18.0975" width="0" layer="20"/>
<wire x1="-249.682" y1="18.0975" x2="-249.682" y2="68.58" width="0" layer="20"/>
<wire x1="-249.682" y1="68.58" x2="-248.412" y2="69.85" width="0" layer="20"/>
<wire x1="-248.412" y1="69.85" x2="-235.712" y2="69.85" width="0" layer="20"/>
<wire x1="-234.442" y1="71.12" x2="-234.442" y2="85.09" width="0" layer="20"/>
<wire x1="-234.442" y1="85.09" x2="-233.172" y2="86.36" width="0" layer="20"/>
<wire x1="-233.172" y1="86.36" x2="-229.6795" y2="86.36" width="0" layer="20"/>
<wire x1="-229.6795" y1="86.36" x2="-229.6795" y2="77.47" width="0" layer="20"/>
<wire x1="-229.6795" y1="77.47" x2="-217.6145" y2="77.47" width="0" layer="20"/>
<wire x1="-217.6145" y1="77.47" x2="-217.6145" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-238.252" y1="74.93" x2="-239.522" y2="73.66" width="0" layer="20"/>
<wire x1="-235.712" y1="69.85" x2="-234.442" y2="71.12" width="0" layer="20"/>
<wire x1="-241.2365" y1="89.535" x2="-260.604" y2="89.535" width="0" layer="20"/>
<wire x1="-260.604" y1="89.535" x2="-261.874" y2="88.265" width="0" layer="20"/>
<wire x1="-261.874" y1="88.265" x2="-261.874" y2="74.93" width="0" layer="20"/>
<wire x1="-263.144" y1="73.66" x2="-275.209" y2="73.66" width="0" layer="20"/>
<wire x1="-275.209" y1="73.66" x2="-276.479" y2="72.39" width="0" layer="20"/>
<wire x1="-276.479" y1="72.39" x2="-276.479" y2="18.0975" width="0" layer="20"/>
<wire x1="-276.479" y1="18.0975" x2="-277.114" y2="17.4625" width="0" layer="20"/>
<wire x1="-277.114" y1="17.4625" x2="-286.639" y2="17.4625" width="0" layer="20"/>
<wire x1="-286.639" y1="17.4625" x2="-287.274" y2="16.8275" width="0" layer="20"/>
<wire x1="-287.274" y1="16.8275" x2="-287.274" y2="-1.397" width="0" layer="20"/>
<wire x1="-287.274" y1="-1.397" x2="-286.639" y2="-2.032" width="0" layer="20"/>
<wire x1="-286.639" y1="-2.032" x2="-268.859" y2="-2.032" width="0" layer="20"/>
<wire x1="-268.859" y1="-2.032" x2="-268.224" y2="-1.397" width="0" layer="20"/>
<wire x1="-268.224" y1="-1.397" x2="-268.224" y2="16.8275" width="0" layer="20"/>
<wire x1="-268.224" y1="16.8275" x2="-268.859" y2="17.4625" width="0" layer="20"/>
<wire x1="-268.859" y1="17.4625" x2="-272.669" y2="17.4625" width="0" layer="20"/>
<wire x1="-272.669" y1="17.4625" x2="-273.304" y2="18.0975" width="0" layer="20"/>
<wire x1="-273.304" y1="18.0975" x2="-273.304" y2="68.58" width="0" layer="20"/>
<wire x1="-273.304" y1="68.58" x2="-272.034" y2="69.85" width="0" layer="20"/>
<wire x1="-272.034" y1="69.85" x2="-259.334" y2="69.85" width="0" layer="20"/>
<wire x1="-258.064" y1="71.12" x2="-258.064" y2="85.09" width="0" layer="20"/>
<wire x1="-258.064" y1="85.09" x2="-256.794" y2="86.36" width="0" layer="20"/>
<wire x1="-256.794" y1="86.36" x2="-253.3015" y2="86.36" width="0" layer="20"/>
<wire x1="-253.3015" y1="86.36" x2="-253.3015" y2="77.47" width="0" layer="20"/>
<wire x1="-253.3015" y1="77.47" x2="-241.2365" y2="77.47" width="0" layer="20"/>
<wire x1="-241.2365" y1="77.47" x2="-241.2365" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-261.874" y1="74.93" x2="-263.144" y2="73.66" width="0" layer="20"/>
<wire x1="-259.334" y1="69.85" x2="-258.064" y2="71.12" width="0" layer="20"/>
<wire x1="-264.8585" y1="89.535" x2="-284.226" y2="89.535" width="0" layer="20"/>
<wire x1="-284.226" y1="89.535" x2="-285.496" y2="88.265" width="0" layer="20"/>
<wire x1="-285.496" y1="88.265" x2="-285.496" y2="74.93" width="0" layer="20"/>
<wire x1="-286.766" y1="73.66" x2="-298.831" y2="73.66" width="0" layer="20"/>
<wire x1="-298.831" y1="73.66" x2="-300.101" y2="72.39" width="0" layer="20"/>
<wire x1="-300.101" y1="72.39" x2="-300.101" y2="18.0975" width="0" layer="20"/>
<wire x1="-300.101" y1="18.0975" x2="-300.736" y2="17.4625" width="0" layer="20"/>
<wire x1="-300.736" y1="17.4625" x2="-310.261" y2="17.4625" width="0" layer="20"/>
<wire x1="-310.261" y1="17.4625" x2="-310.896" y2="16.8275" width="0" layer="20"/>
<wire x1="-310.896" y1="16.8275" x2="-310.896" y2="-1.397" width="0" layer="20"/>
<wire x1="-310.896" y1="-1.397" x2="-310.261" y2="-2.032" width="0" layer="20"/>
<wire x1="-310.261" y1="-2.032" x2="-292.481" y2="-2.032" width="0" layer="20"/>
<wire x1="-292.481" y1="-2.032" x2="-291.846" y2="-1.397" width="0" layer="20"/>
<wire x1="-291.846" y1="-1.397" x2="-291.846" y2="16.8275" width="0" layer="20"/>
<wire x1="-291.846" y1="16.8275" x2="-292.481" y2="17.4625" width="0" layer="20"/>
<wire x1="-292.481" y1="17.4625" x2="-296.291" y2="17.4625" width="0" layer="20"/>
<wire x1="-296.291" y1="17.4625" x2="-296.926" y2="18.0975" width="0" layer="20"/>
<wire x1="-296.926" y1="18.0975" x2="-296.926" y2="68.58" width="0" layer="20"/>
<wire x1="-296.926" y1="68.58" x2="-295.656" y2="69.85" width="0" layer="20"/>
<wire x1="-295.656" y1="69.85" x2="-282.956" y2="69.85" width="0" layer="20"/>
<wire x1="-281.686" y1="71.12" x2="-281.686" y2="85.09" width="0" layer="20"/>
<wire x1="-281.686" y1="85.09" x2="-280.416" y2="86.36" width="0" layer="20"/>
<wire x1="-280.416" y1="86.36" x2="-276.9235" y2="86.36" width="0" layer="20"/>
<wire x1="-276.9235" y1="86.36" x2="-276.9235" y2="77.47" width="0" layer="20"/>
<wire x1="-276.9235" y1="77.47" x2="-264.8585" y2="77.47" width="0" layer="20"/>
<wire x1="-264.8585" y1="77.47" x2="-264.8585" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-285.496" y1="74.93" x2="-286.766" y2="73.66" width="0" layer="20"/>
<wire x1="-282.956" y1="69.85" x2="-281.686" y2="71.12" width="0" layer="20"/>
<wire x1="-288.4805" y1="89.535" x2="-307.848" y2="89.535" width="0" layer="20"/>
<wire x1="-307.848" y1="89.535" x2="-309.118" y2="88.265" width="0" layer="20"/>
<wire x1="-309.118" y1="88.265" x2="-309.118" y2="74.93" width="0" layer="20"/>
<wire x1="-310.388" y1="73.66" x2="-322.453" y2="73.66" width="0" layer="20"/>
<wire x1="-322.453" y1="73.66" x2="-323.723" y2="72.39" width="0" layer="20"/>
<wire x1="-323.723" y1="72.39" x2="-323.723" y2="18.0975" width="0" layer="20"/>
<wire x1="-323.723" y1="18.0975" x2="-324.358" y2="17.4625" width="0" layer="20"/>
<wire x1="-324.358" y1="17.4625" x2="-333.883" y2="17.4625" width="0" layer="20"/>
<wire x1="-333.883" y1="17.4625" x2="-334.518" y2="16.8275" width="0" layer="20"/>
<wire x1="-334.518" y1="16.8275" x2="-334.518" y2="-1.397" width="0" layer="20"/>
<wire x1="-334.518" y1="-1.397" x2="-333.883" y2="-2.032" width="0" layer="20"/>
<wire x1="-333.883" y1="-2.032" x2="-316.103" y2="-2.032" width="0" layer="20"/>
<wire x1="-316.103" y1="-2.032" x2="-315.468" y2="-1.397" width="0" layer="20"/>
<wire x1="-315.468" y1="-1.397" x2="-315.468" y2="16.8275" width="0" layer="20"/>
<wire x1="-315.468" y1="16.8275" x2="-316.103" y2="17.4625" width="0" layer="20"/>
<wire x1="-316.103" y1="17.4625" x2="-319.913" y2="17.4625" width="0" layer="20"/>
<wire x1="-319.913" y1="17.4625" x2="-320.548" y2="18.0975" width="0" layer="20"/>
<wire x1="-320.548" y1="18.0975" x2="-320.548" y2="68.58" width="0" layer="20"/>
<wire x1="-320.548" y1="68.58" x2="-319.278" y2="69.85" width="0" layer="20"/>
<wire x1="-319.278" y1="69.85" x2="-306.578" y2="69.85" width="0" layer="20"/>
<wire x1="-305.308" y1="71.12" x2="-305.308" y2="85.09" width="0" layer="20"/>
<wire x1="-305.308" y1="85.09" x2="-304.038" y2="86.36" width="0" layer="20"/>
<wire x1="-304.038" y1="86.36" x2="-300.5455" y2="86.36" width="0" layer="20"/>
<wire x1="-300.5455" y1="86.36" x2="-300.5455" y2="77.47" width="0" layer="20"/>
<wire x1="-300.5455" y1="77.47" x2="-288.4805" y2="77.47" width="0" layer="20"/>
<wire x1="-288.4805" y1="77.47" x2="-288.4805" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-309.118" y1="74.93" x2="-310.388" y2="73.66" width="0" layer="20"/>
<wire x1="-306.578" y1="69.85" x2="-305.308" y2="71.12" width="0" layer="20"/>
<wire x1="-312.1025" y1="89.535" x2="-331.47" y2="89.535" width="0" layer="20"/>
<wire x1="-331.47" y1="89.535" x2="-332.74" y2="88.265" width="0" layer="20"/>
<wire x1="-332.74" y1="88.265" x2="-332.74" y2="74.93" width="0" layer="20"/>
<wire x1="-334.01" y1="73.66" x2="-346.075" y2="73.66" width="0" layer="20"/>
<wire x1="-346.075" y1="73.66" x2="-347.345" y2="72.39" width="0" layer="20"/>
<wire x1="-347.345" y1="72.39" x2="-347.345" y2="18.0975" width="0" layer="20"/>
<wire x1="-347.345" y1="18.0975" x2="-347.98" y2="17.4625" width="0" layer="20"/>
<wire x1="-347.98" y1="17.4625" x2="-357.505" y2="17.4625" width="0" layer="20"/>
<wire x1="-357.505" y1="17.4625" x2="-358.14" y2="16.8275" width="0" layer="20"/>
<wire x1="-358.14" y1="16.8275" x2="-358.14" y2="-1.397" width="0" layer="20"/>
<wire x1="-358.14" y1="-1.397" x2="-357.505" y2="-2.032" width="0" layer="20"/>
<wire x1="-357.505" y1="-2.032" x2="-339.725" y2="-2.032" width="0" layer="20"/>
<wire x1="-339.725" y1="-2.032" x2="-339.09" y2="-1.397" width="0" layer="20"/>
<wire x1="-339.09" y1="-1.397" x2="-339.09" y2="16.8275" width="0" layer="20"/>
<wire x1="-339.09" y1="16.8275" x2="-339.725" y2="17.4625" width="0" layer="20"/>
<wire x1="-339.725" y1="17.4625" x2="-343.535" y2="17.4625" width="0" layer="20"/>
<wire x1="-343.535" y1="17.4625" x2="-344.17" y2="18.0975" width="0" layer="20"/>
<wire x1="-344.17" y1="18.0975" x2="-344.17" y2="68.58" width="0" layer="20"/>
<wire x1="-344.17" y1="68.58" x2="-342.9" y2="69.85" width="0" layer="20"/>
<wire x1="-342.9" y1="69.85" x2="-330.2" y2="69.85" width="0" layer="20"/>
<wire x1="-328.93" y1="71.12" x2="-328.93" y2="85.09" width="0" layer="20"/>
<wire x1="-328.93" y1="85.09" x2="-327.66" y2="86.36" width="0" layer="20"/>
<wire x1="-327.66" y1="86.36" x2="-324.1675" y2="86.36" width="0" layer="20"/>
<wire x1="-324.1675" y1="86.36" x2="-324.1675" y2="77.47" width="0" layer="20"/>
<wire x1="-324.1675" y1="77.47" x2="-312.1025" y2="77.47" width="0" layer="20"/>
<wire x1="-312.1025" y1="77.47" x2="-312.1025" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-332.74" y1="74.93" x2="-334.01" y2="73.66" width="0" layer="20"/>
<wire x1="-330.2" y1="69.85" x2="-328.93" y2="71.12" width="0" layer="20"/>
<wire x1="-335.7245" y1="89.535" x2="-355.092" y2="89.535" width="0" layer="20"/>
<wire x1="-355.092" y1="89.535" x2="-356.362" y2="88.265" width="0" layer="20"/>
<wire x1="-356.362" y1="88.265" x2="-356.362" y2="74.93" width="0" layer="20"/>
<wire x1="-357.632" y1="73.66" x2="-369.697" y2="73.66" width="0" layer="20"/>
<wire x1="-369.697" y1="73.66" x2="-370.967" y2="72.39" width="0" layer="20"/>
<wire x1="-370.967" y1="72.39" x2="-370.967" y2="18.0975" width="0" layer="20"/>
<wire x1="-370.967" y1="18.0975" x2="-371.602" y2="17.4625" width="0" layer="20"/>
<wire x1="-371.602" y1="17.4625" x2="-381.127" y2="17.4625" width="0" layer="20"/>
<wire x1="-381.127" y1="17.4625" x2="-381.762" y2="16.8275" width="0" layer="20"/>
<wire x1="-381.762" y1="16.8275" x2="-381.762" y2="-1.397" width="0" layer="20"/>
<wire x1="-381.762" y1="-1.397" x2="-381.127" y2="-2.032" width="0" layer="20"/>
<wire x1="-381.127" y1="-2.032" x2="-363.347" y2="-2.032" width="0" layer="20"/>
<wire x1="-363.347" y1="-2.032" x2="-362.712" y2="-1.397" width="0" layer="20"/>
<wire x1="-362.712" y1="-1.397" x2="-362.712" y2="16.8275" width="0" layer="20"/>
<wire x1="-362.712" y1="16.8275" x2="-363.347" y2="17.4625" width="0" layer="20"/>
<wire x1="-363.347" y1="17.4625" x2="-367.157" y2="17.4625" width="0" layer="20"/>
<wire x1="-367.157" y1="17.4625" x2="-367.792" y2="18.0975" width="0" layer="20"/>
<wire x1="-367.792" y1="18.0975" x2="-367.792" y2="68.58" width="0" layer="20"/>
<wire x1="-367.792" y1="68.58" x2="-366.522" y2="69.85" width="0" layer="20"/>
<wire x1="-366.522" y1="69.85" x2="-353.822" y2="69.85" width="0" layer="20"/>
<wire x1="-352.552" y1="71.12" x2="-352.552" y2="85.09" width="0" layer="20"/>
<wire x1="-352.552" y1="85.09" x2="-351.282" y2="86.36" width="0" layer="20"/>
<wire x1="-351.282" y1="86.36" x2="-347.7895" y2="86.36" width="0" layer="20"/>
<wire x1="-347.7895" y1="86.36" x2="-347.7895" y2="77.47" width="0" layer="20"/>
<wire x1="-347.7895" y1="77.47" x2="-335.7245" y2="77.47" width="0" layer="20"/>
<wire x1="-335.7245" y1="77.47" x2="-335.7245" y2="89.535" width="0" layer="20"/>
<text>Pocket NC USB Extension Rev B</text>
<wire x1="-356.362" y1="74.93" x2="-357.632" y2="73.66" width="0" layer="20"/>
<wire x1="-353.822" y1="69.85" x2="-352.552" y2="71.12" width="0" layer="20"/>
</plain>
<libraries>
<library name="PocketNC">
<packages>
<package name="MOLEX-48258-0002">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$8" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$10" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$12" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$13" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$14" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$15" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$16" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$17" library="PocketNC" package="MOLEX-48258-0002" value="MOLEX-48258-0002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="GND"/>
</signal>
<signal name="D-">
<contactref element="U$2" pad="D-"/>
</signal>
<signal name="D+">
<contactref element="U$2" pad="D+"/>
</signal>
<signal name="V+">
<contactref element="U$2" pad="V+"/>
</signal>
<signal name="GND1">
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="D-1">
<contactref element="U$1" pad="D-"/>
</signal>
<signal name="D+1">
<contactref element="U$1" pad="D+"/>
</signal>
<signal name="V+1">
<contactref element="U$1" pad="V+"/>
</signal>
<signal name="GND2">
<contactref element="U$3" pad="GND"/>
</signal>
<signal name="D-2">
<contactref element="U$3" pad="D-"/>
</signal>
<signal name="D+2">
<contactref element="U$3" pad="D+"/>
</signal>
<signal name="V+2">
<contactref element="U$3" pad="V+"/>
</signal>
<signal name="GND3">
<contactref element="U$4" pad="GND"/>
</signal>
<signal name="D-3">
<contactref element="U$4" pad="D-"/>
</signal>
<signal name="D+3">
<contactref element="U$4" pad="D+"/>
</signal>
<signal name="V+3">
<contactref element="U$4" pad="V+"/>
</signal>
<signal name="GND4">
<contactref element="U$5" pad="GND"/>
</signal>
<signal name="D-4">
<contactref element="U$5" pad="D-"/>
</signal>
<signal name="D+4">
<contactref element="U$5" pad="D+"/>
</signal>
<signal name="V+4">
<contactref element="U$5" pad="V+"/>
</signal>
<signal name="GND5">
<contactref element="U$6" pad="GND"/>
</signal>
<signal name="D-5">
<contactref element="U$6" pad="D-"/>
</signal>
<signal name="D+5">
<contactref element="U$6" pad="D+"/>
</signal>
<signal name="V+5">
<contactref element="U$6" pad="V+"/>
</signal>
<signal name="GND6">
<contactref element="U$7" pad="GND"/>
</signal>
<signal name="D-6">
<contactref element="U$7" pad="D-"/>
</signal>
<signal name="D+6">
<contactref element="U$7" pad="D+"/>
</signal>
<signal name="V+6">
<contactref element="U$7" pad="V+"/>
</signal>
<signal name="GND7">
<contactref element="U$8" pad="GND"/>
</signal>
<signal name="D-7">
<contactref element="U$8" pad="D-"/>
</signal>
<signal name="D+7">
<contactref element="U$8" pad="D+"/>
</signal>
<signal name="V+7">
<contactref element="U$8" pad="V+"/>
</signal>
<signal name="GND8">
<contactref element="U$9" pad="GND"/>
</signal>
<signal name="D-8">
<contactref element="U$9" pad="D-"/>
</signal>
<signal name="D+8">
<contactref element="U$9" pad="D+"/>
</signal>
<signal name="V+8">
<contactref element="U$9" pad="V+"/>
</signal>
<signal name="GND9">
<contactref element="U$10" pad="GND"/>
</signal>
<signal name="D-9">
<contactref element="U$10" pad="D-"/>
</signal>
<signal name="D+9">
<contactref element="U$10" pad="D+"/>
</signal>
<signal name="V+9">
<contactref element="U$10" pad="V+"/>
</signal>
<signal name="GND10">
<contactref element="U$11" pad="GND"/>
</signal>
<signal name="D-10">
<contactref element="U$11" pad="D-"/>
</signal>
<signal name="D+10">
<contactref element="U$11" pad="D+"/>
</signal>
<signal name="V+10">
<contactref element="U$11" pad="V+"/>
</signal>
<signal name="GND11">
<contactref element="U$12" pad="GND"/>
</signal>
<signal name="D-11">
<contactref element="U$12" pad="D-"/>
</signal>
<signal name="D+11">
<contactref element="U$12" pad="D+"/>
</signal>
<signal name="V+11">
<contactref element="U$12" pad="V+"/>
</signal>
<signal name="GND12">
<contactref element="U$13" pad="GND"/>
</signal>
<signal name="D-12">
<contactref element="U$13" pad="D-"/>
</signal>
<signal name="D+12">
<contactref element="U$13" pad="D+"/>
</signal>
<signal name="V+12">
<contactref element="U$13" pad="V+"/>
</signal>
<signal name="GND13">
<contactref element="U$14" pad="GND"/>
</signal>
<signal name="D-13">
<contactref element="U$14" pad="D-"/>
</signal>
<signal name="D+13">
<contactref element="U$14" pad="D+"/>
</signal>
<signal name="V+13">
<contactref element="U$14" pad="V+"/>
</signal>
<signal name="GND14">
<contactref element="U$15" pad="GND"/>
</signal>
<signal name="D-14">
<contactref element="U$15" pad="D-"/>
</signal>
<signal name="D+14">
<contactref element="U$15" pad="D+"/>
</signal>
<signal name="V+14">
<contactref element="U$15" pad="V+"/>
</signal>
<signal name="GND15">
<contactref element="U$16" pad="GND"/>
</signal>
<signal name="D-15">
<contactref element="U$16" pad="D-"/>
</signal>
<signal name="D+15">
<contactref element="U$16" pad="D+"/>
</signal>
<signal name="V+15">
<contactref element="U$16" pad="V+"/>
</signal>
<signal name="D-16">
</signal>
<signal name="D+16">
</signal>
<signal name="V+16">
</signal>
<signal name="D-17">
</signal>
<signal name="D+17">
</signal>
<signal name="V+17">
</signal>
<signal name="D-18">
</signal>
<signal name="D+18">
</signal>
<signal name="V+18">
</signal>
<signal name="D-19">
</signal>
<signal name="D+19">
</signal>
<signal name="V+19">
</signal>
<signal name="D-20">
</signal>
<signal name="D+20">
</signal>
<signal name="V+20">
</signal>
<signal name="D-21">
</signal>
<signal name="D+21">
</signal>
<signal name="V+21">
</signal>
<signal name="D-22">
</signal>
<signal name="D+22">
</signal>
<signal name="V+22">
</signal>
<signal name="D-23">
</signal>
<signal name="D+23">
</signal>
<signal name="V+23">
</signal>
<signal name="D-24">
</signal>
<signal name="D+24">
</signal>
<signal name="V+24">
</signal>
<signal name="D-25">
</signal>
<signal name="D+25">
</signal>
<signal name="V+25">
</signal>
<signal name="D-26">
</signal>
<signal name="D+26">
</signal>
<signal name="V+26">
</signal>
<signal name="D-27">
</signal>
<signal name="D+27">
</signal>
<signal name="V+27">
</signal>
<signal name="D-28">
</signal>
<signal name="D+28">
</signal>
<signal name="V+28">
</signal>
<signal name="D-29">
</signal>
<signal name="D+29">
</signal>
<signal name="V+29">
</signal>
<signal name="D-30">
</signal>
<signal name="D+30">
</signal>
<signal name="V+30">
</signal>
<signal name="D-31">
</signal>
<signal name="D+31">
</signal>
<signal name="V+31">
</signal>
<signal name="GND16">
<contactref element="U$17" pad="GND"/>
</signal>
<signal name="D-32">
<contactref element="U$17" pad="D-"/>
</signal>
<signal name="D+32">
<contactref element="U$17" pad="D+"/>
</signal>
<signal name="V+32">
<contactref element="U$17" pad="V+"/>
</signal>
<signal name="GND17">
</signal>
<signal name="D-33">
</signal>
<signal name="D+33">
</signal>
<signal name="V+33">
</signal>
<signal name="GND18">
</signal>
<signal name="D-34">
</signal>
<signal name="D+34">
</signal>
<signal name="V+34">
</signal>
<signal name="GND19">
</signal>
<signal name="D-35">
</signal>
<signal name="D+35">
</signal>
<signal name="V+35">
</signal>
<signal name="GND20">
</signal>
<signal name="D-36">
</signal>
<signal name="D+36">
</signal>
<signal name="V+36">
</signal>
<signal name="GND21">
</signal>
<signal name="D-37">
</signal>
<signal name="D+37">
</signal>
<signal name="V+37">
</signal>
<signal name="GND22">
</signal>
<signal name="D-38">
</signal>
<signal name="D+38">
</signal>
<signal name="V+38">
</signal>
<signal name="GND23">
</signal>
<signal name="D-39">
</signal>
<signal name="D+39">
</signal>
<signal name="V+39">
</signal>
<signal name="GND24">
</signal>
<signal name="D-40">
</signal>
<signal name="D+40">
</signal>
<signal name="V+40">
</signal>
<signal name="GND25">
</signal>
<signal name="D-41">
</signal>
<signal name="D+41">
</signal>
<signal name="V+41">
</signal>
<signal name="GND26">
</signal>
<signal name="D-42">
</signal>
<signal name="D+42">
</signal>
<signal name="V+42">
</signal>
<signal name="GND27">
</signal>
<signal name="D-43">
</signal>
<signal name="D+43">
</signal>
<signal name="V+43">
</signal>
<signal name="GND28">
</signal>
<signal name="D-44">
</signal>
<signal name="D+44">
</signal>
<signal name="V+44">
</signal>
<signal name="GND29">
</signal>
<signal name="D-45">
</signal>
<signal name="D+45">
</signal>
<signal name="V+45">
</signal>
<signal name="GND30">
</signal>
<signal name="D-46">
</signal>
<signal name="D+46">
</signal>
<signal name="V+46">
</signal>
<signal name="GND31">
</signal>
<signal name="D-47">
</signal>
<signal name="D+47">
</signal>
<signal name="V+47">
</signal>
<signal name="GND32">
</signal>
<signal name="D-48">
</signal>
<signal name="D+48">
</signal>
<signal name="V+48">
</signal>
<signal name="GND33">
</signal>
<signal name="D-49">
</signal>
<signal name="D+49">
</signal>
<signal name="V+49">
</signal>
</signals>
</board>
</drawing>
</eagle>
