(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 63)
    (no_connects 0)
    (area 105.182599 70.960001 182.932401 101.934781)
    (thickness 1.6)
    (drawings 22)
    (tracks 202)
    (zones 0)
    (modules 26)
    (nets 32)
  )
  (page A4)
  (title_block
    (title "1UP Audio Repair")
    (date 2018-03-04)
    (rev v0.3)
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 /VOL_ADC)
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 /DAC_L)
  (net 7 "Net-(C8-Pad1)")
  (net 8 /DAC_R)
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(C10-Pad2)")
  (net 13 /TIP_SW)
  (net 14 "Net-(J2-Pad3)")
  (net 15 "Net-(J2-Pad4)")
  (net 16 "Net-(J4-Pad1)")
  (net 17 "Net-(J4-Pad2)")
  (net 18 "Net-(J6-Pad1)")
  (net 19 "Net-(J6-Pad2)")
  (net 20 "Net-(R2-Pad1)")
  (net 21 "Net-(R6-Pad1)")
  (net 22 "Net-(R6-Pad2)")
  (net 23 /~SHUTDOWN)
  (net 24 /MUTE)
  (net 25 "Net-(U2-Pad14)")
  (net 26 +3V3)
  (net 27 "Net-(U2-Pad17)")
  (net 28 "Net-(U2-Pad37)")
  (net 29 "Net-(U2-Pad38)")
  (net 30 "Net-(U2-Pad39)")
  (net 31 "Net-(U2-Pad40)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /DAC_L)
    (add_net /DAC_R)
    (add_net /MUTE)
    (add_net /TIP_SW)
    (add_net /VOL_ADC)
    (add_net /~SHUTDOWN)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad40)")
    (add_net VDD)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.1)
  )
  (net_class "Speaker Wire" ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.1)
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
  )
  (module audio-repair:Switchcraft_35RAPC4BHN3 (layer F.Cu) (tedit 5A9BED16)
    (at 179.08 83.46 180)
    (fp_text reference J2 (at 2.5 7 180) (layer F.Fab))
    (fp_text value Switchcraft_35RAPC4BHN3 (at 8.392 0.402 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 2 0 180) (size 1.66 2.06) (drill 1.36) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at 9.8 -5.2 180) (size 2.06 1.66) (drill 1.36) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 3 thru_hole rect (at 8.4 -2.5 180) (size 2.06 1.66) (drill 1.36) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 4 thru_hole rect (at 13 4 180) (size 1.66 2.06) (drill 1.36) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 5 thru_hole rect (at 5.4 4.5 180) (size 2.06 1.66) (drill 1.36) (layers *.Cu *.Mask)
      (net 10 "Net-(C9-Pad2)"))
  )
  (module audio-repair:1bitsy-stub (layer F.Cu) (tedit 59F8C8AB)
    (at 106.68 93.98 90)
    (fp_text reference U2 (at -2.38 -0.02 180) (layer F.SilkS))
    (fp_text value 1bitsy-basic-stubby (at 14.84 7.41 180) (layer F.Fab))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 +3V3))
    (pad 16 thru_hole circle (at 15.24 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole circle (at 15.24 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 15.24 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 15.24 27.94) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 2.54 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /TIP_SW))
    (pad 32 thru_hole circle (at 2.54 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VOL_ADC))
    (pad 33 thru_hole circle (at 5.08 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /MUTE))
    (pad 34 thru_hole circle (at 5.08 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /~SHUTDOWN))
    (pad 35 thru_hole circle (at 7.62 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /DAC_L))
    (pad 36 thru_hole circle (at 7.62 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /DAC_R))
    (pad 37 thru_hole circle (at 10.16 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U2-Pad37)"))
    (pad 38 thru_hole circle (at 10.16 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad38)"))
    (pad 39 thru_hole circle (at 12.7 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad39)"))
    (pad 40 thru_hole circle (at 12.7 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad40)"))
    (pad 42 thru_hole circle (at 2.54 27.94) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at 2.54 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at 12.7 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BE877)
    (at 146.2652 82.3214)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.4384 0) (layer F.SilkS))
    (fp_text value 10µF (at -3.5172 -0.0254) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BEEB3)
    (at 153.6192 83.0834 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.0574 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BEF75)
    (at 151.1808 83.0834 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.0574 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BE919)
    (at 156.9466 87.63)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.3462) (layer F.SilkS))
    (fp_text value 100nF (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BE7A8)
    (at 147.32 93.968 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.552 0 270) (layer F.SilkS))
    (fp_text value 10nF (at 5.854 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOL_ADC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BE889)
    (at 146.2659 84.328 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.4511 0 180) (layer F.SilkS))
    (fp_text value 1µF (at 3.0099 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BE8A2)
    (at 146.2659 88.392 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.4511 0 180) (layer F.SilkS))
    (fp_text value 220nF (at 3.7719 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /DAC_L))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BE853)
    (at 146.2659 86.36 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.4511 0 180) (layer F.SilkS))
    (fp_text value 220nF (at 3.7719 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /DAC_R))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5A9BF3D6)
    (at 162.7124 86.0552 90)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at -2.5908 0 180) (layer F.SilkS))
    (fp_text value 220µF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5A9BE9C6)
    (at 162.7124 80.8482 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C10 (at -2.7432 0.0254 360) (layer F.SilkS))
    (fp_text value 220µF (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A9BEF48)
    (at 151.384 79.248 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 1.143 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 /TIP_SW))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A9B2FC6)
    (at 144.78 78.74)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.Fab))
    (fp_text value Vin (at 2.794 0) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A9B3F70)
    (at 165.1 93.98)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 5.08) (layer F.Fab))
    (fp_text value Left (at -0.762 -1.9558) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A9B3F74)
    (at 167.64 93.98)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 5.08) (layer F.Fab))
    (fp_text value Right (at 0.762 -1.9558) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BF040)
    (at 158.75 79.248)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.143) (layer F.SilkS))
    (fp_text value 100K (at 0 -3.81) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BE74B)
    (at 149.352 93.98 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 1M (at 5.08 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOL_ADC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BE7B1)
    (at 153.416 93.98 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 33K (at -5.334 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BE7B4)
    (at 155.448 93.98 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 18K (at 5.334 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BE7D3)
    (at 157.48 93.98 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 33K (at -5.334 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BEFFE)
    (at 155.194 79.248 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.143 180) (layer F.SilkS))
    (fp_text value 51K (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /TIP_SW))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BF05E)
    (at 158.75 82.042)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.524) (layer F.SilkS))
    (fp_text value 10K (at 0 -5.334) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:Potentiometer_Bourns_3352T (layer F.Cu) (tedit 59F717EB)
    (at 175.77 93.98 270)
    (fp_text reference RV1 (at 0 0.51 270) (layer F.SilkS))
    (fp_text value 50K (at 6.35 0.002 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 2.875 270) (size 1.1 1.1) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 2.875 270) (size 1.1 1.1) (drill 0.55) (layers *.Cu *.Mask)
      (net 20 "Net-(R2-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 2.875 270) (size 1.1 1.1) (drill 0.55) (layers *.Cu *.Mask)
      (net 1 VDD))
  )
  (module audio-repair:QFN-20-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5A9BF0A5)
    (at 152.4 87.63)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 3.556 2.032) (layer F.SilkS))
    (fp_text value PAM8019KGR (at 0 3.33) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J6-Pad2)"))
    (pad 2 smd oval (at -1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 3 smd oval (at -1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /~SHUTDOWN))
    (pad 4 smd oval (at -1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 5 smd oval (at -1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 6 smd oval (at -1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd oval (at -0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 8 smd oval (at 0 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad1)"))
    (pad 9 smd oval (at 0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /MUTE))
    (pad 10 smd oval (at 1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /TIP_SW))
    (pad 11 smd oval (at 1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd oval (at 1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R6-Pad2)"))
    (pad 13 smd oval (at 1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 14 smd oval (at 1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 15 smd oval (at 1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J4-Pad2)"))
    (pad 16 smd oval (at 1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 17 smd oval (at 0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J4-Pad1)"))
    (pad 18 smd oval (at 0 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd oval (at -0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J6-Pad1)"))
    (pad 20 smd oval (at -1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 21 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 thru_hole circle (at 0 0) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at -0.625 -0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at 0.625 -0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at 0.625 0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at -0.625 0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A9BE7AC)
    (at 151.384 93.98 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 680K (at 5.842 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOL_ADC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "This board is upside down." (at 159.385 82.804) (layer B.SilkS))
  (gr_text v0.3 (at 143.764 93.218) (layer F.SilkS))
  (gr_text "1Bitsy DAC Audio" (at 143.764 91.44) (layer F.SilkS))
  (dimension 20.32 (width 0.15) (layer F.Fab)
    (gr_text "20.320 mm" (at 128.19 87.63 90) (layer F.Fab))
    (feature1 (pts (xy 133.35 97.79) (xy 126.84 97.79)))
    (feature2 (pts (xy 133.35 77.47) (xy 126.84 77.47)))
    (crossbar (pts (xy 129.54 77.47) (xy 129.54 97.79)))
    (arrow1a (pts (xy 129.54 97.79) (xy 128.953579 96.663496)))
    (arrow1b (pts (xy 129.54 97.79) (xy 130.126421 96.663496)))
    (arrow2a (pts (xy 129.54 77.47) (xy 128.953579 78.596504)))
    (arrow2b (pts (xy 129.54 77.47) (xy 130.126421 78.596504)))
  )
  (dimension 45.72 (width 0.15) (layer F.Fab)
    (gr_text "45.720 mm" (at 156.21 72.310001) (layer F.Fab))
    (feature1 (pts (xy 133.35 77.47) (xy 133.35 70.960001)))
    (feature2 (pts (xy 179.07 77.47) (xy 179.07 70.960001)))
    (crossbar (pts (xy 179.07 73.660001) (xy 133.35 73.660001)))
    (arrow1a (pts (xy 133.35 73.660001) (xy 134.476504 73.07358)))
    (arrow1b (pts (xy 133.35 73.660001) (xy 134.476504 74.246422)))
    (arrow2a (pts (xy 179.07 73.660001) (xy 177.943496 73.07358)))
    (arrow2b (pts (xy 179.07 73.660001) (xy 177.943496 74.246422)))
  )
  (gr_arc (start 176.53 95.25) (end 179.07 95.25) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 179.07 77.47) (end 179.07 95.25) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 176.53 97.79) (end 134.62 97.79) (layer Edge.Cuts) (width 0.254))
  (gr_text "-\n" (at 162.56 96.52) (layer F.SilkS))
  (gr_text + (at 162.56 93.98) (layer F.SilkS))
  (gr_text Speakers (at 166.37 90.7542) (layer F.SilkS))
  (gr_arc (start 134.62 96.52) (end 134.62 97.79) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 134.62 77.47) (end 179.07 77.47) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 133.35 91.44) (end 133.35 96.52) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 137.16 90.17) (end 134.62 90.17) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 138.43 88.9) (end 138.43 83.82) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 137.16 81.28) (end 137.16 82.55) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 134.62 81.28) (end 134.62 80.01) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 134.62 78.74) (end 134.62 80.01) (angle 180) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 137.16 83.82) (end 137.16 82.55) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 137.16 88.9) (end 138.43 88.9) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_arc (start 134.62 91.44) (end 133.35 91.44) (angle 90) (layer Edge.Cuts) (width 0.254))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 132.715 76.835) (xy 179.705 76.835) (xy 179.705 98.425) (xy 132.715 98.425)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 132.08 76.2) (xy 180.34 76.2) (xy 180.34 99.06) (xy 132.08 99.06)
      )
    )
  )
)
