(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 21)
    (no_connects 0)
    (area 138.291499 88.380499 160.476001 129.297501)
    (thickness 1.6)
    (drawings 9)
    (tracks 108)
    (zones 0)
    (modules 5)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.6096)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 146.431 98.806)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /3.3V)
  (net 2 "Net-(P1-Pad2)")
  (net 3 /5V)
  (net 4 /DEVICE_RX)
  (net 5 /TEENSY_TX)
  (net 6 /TEENSY_RX)
  (net 7 /DEVICE_TX)
  (net 8 "Net-(U1-Pad2)")
  (net 9 "Net-(U1-Pad3)")
  (net 10 "Net-(U1-Pad4)")
  (net 11 "Net-(U1-Pad5)")
  (net 12 "Net-(U1-Pad6)")
  (net 13 "Net-(U1-Pad7)")
  (net 14 "Net-(U1-Pad8)")
  (net 15 "Net-(U1-Pad9)")
  (net 16 /SPI_CS)
  (net 17 /SPI_MOSI)
  (net 18 /SPI_MISO)
  (net 19 /SPI_CLK)
  (net 20 /AIO0)
  (net 21 /AIO1)
  (net 22 /AIO2)
  (net 23 /AIO3)
  (net 24 /I2C_SDAT)
  (net 25 /I2C_SCLK)
  (net 26 "Net-(U1-Pad20)")
  (net 27 "Net-(U1-Pad21)")
  (net 28 "Net-(U1-Pad22)")
  (net 29 "Net-(U1-Pad23)")
  (net 30 "Net-(U1-Pad25)")
  (net 31 /GND)
  (net 32 "Net-(U1-Pad28)")
  (net 33 "Net-(U1-Pad29)")
  (net 34 "Net-(U1-Pad31)")
  (net 35 "Net-(U1-Pad32)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /5V)
    (add_net /AIO0)
    (add_net /AIO1)
    (add_net /AIO2)
    (add_net /AIO3)
    (add_net /DEVICE_RX)
    (add_net /DEVICE_TX)
    (add_net /GND)
    (add_net /I2C_SCLK)
    (add_net /I2C_SDAT)
    (add_net /SPI_CLK)
    (add_net /SPI_CS)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /TEENSY_RX)
    (add_net /TEENSY_TX)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 147.5105 94.1705 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /3.3V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58AB7631)
    (at 154.686 99.949 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -4.191 -0.0635 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /DEVICE_RX))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /TEENSY_TX))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58AB7634)
    (at 152.527 99.949 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 4.2545 0.127 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /TEENSY_RX))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /DEVICE_TX))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TeensyConverter:CE_Header (layer F.Cu) (tedit 58AB7621)
    (at 146.939 99.187)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference U2 (at 5.3975 -0.635) (layer F.SilkS))
    (fp_text value CE_HEADER (at 1.27 25.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SPI_MOSI))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SPI_MISO))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SPI_CLK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SPI_CS))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /DEVICE_RX))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DEVICE_TX))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /GND))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /3.3V))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /I2C_SCLK))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /I2C_SDAT))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /AIO0))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /AIO1))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /AIO2))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /AIO3))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TeensyConverter:Teensy-32 (layer B.Cu) (tedit 58ABB1C1)
    (at 149.2885 108.6485 180)
    (fp_text reference U1 (at 0 16.51 180) (layer B.SilkS))
    (fp_text value Teensy-3.2 (at 0 19.05 180) (layer B.Fab))
    (pad 0 thru_hole circle (at -7.62 12.7 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /TEENSY_RX))
    (pad 1 thru_hole circle (at -7.62 10.16 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /TEENSY_TX))
    (pad 2 thru_hole circle (at -7.62 7.62 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 5.08 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 2.54 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 0 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at -7.62 -2.54 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at -7.62 -5.08 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 -7.62 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at -7.62 -10.16 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at -7.62 -12.7 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /SPI_CS))
    (pad 11 thru_hole circle (at -7.62 -15.24 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /SPI_MOSI))
    (pad 12 thru_hole circle (at -7.62 -17.78 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /SPI_MISO))
    (pad 13 thru_hole circle (at 7.62 -17.78 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /SPI_CLK))
    (pad 14 thru_hole circle (at 7.62 -15.24 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /AIO0))
    (pad 15 thru_hole circle (at 7.62 -12.7 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /AIO1))
    (pad 16 thru_hole circle (at 7.62 -10.16 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /AIO2))
    (pad 17 thru_hole circle (at 7.62 -7.62 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /AIO3))
    (pad 18 thru_hole circle (at 7.62 -5.08 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /I2C_SDAT))
    (pad 19 thru_hole circle (at 7.62 -2.54 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /I2C_SCLK))
    (pad 20 thru_hole circle (at 7.62 0 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad20)"))
    (pad 21 thru_hole circle (at 7.62 2.54 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 5.08 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 7.62 7.62 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 7.62 10.16 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /3.3V))
    (pad 25 thru_hole circle (at 7.62 12.7 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at 7.62 15.24 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /5V))
    (pad 27 thru_hole circle (at -7.62 15.24 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /GND))
    (pad 28 thru_hole circle (at -5.08 -17.78 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad28)"))
    (pad 29 thru_hole circle (at -2.54 -17.78 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at 0 -17.78 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /GND))
    (pad 31 thru_hole circle (at 2.54 -17.78 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at 5.08 -17.78 180) (size 1.7018 1.7018) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad32)"))
  )
  (gr_text Teensy (at 154.2415 99.2505 90) (layer B.SilkS))
  (gr_text "CE Header" (at 152.654 115.57 90) (layer F.SilkS))
  (gr_line (start 138.3665 88.4555) (end 138.3665 89.4715) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.401 88.4555) (end 138.3665 88.4555) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.401 129.2225) (end 160.401 88.4555) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.3665 129.2225) (end 160.401 129.2225) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.3665 89.154) (end 138.3665 129.2225) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 3.3V (at 144.399 92.456) (layer F.SilkS))
  (gr_text 5V (at 154.8765 92.202) (layer F.SilkS))
  (zone (net 31) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.3665 88.646) (xy 138.3665 129.159) (xy 160.401 129.2225) (xy 160.401 88.4555) (xy 138.3665 88.4555)
      )
    )
  )
)
