(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 58)
    (no_connects 0)
    (area 49.949999 49.949999 150.050001 122.050001)
    (thickness 1.6)
    (drawings 91)
    (tracks 141)
    (zones 0)
    (modules 44)
    (nets 19)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 50 50)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Fabricate/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C3-Pad2)")
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 "Net-(D4-Pad1)")
  (net 9 "Net-(D5-Pad1)")
  (net 10 "Net-(D6-Pad1)")
  (net 11 "Net-(P1-Pad4)")
  (net 12 "Net-(P1-Pad2)")
  (net 13 "Net-(P1-Pad3)")
  (net 14 "Net-(P1-Pad5)")
  (net 15 "Net-(C3-Pad1)")
  (net 16 "Net-(D1-Pad2)")
  (net 17 "Net-(P2-Pad2)")
  (net 18 "Net-(P2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
  )
  (module w_logo:Logo_silk_high_voltage_10x8.5mm (layer B.Cu) (tedit 0)
    (at 128 57 180)
    (descr "High voltage logo, 10x8.5mm")
    (fp_text reference G*** (at 0 -4.43738 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 4.43738 180) (layer B.SilkS) hide)
  )
  (module w_logo:Logo_silk_high_voltage_10x8.5mm (layer B.Cu) (tedit 0)
    (at 72 57 180)
    (descr "High voltage logo, 10x8.5mm")
    (fp_text reference G*** (at 0 -4.43738 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 4.43738 180) (layer B.SilkS) hide)
  )
  (module w_logo:Logo_silk_high_voltage_10x8.5mm (layer F.Cu) (tedit 0)
    (at 69 58)
    (descr "High voltage logo, 10x8.5mm")
    (fp_text reference G*** (at 0 4.43738) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -4.43738) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5867E6FB)
    (at 55.08 116.04)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5867E6FB)
    (at 144.996 116.04)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5867E6FB)
    (at 144.996 56.096)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_ThroughHole:C_Rect_L32_W15_P27 (layer F.Cu) (tedit 58343E39)
    (at 128.27 67.31 270)
    (descr "Film Capacitor Length 32mm x Width 15mm, Pitch 27mm")
    (tags Capacitor)
    (fp_text reference C8 (at 13.5 -8.75 270) (layer F.SilkS))
    (fp_text value C (at 13.5 8.75 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 27 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L32_W15_P27 (layer F.Cu) (tedit 58343E2C)
    (at 100.33 67.31 270)
    (descr "Film Capacitor Length 32mm x Width 15mm, Pitch 27mm")
    (tags Capacitor)
    (fp_text reference C7 (at 13.5 -8.75 270) (layer F.SilkS))
    (fp_text value C (at 13.5 8.75 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 27 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 0)
    (at 134.62 114.3 270)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.4 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.4 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 0)
    (at 134.62 107.95)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 58343DD4)
    (at 125.73 114.3 180)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D1 (at 5.38734 2.53746 180) (layer F.SilkS))
    (fp_text value 1N4001 (at 5.08 -2.54 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16 -0.00254) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 64.77 114.3 180)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D2 (at 1.524 4.064 180) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 180) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 59.69 102.87 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D3 (at 1.524 4.064 90) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 72.39 102.87 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D4 (at 1.524 4.064 90) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 128.27 102.87 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D5 (at 1.524 4.064 90) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 140.97 102.87 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D6 (at 1.524 4.064 90) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 58343D97)
    (at 69.85 114.3)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R1 (at 7.62 -2.54) (layer F.SilkS))
    (fp_text value R (at 7.15 2.7) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 15 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 585EC9DD)
    (at 78.74 106.68)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R2 (at 17.78 0) (layer F.SilkS))
    (fp_text value R (at 6.69 2.78) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 15 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 "Net-(P1-Pad5)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 585EC9E2)
    (at 78.74 102.87)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R3 (at 17.78 0) (layer F.SilkS))
    (fp_text value R (at 8.01 -2.86) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 15 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(P1-Pad4)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 585EC9E9)
    (at 121.92 102.87 180)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R4 (at 17.78 0 180) (layer F.SilkS))
    (fp_text value R (at 7.95 2.14 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(P1-Pad3)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 585EC9EC)
    (at 121.92 106.68 180)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R5 (at 17.78 0 180) (layer F.SilkS))
    (fp_text value R (at 7.62 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(P1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L27_W11_P22 (layer F.Cu) (tedit 58343E21)
    (at 72.352 69.812 270)
    (descr "Film Capacitor Length 27mm x Width 11mm, Pitch 22mm")
    (tags Capacitor)
    (fp_text reference C3 (at 11 -6.75 270) (layer F.SilkS))
    (fp_text value C (at 11 6.75 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 22.352 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L27_W11_P22 (layer F.Cu) (tedit 58343E33)
    (at 100.33 69.85 270)
    (descr "Film Capacitor Length 27mm x Width 11mm, Pitch 22mm")
    (tags Capacitor)
    (fp_text reference C4 (at 11 -6.75 270) (layer F.SilkS))
    (fp_text value C (at 11 6.75 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 22.352 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L27_W11_P22 (layer F.Cu) (tedit 58343E3E)
    (at 128.27 69.85 270)
    (descr "Film Capacitor Length 27mm x Width 11mm, Pitch 22mm")
    (tags Capacitor)
    (fp_text reference C5 (at 11 -6.75 270) (layer F.SilkS))
    (fp_text value C (at 11 6.75 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 22.352 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L32_W15_P27 (layer F.Cu) (tedit 58343E1A)
    (at 72.39 67.31 270)
    (descr "Film Capacitor Length 32mm x Width 15mm, Pitch 27mm")
    (tags Capacitor)
    (fp_text reference C6 (at 13.5 -8.75 270) (layer F.SilkS))
    (fp_text value C (at 13.5 8.75 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 27 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
  )
  (module w_conn_mkds:mkds_1,5-2 (layer F.Cu) (tedit 585DA677)
    (at 86.36 58.42 180)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P2 (at 0 -6.6 180) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 5.9 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P2-Pad2)"))
    (model ${KIWALTER3DMOD}/walter/conn_mkds/mkds_1,5-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mkds:mkds_1,5-2 (layer F.Cu) (tedit 585DA67B)
    (at 114.3 58.42 180)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P3 (at 0 -6.6 180) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 5.9 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P2-Pad1)"))
    (model ${KIWALTER3DMOD}/walter/conn_mkds/mkds_1,5-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-6-3,5-h (layer F.Cu) (tedit 585D9280)
    (at 100.33 114.935)
    (descr "6-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P1 (at 0 5.3) (layer F.SilkS) hide)
    (fp_text value CONN_6 (at 0 -5) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 5.25 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 8.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at -1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at -5.25 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P1-Pad5)"))
    (pad 6 thru_hole circle (at -8.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIWALTER3DMOD}/walter/conn_pt-1_5/pt_1,5-6-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 585ED151)
    (at 63.5 82.55 90)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R6 (at 12.065 -2.54 90) (layer F.SilkS))
    (fp_text value R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 15 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 585ED154)
    (at 91.44 82.55 90)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R7 (at 12.065 -2.54 90) (layer F.SilkS))
    (fp_text value R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 15 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 585ED157)
    (at 119.38 82.55 90)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R8 (at 12.065 -2.54 90) (layer F.SilkS))
    (fp_text value R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 15 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 585EC5DA)
    (at 59.69 86.36)
    (fp_text reference SSR1 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC (at -1.27 -7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad5)"))
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 585EC5DE)
    (at 87.63 86.36)
    (fp_text reference SSR2 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC (at -1.27 -7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad4)"))
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 585EC5E1)
    (at 115.57 86.36)
    (fp_text reference SSR3 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC (at -1.27 -7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad3)"))
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 585EC5E5)
    (at 143.51 86.36)
    (fp_text reference SSR4 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC (at -1.27 -7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5867E43F)
    (at 72.352 88.1)
    (fp_text reference P4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5867E2A4)
    (at 72.352 73.876)
    (fp_text reference P5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5867E565)
    (at 100.292 88.1)
    (fp_text reference P6 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5867E584)
    (at 100.292 73.876)
    (fp_text reference P7 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5867E5BA)
    (at 128.232 88.1)
    (fp_text reference P8 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5867E5AA)
    (at 128.232 73.876)
    (fp_text reference P9 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5867E6FB)
    (at 55.08 56.096)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module w_logo:Logo_silk_high_voltage_10x8.5mm (layer F.Cu) (tedit 0)
    (at 132 58)
    (descr "High voltage logo, 10x8.5mm")
    (fp_text reference G*** (at 0 4.43738) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -4.43738) (layer F.SilkS) hide)
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_5x2mm (layer F.Cu) (tedit 0)
    (at 100.25 63.5)
    (descr "CC BY-NC-SA logo, 5x2mm")
    (fp_text reference G*** (at 0.2 -0.7) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.2 0.2) (layer F.SilkS) hide)
  )
  (gr_arc (start 51 51) (end 50 51) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 51 121) (end 51 122) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149 121) (end 150 121) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149 51) (end 149 50) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 60 (width 0.3) (layer Cmts.User)
    (gr_text "60.000 mm" (at 43.65 86 270) (layer Cmts.User))
    (feature1 (pts (xy 48 116) (xy 42.3 116)))
    (feature2 (pts (xy 48 56) (xy 42.3 56)))
    (crossbar (pts (xy 45 56) (xy 45 116)))
    (arrow1a (pts (xy 45 116) (xy 44.413579 114.873496)))
    (arrow1b (pts (xy 45 116) (xy 45.586421 114.873496)))
    (arrow2a (pts (xy 45 56) (xy 44.413579 57.126504)))
    (arrow2b (pts (xy 45 56) (xy 45.586421 57.126504)))
  )
  (dimension 90 (width 0.3) (layer Cmts.User)
    (gr_text "90.000 mm" (at 100 44.65) (layer Cmts.User))
    (feature1 (pts (xy 145 48) (xy 145 43.3)))
    (feature2 (pts (xy 55 48) (xy 55 43.3)))
    (crossbar (pts (xy 55 46) (xy 145 46)))
    (arrow1a (pts (xy 145 46) (xy 143.873496 46.586421)))
    (arrow1b (pts (xy 145 46) (xy 143.873496 45.413579)))
    (arrow2a (pts (xy 55 46) (xy 56.126504 46.586421)))
    (arrow2b (pts (xy 55 46) (xy 56.126504 45.413579)))
  )
  (gr_text 4 (at 140.932 105.88) (layer F.SilkS))
  (gr_text 3 (at 128.232 105.88) (layer F.SilkS))
  (gr_text 2 (at 72.352 105.88) (layer F.SilkS))
  (gr_text 1 (at 59.652 105.88) (layer F.SilkS))
  (gr_text "Open\nCollector" (at 100.292 107.404) (layer F.SilkS))
  (gr_text 3.2mm (at 59 53) (layer B.SilkS))
  (gr_text 60mm (at 51 86.5 90) (layer B.SilkS))
  (gr_text 90mm (at 100 51) (layer B.SilkS))
  (dimension 72 (width 0.3) (layer Cmts.User)
    (gr_text "72.000 mm" (at 158.35 86 270) (layer Cmts.User))
    (feature1 (pts (xy 154 122) (xy 159.7 122)))
    (feature2 (pts (xy 154 50) (xy 159.7 50)))
    (crossbar (pts (xy 157 50) (xy 157 122)))
    (arrow1a (pts (xy 157 122) (xy 156.413579 120.873496)))
    (arrow1b (pts (xy 157 122) (xy 157.586421 120.873496)))
    (arrow2a (pts (xy 157 50) (xy 156.413579 51.126504)))
    (arrow2b (pts (xy 157 50) (xy 157.586421 51.126504)))
  )
  (dimension 100 (width 0.3) (layer Cmts.User)
    (gr_text "100.000 mm" (at 100 130.35) (layer Cmts.User))
    (feature1 (pts (xy 150 126) (xy 150 131.7)))
    (feature2 (pts (xy 50 126) (xy 50 131.7)))
    (crossbar (pts (xy 50 129) (xy 150 129)))
    (arrow1a (pts (xy 150 129) (xy 148.873496 129.586421)))
    (arrow1b (pts (xy 150 129) (xy 148.873496 128.413579)))
    (arrow2a (pts (xy 50 129) (xy 51.126504 129.586421)))
    (arrow2b (pts (xy 50 129) (xy 51.126504 128.413579)))
  )
  (gr_text 100mm (at 100 121) (layer F.SilkS))
  (gr_text PWR (at 70 118) (layer F.SilkS))
  (gr_text "72mm DIN" (at 149 88.27 90) (layer F.SilkS))
  (gr_text "LINE VOLTAGE!" (at 128.27 63.5) (layer B.SilkS))
  (gr_text "LINE VOLTAGE!" (at 72.39 63.5) (layer B.SilkS))
  (gr_text "LINE\nVOLTAGE!" (at 142.24 62.865) (layer F.SilkS))
  (gr_text "LINE\nVOLTAGE!" (at 58.128 62.7) (layer F.SilkS))
  (gr_text "Fan Speed\nControl" (at 100.33 55.245) (layer F.SilkS))
  (gr_text v2 (at 100.33 59.055) (layer F.SilkS))
  (gr_text jeditekunum (at 100.8 61.43) (layer F.SilkS))
  (gr_text LINE (at 76.835 58.42) (layer F.SilkS))
  (gr_text LOAD (at 123.825 58.42) (layer F.SilkS))
  (gr_text N (at 107.95 58.42) (layer F.SilkS))
  (gr_text N (at 92.71 58.42) (layer F.SilkS))
  (gr_text 3 (at 128.27 81.28) (layer F.SilkS))
  (gr_text 2 (at 100.33 81.28) (layer F.SilkS))
  (gr_text 1 (at 72.39 81.28) (layer F.SilkS))
  (gr_text + (at 109 109.5) (layer F.SilkS))
  (gr_text 4 (at 105.5 110) (layer F.SilkS))
  (gr_text 3 (at 102 110) (layer F.SilkS))
  (gr_text 2 (at 98.5 110) (layer F.SilkS))
  (gr_text 1 (at 95 110) (layer F.SilkS))
  (gr_text G (at 91.5 110) (layer F.SilkS))
  (gr_line (start 149 50) (end 51 50) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 121) (end 150 51) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51 122) (end 149 122) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 51) (end 50 121) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150 122) (xy 50 122) (xy 50 50) (xy 150 50)
      )
    )
    (polygon
      (pts        (xy 52 52) (xy 52 120) (xy 148 120) (xy 148 52)
      )
    )
  )
)
