<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="12.7" y1="83.82" x2="40.005" y2="83.82" width="0" layer="20"/>
<wire x1="40.005" y1="83.82" x2="40.005" y2="108.585" width="0" layer="20"/>
<wire x1="40.005" y1="108.585" x2="12.7" y2="108.585" width="0" layer="20"/>
<wire x1="12.7" y1="108.585" x2="12.7" y2="83.82" width="0" layer="20"/>
</plain>
<libraries>
<library name="rtotte">
<packages>
<package name="ANTENNA_915MHZ">
</package>
<package name="SOP65P640X120-14N">
<description>&lt;b&gt;(ST)14-Lead(TSSOP)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SWITCH_PTS810">
</package>
<package name="0402">
</package>
<package name="0603">
<description>0603 (1608 Metric)</description>
</package>
<package name="LED_0805">
<description>Wurth 0805 LED

Recommended land pattern</description>
</package>
<package name="CRYSTAL_ABM8G">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="rtotte" package="ANTENNA_915MHZ" value="ANTENNA_LOOP_915"/>
<element name="IC1" library="rtotte" package="SOP65P640X120-14N" value="PIC12LF1840T39A">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value="70415120"/>
<attribute name="DESCRIPTION" value="8-Bit MCU 7K Flash 2.5V/3.3V TSSOP14 Microchip PIC12LF1840T39A-I/ST, 8bit PIC Microcontroller, 32MHz, 4 kwords Flash, 14-Pin TSSOP"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PIC12LF1840T39A-I/ST"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7990288"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="rtotte" package="SWITCH_PTS810" value="SWITCH_PTS810_SJM_250"/>
<element name="U$4" library="rtotte" package="SWITCH_PTS810" value="SWITCH_PTS810_SJM_250"/>
<element name="L1" library="rtotte" package="0402" value=""/>
<element name="L3" library="rtotte" package="0402" value=""/>
<element name="C5" library="rtotte" package="0402" value=""/>
<element name="L5" library="rtotte" package="0402" value="120nH"/>
<element name="L2" library="rtotte" package="0402" value=""/>
<element name="L4" library="rtotte" package="0402" value=""/>
<element name="C2" library="rtotte" package="0402" value=""/>
<element name="C3" library="rtotte" package="0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rtotte" package="0402" value="1000pF"/>
<element name="C6" library="rtotte" package="0603" value=""/>
<element name="C7" library="rtotte" package="0603" value=""/>
<element name="R3" library="rtotte" package="0603" value=""/>
<element name="U$5" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$7" library="rtotte" package="LED_0805" value="LED_0805_WURTH"/>
<element name="U$8" library="rtotte" package="LED_0805" value="LED_0805_WURTH"/>
<element name="U$2" library="rtotte" package="CRYSTAL_ABM8G" value="CRYSTAL_4PORT"/>
<element name="U$9" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$10" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$11" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$12" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$13" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U$14" library="rtotte" package="0603" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="L2" pad="P$1"/>
<contactref element="L4" pad="P$1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="C4" pad="P$2"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="8"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$6" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$4" pad="4"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$12" pad="2"/>
<contactref element="U$11" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="RF"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="P$2"/>
<contactref element="L3" pad="P$1"/>
<contactref element="C2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="L3" pad="P$2"/>
<contactref element="C5" pad="P$1"/>
<contactref element="C3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="C2" pad="P$2"/>
<contactref element="L2" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="C3" pad="P$2"/>
<contactref element="L4" pad="P$2"/>
</signal>
<signal name="RFOUT">
<contactref element="L5" pad="P$1"/>
<contactref element="C5" pad="P$2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="C4" pad="P$1"/>
<contactref element="L5" pad="P$2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="C6" pad="1"/>
<contactref element="U$14" pad="2"/>
<contactref element="U$9" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SWITCH0">
<contactref element="IC1" pad="3"/>
<contactref element="U$13" pad="1"/>
<contactref element="U$14" pad="1"/>
<contactref element="U$12" pad="1"/>
</signal>
<signal name="SWITCH1">
<contactref element="IC1" pad="4"/>
<contactref element="U$10" pad="1"/>
<contactref element="U$9" pad="1"/>
<contactref element="U$11" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="LED0">
<contactref element="IC1" pad="13"/>
<contactref element="U$7" pad="PAD_ANODE(+)"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="LED1">
<contactref element="IC1" pad="12"/>
<contactref element="U$8" pad="PAD_ANODE(+)"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="10"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U$7" pad="PAD_CATHODE(-)"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U$8" pad="PAD_CATHODE(-)"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$13" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$10" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
