(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 8)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 17)
    (tracks 38)
    (zones 0)
    (modules 12)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Outputs/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(Q1-Pad1)")
  (net 6 "Net-(Q1-Pad2)")
  (net 7 "Net-(Q2-Pad1)")
  (net 8 "Net-(Q2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
  )
  (module "Local Library:0805" (layer F.Cu) (tedit 5B840685)
    (at 111.75 96.75 270)
    (fp_text reference D1 (at -0.456 2.368 270) (layer F.Fab))
    (fp_text value LED (at -1.956 -1.632 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.3 0 270) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (module "Local Library:0805" (layer F.Cu) (tedit 5B840693)
    (at 111.75 95.25 90)
    (fp_text reference D2 (at 0.29 2.24 90) (layer F.Fab))
    (fp_text value LED (at -0.15 -1.41 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.3 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
  )
  (module "Local Library:0805" (layer F.Cu) (tedit 5B84068E)
    (at 116.25 99 90)
    (fp_text reference Q1 (at 3.52 1.836 90) (layer F.Fab))
    (fp_text value Q_Photo_NPN (at -0.15 -1.41 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 2.3 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad2)"))
  )
  (module "Local Library:0805" (layer F.Cu) (tedit 5B84067E)
    (at 116.25 95.25 90)
    (fp_text reference Q2 (at 5.528 1.408 90) (layer F.Fab))
    (fp_text value Q_Photo_NPN (at -0.15 -1.41 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 2.3 0 90) (size 1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q2-Pad2)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B84000E)
    (at 112.5 99.25)
    (fp_text reference U1 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B8405E0)
    (at 111.5 97.5)
    (fp_text reference U2 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B84000E)
    (at 115.5 99.25)
    (fp_text reference U3 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(Q1-Pad1)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B84000E)
    (at 116.5 97.5)
    (fp_text reference U4 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q1-Pad2)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B84000E)
    (at 116.5 95.75)
    (fp_text reference U5 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(Q2-Pad1)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B84000E)
    (at 116.5 94)
    (fp_text reference U6 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(Q2-Pad2)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B84000E)
    (at 111.5 94)
    (fp_text reference U7 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad2)"))
  )
  (module "Local Library:WirePad" (layer B.Cu) (tedit 5B84000E)
    (at 111.5 95.75)
    (fp_text reference U8 (at 0.04 -3.22) (layer B.Fab))
    (fp_text value WirePad (at -0.02 2.88) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D2-Pad1)"))
  )
  (gr_circle (center 114 96) (end 119 96) (layer Edge.Cuts) (width 0.15))
)
