(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 422)
    (zones 0)
    (modules 72)
    (nets 101)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only yes)
    (trace_min 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.038)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /vcca)
  (net 3 /vccd)
  (net 4 +3V3)
  (net 5 /usb_d+)
  (net 6 /usb_d-)
  (net 7 /usb_vbus)
  (net 8 +5V)
  (net 9 "Net-(C16-Pad1)")
  (net 10 /xo)
  (net 11 /xi)
  (net 12 "Net-(C22-Pad1)")
  (net 13 "Net-(C23-Pad2)")
  (net 14 "Net-(C25-Pad2)")
  (net 15 "Net-(C25-Pad1)")
  (net 16 "Net-(C26-Pad2)")
  (net 17 "Net-(C26-Pad1)")
  (net 18 /dac_l)
  (net 19 /dac_r)
  (net 20 "Net-(C30-Pad1)")
  (net 21 "Net-(C31-Pad1)")
  (net 22 "Net-(C33-Pad2)")
  (net 23 "Net-(C34-Pad2)")
  (net 24 "Net-(C34-Pad1)")
  (net 25 "Net-(J1-Pad4)")
  (net 26 "Net-(J1-Pad3)")
  (net 27 "Net-(J1-Pad2)")
  (net 28 "Net-(J1-Pad6)")
  (net 29 "Net-(J2-Pad20)")
  (net 30 "Net-(J2-Pad19)")
  (net 31 "Net-(J2-Pad18)")
  (net 32 "Net-(J2-Pad17)")
  (net 33 /bt_gp5)
  (net 34 /bt_gp4)
  (net 35 /bt_tx)
  (net 36 /bt_cts)
  (net 37 /bt_rx)
  (net 38 /bt_rts)
  (net 39 /bt_gp3)
  (net 40 "Net-(J2-Pad9)")
  (net 41 /bt_gp2)
  (net 42 /bt_rst)
  (net 43 "Net-(J2-Pad6)")
  (net 44 /bt_gp7)
  (net 45 "Net-(J2-Pad4)")
  (net 46 /bt_gp6)
  (net 47 /xres)
  (net 48 /i2s_mck)
  (net 49 /i2s_lrck)
  (net 50 /i2s_sck)
  (net 51 "Net-(J6-PadR)")
  (net 52 "Net-(J6-PadT)")
  (net 53 "Net-(R4-Pad1)")
  (net 54 "Net-(R10-Pad1)")
  (net 55 /a0)
  (net 56 /a1)
  (net 57 /a2)
  (net 58 "Net-(U1-Pad4)")
  (net 59 "Net-(U2-Pad60)")
  (net 60 "Net-(U2-Pad56)")
  (net 61 "Net-(U2-Pad55)")
  (net 62 "Net-(U2-Pad54)")
  (net 63 /i2s_sdo)
  (net 64 /~mute~)
  (net 65 "Net-(U2-Pad46)")
  (net 66 "Net-(U2-Pad41)")
  (net 67 "Net-(U2-Pad40)")
  (net 68 "Net-(U2-Pad39)")
  (net 69 "Net-(U2-Pad38)")
  (net 70 "Net-(U2-Pad32)")
  (net 71 "Net-(U2-Pad31)")
  (net 72 "Net-(U2-Pad30)")
  (net 73 "Net-(U2-Pad29)")
  (net 74 "Net-(U2-Pad21)")
  (net 75 "Net-(U2-Pad20)")
  (net 76 "Net-(U2-Pad19)")
  (net 77 "Net-(U2-Pad18)")
  (net 78 "Net-(U2-Pad16)")
  (net 79 "Net-(U2-Pad13)")
  (net 80 "Net-(U2-Pad6)")
  (net 81 "Net-(U4-Pad7)")
  (net 82 "Net-(H2-Pad1)")
  (net 83 "Net-(H3-Pad1)")
  (net 84 "Net-(H4-Pad1)")
  (net 85 /sw1)
  (net 86 /sw2)
  (net 87 /sw3)
  (net 88 "Net-(U2-Pad53)")
  (net 89 "Net-(U2-Pad51)")
  (net 90 "Net-(U2-Pad50)")
  (net 91 "Net-(U2-Pad49)")
  (net 92 "Net-(U2-Pad48)")
  (net 93 "Net-(U4-Pad8)")
  (net 94 /as)
  (net 95 "Net-(U2-Pad62)")
  (net 96 "Net-(U2-Pad61)")
  (net 97 /swdio)
  (net 98 /swdck)
  (net 99 "Net-(U2-Pad15)")
  (net 100 "Net-(U2-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /a0)
    (add_net /a1)
    (add_net /a2)
    (add_net /as)
    (add_net /bt_cts)
    (add_net /bt_gp2)
    (add_net /bt_gp3)
    (add_net /bt_gp4)
    (add_net /bt_gp5)
    (add_net /bt_gp6)
    (add_net /bt_gp7)
    (add_net /bt_rst)
    (add_net /bt_rts)
    (add_net /bt_rx)
    (add_net /bt_tx)
    (add_net /dac_l)
    (add_net /dac_r)
    (add_net /i2s_lrck)
    (add_net /i2s_mck)
    (add_net /i2s_sck)
    (add_net /i2s_sdo)
    (add_net /sw1)
    (add_net /sw2)
    (add_net /sw3)
    (add_net /swdck)
    (add_net /swdio)
    (add_net /usb_d+)
    (add_net /usb_d-)
    (add_net /usb_vbus)
    (add_net /vcca)
    (add_net /vccd)
    (add_net /xi)
    (add_net /xo)
    (add_net /xres)
    (add_net /~mute~)
    (add_net GND)
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C33-Pad2)")
    (add_net "Net-(C34-Pad1)")
    (add_net "Net-(C34-Pad2)")
    (add_net "Net-(H2-Pad1)")
    (add_net "Net-(H3-Pad1)")
    (add_net "Net-(H4-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J6-PadR)")
    (add_net "Net-(J6-PadT)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad46)")
    (add_net "Net-(U2-Pad48)")
    (add_net "Net-(U2-Pad49)")
    (add_net "Net-(U2-Pad50)")
    (add_net "Net-(U2-Pad51)")
    (add_net "Net-(U2-Pad53)")
    (add_net "Net-(U2-Pad54)")
    (add_net "Net-(U2-Pad55)")
    (add_net "Net-(U2-Pad56)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad60)")
    (add_net "Net-(U2-Pad61)")
    (add_net "Net-(U2-Pad62)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
  )
  (module Fiducial:Fiducial_0.5mm_Mask1.5mm (layer F.Cu) (tedit 5C18D139)
    (at 127.5 102.75)
    (descr "Circular Fiducial, 0.5mm bare copper, 1.5mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID3 (at 0 -1.7145) (layer F.SilkS) hide)
    (fp_text value ~ (at 0 1.7145) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial:Fiducial_0.5mm_Mask1.5mm (layer F.Cu) (tedit 5C18D139)
    (at 159 131.5)
    (descr "Circular Fiducial, 0.5mm bare copper, 1.5mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID2 (at 0 -1.7145) (layer F.SilkS) hide)
    (fp_text value ~ (at 0 1.7145) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial:Fiducial_0.5mm_Mask1.5mm (layer F.Cu) (tedit 5C18D139)
    (at 93 139.75)
    (descr "Circular Fiducial, 0.5mm bare copper, 1.5mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID1 (at 0 -1.7145) (layer F.SilkS) hide)
    (fp_text value ~ (at 0 1.7145) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Symbol:Symbol_GNU-Logo_SilkscreenTop locked (layer F.Cu) (tedit 0)
    (at 127.25 107)
    (descr "GNU-Logo, GNU-Head, GNU-Kopf, Silkscreen,")
    (tags "GNU-Logo, GNU-Head, GNU-Kopf, Silkscreen,")
    (attr virtual)
    (fp_text reference REF** (at 0 -6.05028) (layer F.SilkS) hide)
    (fp_text value Symbol_GNU-Logo_SilkscreenTop (at 0 9.14908) (layer F.Fab))
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen locked (layer F.Cu) (tedit 0)
    (at 160 112)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:KiCad-Logo2_8mm_SilkScreen locked (layer F.Cu) (tedit 0)
    (at 100.75 132.25)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0 7.62) (layer F.Fab) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 108.75 111.25 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (zone_connect 0)
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /swdio) (zone_connect 0))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /swdck) (zone_connect 0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /xres) (zone_connect 0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3) (zone_connect 0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Mini-B_Wuerth_65100516121_Horizontal (layer F.Cu) (tedit 5EFF75A9)
    (at 94.9 119 270)
    (descr "Mini USB 2.0 Type B SMT Horizontal 5 Contacts (https://katalog.we-online.de/em/datasheet/65100516121.pdf)")
    (tags "Mini USB 2.0 Type B")
    (attr smd)
    (fp_text reference J1 (at 7 0 90) (layer F.SilkS))
    (fp_text value USB_B_Mini (at 0 7.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.2 0 270) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.2 0 270) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 smd rect (at 1.6 -2.6 270) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.8 -2.6 270) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -2.6 270) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.8 -2.6 270) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.6 -2.6 270) (size 0.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /usb_vbus))
    (pad 6 smd rect (at 4.4 -2.6 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -4.4 -2.6 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 4.4 2.9 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -4.4 2.9 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Mini-B_Wuerth_65100516121_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 99.75 96.85 90)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J2 (at -1.5 -3 90) (layer F.SilkS))
    (fp_text value Bluetooth (at 1.27 25.19 90) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /bt_gp5))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /bt_gp4))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /bt_tx))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /bt_cts))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /bt_rx))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /bt_rts))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /bt_gp3))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /bt_gp2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /bt_rst))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /bt_gp7))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /bt_gp6))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5E476F32)
    (at 150.5 132.8)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (attr smd)
    (fp_text reference U4 (at -2 -3.45) (layer F.SilkS))
    (fp_text value TPA6139A2 (at 0 3.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd roundrect (at 2.8625 -1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C31-Pad1)"))
    (pad 13 smd roundrect (at 2.8625 -1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(J6-PadR)"))
    (pad 12 smd roundrect (at 2.8625 -0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(R10-Pad1)"))
    (pad 11 smd roundrect (at 2.8625 0) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 2.8625 0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 9 smd roundrect (at 2.8625 1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C34-Pad1)"))
    (pad 8 smd roundrect (at 2.8625 1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(U4-Pad8)"))
    (pad 7 smd roundrect (at -2.8625 1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U4-Pad7)"))
    (pad 6 smd roundrect (at -2.8625 1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C34-Pad2)"))
    (pad 5 smd roundrect (at -2.8625 0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C33-Pad2)"))
    (pad 4 smd roundrect (at -2.8625 0) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /~mute~))
    (pad 3 smd roundrect (at -2.8625 -0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -2.8625 -1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(J6-PadT)"))
    (pad 1 smd roundrect (at -2.8625 -1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C30-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm_ThermalVias (layer F.Cu) (tedit 5DC5FE75)
    (at 99 108 180)
    (descr "MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference U1 (at 0 -2.45) (layer F.SilkS))
    (fp_text value LT3042xMSE (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.42 0.47 180) (size 0.7 0.79) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.42 -0.47 180) (size 0.7 0.79) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.42 0.47 180) (size 0.7 0.79) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.42 -0.47 180) (size 0.7 0.79) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 11 smd rect (at 0 0 180) (size 1.6 1.8) (layers B.Cu)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0.55 0.65 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 11 thru_hole circle (at -0.55 0.65 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0.55 -0.65 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 11 thru_hole circle (at -0.55 -0.65 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 11 smd rect (at 0 0 180) (size 1.68 1.88) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 10 smd roundrect (at 2.15 -1 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 9 smd roundrect (at 2.15 -0.5 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 8 smd roundrect (at 2.15 0 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at 2.15 0.5 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C16-Pad1)"))
    (pad 6 smd roundrect (at 2.15 1 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (pad 5 smd roundrect (at -2.15 1 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(R4-Pad1)"))
    (pad 4 smd roundrect (at -2.15 0.5 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(U1-Pad4)"))
    (pad 3 smd roundrect (at -2.15 0 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (pad 2 smd roundrect (at -2.15 -0.5 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (pad 1 smd roundrect (at -2.15 -1 180) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H13mm (layer F.Cu) (tedit 5EFF757D)
    (at 154.5 100 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=13mm")
    (tags "tact sw push 6mm")
    (zone_connect 0)
    (fp_text reference SW3 (at 3.25 -2.5) (layer F.SilkS))
    (fp_text value ~ (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 /sw3) (zone_connect 0))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H13mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H13mm (layer F.Cu) (tedit 5EFF7581)
    (at 138 95.5)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=13mm")
    (tags "tact sw push 6mm")
    (zone_connect 0)
    (fp_text reference SW2 (at 3.5 7) (layer F.SilkS))
    (fp_text value ~ (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 86 /sw2) (zone_connect 0))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H13mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H13mm (layer F.Cu) (tedit 5EFF7586)
    (at 134.5 100 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=13mm")
    (tags "tact sw push 6mm")
    (zone_connect 0)
    (fp_text reference SW1 (at 3.25 -2.5) (layer F.SilkS))
    (fp_text value ~ (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 85 /sw1) (zone_connect 0))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H13mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 160.5 151.5)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H4 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value ~ (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 84 "Net-(H4-Pad1)"))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 160.5 96)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H3 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value ~ (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 83 "Net-(H3-Pad1)"))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 92 96)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H2 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value ~ (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 82 "Net-(H2-Pad1)"))
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 92 151.5)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H1 (at 0 -4) (layer F.SilkS))
    (fp_text value ~ (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 134.5 138.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 3 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /as))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117 138.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /as))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_PTV09A-1_Single_Vertical (layer F.Cu) (tedit 5A3D4993)
    (at 133.5 141.5 270)
    (descr "Potentiometer, vertical, Bourns PTV09A-1 Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
    (tags "Potentiometer vertical Bourns PTV09A-1 Single")
    (zone_connect 0)
    (fp_text reference RV3 (at -1.75 3 180) (layer F.SilkS))
    (fp_text value 100k (at 6.05 5.15 90) (layer F.Fab))
    (fp_text user %R (at 2 -2.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7 1.9 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" np_thru_hole circle (at 7 -6.9 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 94 /as) (zone_connect 0))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 57 /a2) (zone_connect 0))
    (pad 3 thru_hole circle (at 0 -5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTV09A-1_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_PTV09A-1_Single_Vertical (layer F.Cu) (tedit 5A3D4993)
    (at 116.5 141.5 270)
    (descr "Potentiometer, vertical, Bourns PTV09A-1 Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
    (tags "Potentiometer vertical Bourns PTV09A-1 Single")
    (zone_connect 0)
    (fp_text reference RV2 (at -1.75 3 180) (layer F.SilkS))
    (fp_text value 100k (at 6.05 5.15 90) (layer F.Fab))
    (fp_text user %R (at 2 -2.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7 1.9 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" np_thru_hole circle (at 7 -6.9 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 94 /as) (zone_connect 0))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 56 /a1) (zone_connect 0))
    (pad 3 thru_hole circle (at 0 -5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTV09A-1_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_PTV09A-1_Single_Vertical (layer F.Cu) (tedit 5A3D4993)
    (at 99.5 141.5 270)
    (descr "Potentiometer, vertical, Bourns PTV09A-1 Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
    (tags "Potentiometer vertical Bourns PTV09A-1 Single")
    (zone_connect 0)
    (fp_text reference RV1 (at -1.75 3 180) (layer F.SilkS))
    (fp_text value 100k (at 6.05 5.15 90) (layer F.Fab))
    (fp_text user %R (at 2 -2.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7 1.9 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" np_thru_hole circle (at 7 -6.9 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 94 /as) (zone_connect 0))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 55 /a0) (zone_connect 0))
    (pad 3 thru_hole circle (at 0 -5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTV09A-1_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_Abracon_ABM3B-4Pin_5.0x3.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 116.5 125 90)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3B http://www.abracon.com/Resonators/abm3b.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.8 90) (layer F.SilkS))
    (fp_text value 12.288MHz (at 0 2.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -2 -1.2 90) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2 -1.2 90) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /xo))
    (pad 2 smd rect (at 2 1.2 90) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2 1.2 90) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /xi))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM3B-4Pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 138.3 109.5)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U3 (at 0 -2.55) (layer F.SilkS))
    (fp_text value CS4344 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at 2.15 -1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C26-Pad2)"))
    (pad 9 smd rect (at 2.15 -0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 8 smd rect (at 2.15 0) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.15 0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C25-Pad2)"))
    (pad 6 smd rect (at 2.15 1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C23-Pad2)"))
    (pad 5 smd rect (at -2.15 1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C22-Pad1)"))
    (pad 4 smd rect (at -2.15 0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /i2s_mck))
    (pad 3 smd rect (at -2.15 0) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 /i2s_lrck))
    (pad 2 smd rect (at -2.15 -0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /i2s_sck))
    (pad 1 smd rect (at -2.15 -1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 /i2s_sdo))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP5.2x5.2mm_ThermalVias (layer F.Cu) (tedit 5DC5F6A6)
    (at 124.5 123 270)
    (descr "QFN, 68 Pin (https://cdn.microsemi.com/documents/1bf6886f-5919-4508-a50b-b1dbf3fdf0f4/download/#page=98), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (zone_connect 2)
    (attr smd)
    (fp_text reference U2 (at -5.5 -4) (layer F.SilkS))
    (fp_text value CY8C5888LTI-LP097 (at 0 5.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd roundrect (at 1.7625 1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at 1.7625 0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at 1.7625 -0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at 1.7625 -1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at 0.5875 1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at 0.5875 0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at 0.5875 -0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at 0.5875 -1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -0.5875 1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -0.5875 0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -0.5875 -0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -0.5875 -1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -1.7625 1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -1.7625 0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -1.7625 -0.5875 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad "" smd roundrect (at -1.7625 -1.7625 270) (size 1.006976 1.006976) (layers F.Paste) (roundrect_rratio 0.248268)
      (zone_connect 2))
    (pad 69 smd rect (at 0 0 270) (size 5.2 5.2) (layers B.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 2.35 2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 1.175 2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 0 2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -1.175 2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -2.35 2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 2.35 1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 1.175 1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 0 1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -1.175 1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -2.35 1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 2.35 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 1.175 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -1.175 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -2.35 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 2.35 -1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 1.175 -1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 0 -1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -1.175 -1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -2.35 -1.175 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 2.35 -2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 1.175 -2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at 0 -2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -1.175 -2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 thru_hole circle (at -2.35 -2.35 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 69 smd rect (at 0 0 270) (size 5.2 5.2) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 68 smd roundrect (at -3.2 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /i2s_lrck) (zone_connect 2))
    (pad 67 smd roundrect (at -2.8 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3) (zone_connect 2))
    (pad 66 smd roundrect (at -2.4 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /i2s_mck) (zone_connect 2))
    (pad 65 smd roundrect (at -2 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /sw1) (zone_connect 2))
    (pad 64 smd roundrect (at -1.6 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 /sw2) (zone_connect 2))
    (pad 63 smd roundrect (at -1.2 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 /sw3) (zone_connect 2))
    (pad 62 smd roundrect (at -0.8 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(U2-Pad62)") (zone_connect 2))
    (pad 61 smd roundrect (at -0.4 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(U2-Pad61)") (zone_connect 2))
    (pad 60 smd roundrect (at 0 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(U2-Pad60)") (zone_connect 2))
    (pad 59 smd roundrect (at 0.4 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3) (zone_connect 2))
    (pad 58 smd roundrect (at 0.8 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 57 smd roundrect (at 1.2 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /vccd) (zone_connect 2))
    (pad 56 smd roundrect (at 1.6 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(U2-Pad56)") (zone_connect 2))
    (pad 55 smd roundrect (at 2 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(U2-Pad55)") (zone_connect 2))
    (pad 54 smd roundrect (at 2.4 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(U2-Pad54)") (zone_connect 2))
    (pad 53 smd roundrect (at 2.8 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(U2-Pad53)") (zone_connect 2))
    (pad 52 smd roundrect (at 3.2 -3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3) (zone_connect 2))
    (pad 51 smd roundrect (at 3.9375 -3.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(U2-Pad51)") (zone_connect 2))
    (pad 50 smd roundrect (at 3.9375 -2.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(U2-Pad50)") (zone_connect 2))
    (pad 49 smd roundrect (at 3.9375 -2.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(U2-Pad49)") (zone_connect 2))
    (pad 48 smd roundrect (at 3.9375 -2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(U2-Pad48)") (zone_connect 2))
    (pad 47 smd roundrect (at 3.9375 -1.6 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /~mute~) (zone_connect 2))
    (pad 46 smd roundrect (at 3.9375 -1.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(U2-Pad46)") (zone_connect 2))
    (pad 45 smd roundrect (at 3.9375 -0.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 44 smd roundrect (at 3.9375 -0.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3) (zone_connect 2))
    (pad 43 smd roundrect (at 3.9375 0 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 42 smd roundrect (at 3.9375 0.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /vcca) (zone_connect 2))
    (pad 41 smd roundrect (at 3.9375 0.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(U2-Pad41)") (zone_connect 2))
    (pad 40 smd roundrect (at 3.9375 1.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(U2-Pad40)") (zone_connect 2))
    (pad 39 smd roundrect (at 3.9375 1.6 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(U2-Pad39)") (zone_connect 2))
    (pad 38 smd roundrect (at 3.9375 2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(U2-Pad38)") (zone_connect 2))
    (pad 37 smd roundrect (at 3.9375 2.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /a2) (zone_connect 2))
    (pad 36 smd roundrect (at 3.9375 2.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /a1) (zone_connect 2))
    (pad 35 smd roundrect (at 3.9375 3.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3) (zone_connect 2))
    (pad 34 smd roundrect (at 3.2 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /a0) (zone_connect 2))
    (pad 33 smd roundrect (at 2.8 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /as) (zone_connect 2))
    (pad 32 smd roundrect (at 2.4 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(U2-Pad32)") (zone_connect 2))
    (pad 31 smd roundrect (at 2 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(U2-Pad31)") (zone_connect 2))
    (pad 30 smd roundrect (at 1.6 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(U2-Pad30)") (zone_connect 2))
    (pad 29 smd roundrect (at 1.2 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(U2-Pad29)") (zone_connect 2))
    (pad 28 smd roundrect (at 0.8 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /xi) (zone_connect 2))
    (pad 27 smd roundrect (at 0.4 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /xo) (zone_connect 2))
    (pad 26 smd roundrect (at 0 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /vccd) (zone_connect 2))
    (pad 25 smd roundrect (at -0.4 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 24 smd roundrect (at -0.8 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3) (zone_connect 2))
    (pad 23 smd roundrect (at -1.2 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /usb_d-) (zone_connect 2))
    (pad 22 smd roundrect (at -1.6 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /usb_d+) (zone_connect 2))
    (pad 21 smd roundrect (at -2 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(U2-Pad21)") (zone_connect 2))
    (pad 20 smd roundrect (at -2.4 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(U2-Pad20)") (zone_connect 2))
    (pad 19 smd roundrect (at -2.8 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U2-Pad19)") (zone_connect 2))
    (pad 18 smd roundrect (at -3.2 3.9375 270) (size 0.2 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U2-Pad18)") (zone_connect 2))
    (pad 17 smd roundrect (at -3.9375 3.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3) (zone_connect 2))
    (pad 16 smd roundrect (at -3.9375 2.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U2-Pad16)") (zone_connect 2))
    (pad 15 smd roundrect (at -3.9375 2.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 "Net-(U2-Pad15)") (zone_connect 2))
    (pad 14 smd roundrect (at -3.9375 2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 "Net-(U2-Pad14)") (zone_connect 2))
    (pad 13 smd roundrect (at -3.9375 1.6 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(U2-Pad13)") (zone_connect 2))
    (pad 12 smd roundrect (at -3.9375 1.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /swdck) (zone_connect 2))
    (pad 11 smd roundrect (at -3.9375 0.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /swdio) (zone_connect 2))
    (pad 10 smd roundrect (at -3.9375 0.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /xres) (zone_connect 2))
    (pad 9 smd roundrect (at -3.9375 0 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 8 smd roundrect (at -3.9375 -0.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 7 smd roundrect (at -3.9375 -0.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd roundrect (at -3.9375 -1.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(U2-Pad6)") (zone_connect 2))
    (pad 5 smd roundrect (at -3.9375 -1.6 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd roundrect (at -3.9375 -2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /bt_rx) (zone_connect 2))
    (pad 3 smd roundrect (at -3.9375 -2.4 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /bt_tx) (zone_connect 2))
    (pad 2 smd roundrect (at -3.9375 -2.8 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /i2s_sdo) (zone_connect 2))
    (pad 1 smd roundrect (at -3.9375 -3.2 270) (size 0.825 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /i2s_sck) (zone_connect 2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-68-1EP_8x8mm_P0.4mm_EP5.2x5.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 150.5 127.25 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (zone_connect 0)
    (fp_text reference R10 (at 10.5 -2.25 90) (layer F.SilkS))
    (fp_text value 82k (at 7.62 2.37 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(R10-Pad1)") (zone_connect 0))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.5 123.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C26-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /dac_r))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.5 123.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -0.2 1.5 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /dac_l))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 157.25 120.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.5 120.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1 -1.43) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.25 106 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.5 1 270) (layer F.SilkS))
    (fp_text value 33.2k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 101 104 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 104 118 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -3 0) (layer F.SilkS))
    (fp_text value 27 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /usb_d-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 104 120 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -3 0) (layer F.SilkS))
    (fp_text value 27 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J1-Pad3)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /usb_d+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 99 127 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_CUI_SJ1-3535NG_Horizontal (layer F.Cu) (tedit 5C301453)
    (at 158 143 270)
    (descr "TRS 3.5mm, horizontal, through-hole, with switch, https://www.cui.com/product/resource/sj1-353xng.pdf")
    (tags "TRS audio jack stereo horizontal")
    (fp_text reference J6 (at -3.5 -3.5 90) (layer F.SilkS))
    (fp_text value Headphones (at 0.1 14.05 90) (layer F.Fab))
    (fp_text user %R (at 0.1 3.8 90) (layer F.Fab))
    (pad RN thru_hole oval (at 0 6.1 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask))
    (pad TN thru_hole oval (at 0 11.6 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask))
    (pad R thru_hole oval (at 2 7.9 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J6-PadR)"))
    (pad T thru_hole oval (at 2 2.4 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J6-PadT)"))
    (pad S thru_hole oval (at 0 0 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3535NG_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 101.75 112.5 270)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value ~ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /usb_vbus))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.2875 136.8 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at -3.2125 -0.2) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C34-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C34-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.5 134.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C33-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 155.75 134.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at -1.25 1.5 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 154.5 127.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 3.3uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /dac_r))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 146.5 127.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 3.3uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /dac_l))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C30-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 157.5 124.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 1.7) (layer F.SilkS))
    (fp_text value 2.7nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /dac_r))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.5 124.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at -3 -0.8) (layer F.SilkS))
    (fp_text value 2.7nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /dac_l))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 101.5 139)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 3.25 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /as))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 154.5 119.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 3.05 0 90) (layer F.SilkS))
    (fp_text value 3.3uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C26-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 146.5 119.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 3.05 0 90) (layer F.SilkS))
    (fp_text value 3.3uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C25-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 138.3 113.5 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 3 0 90) (layer F.SilkS))
    (fp_text value 3.3uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.75 113.25 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -3.5 0.2 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C23-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.3 113.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 3 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 144.3 108.4375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 1.7 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.3 108.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 3 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.5 129.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /xi))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.5 120.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -3 0) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /xo))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 94 109.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 92.25 105.75 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 104 108 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 3 0 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 101 115 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /usb_vbus))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.75 117.75 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 1.75 -1.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.5 124.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 3.25 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.5 127.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 3.25 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.25 131 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 3.25 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.75 129.5 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 2.75 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 105 115 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /usb_d-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 105 123 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /usb_d+))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.75 119 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.5 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 119.5 116.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127 131 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.75 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.75 117.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 3 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.5 126)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.75 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /vccd))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.5 131 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.75 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /vcca))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text https://github.com/half-spin (at 161 126.5 90) (layer F.SilkS))
  (gr_text "No Earbuds Allowed.\nHi-Fi Cans Only." (at 150.5 149.5) (layer F.SilkS))
  (gr_text "This text reduces\nTHD by 0.001%" (at 156 106.25) (layer F.SilkS))
  (gr_text "Half-Spin\nHeadphone DAC Proto V1.0\n2020-07-03" (at 113 101.25) (layer F.SilkS))
  (gr_arc (start 92 96) (end 92 92.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92 151.5) (end 88.5 151.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 160.5 151.5) (end 160.5 155) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 160.5 96) (end 164 96) (angle -90) (layer Edge.Cuts) (width 0.05))
  (dimension 62.5 (width 0.15) (layer Dwgs.User)
    (gr_text "62.500 mm" (at 168.8 123.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 164 155) (xy 168.086421 155)))
    (feature2 (pts (xy 164 92.5) (xy 168.086421 92.5)))
    (crossbar (pts (xy 167.5 92.5) (xy 167.5 155)))
    (arrow1a (pts (xy 167.5 155) (xy 166.913579 153.873496)))
    (arrow1b (pts (xy 167.5 155) (xy 168.086421 153.873496)))
    (arrow2a (pts (xy 167.5 92.5) (xy 166.913579 93.626504)))
    (arrow2b (pts (xy 167.5 92.5) (xy 168.086421 93.626504)))
  )
  (dimension 75.5 (width 0.15) (layer Dwgs.User)
    (gr_text "75.500 mm" (at 126.25 87.7) (layer Dwgs.User))
    (feature1 (pts (xy 164 92.5) (xy 164 88.413579)))
    (feature2 (pts (xy 88.5 92.5) (xy 88.5 88.413579)))
    (crossbar (pts (xy 88.5 89) (xy 164 89)))
    (arrow1a (pts (xy 164 89) (xy 162.873496 89.586421)))
    (arrow1b (pts (xy 164 89) (xy 162.873496 88.413579)))
    (arrow2a (pts (xy 88.5 89) (xy 89.626504 89.586421)))
    (arrow2b (pts (xy 88.5 89) (xy 89.626504 88.413579)))
  )
  (gr_line (start 88.5 151.5) (end 88.5 96) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160.5 155) (end 92 155) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 164 96) (end 164 151.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92 92.5) (end 160.5 92.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 164 155) (xy 88.5 155) (xy 88.5 92.5) (xy 164 92.5)
      )
    )
  )
  (zone (net 8) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 104.75 112.25) (xy 100.5 112.25) (xy 100.5 108) (xy 104.75 108)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 164 108) (xy 138.25 108) (xy 138.25 155) (xy 88.5 155) (xy 88.5 92.5)
        (xy 164 92.5)
      )
    )
    (polygon
      (pts
        (xy 100 107.5) (xy 100 112.75) (xy 105.25 112.75) (xy 105.25 107.5)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 143 155) (xy 137.75 155) (xy 137.75 136) (xy 143 136)
      )
    )
  )
)
