<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="122" y2="0" width="0" layer="20"/>
<wire x1="122" y1="0" x2="122" y2="86" width="0" layer="20"/>
<wire x1="122" y1="86" x2="0" y2="86" width="0" layer="20"/>
<wire x1="0" y1="86" x2="0" y2="0" width="0" layer="20"/>
<hole x="60.935" y="62.173" drill="6.4"/>
<wire x1="19.5" y1="38.5" x2="22" y2="38.5" width="0" layer="20"/>
<wire x1="19.5" y1="40.5" x2="22" y2="40.5" width="0" layer="20"/>
<wire x1="18.5" y1="39.5" x2="19.5" y2="40.5" width="0" layer="20" curve="-90"/>
<wire x1="19.5" y1="38.5" x2="18.5" y2="39.5" width="0" layer="20" curve="-90"/>
<wire x1="23" y1="39.5" x2="22" y2="38.5" width="0" layer="20" curve="-90"/>
<wire x1="22" y1="40.5" x2="23" y2="39.5" width="0" layer="20" curve="-90"/>
<text>CAPS_LOCK</text>
<text>NUM_LOCK</text>
<text>SCROLL_LOCK</text>
<text>KEYPAD</text>
<text>kinX keyboard controller</text>
<text>v2018-04-14</text>
<text>M. Stapelberg / V. Wunsch</text>
<wire x1="100" y1="38.5" x2="102.5" y2="38.5" width="0" layer="20"/>
<wire x1="100" y1="40.5" x2="102.5" y2="40.5" width="0" layer="20"/>
<wire x1="99" y1="39.5" x2="100" y2="40.5" width="0" layer="20" curve="-90"/>
<wire x1="100" y1="38.5" x2="99" y2="39.5" width="0" layer="20" curve="-90"/>
<wire x1="103.5" y1="39.5" x2="102.5" y2="38.5" width="0" layer="20" curve="-90"/>
<wire x1="102.5" y1="40.5" x2="103.5" y2="39.5" width="0" layer="20" curve="-90"/>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>PROGRAM</text>
</plain>
<libraries>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA10-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-molex-39-53">
<packages>
<package name="39-53-2135">
<description>"1.25 FPC CONN ASSY ZF 13"</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="4,1-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.1 mm, round</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
</packages>
</library>
<library name="t32_ref">
<packages>
<package name="LQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="R0603">
</package>
<package name="SOT-223">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;</description>
</package>
<package name="LED-0805">
</package>
<package name="ALPS_SKHH">
</package>
<package name="F0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="mk66fx1m0vmd18">
<packages>
<package name="TQFP144">
<description>&lt;b&gt;TQFP-144&lt;/b&gt;, from Altera.  0.5mm pin pitch.&lt;br&gt;
NOTICE - PCB should be laid out on a 0.5mm grid, or 0.0025" if you have to then finish routing manually.  Use 0.008"max traces with 0.009"min clearances.</description>
</package>
</packages>
</library>
<library name="crystals">
<description>&lt;b&gt;LAB11&lt;/b&gt; - Crystals of various frequencies.</description>
<packages>
<package name="FHXXX">
<description>Pericom Type FH crystals
2.5 mm x 2.0 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="molex-105133-0001">
<packages>
<package name="MOLEX_105133-0001">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="THUMB_LEFT_BAK" library="con-lstb" package="MA10-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_MOUSER" value="538-22-28-4100"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="THUMB_RIGHT_SPC" library="con-lstb" package="MA10-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_MOUSER" value="538-22-28-4100"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RGHT_13_DOWN" library="con-molex-39-53" package="39-53-2135" value="39-53-2355">
<attribute name="DIGIKEY" value="WM14526-ND"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="538-39-53-2135"/>
</element>
<element name="TOP_RIGHT" library="con-molex-39-53" package="39-53-2135" value="39-53-2355">
<attribute name="DIGIKEY" value="WM14526-ND"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="538-39-53-2135"/>
</element>
<element name="TOP_LEFT" library="con-molex-39-53" package="39-53-2135" value="39-53-2355">
<attribute name="DIGIKEY" value="WM14526-ND"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="538-39-53-2135"/>
</element>
<element name="LEFT_13_LT" library="con-molex-39-53" package="39-53-2135" value="39-53-2355">
<attribute name="DIGIKEY" value="WM14526-ND"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="538-39-53-2135"/>
</element>
<element name="LED1" library="led" package="SML1206" value="">
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="604-APT3216QBC/D"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="SML1206" value="">
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="604-APT3216QBC/D"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="SML1206" value="">
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="604-APT3216QBC/D"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="SML1206" value="">
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="604-APT3216QBC/D"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R1206" value="10K">
<attribute name="DIGIKEY" value="311-10.0KFRCT-ND"/>
<attribute name="MPN" value="RC1206FR-0710KL"/>
<attribute name="OC_MOUSER" value="603-RC1206FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R1206" value="10K">
<attribute name="DIGIKEY" value="311-10.0KFRCT-ND"/>
<attribute name="MPN" value="RC1206FR-0710KL"/>
<attribute name="OC_MOUSER" value="603-RC1206FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R1206" value="10K">
<attribute name="DIGIKEY" value="311-10.0KFRCT-ND"/>
<attribute name="MPN" value="RC1206FR-0710KL"/>
<attribute name="OC_MOUSER" value="603-RC1206FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R1206" value="10K">
<attribute name="DIGIKEY" value="311-10.0KFRCT-ND"/>
<attribute name="MPN" value="RC1206FR-0710KL"/>
<attribute name="OC_MOUSER" value="603-RC1206FR-0710KL"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="4,1-PAD" value="MOUNT-PAD-ROUND4.1"/>
<element name="MKL04Z32VLC4" library="t32_ref" package="LQFP32-08" value="MKL04Z32VLC4">
<attribute name="DESC" value="MKL04Z32VLC4 (preprogrammed)"/>
<attribute name="MF" value="PJRC"/>
<attribute name="MPN" value="IC_MKL04Z32_TQFP32"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="LQFP-32"/>
<attribute name="TYPE" value="Microcontroller"/>
</element>
<element name="G1" library="crystals" package="FHXXX" value="16MHz">
<attribute name="DIGIKEY" value="SER4068CT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="MPN" value="FH1600015"/>
<attribute name="OC_MOUSER" value="729-FH1600015"/>
<attribute name="VALUE"/>
</element>
<element name="G2" library="t32_ref" package="TC26H" value="32.768kHz">
<attribute name="DESC" value="32.768kHz / 12.5pF / 20ppm"/>
<attribute name="MF" value="Citizen FineDevice"/>
<attribute name="MPN" value=" CFS206-32.768KDZF-UB"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="695-CFS206-327KF-U"/>
<attribute name="PACKAGE" value="TC-26H"/>
<attribute name="TYPE" value="Crystal"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="t32_ref" package="C0805" value="2.2uF">
<attribute name="DESC" value="2.2uF / 25 VDC / X7R "/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="TMK212B7225KG-TR"/>
<attribute name="OC_MOUSER" value="963-TMK212B7225KG-TR"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="t32_ref" package="C0805" value="2.2uF">
<attribute name="DESC" value="2.2uF / 25 VDC / X7R "/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="TMK212B7225KG-TR"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="963-TMK212B7225KG-TR"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="t32_ref" package="R0603" value="33R">
<attribute name="DESC" value="33R / 1% / 0.25 W"/>
<attribute name="MF" value="Panasonic"/>
<attribute name="MPN" value="ERJ-PA3F33R0V"/>
<attribute name="OC_MOUSER" value="667-ERJ-PA3F33R0V"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Resistor"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="t32_ref" package="R0603" value="470R">
<attribute name="DESC" value="470R / 1 % /  0.1 W"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MPN" value="CRCW0603470RFKEA"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="71-CRCW0603-470-E3"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Resistor"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="t32_ref" package="R0603" value="33R">
<attribute name="DESC" value="33R / 1% / 0.25 W"/>
<attribute name="MF" value="Panasonic"/>
<attribute name="MPN" value="ERJ-PA3F33R0V"/>
<attribute name="OC_MOUSER" value="667-ERJ-PA3F33R0V"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Resistor"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="t32_ref" package="SOT-223" value="MCP1825S">
<attribute name="DESC" value="3.3V 500mA"/>
<attribute name="DIGIKEY" value="MCP1825S-3302E/DB-ND"/>
<attribute name="MF" value="Microchip Technology"/>
<attribute name="MPN" value="MCP1825S-3302E/DB"/>
<attribute name="OC_MOUSER" value="579-MCP1825S-3302EDB"/>
<attribute name="PACKAGE" value="SOT-223-3"/>
<attribute name="TYPE" value="Voltage regulator"/>
<attribute name="VALUE"/>
</element>
<element name="LED_PWR" library="t32_ref" package="LED-0805" value="">
<attribute name="DESC" value="orange"/>
<attribute name="MF" value="ROHM Semiconductor"/>
<attribute name="MPN" value="SML-211DTT86"/>
<attribute name="OC_MOUSER" value="755-SML-211DTT86"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="TYPE" value="LED"/>
</element>
<element name="S1" library="t32_ref" package="ALPS_SKHH" value="">
<attribute name="DESC" value="SPST"/>
<attribute name="MF" value="ALPS"/>
<attribute name="MPN" value="SKHHPKA010"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="688-SKHHPK"/>
<attribute name="PACKAGE" value="6x6x5 MM"/>
<attribute name="TYPE" value="Tactile switch"/>
</element>
<element name="R12" library="t32_ref" package="F0805" value="FUSE">
<attribute name="DESC" value="6V / 0.5A"/>
<attribute name="DIGIKEY" value="507-1813-1-ND"/>
<attribute name="MF" value="Bel Fuse"/>
<attribute name="MPN" value="0ZCK0050FF2E"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="530-0ZCK0050FF2E"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="TYPE" value="PPTC"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="mk66fx1m0vmd18" package="TQFP144" value="MK66FX1M0VLQ18">
<attribute name="DIGIKEY" value="568-13334-ND"/>
<attribute name="OC_MOUSER" value="841-MK66FX1M0VLQ18"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="t32_ref" package="R0603" value="33R">
<attribute name="DESC" value="33R / 1% / 0.25 W"/>
<attribute name="MF" value="Panasonic"/>
<attribute name="MPN" value="ERJ-PA3F33R0V"/>
<attribute name="OC_MOUSER" value="667-ERJ-PA3F33R0V"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Resistor"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="t32_ref" package="R0603" value="33R">
<attribute name="DESC" value="33R / 1% / 0.25 W"/>
<attribute name="MF" value="Panasonic"/>
<attribute name="MPN" value="ERJ-PA3F33R0V"/>
<attribute name="OC_MOUSER" value="667-ERJ-PA3F33R0V"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Resistor"/>
<attribute name="VALUE"/>
</element>
<element name="USBFS" library="molex-105133-0001" package="MOLEX_105133-0001" value="105133-0001">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Conn Micro USB Type B RCP 5 POS 0.65mm Solder RA SMD 5 Terminal 1 Port Embossed T/R "/>
<attribute name="DIGIKEY" value="WM10134CT-ND"/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="105133-0011"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="538-105133-0011"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="0.48 USD"/>
</element>
<element name="USBHS" library="molex-105133-0001" package="MOLEX_105133-0001" value="105133-0001">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Conn Micro USB Type B RCP 5 POS 0.65mm Solder RA SMD 5 Terminal 1 Port Embossed T/R "/>
<attribute name="DIGIKEY" value="WM10134CT-ND"/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="105133-0011"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="538-105133-0011"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="0.48 USD"/>
</element>
<element name="PROGHEAD" library="pinhead" package="1X04/90" value="">
<attribute name="OC_MOUSER" value="649-68016-404HLF"/>
</element>
<element name="UART0" library="pinhead" package="1X04/90" value="">
<attribute name="OC_MOUSER" value="649-68016-404HLF"/>
</element>
<element name="C6" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="t32_ref" package="C0603" value="0.1uF">
<attribute name="DESC" value="0.1uF / 16VDC /  X7R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="GRM188R71C104KA01D"/>
<attribute name="OC_MOUSER" value="80-C0603C104M4R7411"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Capacitor"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MKL04Z32VLC4" pad="6"/>
<contactref element="MKL04Z32VLC4" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="T1" pad="2"/>
<contactref element="T1" pad="PAD"/>
<contactref element="R8" pad="1"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="71"/>
<contactref element="G1" pad="4"/>
<contactref element="G1" pad="2"/>
<contactref element="USBFS" pad="P$1"/>
<contactref element="USBFS" pad="P$2"/>
<contactref element="USBHS" pad="P$1"/>
<contactref element="USBHS" pad="P$2"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="33"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="17"/>
<contactref element="U$1" pad="44"/>
<contactref element="U$1" pad="93"/>
<contactref element="U$1" pad="107"/>
<contactref element="U$1" pad="121"/>
<contactref element="U$1" pad="134"/>
<contactref element="U$1" pad="57"/>
<contactref element="PROGHEAD" pad="3"/>
<contactref element="PROGHEAD" pad="4"/>
<contactref element="UART0" pad="1"/>
<contactref element="UART0" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="USBHS" pad="P$3"/>
<contactref element="USBFS" pad="P$3"/>
<contactref element="USBFS" pad="5"/>
<contactref element="USBHS" pad="5"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="24"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="ROW_8">
<contactref element="THUMB_RIGHT_SPC" pad="5"/>
<contactref element="RGHT_13_DOWN" pad="P$2"/>
<contactref element="U$1" pad="79"/>
</signal>
<signal name="ROW_6">
<contactref element="THUMB_RIGHT_SPC" pad="6"/>
<contactref element="RGHT_13_DOWN" pad="P$1"/>
<contactref element="U$1" pad="80"/>
</signal>
<signal name="ROW_F2">
<contactref element="TOP_RIGHT" pad="P$4"/>
<contactref element="TOP_RIGHT" pad="P$7"/>
<contactref element="TOP_RIGHT" pad="P$12"/>
<contactref element="TOP_LEFT" pad="P$4"/>
<contactref element="TOP_LEFT" pad="P$7"/>
<contactref element="TOP_LEFT" pad="P$11"/>
<contactref element="U$1" pad="138"/>
</signal>
<signal name="ROW_F1">
<contactref element="TOP_RIGHT" pad="P$6"/>
<contactref element="TOP_RIGHT" pad="P$13"/>
<contactref element="TOP_LEFT" pad="P$3"/>
<contactref element="TOP_LEFT" pad="P$6"/>
<contactref element="TOP_LEFT" pad="P$10"/>
<contactref element="TOP_RIGHT" pad="P$3"/>
<contactref element="U$1" pad="137"/>
</signal>
<signal name="ROW_ESC">
<contactref element="TOP_RIGHT" pad="P$9"/>
<contactref element="TOP_LEFT" pad="P$2"/>
<contactref element="U$1" pad="136"/>
</signal>
<signal name="ROW_2">
<contactref element="THUMB_LEFT_BAK" pad="8"/>
<contactref element="LEFT_13_LT" pad="P$6"/>
<contactref element="U$1" pad="112"/>
</signal>
<signal name="ROW_9">
<contactref element="THUMB_RIGHT_SPC" pad="3"/>
<contactref element="RGHT_13_DOWN" pad="P$12"/>
<contactref element="U$1" pad="76"/>
</signal>
<signal name="ROW_7">
<contactref element="THUMB_RIGHT_SPC" pad="4"/>
<contactref element="RGHT_13_DOWN" pad="P$3"/>
<contactref element="U$1" pad="78"/>
</signal>
<signal name="COL1">
<contactref element="LEFT_13_LT" pad="P$9"/>
<contactref element="RGHT_13_DOWN" pad="P$9"/>
<contactref element="TOP_LEFT" pad="P$5"/>
<contactref element="U$1" pad="128"/>
</signal>
<signal name="COL2">
<contactref element="LEFT_13_LT" pad="P$11"/>
<contactref element="RGHT_13_DOWN" pad="P$8"/>
<contactref element="TOP_LEFT" pad="P$1"/>
<contactref element="U$1" pad="129"/>
</signal>
<signal name="COL4">
<contactref element="LEFT_13_LT" pad="P$13"/>
<contactref element="RGHT_13_DOWN" pad="P$4"/>
<contactref element="TOP_RIGHT" pad="P$5"/>
<contactref element="U$1" pad="131"/>
</signal>
<signal name="COL5">
<contactref element="THUMB_LEFT_BAK" pad="5"/>
<contactref element="THUMB_RIGHT_SPC" pad="8"/>
<contactref element="TOP_RIGHT" pad="P$10"/>
<contactref element="TOP_RIGHT" pad="P$11"/>
<contactref element="U$1" pad="132"/>
</signal>
<signal name="COL6">
<contactref element="THUMB_LEFT_BAK" pad="4"/>
<contactref element="THUMB_RIGHT_SPC" pad="7"/>
<contactref element="U$1" pad="133"/>
</signal>
<signal name="COL3">
<contactref element="LEFT_13_LT" pad="P$12"/>
<contactref element="TOP_RIGHT" pad="P$8"/>
<contactref element="RGHT_13_DOWN" pad="P$7"/>
<contactref element="U$1" pad="130"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$2">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$14">
<contactref element="LED4" pad="C"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R3" pad="1"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="VCC">
</signal>
<signal name="ROW_4">
<contactref element="THUMB_LEFT_BAK" pad="2"/>
<contactref element="LEFT_13_LT" pad="P$3"/>
<contactref element="U$1" pad="110"/>
</signal>
<signal name="ROW_5">
<contactref element="THUMB_LEFT_BAK" pad="1"/>
<contactref element="LEFT_13_LT" pad="P$2"/>
<contactref element="U$1" pad="109"/>
</signal>
<signal name="ROW_3">
<contactref element="THUMB_LEFT_BAK" pad="3"/>
<contactref element="LEFT_13_LT" pad="P$4"/>
<contactref element="U$1" pad="111"/>
</signal>
<signal name="ROW_1">
<contactref element="LEFT_13_LT" pad="P$7"/>
<contactref element="U$1" pad="113"/>
</signal>
<signal name="ROW_EQL">
<contactref element="LEFT_13_LT" pad="P$8"/>
<contactref element="U$1" pad="114"/>
</signal>
<signal name="ROW_0">
<contactref element="RGHT_13_DOWN" pad="P$13"/>
<contactref element="U$1" pad="75"/>
</signal>
<signal name="ROW_MIN">
<contactref element="RGHT_13_DOWN" pad="P$6"/>
<contactref element="U$1" pad="77"/>
</signal>
<signal name="COL0">
<contactref element="LEFT_13_LT" pad="P$1"/>
<contactref element="RGHT_13_DOWN" pad="P$10"/>
<contactref element="TOP_LEFT" pad="P$8"/>
<contactref element="U$1" pad="127"/>
</signal>
<signal name="LED_KEYPAD">
<contactref element="R4" pad="2"/>
<contactref element="U$1" pad="102"/>
</signal>
<signal name="LED_SCROLL_LOCK">
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="103"/>
</signal>
<signal name="LED_NUM_LOCK">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="104"/>
</signal>
<signal name="LED_CAPS_LOCK">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="105"/>
</signal>
<signal name="SWD_CLK">
<contactref element="MKL04Z32VLC4" pad="16"/>
<contactref element="U$1" pad="50"/>
</signal>
<signal name="N$18">
<contactref element="G1" pad="1"/>
<contactref element="U$1" pad="73"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="72"/>
<contactref element="G1" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="G2" pad="2"/>
<contactref element="U$1" pad="40"/>
</signal>
<signal name="N$21">
<contactref element="G2" pad="1"/>
<contactref element="U$1" pad="41"/>
</signal>
<signal name="D0F_P">
<contactref element="R7" pad="2"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="D0_P">
<contactref element="R7" pad="1"/>
<contactref element="USBFS" pad="3"/>
</signal>
<signal name="D0_N">
<contactref element="R5" pad="1"/>
<contactref element="USBFS" pad="2"/>
</signal>
<signal name="USBFS_VBUS">
<contactref element="C3" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="USBFS" pad="1"/>
</signal>
<signal name="PTA1">
<contactref element="MKL04Z32VLC4" pad="10"/>
<contactref element="U$1" pad="51"/>
</signal>
<signal name="N$41">
<contactref element="LED_PWR" pad="+"/>
<contactref element="U$1" pad="106"/>
</signal>
<signal name="N$70">
<contactref element="MKL04Z32VLC4" pad="18"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="PROGHEAD" pad="1"/>
</signal>
<signal name="RESET_B">
<contactref element="MKL04Z32VLC4" pad="25"/>
<contactref element="MKL04Z32VLC4" pad="8"/>
<contactref element="U$1" pad="74"/>
</signal>
<signal name="SWD_DIO">
<contactref element="MKL04Z32VLC4" pad="15"/>
<contactref element="U$1" pad="53"/>
</signal>
<signal name="N$80">
<contactref element="R8" pad="2"/>
<contactref element="LED_PWR" pad="-"/>
</signal>
<signal name="PTA2">
<contactref element="MKL04Z32VLC4" pad="17"/>
<contactref element="U$1" pad="52"/>
</signal>
<signal name="D0F_N">
<contactref element="U$1" pad="20"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="D1F_P">
<contactref element="U$1" pad="25"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D1_P">
<contactref element="R6" pad="1"/>
<contactref element="USBHS" pad="3"/>
</signal>
<signal name="D1F_N">
<contactref element="U$1" pad="26"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="D1_N">
<contactref element="R9" pad="1"/>
<contactref element="USBHS" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="C12" pad="1"/>
<contactref element="MKL04Z32VLC4" pad="3"/>
<contactref element="MKL04Z32VLC4" pad="4"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="32"/>
<contactref element="U$1" pad="31"/>
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="43"/>
<contactref element="U$1" pad="70"/>
<contactref element="U$1" pad="94"/>
<contactref element="U$1" pad="108"/>
<contactref element="U$1" pad="122"/>
<contactref element="U$1" pad="135"/>
<contactref element="U$1" pad="56"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="U$1" pad="42"/>
<contactref element="U$1" pad="21"/>
<contactref element="PROGHEAD" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="T1" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$7">
<contactref element="R12" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="VREG_IN0">
<contactref element="U$1" pad="22"/>
</signal>
<signal name="VREG_IN1">
<contactref element="U$1" pad="23"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="66"/>
<contactref element="UART0" pad="3"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="67"/>
<contactref element="UART0" pad="2"/>
</signal>
<signal name="USBHS_VBUS">
<contactref element="USBHS" pad="1"/>
<contactref element="U$1" pad="27"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
