(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.01)
    (solder_mask_min_width 0.01)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J3_S4-Pin_1-Pad1)")
  (net 2 "Net-(J83-Pin_5)")
  (net 3 "Net-(J84-Pin_1)")
  (net 4 "Net-(J84-Pin_3)")
  (net 5 "Net-(J84-Pin_5)")
  (net 6 "Net-(J85-Pin_1)")
  (net 7 "Net-(J85-Pin_3)")
  (net 8 "Net-(J85-Pin_5)")
  (net 9 "Net-(J86-Pin_1)")
  (net 10 "Net-(J86-Pin_3)")
  (net 11 "Net-(J86-Pin_5)")
  (net 12 "Net-(J87-Pin_1)")
  (net 13 "Net-(J87-Pin_3)")
  (net 14 "Net-(J87-Pin_5)")
  (net 15 "Net-(J88-Pin_1)")
  (net 16 "Net-(J88-Pin_3)")
  (net 17 "Net-(J88-Pin_5)")
  (net 18 "Net-(J67-Pin_2)")
  (net 19 "Net-(J67-Pin_4)")
  (net 20 "Net-(J68-Pin_1)")
  (net 21 "Net-(J68-Pin_3)")
  (net 22 "Net-(J68-Pin_5)")
  (net 23 "Net-(J69-Pin_1)")
  (net 24 "Net-(J69-Pin_3)")
  (net 25 "Net-(J69-Pin_5)")
  (net 26 "Net-(J70-Pin_1)")
  (net 27 "Net-(J70-Pin_3)")
  (net 28 "Net-(J70-Pin_5)")
  (net 29 "Net-(J71-Pin_1)")
  (net 30 "Net-(J71-Pin_3)")
  (net 31 "Net-(J71-Pin_5)")
  (net 32 "Net-(J72-Pin_1)")
  (net 33 "Net-(J72-Pin_3)")
  (net 34 "Net-(J72-Pin_5)")
  (net 35 "Net-(J73-Pin_1)")
  (net 36 "Net-(J73-Pin_3)")
  (net 37 "Net-(J73-Pin_5)")
  (net 38 "Net-(J74-Pin_1)")
  (net 39 "Net-(J74-Pin_3)")
  (net 40 "Net-(J74-Pin_5)")
  (net 41 "Net-(J75-Pin_1)")
  (net 42 "Net-(J75-Pin_3)")
  (net 43 "Net-(J75-Pin_5)")
  (net 44 "Net-(J76-Pin_1)")
  (net 45 "Net-(J76-Pin_3)")
  (net 46 "Net-(J76-Pin_5)")
  (net 47 "Net-(J77-Pin_1)")
  (net 48 "Net-(J77-Pin_3)")
  (net 49 "Net-(J77-Pin_5)")
  (net 50 "Net-(J78-Pin_2)")
  (net 51 "Net-(J78-Pin_4)")
  (net 52 "Net-(J79-Pin_1)")
  (net 53 "Net-(J79-Pin_3)")
  (net 54 "Net-(J79-Pin_5)")
  (net 55 "Net-(J80-Pin_1)")
  (net 56 "Net-(J80-Pin_3)")
  (net 57 "Net-(J80-Pin_5)")
  (net 58 "Net-(J81-Pin_1)")
  (net 59 "Net-(J81-Pin_3)")
  (net 60 "Net-(J81-Pin_5)")
  (net 61 "Net-(J82-Pin_1)")
  (net 62 "Net-(J82-Pin_3)")
  (net 63 "Net-(J82-Pin_5)")
  (net 64 "Net-(J83-Pin_1)")
  (net 65 "Net-(J83-Pin_3)")
  (net 66 "Net-(J50-Pin_3)")
  (net 67 "Net-(J50-Pin_1)")
  (net 68 "Net-(J49-Pin_5)")
  (net 69 "Net-(J49-Pin_3)")
  (net 70 "Net-(J49-Pin_1)")
  (net 71 "Net-(J48-Pin_5)")
  (net 72 "Net-(J48-Pin_3)")
  (net 73 "Net-(J48-Pin_1)")
  (net 74 "Net-(J47-Pin_5)")
  (net 75 "Net-(J47-Pin_3)")
  (net 76 "Net-(J47-Pin_1)")
  (net 77 "Net-(J46-Pin_5)")
  (net 78 "Net-(J46-Pin_3)")
  (net 79 "Net-(J46-Pin_1)")
  (net 80 "Net-(J45-Pin_4)")
  (net 81 "Net-(J45-Pin_2)")
  (net 82 "Net-(J66-Pin_5)")
  (net 83 "Net-(J66-Pin_3)")
  (net 84 "Net-(J66-Pin_1)")
  (net 85 "Net-(J65-Pin_5)")
  (net 86 "Net-(J65-Pin_3)")
  (net 87 "Net-(J65-Pin_1)")
  (net 88 "Net-(J64-Pin_5)")
  (net 89 "Net-(J64-Pin_3)")
  (net 90 "Net-(J64-Pin_1)")
  (net 91 "Net-(J63-Pin_5)")
  (net 92 "Net-(J63-Pin_3)")
  (net 93 "Net-(J63-Pin_1)")
  (net 94 "Net-(J62-Pin_1)")
  (net 95 "Net-(J62-Pin_3)")
  (net 96 "Net-(J62-Pin_5)")
  (net 97 "Net-(J61-Pin_1)")
  (net 98 "Net-(J61-Pin_3)")
  (net 99 "Net-(J61-Pin_5)")
  (net 100 "Net-(J60-Pin_1)")
  (net 101 "Net-(J60-Pin_3)")
  (net 102 "Net-(J60-Pin_5)")
  (net 103 "Net-(J59-Pin_1)")
  (net 104 "Net-(J59-Pin_3)")
  (net 105 "Net-(J59-Pin_5)")
  (net 106 "Net-(J58-Pin_1)")
  (net 107 "Net-(J58-Pin_3)")
  (net 108 "Net-(J58-Pin_5)")
  (net 109 "Net-(J57-Pin_1)")
  (net 110 "Net-(J57-Pin_3)")
  (net 111 "Net-(J57-Pin_5)")
  (net 112 "Net-(J56-Pin_4)")
  (net 113 "Net-(J56-Pin_2)")
  (net 114 "Net-(J55-Pin_5)")
  (net 115 "Net-(J55-Pin_3)")
  (net 116 "Net-(J55-Pin_1)")
  (net 117 "Net-(J54-Pin_5)")
  (net 118 "Net-(J54-Pin_3)")
  (net 119 "Net-(J54-Pin_1)")
  (net 120 "Net-(J53-Pin_5)")
  (net 121 "Net-(J53-Pin_3)")
  (net 122 "Net-(J53-Pin_1)")
  (net 123 "Net-(J52-Pin_5)")
  (net 124 "Net-(J52-Pin_3)")
  (net 125 "Net-(J52-Pin_1)")
  (net 126 "Net-(J51-Pin_5)")
  (net 127 "Net-(J51-Pin_3)")
  (net 128 "Net-(J51-Pin_1)")
  (net 129 "Net-(J50-Pin_5)")
  (net 130 "Net-(J39-Pin_5)")
  (net 131 "Net-(J40-Pin_1)")
  (net 132 "Net-(J40-Pin_3)")
  (net 133 "Net-(J40-Pin_5)")
  (net 134 "Net-(J41-Pin_1)")
  (net 135 "Net-(J41-Pin_3)")
  (net 136 "Net-(J41-Pin_5)")
  (net 137 "Net-(J42-Pin_1)")
  (net 138 "Net-(J42-Pin_3)")
  (net 139 "Net-(J42-Pin_5)")
  (net 140 "Net-(J43-Pin_1)")
  (net 141 "Net-(J43-Pin_3)")
  (net 142 "Net-(J43-Pin_5)")
  (net 143 "Net-(J44-Pin_1)")
  (net 144 "Net-(J44-Pin_3)")
  (net 145 "Net-(J44-Pin_5)")
  (net 146 "Net-(J23-Pin_2)")
  (net 147 "Net-(J23-Pin_4)")
  (net 148 "Net-(J24-Pin_1)")
  (net 149 "Net-(J24-Pin_3)")
  (net 150 "Net-(J24-Pin_5)")
  (net 151 "Net-(J25-Pin_1)")
  (net 152 "Net-(J25-Pin_3)")
  (net 153 "Net-(J25-Pin_5)")
  (net 154 "Net-(J26-Pin_1)")
  (net 155 "Net-(J26-Pin_3)")
  (net 156 "Net-(J26-Pin_5)")
  (net 157 "Net-(J27-Pin_1)")
  (net 158 "Net-(J27-Pin_3)")
  (net 159 "Net-(J27-Pin_5)")
  (net 160 "Net-(J28-Pin_1)")
  (net 161 "Net-(J28-Pin_3)")
  (net 162 "Net-(J28-Pin_5)")
  (net 163 "Net-(J29-Pin_1)")
  (net 164 "Net-(J29-Pin_3)")
  (net 165 "Net-(J29-Pin_5)")
  (net 166 "Net-(J30-Pin_1)")
  (net 167 "Net-(J30-Pin_3)")
  (net 168 "Net-(J30-Pin_5)")
  (net 169 "Net-(J31-Pin_1)")
  (net 170 "Net-(J31-Pin_3)")
  (net 171 "Net-(J31-Pin_5)")
  (net 172 "Net-(J32-Pin_1)")
  (net 173 "Net-(J32-Pin_3)")
  (net 174 "Net-(J32-Pin_5)")
  (net 175 "Net-(J33-Pin_1)")
  (net 176 "Net-(J33-Pin_3)")
  (net 177 "Net-(J33-Pin_5)")
  (net 178 "Net-(J34-Pin_2)")
  (net 179 "Net-(J34-Pin_4)")
  (net 180 "Net-(J35-Pin_1)")
  (net 181 "Net-(J35-Pin_3)")
  (net 182 "Net-(J35-Pin_5)")
  (net 183 "Net-(J36-Pin_1)")
  (net 184 "Net-(J36-Pin_3)")
  (net 185 "Net-(J36-Pin_5)")
  (net 186 "Net-(J37-Pin_1)")
  (net 187 "Net-(J37-Pin_3)")
  (net 188 "Net-(J37-Pin_5)")
  (net 189 "Net-(J38-Pin_1)")
  (net 190 "Net-(J38-Pin_3)")
  (net 191 "Net-(J38-Pin_5)")
  (net 192 "Net-(J39-Pin_1)")
  (net 193 "Net-(J39-Pin_3)")
  (net 194 "Net-(J6-Pin_5)")
  (net 195 "Net-(J7-Pin_1)")
  (net 196 "Net-(J7-Pin_3)")
  (net 197 "Net-(J7-Pin_5)")
  (net 198 "Net-(J8-Pin_1)")
  (net 199 "Net-(J8-Pin_3)")
  (net 200 "Net-(J8-Pin_5)")
  (net 201 "Net-(J9-Pin_1)")
  (net 202 "Net-(J9-Pin_3)")
  (net 203 "Net-(J9-Pin_5)")
  (net 204 "Net-(J10-Pin_1)")
  (net 205 "Net-(J10-Pin_3)")
  (net 206 "Net-(J10-Pin_5)")
  (net 207 "Net-(J11-Pin_1)")
  (net 208 "Net-(J11-Pin_3)")
  (net 209 "Net-(J11-Pin_5)")
  (net 210 "Net-(J12-Pin_2)")
  (net 211 "Net-(J12-Pin_4)")
  (net 212 "Net-(J13-Pin_5)")
  (net 213 "Net-(J13-Pin_3)")
  (net 214 "Net-(J13-Pin_1)")
  (net 215 "Net-(J14-Pin_5)")
  (net 216 "Net-(J14-Pin_3)")
  (net 217 "Net-(J14-Pin_1)")
  (net 218 "Net-(J15-Pin_5)")
  (net 219 "Net-(J15-Pin_3)")
  (net 220 "Net-(J15-Pin_1)")
  (net 221 "Net-(J16-Pin_5)")
  (net 222 "Net-(J16-Pin_3)")
  (net 223 "Net-(J16-Pin_1)")
  (net 224 "Net-(J17-Pin_5)")
  (net 225 "Net-(J17-Pin_3)")
  (net 226 "Net-(J17-Pin_1)")
  (net 227 "Net-(J18-Pin_5)")
  (net 228 "Net-(J18-Pin_3)")
  (net 229 "Net-(J18-Pin_1)")
  (net 230 "Net-(J19-Pin_1)")
  (net 231 "Net-(J19-Pin_3)")
  (net 232 "Net-(J19-Pin_5)")
  (net 233 "Net-(J20-Pin_1)")
  (net 234 "Net-(J20-Pin_3)")
  (net 235 "Net-(J20-Pin_5)")
  (net 236 "Net-(J21-Pin_1)")
  (net 237 "Net-(J21-Pin_3)")
  (net 238 "Net-(J21-Pin_5)")
  (net 239 "Net-(J22-Pin_1)")
  (net 240 "Net-(J22-Pin_3)")
  (net 241 "Net-(J22-Pin_5)")
  (net 242 "Net-(J1-Pin_2)")
  (net 243 "Net-(J1-Pin_4)")
  (net 244 "Net-(J2-Pin_1)")
  (net 245 "Net-(J2-Pin_3)")
  (net 246 "Net-(J2-Pin_5)")
  (net 247 "Net-(J3-Pin_1)")
  (net 248 "Net-(J3-Pin_3)")
  (net 249 "Net-(J3-Pin_5)")
  (net 250 "Net-(J4-Pin_1)")
  (net 251 "Net-(J4-Pin_3)")
  (net 252 "Net-(J4-Pin_5)")
  (net 253 "Net-(J5-Pin_1)")
  (net 254 "Net-(J5-Pin_3)")
  (net 255 "Net-(J5-Pin_5)")
  (net 256 "Net-(J6-Pin_1)")
  (net 257 "Net-(J6-Pin_3)")
  (net 258 "Net-(J6-Pin_4)")
  (net 259 "Net-(J6-Pin_6)")
  (net 260 "Net-(J7-Pin_2)")
  (net 261 "Net-(J7-Pin_4)")
  (net 262 "Net-(J7-Pin_6)")
  (net 263 "Net-(J8-Pin_2)")
  (net 264 "Net-(J8-Pin_4)")
  (net 265 "Net-(J8-Pin_6)")
  (net 266 "Net-(J89-Pin_9)")
  (net 267 "Net-(J89-Pin_10)")
  (net 268 "Net-(J89-Pin_11)")
  (net 269 "Net-(J10-Pin_2)")
  (net 270 "Net-(J10-Pin_4)")
  (net 271 "Net-(J10-Pin_6)")
  (net 272 "Net-(J11-Pin_2)")
  (net 273 "Net-(J11-Pin_4)")
  (net 274 "Net-(J12-Pin_1)")
  (net 275 "Net-(J12-Pin_3)")
  (net 276 "Net-(J12-Pin_5)")
  (net 277 "Net-(J13-Pin_2)")
  (net 278 "Net-(J13-Pin_4)")
  (net 279 "Net-(J13-Pin_6)")
  (net 280 "Net-(J14-Pin_2)")
  (net 281 "Net-(J14-Pin_4)")
  (net 282 "Net-(J14-Pin_6)")
  (net 283 "Net-(J15-Pin_2)")
  (net 284 "Net-(J15-Pin_4)")
  (net 285 "Net-(J15-Pin_6)")
  (net 286 "Net-(J16-Pin_2)")
  (net 287 "Net-(J16-Pin_4)")
  (net 288 "Net-(J16-Pin_6)")
  (net 289 "Net-(J17-Pin_2)")
  (net 290 "Net-(J17-Pin_4)")
  (net 291 "Net-(J17-Pin_6)")
  (net 292 "Net-(J18-Pin_2)")
  (net 293 "Net-(J18-Pin_4)")
  (net 294 "Net-(J18-Pin_6)")
  (net 295 "Net-(J19-Pin_2)")
  (net 296 "Net-(J19-Pin_4)")
  (net 297 "Net-(J19-Pin_6)")
  (net 298 "Net-(J20-Pin_2)")
  (net 299 "Net-(J20-Pin_4)")
  (net 300 "Net-(J20-Pin_6)")
  (net 301 "Net-(J21-Pin_2)")
  (net 302 "Net-(J21-Pin_4)")
  (net 303 "Net-(J21-Pin_6)")
  (net 304 "Net-(J22-Pin_2)")
  (net 305 "Net-(J22-Pin_4)")
  (net 306 "Net-(J1-Pin_1)")
  (net 307 "Net-(J1-Pin_3)")
  (net 308 "Net-(J1-Pin_5)")
  (net 309 "Net-(J2-Pin_2)")
  (net 310 "Net-(J2-Pin_4)")
  (net 311 "Net-(J2-Pin_6)")
  (net 312 "Net-(J3-Pin_2)")
  (net 313 "Net-(J3-Pin_4)")
  (net 314 "Net-(J3-Pin_6)")
  (net 315 "Net-(J4-Pin_2)")
  (net 316 "Net-(J4-Pin_4)")
  (net 317 "Net-(J4-Pin_6)")
  (net 318 "Net-(J5-Pin_2)")
  (net 319 "Net-(J5-Pin_4)")
  (net 320 "Net-(J5-Pin_6)")
  (net 321 "Net-(J6-Pin_2)")
  (net 322 "Net-(J83-Pin_4)")
  (net 323 "Net-(J83-Pin_6)")
  (net 324 "Net-(J84-Pin_2)")
  (net 325 "Net-(J84-Pin_4)")
  (net 326 "Net-(J84-Pin_6)")
  (net 327 "Net-(J85-Pin_2)")
  (net 328 "Net-(J85-Pin_4)")
  (net 329 "Net-(J85-Pin_6)")
  (net 330 "Net-(J86-Pin_2)")
  (net 331 "Net-(J86-Pin_4)")
  (net 332 "Net-(J86-Pin_6)")
  (net 333 "Net-(J87-Pin_2)")
  (net 334 "Net-(J87-Pin_4)")
  (net 335 "Net-(J87-Pin_6)")
  (net 336 "Net-(J88-Pin_2)")
  (net 337 "Net-(J88-Pin_4)")
  (net 338 "Net-(J67-Pin_1)")
  (net 339 "Net-(J67-Pin_3)")
  (net 340 "Net-(J67-Pin_5)")
  (net 341 "Net-(J68-Pin_2)")
  (net 342 "Net-(J68-Pin_4)")
  (net 343 "Net-(J68-Pin_6)")
  (net 344 "Net-(J69-Pin_2)")
  (net 345 "Net-(J69-Pin_4)")
  (net 346 "Net-(J69-Pin_6)")
  (net 347 "Net-(J70-Pin_2)")
  (net 348 "Net-(J70-Pin_4)")
  (net 349 "Net-(J70-Pin_6)")
  (net 350 "Net-(J71-Pin_2)")
  (net 351 "Net-(J71-Pin_4)")
  (net 352 "Net-(J71-Pin_6)")
  (net 353 "Net-(J72-Pin_2)")
  (net 354 "Net-(J72-Pin_4)")
  (net 355 "Net-(J72-Pin_6)")
  (net 356 "Net-(J73-Pin_2)")
  (net 357 "Net-(J73-Pin_4)")
  (net 358 "Net-(J73-Pin_6)")
  (net 359 "Net-(J74-Pin_2)")
  (net 360 "Net-(J74-Pin_4)")
  (net 361 "Net-(J74-Pin_6)")
  (net 362 "Net-(J75-Pin_2)")
  (net 363 "Net-(J75-Pin_4)")
  (net 364 "Net-(J75-Pin_6)")
  (net 365 "Net-(J76-Pin_2)")
  (net 366 "Net-(J76-Pin_4)")
  (net 367 "Net-(J76-Pin_6)")
  (net 368 "Net-(J77-Pin_2)")
  (net 369 "Net-(J77-Pin_4)")
  (net 370 "Net-(J78-Pin_1)")
  (net 371 "Net-(J78-Pin_3)")
  (net 372 "Net-(J78-Pin_5)")
  (net 373 "Net-(J79-Pin_2)")
  (net 374 "Net-(J79-Pin_4)")
  (net 375 "Net-(J79-Pin_6)")
  (net 376 "Net-(J80-Pin_2)")
  (net 377 "Net-(J80-Pin_4)")
  (net 378 "Net-(J80-Pin_6)")
  (net 379 "Net-(J81-Pin_2)")
  (net 380 "Net-(J81-Pin_4)")
  (net 381 "Net-(J81-Pin_6)")
  (net 382 "Net-(J82-Pin_2)")
  (net 383 "Net-(J82-Pin_4)")
  (net 384 "Net-(J82-Pin_6)")
  (net 385 "Net-(J83-Pin_2)")
  (net 386 "Net-(J50-Pin_4)")
  (net 387 "Net-(J50-Pin_6)")
  (net 388 "Net-(J51-Pin_2)")
  (net 389 "Net-(J51-Pin_4)")
  (net 390 "Net-(J51-Pin_6)")
  (net 391 "Net-(J52-Pin_2)")
  (net 392 "Net-(J52-Pin_4)")
  (net 393 "Net-(J52-Pin_6)")
  (net 394 "Net-(J53-Pin_2)")
  (net 395 "Net-(J53-Pin_4)")
  (net 396 "Net-(J53-Pin_6)")
  (net 397 "Net-(J54-Pin_2)")
  (net 398 "Net-(J54-Pin_4)")
  (net 399 "Net-(J54-Pin_6)")
  (net 400 "Net-(J55-Pin_2)")
  (net 401 "Net-(J55-Pin_4)")
  (net 402 "Net-(J56-Pin_1)")
  (net 403 "Net-(J56-Pin_3)")
  (net 404 "Net-(J56-Pin_5)")
  (net 405 "Net-(J57-Pin_2)")
  (net 406 "Net-(J57-Pin_4)")
  (net 407 "Net-(J57-Pin_6)")
  (net 408 "Net-(J58-Pin_2)")
  (net 409 "Net-(J58-Pin_4)")
  (net 410 "Net-(J58-Pin_6)")
  (net 411 "Net-(J59-Pin_2)")
  (net 412 "Net-(J59-Pin_4)")
  (net 413 "Net-(J59-Pin_6)")
  (net 414 "Net-(J60-Pin_2)")
  (net 415 "Net-(J60-Pin_4)")
  (net 416 "Net-(J60-Pin_6)")
  (net 417 "Net-(J61-Pin_2)")
  (net 418 "Net-(J61-Pin_4)")
  (net 419 "Net-(J61-Pin_6)")
  (net 420 "Net-(J62-Pin_2)")
  (net 421 "Net-(J62-Pin_4)")
  (net 422 "Net-(J62-Pin_6)")
  (net 423 "Net-(J63-Pin_2)")
  (net 424 "Net-(J63-Pin_4)")
  (net 425 "Net-(J63-Pin_6)")
  (net 426 "Net-(J64-Pin_2)")
  (net 427 "Net-(J64-Pin_4)")
  (net 428 "Net-(J64-Pin_6)")
  (net 429 "Net-(J65-Pin_2)")
  (net 430 "Net-(J65-Pin_4)")
  (net 431 "Net-(J65-Pin_6)")
  (net 432 "Net-(J66-Pin_2)")
  (net 433 "Net-(J66-Pin_4)")
  (net 434 "Net-(J45-Pin_1)")
  (net 435 "Net-(J45-Pin_3)")
  (net 436 "Net-(J45-Pin_5)")
  (net 437 "Net-(J46-Pin_2)")
  (net 438 "Net-(J46-Pin_4)")
  (net 439 "Net-(J46-Pin_6)")
  (net 440 "Net-(J47-Pin_2)")
  (net 441 "Net-(J47-Pin_4)")
  (net 442 "Net-(J47-Pin_6)")
  (net 443 "Net-(J48-Pin_2)")
  (net 444 "Net-(J48-Pin_4)")
  (net 445 "Net-(J48-Pin_6)")
  (net 446 "Net-(J49-Pin_2)")
  (net 447 "Net-(J49-Pin_4)")
  (net 448 "Net-(J49-Pin_6)")
  (net 449 "Net-(J50-Pin_2)")
  (net 450 "Net-(J39-Pin_4)")
  (net 451 "Net-(J39-Pin_6)")
  (net 452 "Net-(J40-Pin_2)")
  (net 453 "Net-(J40-Pin_4)")
  (net 454 "Net-(J40-Pin_6)")
  (net 455 "Net-(J41-Pin_2)")
  (net 456 "Net-(J41-Pin_4)")
  (net 457 "Net-(J41-Pin_6)")
  (net 458 "Net-(J42-Pin_2)")
  (net 459 "Net-(J42-Pin_4)")
  (net 460 "Net-(J42-Pin_6)")
  (net 461 "Net-(J43-Pin_2)")
  (net 462 "Net-(J43-Pin_4)")
  (net 463 "Net-(J43-Pin_6)")
  (net 464 "Net-(J44-Pin_2)")
  (net 465 "Net-(J44-Pin_4)")
  (net 466 "Net-(J23-Pin_1)")
  (net 467 "Net-(J23-Pin_3)")
  (net 468 "Net-(J23-Pin_5)")
  (net 469 "Net-(J24-Pin_2)")
  (net 470 "Net-(J24-Pin_4)")
  (net 471 "Net-(J24-Pin_6)")
  (net 472 "Net-(J25-Pin_2)")
  (net 473 "Net-(J25-Pin_4)")
  (net 474 "Net-(J25-Pin_6)")
  (net 475 "Net-(J26-Pin_2)")
  (net 476 "Net-(J26-Pin_4)")
  (net 477 "Net-(J26-Pin_6)")
  (net 478 "Net-(J27-Pin_2)")
  (net 479 "Net-(J27-Pin_4)")
  (net 480 "Net-(J27-Pin_6)")
  (net 481 "Net-(J28-Pin_2)")
  (net 482 "Net-(J28-Pin_4)")
  (net 483 "Net-(J28-Pin_6)")
  (net 484 "Net-(J29-Pin_2)")
  (net 485 "Net-(J29-Pin_4)")
  (net 486 "Net-(J29-Pin_6)")
  (net 487 "Net-(J30-Pin_2)")
  (net 488 "Net-(J30-Pin_4)")
  (net 489 "Net-(J30-Pin_6)")
  (net 490 "Net-(J31-Pin_2)")
  (net 491 "Net-(J31-Pin_4)")
  (net 492 "Net-(J31-Pin_6)")
  (net 493 "Net-(J32-Pin_2)")
  (net 494 "Net-(J32-Pin_4)")
  (net 495 "Net-(J32-Pin_6)")
  (net 496 "Net-(J33-Pin_2)")
  (net 497 "Net-(J33-Pin_4)")
  (net 498 "Net-(J34-Pin_1)")
  (net 499 "Net-(J34-Pin_3)")
  (net 500 "Net-(J34-Pin_5)")
  (net 501 "Net-(J35-Pin_2)")
  (net 502 "Net-(J35-Pin_4)")
  (net 503 "Net-(J35-Pin_6)")
  (net 504 "Net-(J36-Pin_2)")
  (net 505 "Net-(J36-Pin_4)")
  (net 506 "Net-(J36-Pin_6)")
  (net 507 "Net-(J37-Pin_2)")
  (net 508 "Net-(J37-Pin_4)")
  (net 509 "Net-(J37-Pin_6)")
  (net 510 "Net-(J38-Pin_2)")
  (net 511 "Net-(J38-Pin_4)")
  (net 512 "Net-(J38-Pin_6)")
  (net 513 "Net-(J39-Pin_2)")
  (net 514 "unconnected-(J3_S3-Pin_1-Pad1)")
  (net 515 "unconnected-(J3_S2-Pin_1-Pad1)")
  (net 516 "unconnected-(J3_S1-Pin_1-Pad1)")
  (net 517 "unconnected-(J_G1-Pin_1-Pad1)")
  (net 518 "unconnected-(J_G2-Pin_1-Pad1)")
  (net 519 "unconnected-(J_G3-Pin_1-Pad1)")
  (net 520 "unconnected-(J_G4-Pin_1-Pad1)")
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 180.362431 110.105584 -108.408636)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J27" (at 0 -1.695 -108.408636) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -108.408636) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -18.408636) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 251.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 157 "Net-(J27-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 251.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 478 "Net-(J27-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 251.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 158 "Net-(J27-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 251.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 479 "Net-(J27-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 251.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 159 "Net-(J27-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 251.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 480 "Net-(J27-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 166.328644 127.520455 -149.317727)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J37" (at 0 -1.695 -149.317727) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -149.317727) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -59.317727) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 210.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 186 "Net-(J37-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 210.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 507 "Net-(J37-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 210.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 187 "Net-(J37-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 210.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 508 "Net-(J37-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 210.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 188 "Net-(J37-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 210.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 509 "Net-(J37-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 133.671359 127.520457 149.318633)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J81" (at 0 -1.695 149.318633) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 149.318633) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 239.318633) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 149.318633) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(J81-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 149.318633) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 379 "Net-(J81-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 149.318633) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(J81-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 149.318633) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 380 "Net-(J81-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 149.318633) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(J81-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 149.318633) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 381 "Net-(J81-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 178.61521 114.323748 -116.590454)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J29" (at 0 -1.695 -116.590454) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -116.590454) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -26.590454) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 243.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 163 "Net-(J29-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 243.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 484 "Net-(J29-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 243.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 164 "Net-(J29-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 243.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 485 "Net-(J29-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 243.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 165 "Net-(J29-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 243.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 486 "Net-(J29-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.81665 96.579353 -83.863181)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J21" (at 0 -1.695 -83.863181) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -83.863181) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 6.136819) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 276.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 236 "Net-(J21-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 276.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 301 "Net-(J21-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 276.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 237 "Net-(J21-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 276.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 302 "Net-(J21-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 276.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 238 "Net-(J21-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 276.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 303 "Net-(J21-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 146.579357 131.81665 173.864087)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J87" (at 0 -1.695 173.864087) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 173.864087) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 263.864087) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 173.864087) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J87-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 173.864087) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 333 "Net-(J87-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 173.864087) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J87-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 173.864087) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 334 "Net-(J87-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 173.864087) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J87-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 173.864087) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 335 "Net-(J87-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 173.420627 121.805372 -132.95409)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J33" (at 0 -1.695 -132.95409) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -132.95409) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -42.95409) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 227.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 175 "Net-(J33-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 227.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 496 "Net-(J33-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 227.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 176 "Net-(J33-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 227.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 497 "Net-(J33-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 227.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 177 "Net-(J33-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.81665 103.420641 -96.135909)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J24" (at 0 -1.695 -96.135909) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -96.135909) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -6.135909) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 263.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 148 "Net-(J24-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 263.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 469 "Net-(J24-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 263.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 149 "Net-(J24-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 263.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 470 "Net-(J24-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 263.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 150 "Net-(J24-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 263.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 471 "Net-(J24-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 120.435855 112.245871 112.500452)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J72" (at 0 -1.695 112.500452) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 112.500452) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 202.500452) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 112.500452) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(J72-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 112.500452) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 353 "Net-(J72-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 112.500452) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(J72-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 112.500452) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 354 "Net-(J72-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 112.500452) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(J72-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 112.500452) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 355 "Net-(J72-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 157.913811 131.005994 -165.681363)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J41" (at 0 -1.695 -165.681363) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -165.681363) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -75.681363) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 194.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 134 "Net-(J41-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 194.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 455 "Net-(J41-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 194.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 135 "Net-(J41-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 194.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 456 "Net-(J41-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 194.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 136 "Net-(J41-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 194.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 457 "Net-(J41-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex" (layer "F.Cu")
    (at 198 59)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J89" (at -0.175 -7.8) (layer "F.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 14.374) (layer "F.Fab"))
    (pad "1" smd rect (at 0.645 0.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "Net-(J6-Pin_4)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 0.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "Net-(J6-Pin_6)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 1.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "Net-(J7-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 1.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "Net-(J7-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 1.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "Net-(J7-Pin_6)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 2.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "Net-(J8-Pin_2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 2.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "Net-(J8-Pin_4)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 3.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "Net-(J8-Pin_6)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 3.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "Net-(J89-Pin_9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 3.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "Net-(J89-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 4.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "Net-(J89-Pin_11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 4.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "Net-(J10-Pin_2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 5.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "Net-(J10-Pin_4)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 5.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "Net-(J10-Pin_6)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 5.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "Net-(J11-Pin_2)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 6.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "Net-(J11-Pin_4)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 6.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "Net-(J12-Pin_1)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 7.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 275 "Net-(J12-Pin_3)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 7.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 276 "Net-(J12-Pin_5)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 7.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "Net-(J13-Pin_2)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 8.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "Net-(J13-Pin_4)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 8.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "Net-(J13-Pin_6)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 9.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "Net-(J14-Pin_2)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 9.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "Net-(J14-Pin_4)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 9.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "Net-(J14-Pin_6)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 10.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "Net-(J15-Pin_2)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 10.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "Net-(J15-Pin_4)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 11.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "Net-(J15-Pin_6)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 11.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "Net-(J16-Pin_2)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 11.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "Net-(J16-Pin_4)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 12.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "Net-(J16-Pin_6)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 12.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "Net-(J17-Pin_2)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 12.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "Net-(J17-Pin_4)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 12.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "Net-(J17-Pin_6)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 11.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "Net-(J18-Pin_2)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 11.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 293 "Net-(J18-Pin_4)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 11.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "Net-(J18-Pin_6)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 10.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "Net-(J19-Pin_2)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 10.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "Net-(J19-Pin_4)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 9.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "Net-(J19-Pin_6)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 9.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "Net-(J20-Pin_2)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 9.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "Net-(J20-Pin_4)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 8.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "Net-(J20-Pin_6)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 8.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "Net-(J21-Pin_2)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 7.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 302 "Net-(J21-Pin_4)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 7.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "Net-(J21-Pin_6)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 7.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 304 "Net-(J22-Pin_2)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 6.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 305 "Net-(J22-Pin_4)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 6.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "Net-(J1-Pin_1)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 5.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "Net-(J1-Pin_3)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 5.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "Net-(J1-Pin_5)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 5.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "Net-(J2-Pin_2)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 4.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "Net-(J2-Pin_4)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 4.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "Net-(J2-Pin_6)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 3.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "Net-(J3-Pin_2)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 3.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "Net-(J3-Pin_4)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 3.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "Net-(J3-Pin_6)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 2.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "Net-(J4-Pin_2)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 2.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "Net-(J4-Pin_4)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 1.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "Net-(J4-Pin_6)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 1.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "Net-(J5-Pin_2)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 1.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "Net-(J5-Pin_4)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 0.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "Net-(J5-Pin_6)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 0.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "Net-(J6-Pin_2)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex_Back" (layer "F.Cu")
    (at 206.865 59)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J92" (at -0.175 -7.8) (layer "F.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 14.374) (layer "F.Fab"))
    (pad "1" smd rect (at 0.645 0.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "Net-(J39-Pin_5)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 0.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "Net-(J40-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 1.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "Net-(J40-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 1.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "Net-(J40-Pin_5)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 1.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "Net-(J41-Pin_1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 2.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 135 "Net-(J41-Pin_3)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 2.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "Net-(J41-Pin_5)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 3.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "Net-(J42-Pin_1)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 3.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "Net-(J42-Pin_3)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 3.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "Net-(J42-Pin_5)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 4.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "Net-(J43-Pin_1)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 4.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "Net-(J43-Pin_3)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 5.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "Net-(J43-Pin_5)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 5.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "Net-(J44-Pin_1)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 5.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 144 "Net-(J44-Pin_3)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 6.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 145 "Net-(J44-Pin_5)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 6.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "Net-(J23-Pin_2)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 7.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "Net-(J23-Pin_4)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 7.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "Net-(J24-Pin_1)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 7.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "Net-(J24-Pin_3)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 8.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 150 "Net-(J24-Pin_5)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 8.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 151 "Net-(J25-Pin_1)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 9.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "Net-(J25-Pin_3)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 9.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 153 "Net-(J25-Pin_5)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 9.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "Net-(J26-Pin_1)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 10.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "Net-(J26-Pin_3)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 10.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "Net-(J26-Pin_5)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 11.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "Net-(J27-Pin_1)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 11.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "Net-(J27-Pin_3)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 11.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "Net-(J27-Pin_5)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 12.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 160 "Net-(J28-Pin_1)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 12.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "Net-(J28-Pin_3)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 12.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 162 "Net-(J28-Pin_5)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 12.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 163 "Net-(J29-Pin_1)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 11.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 164 "Net-(J29-Pin_3)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 11.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 165 "Net-(J29-Pin_5)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 11.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 166 "Net-(J30-Pin_1)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 10.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 167 "Net-(J30-Pin_3)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 10.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 168 "Net-(J30-Pin_5)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 9.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 169 "Net-(J31-Pin_1)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 9.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 170 "Net-(J31-Pin_3)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 9.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 171 "Net-(J31-Pin_5)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 8.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "Net-(J32-Pin_1)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 8.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 173 "Net-(J32-Pin_3)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 7.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 174 "Net-(J32-Pin_5)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 7.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 175 "Net-(J33-Pin_1)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 7.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 176 "Net-(J33-Pin_3)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 6.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 177 "Net-(J33-Pin_5)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 6.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 178 "Net-(J34-Pin_2)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 5.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 179 "Net-(J34-Pin_4)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 5.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 180 "Net-(J35-Pin_1)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 5.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 181 "Net-(J35-Pin_3)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 4.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 182 "Net-(J35-Pin_5)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 4.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 183 "Net-(J36-Pin_1)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 3.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 184 "Net-(J36-Pin_3)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 3.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 185 "Net-(J36-Pin_5)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 3.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 186 "Net-(J37-Pin_1)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 2.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 187 "Net-(J37-Pin_3)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 2.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 188 "Net-(J37-Pin_5)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 1.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 189 "Net-(J38-Pin_1)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 1.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 190 "Net-(J38-Pin_3)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 1.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 191 "Net-(J38-Pin_5)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 0.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 192 "Net-(J39-Pin_1)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 0.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 193 "Net-(J39-Pin_3)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_STIM" (layer "F.Cu")
    (at 150 76)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3_S2" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 -2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 515 "unconnected-(J3_S2-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 120.435854 87.754132 67.500453)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J61" (at 0 -1.695 67.500453) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 67.500453) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 157.500453) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 67.500453) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 97 "Net-(J61-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 67.500453) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 417 "Net-(J61-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 67.500453) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 98 "Net-(J61-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 67.500453) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 418 "Net-(J61-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 67.500453) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 99 "Net-(J61-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 67.500453) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 419 "Net-(J61-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 164.323754 128.615208 -153.408636)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J38" (at 0 -1.695 -153.408636) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -153.408636) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -63.408636) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 206.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 189 "Net-(J38-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 206.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 510 "Net-(J38-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 206.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 190 "Net-(J38-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 206.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 511 "Net-(J38-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 206.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 191 "Net-(J38-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 206.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 512 "Net-(J38-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 164.323748 71.38479 -26.590454)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at 0 -1.695 -26.590454) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -26.590454) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 63.409546) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 333.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 195 "Net-(J7-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 333.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 260 "Net-(J7-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 333.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 196 "Net-(J7-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 333.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 261 "Net-(J7-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 333.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 197 "Net-(J7-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 333.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 262 "Net-(J7-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 151.142158 131.979611 -177.95409)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J44" (at 0 -1.695 -177.95409) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -177.95409) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -87.95409) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 182.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 143 "Net-(J44-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 182.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 464 "Net-(J44-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 182.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 144 "Net-(J44-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 182.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 465 "Net-(J44-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 182.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 145 "Net-(J44-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 148.857846 131.979611 177.954996)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J88" (at 0 -1.695 177.954996) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 177.954996) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 267.954996) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 177.954996) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J88-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 177.954996) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 336 "Net-(J88-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 177.954996) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J88-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 177.954996) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 337 "Net-(J88-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 177.954996) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(J88-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 162.245867 70.435853 -22.499545)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -1.695 -22.499545) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -22.499545) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 67.500455) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 337.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 256 "Net-(J6-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 337.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 321 "Net-(J6-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 337.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 257 "Net-(J6-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 337.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 258 "Net-(J6-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 337.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 194 "Net-(J6-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 337.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 259 "Net-(J6-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_GND" (layer "F.Cu")
    (at 133.096 83.058)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J_G2" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -0.066 -0.028) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 518 "unconnected-(J_G2-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.49156 105.6817 -100.226818)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J25" (at 0 -1.695 -100.226818) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -100.226818) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -10.226818) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 259.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 151 "Net-(J25-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 259.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 472 "Net-(J25-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 259.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 152 "Net-(J25-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 259.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 473 "Net-(J25-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 259.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 153 "Net-(J25-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 259.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 474 "Net-(J25-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.005994 92.086189 -75.681363)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J19" (at 0 -1.695 -75.681363) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -75.681363) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 14.318637) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 284.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 230 "Net-(J19-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 284.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 295 "Net-(J19-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 284.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 231 "Net-(J19-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 284.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 296 "Net-(J19-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 284.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 232 "Net-(J19-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 284.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 297 "Net-(J19-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 144.318298 131.491559 169.773178)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J86" (at 0 -1.695 169.773178) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 169.773178) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 259.773178) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 169.773178) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J86-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 169.773178) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 330 "Net-(J86-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 169.773178) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J86-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 169.773178) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 331 "Net-(J86-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 169.773178) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J86-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 169.773178) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 332 "Net-(J86-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 173.420623 78.194624 -47.045)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J12" (at 0 -1.695 -47.045) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -47.045) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 42.955) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 312.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 274 "Net-(J12-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 312.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 210 "Net-(J12-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 312.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 275 "Net-(J12-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 312.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 211 "Net-(J12-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 312.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 276 "Net-(J12-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.979611 98.857842 -87.95409)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J22" (at 0 -1.695 -87.95409) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -87.95409) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 2.04591) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 272.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 239 "Net-(J22-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 272.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 304 "Net-(J22-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 272.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 240 "Net-(J22-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 272.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 305 "Net-(J22-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 272.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 241 "Net-(J22-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 125.083471 120.079009 128.864088)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J76" (at 0 -1.695 128.864088) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 128.864088) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 218.864088) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 128.864088) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(J76-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 128.864088) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 365 "Net-(J76-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 128.864088) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(J76-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 128.864088) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 366 "Net-(J76-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 128.864088) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(J76-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 128.864088) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 367 "Net-(J76-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_STIM" (layer "F.Cu")
    (at 174 100)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3_S1" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 -2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 516 "unconnected-(J3_S1-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 131.749676 126.285466 145.227724)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J80" (at 0 -1.695 145.227724) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 145.227724) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 235.227724) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 145.227724) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(J80-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 145.227724) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 376 "Net-(J80-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 145.227724) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J80-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 145.227724) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 377 "Net-(J80-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 145.227724) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(J80-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 145.227724) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 378 "Net-(J80-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 176.285464 81.749673 -55.226818)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J14" (at 0 -1.695 -55.226818) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -55.226818) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 34.773182) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 304.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 217 "Net-(J14-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 304.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 280 "Net-(J14-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 304.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 216 "Net-(J14-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 304.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 281 "Net-(J14-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 304.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 215 "Net-(J14-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 304.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 282 "Net-(J14-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 137.754131 129.564146 157.500451)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J83" (at 0 -1.695 157.500451) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 157.500451) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 247.500451) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 157.500451) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(J83-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 157.500451) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 385 "Net-(J83-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 157.500451) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(J83-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 157.500451) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 322 "Net-(J83-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 157.500451) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J83-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 157.500451) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 323 "Net-(J83-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 126.579374 78.194627 47.045908)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J56" (at 0 -1.695 47.045908) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 47.045908) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 137.045908) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 47.045908) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 402 "Net-(J56-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 47.045908) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 113 "Net-(J56-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 47.045908) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 403 "Net-(J56-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 47.045908) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 112 "Net-(J56-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 47.045908) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 404 "Net-(J56-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 123.714535 118.250326 124.773179)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J75" (at 0 -1.695 124.773179) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 124.773179) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 214.773179) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 124.773179) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(J75-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 124.773179) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 362 "Net-(J75-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 124.773179) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(J75-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 124.773179) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 363 "Net-(J75-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 124.773179) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(J75-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 124.773179) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 364 "Net-(J75-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 148.857843 68.020389 2.045909)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J45" (at 0 -1.695 2.045909) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 2.045909) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 92.045909) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 2.045909) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 434 "Net-(J45-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 2.045909) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(J45-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 2.045909) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 435 "Net-(J45-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 2.045909) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 80 "Net-(J45-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 2.045909) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 436 "Net-(J45-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 177.520458 116.328639 -120.681363)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J30" (at 0 -1.695 -120.681363) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -120.681363) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -30.681363) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 239.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 166 "Net-(J30-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 239.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 487 "Net-(J30-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 239.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 167 "Net-(J30-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 239.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 488 "Net-(J30-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 239.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 168 "Net-(J30-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 239.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 489 "Net-(J30-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 121.384791 114.323752 116.591361)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J73" (at 0 -1.695 116.591361) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 116.591361) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 206.591361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 116.591361) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(J73-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 116.591361) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 356 "Net-(J73-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 116.591361) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(J73-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 116.591361) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 357 "Net-(J73-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 116.591361) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(J73-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 116.591361) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 358 "Net-(J73-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 142.086189 68.994006 14.318636)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J48" (at 0 -1.695 14.318636) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 14.318636) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 104.318636) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 14.318636) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(J48-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 14.318636) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 443 "Net-(J48-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 14.318636) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(J48-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 14.318636) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 444 "Net-(J48-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 14.318636) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(J48-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 14.318636) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 445 "Net-(J48-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 123.714534 81.749677 55.227726)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J58" (at 0 -1.695 55.227726) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 55.227726) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 145.227726) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 55.227726) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 106 "Net-(J58-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 55.227726) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 408 "Net-(J58-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 55.227726) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 107 "Net-(J58-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 55.227726) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 409 "Net-(J58-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 55.227726) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 108 "Net-(J58-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 55.227726) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 410 "Net-(J58-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 155.681706 131.491558 -169.772272)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J42" (at 0 -1.695 -169.772272) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -169.772272) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -79.772272) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 190.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 137 "Net-(J42-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 190.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 458 "Net-(J42-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 190.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 138 "Net-(J42-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 190.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 459 "Net-(J42-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 190.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 139 "Net-(J42-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 190.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 460 "Net-(J42-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 153.420641 68.18335 -6.135909)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -1.695 -6.135909) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -6.135909) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 83.864091) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 353.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 244 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 353.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 309 "Net-(J2-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 353.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 245 "Net-(J2-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 353.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 310 "Net-(J2-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 353.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 246 "Net-(J2-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 353.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 311 "Net-(J2-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 146.579353 68.18335 6.136818)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J46" (at 0 -1.695 6.136818) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 6.136818) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 96.136818) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 6.136818) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(J46-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 6.136818) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 437 "Net-(J46-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 6.136818) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(J46-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 6.136818) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 438 "Net-(J46-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 6.136818) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(J46-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 6.136818) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 439 "Net-(J46-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 179.564147 112.245867 -112.499545)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J28" (at 0 -1.695 -112.499545) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -112.499545) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -22.499545) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 247.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 160 "Net-(J28-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 247.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 481 "Net-(J28-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 247.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 161 "Net-(J28-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 247.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 482 "Net-(J28-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 247.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 162 "Net-(J28-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 247.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 483 "Net-(J28-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_GND" (layer "F.Cu")
    (at 133.03 116.97)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J_G1" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 517 "unconnected-(J_G1-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_GND" (layer "F.Cu")
    (at 166.97 83.03)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J_G4" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 520 "unconnected-(J_G4-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 135.676247 71.384792 26.591363)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J51" (at 0 -1.695 26.591363) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 26.591363) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 116.591363) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 26.591363) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 128 "Net-(J51-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 26.591363) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 388 "Net-(J51-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 26.591363) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 127 "Net-(J51-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 26.591363) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 389 "Net-(J51-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 26.591363) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 126 "Net-(J51-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 26.591363) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 390 "Net-(J51-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 166.328639 72.479542 -30.681363)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -1.695 -30.681363) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -30.681363) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 59.318637) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 329.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 198 "Net-(J8-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 329.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 263 "Net-(J8-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 329.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 199 "Net-(J8-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 329.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 264 "Net-(J8-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 329.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 200 "Net-(J8-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 329.318637) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 265 "Net-(J8-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 174.916532 120.079006 -128.863181)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J32" (at 0 -1.695 -128.863181) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -128.863181) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -38.863181) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 231.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 172 "Net-(J32-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 231.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 493 "Net-(J32-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 231.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 173 "Net-(J32-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 231.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 494 "Net-(J32-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 231.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 174 "Net-(J32-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 231.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 495 "Net-(J32-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.979611 101.142152 -92.045)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J23" (at 0 -1.695 -92.045) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -92.045) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -2.045) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 267.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 466 "Net-(J23-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 267.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 146 "Net-(J23-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 267.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 467 "Net-(J23-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 267.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 147 "Net-(J23-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 267.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 468 "Net-(J23-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 157.913805 68.994005 -14.317727)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -1.695 -14.317727) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -14.317727) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 75.682273) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 345.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 250 "Net-(J4-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 345.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 315 "Net-(J4-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 345.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 251 "Net-(J4-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 345.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 316 "Net-(J4-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 345.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 252 "Net-(J4-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 345.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 317 "Net-(J4-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_STIM" (layer "F.Cu")
    (at 126 100)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3_S3" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 -2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 514 "unconnected-(J3_S3-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.508441 94.318299 79.77318)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J64" (at 0 -1.695 79.77318) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 79.77318) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 169.77318) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 79.77318) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(J64-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 79.77318) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 426 "Net-(J64-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 79.77318) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(J64-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 79.77318) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 427 "Net-(J64-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 79.77318) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(J64-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 79.77318) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 428 "Net-(J64-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 168.250322 73.714533 -34.772272)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -1.695 -34.772272) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -34.772272) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 55.227728) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 325.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 201 "Net-(J9-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 325.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 266 "Net-(J89-Pin_9)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 325.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 202 "Net-(J9-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 325.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 267 "Net-(J89-Pin_10)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 325.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 203 "Net-(J9-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 325.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 268 "Net-(J89-Pin_11)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 171.805372 76.579373 -42.95409)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 0 -1.695 -42.95409) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -42.95409) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 47.04591) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 317.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 207 "Net-(J11-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 317.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 272 "Net-(J11-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 317.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 208 "Net-(J11-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 317.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 273 "Net-(J11-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 317.04591) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 209 "Net-(J11-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.508441 105.681704 100.227725)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J69" (at 0 -1.695 100.227725) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 100.227725) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 190.227725) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 100.227725) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J69-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 100.227725) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 344 "Net-(J69-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 100.227725) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(J69-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 100.227725) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 345 "Net-(J69-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 100.227725) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(J69-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 100.227725) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 346 "Net-(J69-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 168.250327 126.285464 -145.226818)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J36" (at 0 -1.695 -145.226818) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -145.226818) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -55.226818) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 214.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 183 "Net-(J36-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 214.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 504 "Net-(J36-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 214.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 184 "Net-(J36-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 214.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 505 "Net-(J36-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 214.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 185 "Net-(J36-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 214.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 506 "Net-(J36-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 179.564144 87.754127 -67.499545)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J17" (at 0 -1.695 -67.499545) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -67.499545) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 22.500455) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 292.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 226 "Net-(J17-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 292.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 289 "Net-(J17-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 292.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 225 "Net-(J17-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 292.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 290 "Net-(J17-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 292.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 224 "Net-(J17-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 292.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 291 "Net-(J17-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 122.479544 116.328642 120.68227)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J74" (at 0 -1.695 120.68227) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 120.68227) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 210.68227) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 120.68227) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(J74-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 120.68227) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 359 "Net-(J74-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 120.68227) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(J74-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 120.68227) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 360 "Net-(J74-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 120.68227) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(J74-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 120.68227) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 361 "Net-(J74-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 180.362428 89.89441 -71.590454)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J18" (at 0 -1.695 -71.590454) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -71.590454) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 18.409546) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 288.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 229 "Net-(J18-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 288.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 292 "Net-(J18-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 288.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 228 "Net-(J18-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 288.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 293 "Net-(J18-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 288.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 227 "Net-(J18-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 288.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 294 "Net-(J18-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 139.894411 69.637571 18.409545)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J49" (at 0 -1.695 18.409545) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 18.409545) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 108.409545) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 18.409545) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(J49-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 18.409545) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 446 "Net-(J49-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 18.409545) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(J49-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 18.409545) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 447 "Net-(J49-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 18.409545) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(J49-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 18.409545) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 448 "Net-(J49-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 170.079006 75.083468 -38.863181)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J10" (at 0 -1.695 -38.863181) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -38.863181) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 51.136819) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 321.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 204 "Net-(J10-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 321.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 269 "Net-(J10-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 321.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 205 "Net-(J10-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 321.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 270 "Net-(J10-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 321.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 206 "Net-(J10-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 321.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 271 "Net-(J10-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 121.38479 85.676251 63.409544)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J60" (at 0 -1.695 63.409544) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 63.409544) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 153.409544) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 63.409544) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(J60-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 63.409544) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 414 "Net-(J60-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 63.409544) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 101 "Net-(J60-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 63.409544) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 415 "Net-(J60-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 63.409544) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 102 "Net-(J60-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 63.409544) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 416 "Net-(J60-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.491558 94.318294 -79.772272)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J20" (at 0 -1.695 -79.772272) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -79.772272) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 10.227728) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 280.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 233 "Net-(J20-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 280.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 298 "Net-(J20-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 280.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 234 "Net-(J20-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 280.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 299 "Net-(J20-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 280.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 235 "Net-(J20-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 280.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 300 "Net-(J20-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 126.579376 121.805375 132.954997)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J77" (at 0 -1.695 132.954997) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 132.954997) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 222.954997) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 132.954997) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(J77-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 132.954997) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 368 "Net-(J77-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 132.954997) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(J77-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 132.954997) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 369 "Net-(J77-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 132.954997) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(J77-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 171.805376 123.420623 -137.045)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J34" (at 0 -1.695 -137.045) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -137.045) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -47.045) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 222.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 498 "Net-(J34-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 222.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 178 "Net-(J34-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 222.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 499 "Net-(J34-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 222.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 179 "Net-(J34-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 222.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 500 "Net-(J34-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 144.318295 68.508441 10.227727)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J47" (at 0 -1.695 10.227727) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 10.227727) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 100.227727) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 10.227727) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 76 "Net-(J47-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 10.227727) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 440 "Net-(J47-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 10.227727) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(J47-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 10.227727) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 441 "Net-(J47-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 10.227727) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(J47-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 10.227727) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 442 "Net-(J47-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 135.67625 128.615209 153.409542)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J82" (at 0 -1.695 153.409542) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 153.409542) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 243.409542) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 153.409542) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(J82-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 153.409542) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 382 "Net-(J82-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 153.409542) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(J82-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 153.409542) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 383 "Net-(J82-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 153.409542) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(J82-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 153.409542) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 384 "Net-(J82-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 119.637571 110.105588 108.409543)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J71" (at 0 -1.695 108.409543) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 108.409543) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 198.409543) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 108.409543) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(J71-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 108.409543) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 350 "Net-(J71-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 108.409543) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(J71-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 108.409543) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 351 "Net-(J71-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 108.409543) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(J71-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 108.409543) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 352 "Net-(J71-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 125.083469 79.920993 51.136817)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J57" (at 0 -1.695 51.136817) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 51.136817) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 141.136817) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 51.136817) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 109 "Net-(J57-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 51.136817) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 405 "Net-(J57-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 51.136817) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 110 "Net-(J57-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 51.136817) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 406 "Net-(J57-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 51.136817) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 111 "Net-(J57-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 51.136817) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 407 "Net-(J57-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 128.194626 123.420626 137.045906)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J78" (at 0 -1.695 137.045906) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 137.045906) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 227.045906) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 137.045906) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 370 "Net-(J78-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 137.045906) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(J78-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 137.045906) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 371 "Net-(J78-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 137.045906) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(J78-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 137.045906) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 372 "Net-(J78-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 162.245873 129.564144 -157.499545)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J39" (at 0 -1.695 -157.499545) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -157.499545) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -67.499545) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 202.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 192 "Net-(J39-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 202.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 513 "Net-(J39-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 202.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 193 "Net-(J39-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 202.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 450 "Net-(J39-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 202.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 130 "Net-(J39-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 202.500455) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 451 "Net-(J39-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 151.142152 68.020389 -2.045)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -1.695 -2.045) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 -2.045) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 87.955) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 357.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 306 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 357.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 242 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 357.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 307 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 357.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 243 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 357.955) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 308 "Net-(J1-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 153.420647 131.81665 -173.863181)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J43" (at 0 -1.695 -173.863181) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -173.863181) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -83.863181) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 186.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 140 "Net-(J43-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 186.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 461 "Net-(J43-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 186.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 141 "Net-(J43-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 186.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 462 "Net-(J43-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 186.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 142 "Net-(J43-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 186.136819) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 463 "Net-(J43-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 155.6817 68.50844 -10.226818)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -1.695 -10.226818) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -10.226818) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 79.773182) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 349.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 247 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 349.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 312 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 349.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 248 "Net-(J3-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 349.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 313 "Net-(J3-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 349.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 249 "Net-(J3-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 349.773182) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 314 "Net-(J3-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.18335 103.420645 96.136816)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J68" (at 0 -1.695 96.136816) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 96.136816) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 186.136816) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 96.136816) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(J68-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 96.136816) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 341 "Net-(J68-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 96.136816) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(J68-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 96.136816) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 342 "Net-(J68-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 96.136816) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(J68-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 96.136816) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 343 "Net-(J68-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 139.894414 130.36243 161.59136)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J84" (at 0 -1.695 161.59136) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 161.59136) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 251.59136) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 161.59136) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J84-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 161.59136) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 324 "Net-(J84-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 161.59136) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J84-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 161.59136) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 325 "Net-(J84-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 161.59136) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J84-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 161.59136) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 326 "Net-(J84-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 174.916527 79.920989 -51.135909)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J13" (at 0 -1.695 -51.135909) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -51.135909) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 38.864091) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 308.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 214 "Net-(J13-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 308.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 277 "Net-(J13-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 308.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 213 "Net-(J13-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 308.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 278 "Net-(J13-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 308.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 212 "Net-(J13-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 308.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 279 "Net-(J13-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 122.479543 83.67136 59.318635)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J59" (at 0 -1.695 59.318635) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 59.318635) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 149.318635) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 59.318635) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 103 "Net-(J59-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 59.318635) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 411 "Net-(J59-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 59.318635) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 104 "Net-(J59-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 59.318635) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 412 "Net-(J59-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 59.318635) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 105 "Net-(J59-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 59.318635) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 413 "Net-(J59-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 128.194624 76.579376 42.954999)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J55" (at 0 -1.695 42.954999) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 42.954999) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 132.954999) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 42.954999) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 116 "Net-(J55-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 42.954999) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 400 "Net-(J55-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 42.954999) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 115 "Net-(J55-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 42.954999) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 401 "Net-(J55-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 42.954999) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(J55-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.994006 107.913809 104.318634)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J70" (at 0 -1.695 104.318634) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 104.318634) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 194.318634) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 104.318634) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J70-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 104.318634) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 347 "Net-(J70-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 104.318634) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(J70-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 104.318634) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 348 "Net-(J70-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 104.318634) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(J70-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 104.318634) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 349 "Net-(J70-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 142.086192 131.005994 165.682269)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J85" (at 0 -1.695 165.682269) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 165.682269) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 255.682269) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 165.682269) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J85-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 165.682269) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 327 "Net-(J85-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 165.682269) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J85-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 165.682269) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 328 "Net-(J85-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 165.682269) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J85-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 165.682269) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 329 "Net-(J85-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_STIM" (layer "F.Cu")
    (at 150 124)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3_S4" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 -2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(J3_S4-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.994005 92.086194 75.682271)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J63" (at 0 -1.695 75.682271) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 75.682271) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 165.682271) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 75.682271) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(J63-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 75.682271) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 423 "Net-(J63-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 75.682271) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 92 "Net-(J63-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 75.682271) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 424 "Net-(J63-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 75.682271) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(J63-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 75.682271) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 425 "Net-(J63-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 160.105584 69.637569 -18.408636)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -1.695 -18.408636) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -18.408636) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 71.591364) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 341.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 253 "Net-(J5-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 341.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 318 "Net-(J5-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 341.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 254 "Net-(J5-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 341.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 319 "Net-(J5-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 341.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 255 "Net-(J5-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 341.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 320 "Net-(J5-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex_Back" (layer "F.Cu")
    (at 198 59)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J91" (at -0.175 -7.8) (layer "F.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 14.374) (layer "F.Fab"))
    (pad "1" smd rect (at 0.645 0.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 194 "Net-(J6-Pin_5)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 0.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 195 "Net-(J7-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 1.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 196 "Net-(J7-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 1.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 197 "Net-(J7-Pin_5)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 1.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 198 "Net-(J8-Pin_1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 2.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 199 "Net-(J8-Pin_3)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 2.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 200 "Net-(J8-Pin_5)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 3.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 201 "Net-(J9-Pin_1)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 3.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 202 "Net-(J9-Pin_3)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 3.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 203 "Net-(J9-Pin_5)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 4.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 204 "Net-(J10-Pin_1)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 4.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 205 "Net-(J10-Pin_3)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 5.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 206 "Net-(J10-Pin_5)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 5.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 207 "Net-(J11-Pin_1)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 5.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 208 "Net-(J11-Pin_3)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 6.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 209 "Net-(J11-Pin_5)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 6.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 210 "Net-(J12-Pin_2)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 7.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 211 "Net-(J12-Pin_4)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 7.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 212 "Net-(J13-Pin_5)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 7.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 213 "Net-(J13-Pin_3)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 8.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 214 "Net-(J13-Pin_1)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 8.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 215 "Net-(J14-Pin_5)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 9.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 216 "Net-(J14-Pin_3)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 9.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 217 "Net-(J14-Pin_1)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 9.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 218 "Net-(J15-Pin_5)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 10.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 219 "Net-(J15-Pin_3)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 10.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 220 "Net-(J15-Pin_1)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 11.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 221 "Net-(J16-Pin_5)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 11.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 222 "Net-(J16-Pin_3)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 11.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 223 "Net-(J16-Pin_1)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 12.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 224 "Net-(J17-Pin_5)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 12.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 225 "Net-(J17-Pin_3)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 12.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 226 "Net-(J17-Pin_1)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 12.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 227 "Net-(J18-Pin_5)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 11.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 228 "Net-(J18-Pin_3)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 11.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 229 "Net-(J18-Pin_1)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 11.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 230 "Net-(J19-Pin_1)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 10.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 231 "Net-(J19-Pin_3)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 10.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 232 "Net-(J19-Pin_5)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 9.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 233 "Net-(J20-Pin_1)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 9.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 234 "Net-(J20-Pin_3)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 9.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 235 "Net-(J20-Pin_5)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 8.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 236 "Net-(J21-Pin_1)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 8.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 237 "Net-(J21-Pin_3)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 7.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 238 "Net-(J21-Pin_5)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 7.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 239 "Net-(J22-Pin_1)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 7.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 240 "Net-(J22-Pin_3)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 6.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 241 "Net-(J22-Pin_5)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 6.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 242 "Net-(J1-Pin_2)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 5.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 243 "Net-(J1-Pin_4)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 5.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 244 "Net-(J2-Pin_1)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 5.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 245 "Net-(J2-Pin_3)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 4.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 246 "Net-(J2-Pin_5)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 4.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 247 "Net-(J3-Pin_1)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 3.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 248 "Net-(J3-Pin_3)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 3.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 249 "Net-(J3-Pin_5)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 3.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 250 "Net-(J4-Pin_1)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 2.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 251 "Net-(J4-Pin_3)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 2.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 252 "Net-(J4-Pin_5)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 1.9) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 253 "Net-(J5-Pin_1)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 1.5) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 254 "Net-(J5-Pin_3)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 1.1) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 255 "Net-(J5-Pin_5)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 0.7) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 256 "Net-(J6-Pin_1)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 0.3) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 257 "Net-(J6-Pin_3)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.020389 98.857847 87.954998)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J66" (at 0 -1.695 87.954998) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 87.954998) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 177.954998) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 87.954998) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 84 "Net-(J66-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 87.954998) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 432 "Net-(J66-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 87.954998) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 83 "Net-(J66-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 87.954998) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 433 "Net-(J66-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 87.954998) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 82 "Net-(J66-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 177.520455 83.671356 -59.317727)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J15" (at 0 -1.695 -59.317727) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -59.317727) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 30.682273) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 300.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 220 "Net-(J15-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 300.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 283 "Net-(J15-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 300.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 219 "Net-(J15-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 300.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 284 "Net-(J15-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 300.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 218 "Net-(J15-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 300.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 285 "Net-(J15-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 129.92099 75.083472 38.86409)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J54" (at 0 -1.695 38.86409) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 38.86409) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 128.86409) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 38.86409) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 119 "Net-(J54-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 38.86409) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 397 "Net-(J54-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 38.86409) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 118 "Net-(J54-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 38.86409) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 398 "Net-(J54-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 38.86409) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 117 "Net-(J54-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 38.86409) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 399 "Net-(J54-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 119.63757 89.894415 71.591362)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J62" (at 0 -1.695 71.591362) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 71.591362) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 161.591362) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 71.591362) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(J62-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 71.591362) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 420 "Net-(J62-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 71.591362) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 95 "Net-(J62-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 71.591362) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 421 "Net-(J62-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 71.591362) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 96 "Net-(J62-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 71.591362) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 422 "Net-(J62-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x05_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.020389 101.142156 92.045907)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J67" (at 0 -1.695 92.045907) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 6.775 92.045907) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 182.045907) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 92.045907) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 338 "Net-(J67-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 92.045907) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(J67-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 92.045907) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 339 "Net-(J67-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 92.045907) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J67-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 92.045907) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 340 "Net-(J67-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 137.754128 70.435855 22.500454)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J50" (at 0 -1.695 22.500454) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 22.500454) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 112.500454) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 22.500454) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(J50-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 22.500454) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 449 "Net-(J50-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 22.500454) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(J50-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 22.500454) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 386 "Net-(J50-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 22.500454) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 129 "Net-(J50-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 22.500454) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 387 "Net-(J50-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 170.079011 124.916527 -141.135909)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J35" (at 0 -1.695 -141.135909) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -141.135909) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -51.135909) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 218.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 180 "Net-(J35-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 218.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 501 "Net-(J35-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 218.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 181 "Net-(J35-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 218.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 502 "Net-(J35-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 218.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 182 "Net-(J35-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 218.864091) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 503 "Net-(J35-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 181.005995 107.913805 -104.317727)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J26" (at 0 -1.695 -104.317727) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -104.317727) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -14.317727) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 255.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 154 "Net-(J26-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 255.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 475 "Net-(J26-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 255.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 155 "Net-(J26-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 255.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 476 "Net-(J26-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 255.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 156 "Net-(J26-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 255.682273) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 477 "Net-(J26-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex" (layer "F.Cu")
    (at 206.865 59)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J90" (at -0.175 -7.8) (layer "F.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 14.374) (layer "F.Fab"))
    (pad "1" smd rect (at 0.645 0.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 450 "Net-(J39-Pin_4)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 0.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "Net-(J39-Pin_6)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 1.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "Net-(J40-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 1.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "Net-(J40-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 1.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "Net-(J40-Pin_6)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 2.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "Net-(J41-Pin_2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 2.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "Net-(J41-Pin_4)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 3.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "Net-(J41-Pin_6)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 3.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "Net-(J42-Pin_2)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 3.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "Net-(J42-Pin_4)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 4.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "Net-(J42-Pin_6)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 4.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "Net-(J43-Pin_2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 5.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "Net-(J43-Pin_4)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 5.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "Net-(J43-Pin_6)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 5.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "Net-(J44-Pin_2)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 6.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "Net-(J44-Pin_4)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 6.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "Net-(J23-Pin_1)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 7.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "Net-(J23-Pin_3)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 7.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "Net-(J23-Pin_5)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 7.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "Net-(J24-Pin_2)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 8.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "Net-(J24-Pin_4)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 8.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "Net-(J24-Pin_6)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 9.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "Net-(J25-Pin_2)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 9.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "Net-(J25-Pin_4)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 9.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "Net-(J25-Pin_6)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 10.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "Net-(J26-Pin_2)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 10.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "Net-(J26-Pin_4)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 11.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "Net-(J26-Pin_6)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 11.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "Net-(J27-Pin_2)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 11.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "Net-(J27-Pin_4)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 12.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 480 "Net-(J27-Pin_6)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 12.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "Net-(J28-Pin_2)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 12.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "Net-(J28-Pin_4)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 12.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 483 "Net-(J28-Pin_6)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 11.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 484 "Net-(J29-Pin_2)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 11.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "Net-(J29-Pin_4)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 11.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "Net-(J29-Pin_6)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 10.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 487 "Net-(J30-Pin_2)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 10.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "Net-(J30-Pin_4)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 9.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 489 "Net-(J30-Pin_6)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 9.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 490 "Net-(J31-Pin_2)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 9.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 491 "Net-(J31-Pin_4)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 8.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "Net-(J31-Pin_6)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 8.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "Net-(J32-Pin_2)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 7.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "Net-(J32-Pin_4)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 7.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "Net-(J32-Pin_6)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 7.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "Net-(J33-Pin_2)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 6.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "Net-(J33-Pin_4)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 6.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "Net-(J34-Pin_1)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 5.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "Net-(J34-Pin_3)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 5.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "Net-(J34-Pin_5)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 5.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "Net-(J35-Pin_2)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 4.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "Net-(J35-Pin_4)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 4.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 503 "Net-(J35-Pin_6)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 3.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 504 "Net-(J36-Pin_2)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 3.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 505 "Net-(J36-Pin_4)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 3.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 506 "Net-(J36-Pin_6)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 2.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "Net-(J37-Pin_2)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 2.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 508 "Net-(J37-Pin_4)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 1.9) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 509 "Net-(J37-Pin_6)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 1.5) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 510 "Net-(J38-Pin_2)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 1.1) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 511 "Net-(J38-Pin_4)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 0.7) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 512 "Net-(J38-Pin_6)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 0.3) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 513 "Net-(J39-Pin_2)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 176.285467 118.250322 -124.772272)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J31" (at 0 -1.695 -124.772272) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -124.772272) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -34.772272) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 235.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 169 "Net-(J31-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 235.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 490 "Net-(J31-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 235.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 170 "Net-(J31-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 235.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 491 "Net-(J31-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 235.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 171 "Net-(J31-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 235.227728) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 492 "Net-(J31-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 131.749673 73.714536 34.773181)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J53" (at 0 -1.695 34.773181) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 34.773181) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 124.773181) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 34.773181) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 122 "Net-(J53-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 34.773181) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 394 "Net-(J53-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 34.773181) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 121 "Net-(J53-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 34.773181) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 395 "Net-(J53-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 34.773181) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 120 "Net-(J53-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 34.773181) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 396 "Net-(J53-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 118.18335 96.579358 83.864089)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J65" (at 0 -1.695 83.864089) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 83.864089) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 173.864089) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 83.864089) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(J65-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 83.864089) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 429 "Net-(J65-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 83.864089) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 86 "Net-(J65-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 83.864089) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 430 "Net-(J65-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 83.864089) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(J65-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 83.864089) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 431 "Net-(J65-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 160.10559 130.362428 -161.590454)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J40" (at 0 -1.695 -161.590454) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -161.590454) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 -71.590454) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 198.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 131 "Net-(J40-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 198.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 452 "Net-(J40-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 198.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 132 "Net-(J40-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 198.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 453 "Net-(J40-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 198.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 133 "Net-(J40-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 198.409546) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 454 "Net-(J40-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 178.615208 85.676246 -63.408636)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J16" (at 0 -1.695 -63.408636) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 -63.408636) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 26.591364) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 296.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 223 "Net-(J16-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 296.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 286 "Net-(J16-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 296.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 222 "Net-(J16-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 296.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 287 "Net-(J16-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 296.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 221 "Net-(J16-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 296.591364) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 288 "Net-(J16-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 133.671357 72.479545 30.682272)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J52" (at 0 -1.695 30.682272) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 30.682272) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 120.682272) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 30.682272) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 125 "Net-(J52-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 30.682272) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 391 "Net-(J52-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 30.682272) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 124 "Net-(J52-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 30.682272) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 392 "Net-(J52-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 30.682272) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 123 "Net-(J52-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 30.682272) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 393 "Net-(J52-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x01_P1.27mm_Vertical_0.483_GND" (layer "F.Cu")
    (at 166.97 116.97)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J_G3" (at 0 -1.695) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 1.695) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 519 "unconnected-(J_G3-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_1x06_P1.5mm_Vertical" (layer "F.Cu")
    (at 129.920992 124.91653 141.136815)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J79" (at 0 -1.695 141.136815) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 6.775 141.136815) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 231.136815) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 141.136815) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(J79-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.5 141.136815) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 373 "Net-(J79-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 3 141.136815) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(J79-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 4.5 141.136815) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 374 "Net-(J79-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 6 141.136815) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(J79-Pin_5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 7.5 141.136815) (size 1 1) (drill 0.483) (layers "*.Cu" "*.Mask")
      (net 375 "Net-(J79-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex_Back" (layer "B.Cu")
    (at 102 59 180)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J93" (at -0.175 7.8) (layer "B.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 -14.374) (layer "B.Fab"))
    (pad "1" smd rect (at 0.645 -0.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 386 "Net-(J50-Pin_4)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 -0.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 387 "Net-(J50-Pin_6)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 -1.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 388 "Net-(J51-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 -1.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 389 "Net-(J51-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 -1.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 390 "Net-(J51-Pin_6)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 -2.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "Net-(J52-Pin_2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 -2.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 392 "Net-(J52-Pin_4)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 -3.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 393 "Net-(J52-Pin_6)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 -3.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 394 "Net-(J53-Pin_2)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 -3.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 395 "Net-(J53-Pin_4)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 -4.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "Net-(J53-Pin_6)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 -4.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "Net-(J54-Pin_2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 -5.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "Net-(J54-Pin_4)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 -5.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "Net-(J54-Pin_6)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 -5.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 400 "Net-(J55-Pin_2)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 -6.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 401 "Net-(J55-Pin_4)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 -6.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 402 "Net-(J56-Pin_1)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 -7.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 403 "Net-(J56-Pin_3)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 -7.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "Net-(J56-Pin_5)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 -7.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "Net-(J57-Pin_2)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 -8.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "Net-(J57-Pin_4)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 -8.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "Net-(J57-Pin_6)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 -9.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "Net-(J58-Pin_2)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 -9.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "Net-(J58-Pin_4)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 -9.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "Net-(J58-Pin_6)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 -10.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "Net-(J59-Pin_2)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 -10.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "Net-(J59-Pin_4)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 -11.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "Net-(J59-Pin_6)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 -11.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "Net-(J60-Pin_2)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 -11.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 415 "Net-(J60-Pin_4)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 -12.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "Net-(J60-Pin_6)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 -12.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 417 "Net-(J61-Pin_2)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 -12.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "Net-(J61-Pin_4)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 -12.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "Net-(J61-Pin_6)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 -11.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "Net-(J62-Pin_2)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 -11.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "Net-(J62-Pin_4)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 -11.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "Net-(J62-Pin_6)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 -10.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "Net-(J63-Pin_2)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 -10.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "Net-(J63-Pin_4)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 -9.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "Net-(J63-Pin_6)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 -9.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "Net-(J64-Pin_2)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 -9.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "Net-(J64-Pin_4)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 -8.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 428 "Net-(J64-Pin_6)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 -8.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "Net-(J65-Pin_2)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 -7.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "Net-(J65-Pin_4)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 -7.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 431 "Net-(J65-Pin_6)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 -7.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 432 "Net-(J66-Pin_2)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 -6.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "Net-(J66-Pin_4)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 -6.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 434 "Net-(J45-Pin_1)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 -5.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "Net-(J45-Pin_3)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 -5.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 436 "Net-(J45-Pin_5)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 -5.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 437 "Net-(J46-Pin_2)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 -4.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 438 "Net-(J46-Pin_4)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 -4.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 439 "Net-(J46-Pin_6)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 -3.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "Net-(J47-Pin_2)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 -3.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 441 "Net-(J47-Pin_4)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 -3.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 442 "Net-(J47-Pin_6)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 -2.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "Net-(J48-Pin_2)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 -2.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 444 "Net-(J48-Pin_4)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 -1.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 445 "Net-(J48-Pin_6)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 -1.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "Net-(J49-Pin_2)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 -1.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "Net-(J49-Pin_4)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 -0.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 448 "Net-(J49-Pin_6)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 -0.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "Net-(J50-Pin_2)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex" (layer "B.Cu")
    (at 102 59 180)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J95" (at -0.175 7.8) (layer "B.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 -14.374) (layer "B.Fab"))
    (pad "1" smd rect (at 0.645 -0.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "Net-(J50-Pin_5)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 -0.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "Net-(J51-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 -1.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "Net-(J51-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 -1.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "Net-(J51-Pin_5)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 -1.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "Net-(J52-Pin_1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 -2.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "Net-(J52-Pin_3)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 -2.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "Net-(J52-Pin_5)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 -3.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "Net-(J53-Pin_1)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 -3.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "Net-(J53-Pin_3)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 -3.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "Net-(J53-Pin_5)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 -4.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 119 "Net-(J54-Pin_1)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 -4.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "Net-(J54-Pin_3)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 -5.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "Net-(J54-Pin_5)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 -5.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 116 "Net-(J55-Pin_1)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 -5.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "Net-(J55-Pin_3)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 -6.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "Net-(J55-Pin_5)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 -6.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 113 "Net-(J56-Pin_2)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 -7.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "Net-(J56-Pin_4)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 -7.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "Net-(J57-Pin_5)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 -7.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "Net-(J57-Pin_3)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 -8.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "Net-(J57-Pin_1)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 -8.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "Net-(J58-Pin_5)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 -9.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "Net-(J58-Pin_3)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 -9.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "Net-(J58-Pin_1)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 -9.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "Net-(J59-Pin_5)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 -10.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "Net-(J59-Pin_3)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 -10.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "Net-(J59-Pin_1)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 -11.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "Net-(J60-Pin_5)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 -11.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "Net-(J60-Pin_3)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 -11.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "Net-(J60-Pin_1)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 -12.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "Net-(J61-Pin_5)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 -12.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "Net-(J61-Pin_3)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 -12.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "Net-(J61-Pin_1)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 -12.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "Net-(J62-Pin_5)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 -11.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "Net-(J62-Pin_3)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 -11.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "Net-(J62-Pin_1)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 -11.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "Net-(J63-Pin_1)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 -10.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(J63-Pin_3)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 -10.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "Net-(J63-Pin_5)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 -9.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "Net-(J64-Pin_1)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 -9.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "Net-(J64-Pin_3)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 -9.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "Net-(J64-Pin_5)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 -8.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "Net-(J65-Pin_1)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 -8.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "Net-(J65-Pin_3)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 -7.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "Net-(J65-Pin_5)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 -7.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "Net-(J66-Pin_1)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 -7.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "Net-(J66-Pin_3)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 -6.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "Net-(J66-Pin_5)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 -6.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "Net-(J45-Pin_2)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 -5.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "Net-(J45-Pin_4)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 -5.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "Net-(J46-Pin_1)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 -5.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "Net-(J46-Pin_3)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 -4.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "Net-(J46-Pin_5)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 -4.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "Net-(J47-Pin_1)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 -3.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "Net-(J47-Pin_3)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 -3.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "Net-(J47-Pin_5)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 -3.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "Net-(J48-Pin_1)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 -2.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "Net-(J48-Pin_3)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 -2.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "Net-(J48-Pin_5)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 -1.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "Net-(J49-Pin_1)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 -1.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "Net-(J49-Pin_3)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 -1.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "Net-(J49-Pin_5)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 -0.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "Net-(J50-Pin_1)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 -0.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "Net-(J50-Pin_3)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex_Back" (layer "B.Cu")
    (at 93.135 59 180)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J96" (at -0.175 7.8) (layer "B.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 -14.374) (layer "B.Fab"))
    (pad "1" smd rect (at 0.645 -0.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J83-Pin_5)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 -0.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J84-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 -1.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J84-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 -1.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J84-Pin_5)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 -1.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J85-Pin_1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 -2.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J85-Pin_3)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 -2.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J85-Pin_5)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 -3.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(J86-Pin_1)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 -3.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(J86-Pin_3)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 -3.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(J86-Pin_5)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 -4.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(J87-Pin_1)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 -4.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J87-Pin_3)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 -5.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J87-Pin_5)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 -5.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(J88-Pin_1)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 -5.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J88-Pin_3)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 -6.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J88-Pin_5)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 -6.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(J67-Pin_2)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 -7.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J67-Pin_4)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 -7.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(J68-Pin_1)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 -7.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(J68-Pin_3)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 -8.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(J68-Pin_5)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 -8.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(J69-Pin_1)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 -9.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(J69-Pin_3)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 -9.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(J69-Pin_5)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 -9.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(J70-Pin_1)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 -10.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(J70-Pin_3)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 -10.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(J70-Pin_5)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 -11.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(J71-Pin_1)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 -11.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(J71-Pin_3)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 -11.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(J71-Pin_5)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 -12.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(J72-Pin_1)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 -12.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(J72-Pin_3)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 -12.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(J72-Pin_5)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 -12.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(J73-Pin_1)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 -11.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(J73-Pin_3)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 -11.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(J73-Pin_5)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 -11.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J74-Pin_1)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 -10.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(J74-Pin_3)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 -10.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(J74-Pin_5)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 -9.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(J75-Pin_1)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 -9.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(J75-Pin_3)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 -9.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(J75-Pin_5)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 -8.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(J76-Pin_1)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 -8.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(J76-Pin_3)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 -7.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(J76-Pin_5)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 -7.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(J77-Pin_1)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 -7.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(J77-Pin_3)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 -6.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(J77-Pin_5)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 -6.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(J78-Pin_2)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 -5.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(J78-Pin_4)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 -5.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(J79-Pin_1)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 -5.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(J79-Pin_3)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 -4.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(J79-Pin_5)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 -4.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(J80-Pin_1)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 -3.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(J80-Pin_3)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 -3.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(J80-Pin_5)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 -3.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(J81-Pin_1)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 -2.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(J81-Pin_3)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 -2.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(J81-Pin_5)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 -1.9 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(J82-Pin_1)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 -1.5 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(J82-Pin_3)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 -1.1 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(J82-Pin_5)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 -0.7 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(J83-Pin_1)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 -0.3 180) (size 0.66 0.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(J83-Pin_3)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MEAboard_512_footprint:PinHeader_2x32_P0.4mm_Vertical_SMD_Molex" (layer "B.Cu")
    (at 93.135 59 180)
    (descr "surface-mounted straight pin header, 2x32, 0.4mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x32 0.4mm double row")
    (property "Sheetfile" "MEAboard_new.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J94" (at -0.175 7.8) (layer "B.SilkS"))
    (fp_text value "Conn_02x32_Counter_Clockwise" (at 1.5 -14.374) (layer "B.Fab"))
    (pad "1" smd rect (at 0.645 -0.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 322 "Net-(J83-Pin_4)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.645 -0.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 323 "Net-(J83-Pin_6)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 0.645 -1.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 324 "Net-(J84-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.645 -1.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 325 "Net-(J84-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.645 -1.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 326 "Net-(J84-Pin_6)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0.645 -2.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 327 "Net-(J85-Pin_2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 0.645 -2.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 328 "Net-(J85-Pin_4)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0.645 -3.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 329 "Net-(J85-Pin_6)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.645 -3.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 330 "Net-(J86-Pin_2)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 0.645 -3.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 331 "Net-(J86-Pin_4)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 0.645 -4.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 332 "Net-(J86-Pin_6)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 0.645 -4.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 333 "Net-(J87-Pin_2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 0.645 -5.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 334 "Net-(J87-Pin_4)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 0.645 -5.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 335 "Net-(J87-Pin_6)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 0.645 -5.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 336 "Net-(J88-Pin_2)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 0.645 -6.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 337 "Net-(J88-Pin_4)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 0.645 -6.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 338 "Net-(J67-Pin_1)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 0.645 -7.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 339 "Net-(J67-Pin_3)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.645 -7.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 340 "Net-(J67-Pin_5)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.645 -7.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 341 "Net-(J68-Pin_2)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.645 -8.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 342 "Net-(J68-Pin_4)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.645 -8.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 343 "Net-(J68-Pin_6)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 0.645 -9.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 344 "Net-(J69-Pin_2)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.645 -9.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 345 "Net-(J69-Pin_4)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.645 -9.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 346 "Net-(J69-Pin_6)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 0.645 -10.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 347 "Net-(J70-Pin_2)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 0.645 -10.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 348 "Net-(J70-Pin_4)") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 0.645 -11.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 349 "Net-(J70-Pin_6)") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 0.645 -11.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 350 "Net-(J71-Pin_2)") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 0.645 -11.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 351 "Net-(J71-Pin_4)") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 0.645 -12.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 352 "Net-(J71-Pin_6)") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 0.645 -12.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 353 "Net-(J72-Pin_2)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 2.355 -12.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 354 "Net-(J72-Pin_4)") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 2.355 -12.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 355 "Net-(J72-Pin_6)") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 2.355 -11.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 356 "Net-(J73-Pin_2)") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 2.355 -11.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 357 "Net-(J73-Pin_4)") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 2.355 -11.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 358 "Net-(J73-Pin_6)") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 2.355 -10.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 359 "Net-(J74-Pin_2)") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 2.355 -10.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 360 "Net-(J74-Pin_4)") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at 2.355 -9.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 361 "Net-(J74-Pin_6)") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at 2.355 -9.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 362 "Net-(J75-Pin_2)") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at 2.355 -9.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 363 "Net-(J75-Pin_4)") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at 2.355 -8.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 364 "Net-(J75-Pin_6)") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at 2.355 -8.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 365 "Net-(J76-Pin_2)") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at 2.355 -7.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 366 "Net-(J76-Pin_4)") (pinfunction "Pin_45") (pintype "passive"))
    (pad "46" smd rect (at 2.355 -7.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 367 "Net-(J76-Pin_6)") (pinfunction "Pin_46") (pintype "passive"))
    (pad "47" smd rect (at 2.355 -7.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 368 "Net-(J77-Pin_2)") (pinfunction "Pin_47") (pintype "passive"))
    (pad "48" smd rect (at 2.355 -6.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 369 "Net-(J77-Pin_4)") (pinfunction "Pin_48") (pintype "passive"))
    (pad "49" smd rect (at 2.355 -6.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 370 "Net-(J78-Pin_1)") (pinfunction "Pin_49") (pintype "passive"))
    (pad "50" smd rect (at 2.355 -5.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 371 "Net-(J78-Pin_3)") (pinfunction "Pin_50") (pintype "passive"))
    (pad "51" smd rect (at 2.355 -5.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 372 "Net-(J78-Pin_5)") (pinfunction "Pin_51") (pintype "passive"))
    (pad "52" smd rect (at 2.355 -5.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 373 "Net-(J79-Pin_2)") (pinfunction "Pin_52") (pintype "passive"))
    (pad "53" smd rect (at 2.355 -4.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 374 "Net-(J79-Pin_4)") (pinfunction "Pin_53") (pintype "passive"))
    (pad "54" smd rect (at 2.355 -4.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 375 "Net-(J79-Pin_6)") (pinfunction "Pin_54") (pintype "passive"))
    (pad "55" smd rect (at 2.355 -3.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 376 "Net-(J80-Pin_2)") (pinfunction "Pin_55") (pintype "passive"))
    (pad "56" smd rect (at 2.355 -3.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 377 "Net-(J80-Pin_4)") (pinfunction "Pin_56") (pintype "passive"))
    (pad "57" smd rect (at 2.355 -3.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 378 "Net-(J80-Pin_6)") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" smd rect (at 2.355 -2.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 379 "Net-(J81-Pin_2)") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" smd rect (at 2.355 -2.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 380 "Net-(J81-Pin_4)") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" smd rect (at 2.355 -1.9 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 381 "Net-(J81-Pin_6)") (pinfunction "Pin_60") (pintype "passive"))
    (pad "61" smd rect (at 2.355 -1.5 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 382 "Net-(J82-Pin_2)") (pinfunction "Pin_61") (pintype "passive"))
    (pad "62" smd rect (at 2.355 -1.1 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 383 "Net-(J82-Pin_4)") (pinfunction "Pin_62") (pintype "passive"))
    (pad "63" smd rect (at 2.355 -0.7 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 384 "Net-(J82-Pin_6)") (pinfunction "Pin_63") (pintype "passive"))
    (pad "64" smd rect (at 2.355 -0.3 180) (size 0.66 0.22) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 385 "Net-(J83-Pin_2)") (pinfunction "Pin_64") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x32_P1.00mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 226 50.75) (end 226 102)
    (layer "Edge.Cuts"))
  (gr_line (start 150 151.961524) (end 120 151.961524)
    (layer "Edge.Cuts"))
  (gr_line (start 74 50.75) (end 74 102)
    (layer "Edge.Cuts"))
  (gr_circle (center 125.4 144.16) (end 127.55 144.16)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 150 50.75) (end 74 50.75)
    (layer "Edge.Cuts"))
  (gr_circle (center 134.125 60.75) (end 136.275 60.75)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 150 100) (end 173 100)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 105 100) (end 106.6 100)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 74 102) (end 90 102)
    (layer "Edge.Cuts"))
  (gr_circle (center 165.875 60.75) (end 168.025 60.75)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 210 102) (mid 201.693575 131) (end 180 151.961524)
    (layer "Edge.Cuts"))
  (gr_arc (start 120 151.961524) (mid 98.306425 131) (end 90 102)
    (layer "Edge.Cuts"))
  (gr_circle (center 174.6 144.16) (end 176.75 144.16)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 150 50.75) (end 226 50.75)
    (layer "Edge.Cuts"))
  (gr_line (start 210 102) (end 226 102)
    (layer "Edge.Cuts"))
  (gr_line (start 150 151.961524) (end 180 151.961524)
    (layer "Edge.Cuts"))
  (gr_circle (center 195 100) (end 196.6 100)
    (fill none) (layer "Edge.Cuts"))
)
