(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 215)
    (no_connects 0)
    (area 36.493999 112.799 130.035001 155.3765)
    (thickness 1.6)
    (drawings 46)
    (tracks 655)
    (zones 0)
    (modules 63)
    (nets 64)
  )
  (page A4)
  (layers
    (0 Front signal)
    (1 Ground_1 power)
    (2 Ground_2 power)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.152)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.151)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.152)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.075)
    (aux_axis_origin 38.735 154.94)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 PVDD_1V8)
  (net 2 GND)
  (net 3 1V8)
  (net 4 3V3)
  (net 5 5V)
  (net 6 "Net-(C10-Pad1)")
  (net 7 AVDD_1V8)
  (net 8 TXC+)
  (net 9 TX0-)
  (net 10 TX0+)
  (net 11 TX1-)
  (net 12 TX1+)
  (net 13 TX2-)
  (net 14 TX2+)
  (net 15 TXC-)
  (net 16 DDCSCL)
  (net 17 DDCSDA)
  (net 18 HPD)
  (net 19 "Net-(L1-Pad2)")
  (net 20 "Net-(P2-Pad2)")
  (net 21 "Net-(P2-Pad4)")
  (net 22 "Net-(P2-Pad6)")
  (net 23 "Net-(P2-Pad8)")
  (net 24 "Net-(P3-Pad2)")
  (net 25 "Net-(P3-Pad3)")
  (net 26 "Net-(P3-Pad4)")
  (net 27 "Net-(R3-Pad1)")
  (net 28 "Net-(R8-Pad1)")
  (net 29 "Net-(P4-Pad2)")
  (net 30 "Net-(P4-Pad4)")
  (net 31 "Net-(P4-Pad6)")
  (net 32 "Net-(P4-Pad8)")
  (net 33 "Net-(P4-Pad10)")
  (net 34 "Net-(P4-Pad12)")
  (net 35 "Net-(P4-Pad14)")
  (net 36 "Net-(P4-Pad16)")
  (net 37 "Net-(P5-Pad2)")
  (net 38 "Net-(P5-Pad4)")
  (net 39 "Net-(P5-Pad6)")
  (net 40 "Net-(P5-Pad8)")
  (net 41 "Net-(P5-Pad10)")
  (net 42 "Net-(P5-Pad12)")
  (net 43 "Net-(P5-Pad14)")
  (net 44 "Net-(P5-Pad16)")
  (net 45 "Net-(P6-Pad2)")
  (net 46 "Net-(P6-Pad4)")
  (net 47 "Net-(P6-Pad6)")
  (net 48 "Net-(P6-Pad8)")
  (net 49 "Net-(P6-Pad10)")
  (net 50 "Net-(P6-Pad12)")
  (net 51 "Net-(P6-Pad14)")
  (net 52 "Net-(P6-Pad16)")
  (net 53 "Net-(P7-Pad2)")
  (net 54 "Net-(P7-Pad4)")
  (net 55 "Net-(P7-Pad6)")
  (net 56 "Net-(P7-Pad8)")
  (net 57 "Net-(P7-Pad10)")
  (net 58 "Net-(P7-Pad12)")
  (net 59 "Net-(P7-Pad14)")
  (net 60 "Net-(P7-Pad16)")
  (net 61 "Net-(U4-Pad3)")
  (net 62 "Net-(U5-Pad3)")
  (net 63 "Net-(U6-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.151)
    (trace_width 0.152)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net DDCSCL)
    (add_net DDCSDA)
    (add_net GND)
    (add_net HPD)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P4-Pad10)")
    (add_net "Net-(P4-Pad12)")
    (add_net "Net-(P4-Pad14)")
    (add_net "Net-(P4-Pad16)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P5-Pad10)")
    (add_net "Net-(P5-Pad12)")
    (add_net "Net-(P5-Pad14)")
    (add_net "Net-(P5-Pad16)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P5-Pad6)")
    (add_net "Net-(P5-Pad8)")
    (add_net "Net-(P6-Pad10)")
    (add_net "Net-(P6-Pad12)")
    (add_net "Net-(P6-Pad14)")
    (add_net "Net-(P6-Pad16)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad6)")
    (add_net "Net-(P6-Pad8)")
    (add_net "Net-(P7-Pad10)")
    (add_net "Net-(P7-Pad12)")
    (add_net "Net-(P7-Pad14)")
    (add_net "Net-(P7-Pad16)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P7-Pad6)")
    (add_net "Net-(P7-Pad8)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U6-Pad3)")
    (add_net TX0+)
    (add_net TX0-)
    (add_net TX1+)
    (add_net TX1-)
    (add_net TX2+)
    (add_net TX2-)
    (add_net TXC+)
    (add_net TXC-)
  )
  (net_class power ""
    (clearance 0.151)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 1V8)
    (add_net 3V3)
    (add_net 5V)
    (add_net AVDD_1V8)
    (add_net PVDD_1V8)
  )
  (module my-libs:MountHole (layer Front) (tedit 58B9DB90)
    (at 43.1165 117.475)
    (fp_text reference REF** (at 0 4) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -3.75) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module my-libs:MountHole (layer Front) (tedit 58B9DBCD)
    (at 43.18 150.3505)
    (fp_text reference REF** (at 0 4) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -3.75) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module my-libs:MountHole (layer Front) (tedit 58B9DBBD)
    (at 125.7935 117.5385)
    (fp_text reference REF** (at 0 4) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -3.75) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 103.1748 120.7516)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 111.76 134.6708)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 111.76 140.3096)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 111.76 146.6596)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 111.76 145.1356)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 96.012 134.1628)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 93.4212 127.2032)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 96.0628 130.2385)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89EA1)
    (at 58.166 142.24)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.334 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B99EA3)
    (at 64.817 130.556)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B99EB5)
    (at 59.817 130.556)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 73.5 142.24)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 68.5 142.24)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB29A7)
    (at 103.2456 122.2756)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.1248 0) (layer B.SilkS))
    (fp_text value 10u (at -3.6776 0) (layer B.Fab))
    (fp_text user %R (at 2.8248 0) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 1 PVDD_1V8))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2AC8)
    (at 87.376 124.714 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.84 0 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 2.54 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 3 1V8))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2A09)
    (at 77.47 139.954 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.86 0 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 2.56 0 360) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 3 1V8))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB29DA)
    (at 99.314 134.112 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.651 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.524 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 3 1V8))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2AD6)
    (at 89.281 124.714 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.84 0 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 2.54 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 3 1V8))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB29EE)
    (at 81.915 139.065 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.86 0 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 2.56 0 360) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 4 3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB29D0)
    (at 113.995996 117.348 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.997996 0 180) (layer B.SilkS))
    (fp_text value 10u (at -3.556 0 180) (layer B.Fab) hide)
    (fp_text user %R (at 3.378996 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 5 5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB29CC)
    (at 113.995996 115.316 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 2.997996 0 180) (layer B.SilkS))
    (fp_text value 100n (at -4.064 0 180) (layer B.Fab) hide)
    (fp_text user %R (at 3.378996 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 5 5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2B12)
    (at 119.049004 131.2545 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 2.9289 0.026196 180) (layer B.SilkS))
    (fp_text value 10u (at 3.556 0 90) (layer B.Fab) hide)
    (fp_text user %R (at 3.2385 0.076996 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB29B6)
    (at 121.081004 131.2545 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0.0127 2.058196 180) (layer B.SilkS))
    (fp_text value 100n (at 4.064 0 90) (layer B.Fab) hide)
    (fp_text user %R (at 3.7465 0.076996 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB298C)
    (at 103.2456 128.27)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 3.3788 0) (layer B.SilkS))
    (fp_text value 10u (at -3.6776 0) (layer B.Fab))
    (fp_text user %R (at 3.6884 0) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 7 AVDD_1V8))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2A26)
    (at 75.712 132.08 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.3728 -0.0254 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 2.56 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 7 AVDD_1V8))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2AA4)
    (at 79.522 127.762 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 3.3728 0 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 2.54 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 7 AVDD_1V8))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2A21)
    (at 75.712 133.858 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 3.3728 0 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 2.56 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 7 AVDD_1V8))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2A88)
    (at 82.824 124.714 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 3.4236 0 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 2.54 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 1 PVDD_1V8))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2A78)
    (at 82.824 122.936 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 3.3982 0 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 180) (layer B.Fab) hide)
    (fp_text user %R (at 2.54 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 1 PVDD_1V8))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2949)
    (at 103.2456 140.97)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 3.3582 0.0254) (layer B.SilkS))
    (fp_text value 10u (at -3.6776 0) (layer B.Fab))
    (fp_text user %R (at 3.6884 0) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 4 3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Back) (tedit 58BB2973)
    (at 103.2456 134.62)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 3.3788 0) (layer B.SilkS))
    (fp_text value 10u (at -3.556 0) (layer B.Fab) hide)
    (fp_text user %R (at 3.6884 0) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 3 1V8))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer Back) (tedit 58BB2996)
    (at 104 125)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L1 (at 4.0976 -0.032) (layer B.SilkS))
    (fp_text value 10u (at -4.686 -0.032) (layer B.Fab))
    (fp_text user %R (at 4.204 -0.032) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 1 PVDD_1V8))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 19 "Net-(L1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer Back) (tedit 58BB2987)
    (at 104 130.81)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L2 (at 3.8992 0) (layer B.SilkS))
    (fp_text value 10u (at -4.686 0) (layer B.Fab))
    (fp_text user %R (at 4.204 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 7 AVDD_1V8))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 19 "Net-(L1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer Back) (tedit 58BB2941)
    (at 104 143.51)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L3 (at 3.8992 -0.0254) (layer B.SilkS))
    (fp_text value 10u (at -4.686 0) (layer B.Fab))
    (fp_text user %R (at 4.204 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 4 3V3))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer Back) (tedit 58BB2962)
    (at 104 137.16)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L4 (at 4.0516 0.0254) (layer B.SilkS))
    (fp_text value 10u (at -4.686 0) (layer B.Fab))
    (fp_text user %R (at 4.204 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 3 1V8))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers Back B.Paste B.Mask)
      (net 19 "Net-(L1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer Front) (tedit 58B8A21D)
    (at 119.126 115.2525)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at 2.54 -0.9525) (layer F.SilkS) hide)
    (fp_text value 5V (at 2.54 2.6035) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer Front) (tedit 58B8A40C)
    (at 48.26 143.891)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P3 (at 0 9.906) (layer F.SilkS) hide)
    (fp_text value I2C_INT (at 2.286 4.064 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P3-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB285A)
    (at 67.31 128.19 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.7902 -0.0254 360) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.794 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 5 5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 16 DDCSCL))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB2865)
    (at 70.104 127.809 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.794 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 5 5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 17 DDCSDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB2892)
    (at 79.502 127.762 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.2004 0 180) (layer F.SilkS))
    (fp_text value 887R (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.2004 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 27 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB287E)
    (at 77.47 125.984 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.0734 0.0254 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.1496 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 18 HPD))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB28AC)
    (at 58.547 146.685 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.794 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 4 3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 26 "Net-(P3-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB28B2)
    (at 54.483 147.654 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.794 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 4 3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 25 "Net-(P3-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB28B8)
    (at 52.451 144.987 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.8664 0 180) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at -2.794 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 4 3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 24 "Net-(P3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Front) (tedit 58BB28DE)
    (at 69.977 134.239 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -0.0254 1.3462 360) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 2.794 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 28 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer Back) (tedit 58BB2931)
    (at 114.036 126.094 270)
    (descr TO-252-2Lead)
    (attr smd)
    (fp_text reference U2 (at -0.618 0.244 360) (layer B.SilkS))
    (fp_text value NCP1117DT33G (at 0.254 -4.572 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -3.7 2.29) (size 2 3.5) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.7 -2.29) (size 2 3.5) (layers Back B.Paste B.Mask)
      (net 5 5V))
    (pad 2 smd rect (at 3.7 -0.01) (size 7 7) (layers Back B.Paste B.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes\TO-252-2Lead.wrl
      (at (xyz -0.1377952755905512 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer Back) (tedit 58BB293B)
    (at 116.322 139.81 270)
    (descr TO-252-2Lead)
    (attr smd)
    (fp_text reference U3 (at -0.618 -0.01 360) (layer B.SilkS))
    (fp_text value NCP1117DT18G (at 0.254 -4.572 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -3.7 2.29) (size 2 3.5) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.7 -2.29) (size 2 3.5) (layers Back B.Paste B.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 3.7 -0.01) (size 7 7) (layers Back B.Paste B.Mask)
      (net 19 "Net-(L1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes\TO-252-2Lead.wrl
      (at (xyz -0.1377952755905512 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer Front) (tedit 58BB283C)
    (at 63.9445 136.0805)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U5 (at 0.0889 0.8255) (layer F.SilkS))
    (fp_text value TVS_DIODE_3.3VWM_10VC_SMD (at 0 2.6) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 11 TX1-))
    (pad 2 smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 12 TX1+))
    (pad 3 smd rect (at -2.2 0) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 62 "Net-(U5-Pad3)"))
    (pad 4 smd rect (at -2.2 0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 13 TX2-))
    (pad 5 smd rect (at -2.2 1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 14 TX2+))
    (pad 6 smd rect (at 2.2 1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 14 TX2+))
    (pad 7 smd rect (at 2.2 0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 13 TX2-))
    (pad 8 smd rect (at 2.2 0) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 12 TX1+))
    (pad 10 smd rect (at 2.2 -1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 11 TX1-))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer Front) (tedit 58BB282C)
    (at 61.341 128.143 180)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U6 (at 0 -0.8382 180) (layer F.SilkS))
    (fp_text value TVS_DIODE_3.3VWM_10VC_SMD (at 0 2.6 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 16 DDCSCL))
    (pad 2 smd rect (at -2.2 -0.5 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 17 DDCSDA))
    (pad 3 smd rect (at -2.2 0 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 63 "Net-(U6-Pad3)"))
    (pad 4 smd rect (at -2.2 0.5 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 5 5V))
    (pad 5 smd rect (at -2.2 1 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 18 HPD))
    (pad 6 smd rect (at 2.2 1 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 18 HPD))
    (pad 7 smd rect (at 2.2 0.5 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 5 5V))
    (pad 8 smd rect (at 2.2 0 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.2 -0.5 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 17 DDCSDA))
    (pad 10 smd rect (at 2.2 -1 180) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 16 DDCSCL))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm (layer Front) (tedit 58B87763)
    (at 67.564 115.2525 270)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference P4 (at 1.016 20.066 270) (layer F.SilkS) hide)
    (fp_text value AUDIO (at 1.27 20.17 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P4-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P4-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P4-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P4-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P4-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P4-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm (layer Front) (tedit 58B8A88A)
    (at 61.341 152.7195 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference P5 (at 1.27 -2.39 90) (layer F.SilkS) hide)
    (fp_text value RED (at 1.3355 -2.413 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P5-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P5-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P5-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P5-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P5-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P5-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P5-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm (layer Front) (tedit 58B8A404)
    (at 86.741 152.7195 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference P6 (at 1.27 -2.39 90) (layer F.SilkS) hide)
    (fp_text value GREEN (at 1.3355 -2.413 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P6-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P6-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P6-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P6-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P6-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P6-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm (layer Front) (tedit 58B877A9)
    (at 104.4575 115.2525 270)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference P7 (at 1.27 -2.39 270) (layer F.SilkS) hide)
    (fp_text value BLUE (at 1.27 20.17 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P7-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P7-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P7-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P7-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P7-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P7-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P7-Pad16)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer Front) (tedit 58C85B94)
    (at 81.0895 115.2525 270)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference P2 (at 1.27 -2.39 270) (layer F.SilkS) hide)
    (fp_text value SYNC (at 1.27 10.01 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P2-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module my-libs:VIA-0.6mm (layer Front) (tedit 58B89DED)
    (at 63.5 142.24)
    (fp_text reference REF** (at 0.5 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0.25 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module my-libs:MountHole (layer Front) (tedit 58B9DBC6)
    (at 125.73 150.16)
    (fp_text reference REF** (at 0 4) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -3.75) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer Front) (tedit 58BB2833)
    (at 63.9445 132.6515)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U4 (at 0.0515 0.846999) (layer F.SilkS))
    (fp_text value TVS_DIODE_3.3VWM_10VC_SMD (at 0 2.6) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 15 TXC-))
    (pad 2 smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 8 TXC+))
    (pad 3 smd rect (at -2.2 0) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 61 "Net-(U4-Pad3)"))
    (pad 4 smd rect (at -2.2 0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 9 TX0-))
    (pad 5 smd rect (at -2.2 1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 10 TX0+))
    (pad 6 smd rect (at 2.2 1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 10 TX0+))
    (pad 7 smd rect (at 2.2 0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 9 TX0-))
    (pad 8 smd rect (at 2.2 0) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 8 TXC+))
    (pad 10 smd rect (at 2.2 -1) (size 1.4 0.3) (layers Front F.Paste F.Mask)
      (net 15 TXC-))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my-libs:OSHW-logo_10mm (layer Front) (tedit 0)
    (at 116.2304 125.4252)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value REF (at 0 0) (layer F.SilkS) hide)
  )
  (module hdmi:hdmi_new (layer Front) (tedit 58D94CA0)
    (at 46.72 132.338 270)
    (fp_text reference J1 (at 7.0064 -3.3688 360) (layer F.SilkS))
    (fp_text value HDMI (at 0.25 3.556 270) (layer F.SilkS) hide)
    (pad 10 smd rect (at 0.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 8 TXC+))
    (pad 9 smd rect (at 0.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 9 TX0-))
    (pad 8 smd rect (at 1.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 1.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 10 TX0+))
    (pad 6 smd rect (at 2.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 11 TX1-))
    (pad 5 smd rect (at 2.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 3.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 12 TX1+))
    (pad 3 smd rect (at 3.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 13 TX2-))
    (pad 2 smd rect (at 4.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 14 TX2+))
    (pad 11 smd rect (at -0.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -0.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 15 TXC-))
    (pad 13 smd rect (at -1.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -1.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at -2.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 16 DDCSCL))
    (pad 16 smd rect (at -2.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 17 DDCSDA))
    (pad 17 smd rect (at -3.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at -3.75 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 5 5V))
    (pad 19 smd rect (at -4.25 -1.3 270) (size 0.3 2.75) (layers Front F.Paste F.Mask)
      (net 18 HPD))
    (pad 0 thru_hole circle (at -7.25 0 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 0 thru_hole circle (at 7.25 0 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 0 thru_hole circle (at -7.85 4.9 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 0 thru_hole circle (at 7.85 4.9 270) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module my-libs:HTQFP-64_1EP_10x10mm_Pitch0.5mm_ThermalPad3 (layer Front) (tedit 58C85BC3)
    (at 86.36 134.112 270)
    (descr "64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [HTQFP] thermal pad")
    (tags "HTQFP-64 Pitch 0.5 ")
    (attr smd)
    (fp_text reference U1 (at -5.842 -5.588 360) (layer F.SilkS))
    (fp_text value ADV7513 (at 0 8.25 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -6.2 -3.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 3 1V8))
    (pad 2 smd rect (at -6.2 -3.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 23 "Net-(P2-Pad8)"))
    (pad 3 smd rect (at -6.2 -2.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 29 "Net-(P4-Pad2)"))
    (pad 4 smd rect (at -6.2 -2.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 30 "Net-(P4-Pad4)"))
    (pad 5 smd rect (at -6.2 -1.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 31 "Net-(P4-Pad6)"))
    (pad 6 smd rect (at -6.2 -1.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 32 "Net-(P4-Pad8)"))
    (pad 7 smd rect (at -6.2 -0.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 33 "Net-(P4-Pad10)"))
    (pad 8 smd rect (at -6.2 -0.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 34 "Net-(P4-Pad12)"))
    (pad 9 smd rect (at -6.2 0.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 35 "Net-(P4-Pad14)"))
    (pad 10 smd rect (at -6.2 0.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 36 "Net-(P4-Pad16)"))
    (pad 11 smd rect (at -6.2 1.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 3 1V8))
    (pad 12 smd rect (at -6.2 1.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 1 PVDD_1V8))
    (pad 13 smd rect (at -6.2 2.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 1 PVDD_1V8))
    (pad 14 smd rect (at -6.2 2.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 27 "Net-(R3-Pad1)"))
    (pad 15 smd rect (at -6.2 3.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 7 AVDD_1V8))
    (pad 16 smd rect (at -6.2 3.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 18 HPD))
    (pad 17 smd rect (at -3.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 15 TXC-))
    (pad 18 smd rect (at -3.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 8 TXC+))
    (pad 19 smd rect (at -2.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 7 AVDD_1V8))
    (pad 20 smd rect (at -2.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 9 TX0-))
    (pad 21 smd rect (at -1.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 10 TX0+))
    (pad 22 smd rect (at -1.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 28 "Net-(R8-Pad1)"))
    (pad 23 smd rect (at -0.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 11 TX1-))
    (pad 24 smd rect (at -0.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 12 TX1+))
    (pad 25 smd rect (at 0.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 7 AVDD_1V8))
    (pad 26 smd rect (at 0.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 13 TX2-))
    (pad 27 smd rect (at 1.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 14 TX2+))
    (pad 28 smd rect (at 1.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 24 "Net-(P3-Pad2)"))
    (pad 29 smd rect (at 2.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 4 3V3))
    (pad 30 smd rect (at 2.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 31 smd rect (at 3.25 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 3 1V8))
    (pad 32 smd rect (at 3.75 6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 33 smd rect (at 6.2 3.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 16 DDCSCL))
    (pad 34 smd rect (at 6.2 3.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 17 DDCSDA))
    (pad 35 smd rect (at 6.2 2.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 25 "Net-(P3-Pad3)"))
    (pad 36 smd rect (at 6.2 2.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 26 "Net-(P3-Pad4)"))
    (pad 37 smd rect (at 6.2 1.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 37 "Net-(P5-Pad2)"))
    (pad 38 smd rect (at 6.2 1.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 38 "Net-(P5-Pad4)"))
    (pad 39 smd rect (at 6.2 0.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 39 "Net-(P5-Pad6)"))
    (pad 40 smd rect (at 6.2 0.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 40 "Net-(P5-Pad8)"))
    (pad 41 smd rect (at 6.2 -0.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 41 "Net-(P5-Pad10)"))
    (pad 42 smd rect (at 6.2 -0.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 42 "Net-(P5-Pad12)"))
    (pad 43 smd rect (at 6.2 -1.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 43 "Net-(P5-Pad14)"))
    (pad 44 smd rect (at 6.2 -1.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 44 "Net-(P5-Pad16)"))
    (pad 45 smd rect (at 6.2 -2.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 45 "Net-(P6-Pad2)"))
    (pad 46 smd rect (at 6.2 -2.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 46 "Net-(P6-Pad4)"))
    (pad 47 smd rect (at 6.2 -3.25 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 47 "Net-(P6-Pad6)"))
    (pad 48 smd rect (at 6.2 -3.75 270) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 48 "Net-(P6-Pad8)"))
    (pad 49 smd rect (at 3.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 49 "Net-(P6-Pad10)"))
    (pad 50 smd rect (at 3.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 50 "Net-(P6-Pad12)"))
    (pad 51 smd rect (at 2.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 3 1V8))
    (pad 52 smd rect (at 2.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 51 "Net-(P6-Pad14)"))
    (pad 53 smd rect (at 1.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 22 "Net-(P2-Pad6)"))
    (pad 54 smd rect (at 1.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 52 "Net-(P6-Pad16)"))
    (pad 55 smd rect (at 0.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 53 "Net-(P7-Pad2)"))
    (pad 56 smd rect (at 0.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 54 "Net-(P7-Pad4)"))
    (pad 57 smd rect (at -0.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 55 "Net-(P7-Pad6)"))
    (pad 58 smd rect (at -0.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 56 "Net-(P7-Pad8)"))
    (pad 59 smd rect (at -1.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 57 "Net-(P7-Pad10)"))
    (pad 60 smd rect (at -1.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 58 "Net-(P7-Pad12)"))
    (pad 61 smd rect (at -2.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 59 "Net-(P7-Pad14)"))
    (pad 62 smd rect (at -2.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 60 "Net-(P7-Pad16)"))
    (pad 63 smd rect (at -3.25 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 20 "Net-(P2-Pad2)"))
    (pad 64 smd rect (at -3.75 -6.2) (size 2.5 0.3) (layers Front F.Paste F.Mask)
      (net 21 "Net-(P2-Pad4)"))
    (pad 65 smd rect (at 0 0 270) (size 5.2 5.2) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 65 smd rect (at 0 0 270) (size 5.2 5.2) (layers Back B.Paste B.Mask)
      (net 2 GND))
    (pad 65 thru_hole circle (at 0 0 270) (size 4.5 4.5) (drill 4) (layers *.Cu)
      (net 2 GND))
    (model Housings_QFP.3dshapes/TQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "by chriz2600\ngithub.com/chriz2600/ADV7513" (at 116.2558 139.4206) (layer F.SilkS))
  (gr_text "ADV7513 \nDevelopment Board" (at 116.2304 134.9502) (layer F.SilkS))
  (gr_text SPFMDBC (at 116.205 131.0894) (layer F.SilkS))
  (gr_text "GND\nINT 28\nI2C SCL 35\nI2C SDA 36\n" (at 46.482 144.8054) (layer F.SilkS))
  (gr_text "<- All GND" (at 110.236 152.654) (layer F.SilkS))
  (gr_text "DATA23 37" (at 61.3664 148.5 90) (layer F.SilkS))
  (gr_text "DATA22 38" (at 63.9064 148.5 90) (layer F.SilkS))
  (gr_text "DATA21 39" (at 66.4464 148.5 90) (layer F.SilkS))
  (gr_text "DATA20 40" (at 68.9864 148.5 90) (layer F.SilkS))
  (gr_text "DATA19 41" (at 71.5264 148.5 90) (layer F.SilkS))
  (gr_text "DATA18 42" (at 74.0664 148.5 90) (layer F.SilkS))
  (gr_text "DATA17 43" (at 76.6064 148.5 90) (layer F.SilkS))
  (gr_text "DATA16 44" (at 79.1464 148.5 90) (layer F.SilkS))
  (gr_text "DATA15 45" (at 86.7664 148.5 90) (layer F.SilkS))
  (gr_text "DATA14 46" (at 89.3064 148.5 90) (layer F.SilkS))
  (gr_text "DATA13 47" (at 91.8464 148.5 90) (layer F.SilkS))
  (gr_text "DATA12 48" (at 94.3864 148.5 90) (layer F.SilkS))
  (gr_text "DATA11 49" (at 96.9264 148.5 90) (layer F.SilkS))
  (gr_text "DATA10 50" (at 99.4664 148.5 90) (layer F.SilkS))
  (gr_text "DATA9 52" (at 102.0064 148.5 90) (layer F.SilkS))
  (gr_text "DATA8 54" (at 104.5464 148.5 90) (layer F.SilkS))
  (gr_text "DATA7 55" (at 104.4956 119.5 90) (layer F.SilkS))
  (gr_text "DATA6 56" (at 101.9556 119.5 90) (layer F.SilkS))
  (gr_text "DATA5 57" (at 99.4156 119.5 90) (layer F.SilkS))
  (gr_text "DATA4 58" (at 96.8756 119.5 90) (layer F.SilkS))
  (gr_text "DATA3 59" (at 94.2848 119.5 90) (layer F.SilkS))
  (gr_text "DATA2 60" (at 91.7448 119.5 90) (layer F.SilkS))
  (gr_text "DATA1 61" (at 89.2556 119.5 90) (layer F.SilkS))
  (gr_text "DATA0 62" (at 86.7156 119.5 90) (layer F.SilkS))
  (gr_text "DE 63" (at 81.1022 119.5 90) (layer F.SilkS))
  (gr_text "HSYNC 64" (at 78.5368 119.5 90) (layer F.SilkS))
  (gr_text "CLK 53" (at 75.9968 119.5 90) (layer F.SilkS))
  (gr_text "VSYNC 2" (at 73.4568 119.5 90) (layer F.SilkS))
  (gr_text "LRCLK 10" (at 49.784 119.5 90) (layer F.SilkS))
  (gr_text "SCLK 9" (at 52.324 119.5 90) (layer F.SilkS))
  (gr_text "I2CS3 8" (at 54.864 119.5 90) (layer F.SilkS))
  (gr_text "I2CS2 7" (at 57.4294 119.5 90) (layer F.SilkS))
  (gr_text "I2CS1 6" (at 59.944 119.5 90) (layer F.SilkS))
  (gr_text "I2CS0 5" (at 62.5094 119.5 90) (layer F.SilkS))
  (gr_text "MCLK 4" (at 64.9986 119.5 90) (layer F.SilkS))
  (gr_text "SPDIF 3" (at 67.564 119.5 90) (layer F.SilkS))
  (gr_text "<- All GND ->" (at 111.76 115.1636) (layer F.SilkS))
  (gr_line (start 38.72 113.03) (end 38.72 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.96 113.03) (end 38.72 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.96 154.94) (end 129.96 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.72 154.94) (end 129.96 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer Ground_1) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.9255 113.2205) (xy 129.794 113.2205) (xy 129.794 154.7495) (xy 38.9255 154.7495)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.9255 113.2205) (xy 129.794 113.2205) (xy 129.794 154.7495) (xy 38.9255 154.7495)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Ground_2) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.9255 113.2205) (xy 129.794 113.2205) (xy 129.794 154.7495) (xy 38.9255 154.7495)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.9255 113.2205) (xy 38.9255 154.7495) (xy 129.794 154.7495) (xy 129.794 113.2205)
      )
    )
  )
)
