(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 34)
    (tracks 152)
    (zones 0)
    (modules 9)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad11)")
  (net 2 "Net-(J1-Pad10)")
  (net 3 "Net-(J1-Pad9)")
  (net 4 "Net-(J1-Pad8)")
  (net 5 "Net-(J1-Pad7)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad5)")
  (net 8 "Net-(J1-Pad4)")
  (net 9 "Net-(J1-Pad3)")
  (net 10 "Net-(J1-Pad2)")
  (net 11 "Net-(J1-Pad1)")
  (net 12 "Net-(J1-Pad18)")
  (net 13 "Net-(J1-Pad17)")
  (net 14 "Net-(J1-Pad16)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad14)")
  (net 17 "Net-(J1-Pad13)")
  (net 18 "Net-(J1-Pad12)")
  (net 19 "Net-(SW1-Pad1)")
  (net 20 "Net-(SW2-Pad1)")
  (net 21 "Net-(SW3-Pad1)")
  (net 22 "Net-(SW4-Pad1)")
  (net 23 "Net-(SW5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(SW3-Pad1)")
    (add_net "Net-(SW4-Pad1)")
    (add_net "Net-(SW5-Pad1)")
  )
  (module "my library:Phoenix_16_pin_5mm_terminal_block" (layer B.Cu) (tedit 5D6B1A83)
    (at 113.03 59.69)
    (fp_text reference J2 (at 2 1) (layer B.SilkS))
    (fp_text value "LED terminals" (at 20 1) (layer B.Fab))
    (pad 16 thru_hole circle (at 77.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad9)"))
    (pad 15 thru_hole circle (at 72.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 14 thru_hole circle (at 67.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad18)"))
    (pad 13 thru_hole circle (at 62.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 12 thru_hole circle (at 57.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad17)"))
    (pad 11 thru_hole circle (at 52.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 10 thru_hole circle (at 47.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad16)"))
    (pad 9 thru_hole circle (at 42.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 8 thru_hole circle (at 37.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 7 thru_hole circle (at 32.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 6 thru_hole circle (at 27.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad13)"))
    (pad 5 thru_hole circle (at 22.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 17.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad14)"))
    (pad 3 thru_hole circle (at 12.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad12)"))
    (pad 1 thru_hole circle (at 2.5 -5) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x18_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 63.5 54.102 270)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x18_Female (at 2.794 -18.288) (layer B.Fab) hide)
    (fp_text user %R (at 0 -21.59) (layer B.Fab))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x18_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "my library:Mini_Toggle_3pin" (layer F.Cu) (tedit 5D619F92)
    (at 210.82 62.992)
    (descr "mini toggle switch, 1/4 in., 0.185\" pin spacing, 0.73\" pin hole")
    (tags "M2011SS1W03, M2018SS1W03")
    (fp_text reference SW7 (at -6.096 10.414) (layer F.SilkS))
    (fp_text value Rate (at -6.35 4.572) (layer B.SilkS))
    (pad 3 thru_hole circle (at 0 9.4) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad10)"))
    (pad 2 thru_hole circle (at 0 4.7) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad11)"))
  )
  (module "my library:Mini_Toggle_3pin" (layer F.Cu) (tedit 5D619F92)
    (at 58.42 62.992)
    (descr "mini toggle switch, 1/4 in., 0.185\" pin spacing, 0.73\" pin hole")
    (tags "M2011SS1W03, M2018SS1W03")
    (fp_text reference SW6 (at 6.35 10.922) (layer F.SilkS))
    (fp_text value Master (at 5.08 4.318 270 unlocked) (layer B.SilkS))
    (pad 3 thru_hole circle (at 0 9.4) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 4.7) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad4)"))
  )
  (module "my library:Mini_Toggle_3pin" (layer F.Cu) (tedit 5D619F92)
    (at 185.42 62.992)
    (descr "mini toggle switch, 1/4 in., 0.185\" pin spacing, 0.73\" pin hole")
    (tags "M2011SS1W03, M2018SS1W03")
    (fp_text reference SW5 (at -6.26533 10.414) (layer F.SilkS))
    (fp_text value Auto (at -6.13833 4.572) (layer B.SilkS))
    (pad 3 thru_hole circle (at 0 9.4) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad9)"))
    (pad 2 thru_hole circle (at 0 4.7) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 23 "Net-(SW5-Pad1)"))
  )
  (module "my library:Mini_Toggle_3pin" (layer F.Cu) (tedit 5D619F92)
    (at 160.02 62.992)
    (descr "mini toggle switch, 1/4 in., 0.185\" pin spacing, 0.73\" pin hole")
    (tags "M2011SS1W03, M2018SS1W03")
    (fp_text reference SW4 (at -6.180664 10.668) (layer F.SilkS))
    (fp_text value SW4 (at -5.926664 4.572) (layer B.SilkS))
    (pad 3 thru_hole circle (at 0 9.4) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (pad 2 thru_hole circle (at 0 4.7) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 22 "Net-(SW4-Pad1)"))
  )
  (module "my library:Mini_Toggle_3pin" (layer F.Cu) (tedit 5D619F92)
    (at 134.62 62.992)
    (descr "mini toggle switch, 1/4 in., 0.185\" pin spacing, 0.73\" pin hole")
    (tags "M2011SS1W03, M2018SS1W03")
    (fp_text reference SW3 (at -6.095998 10.668) (layer F.SilkS))
    (fp_text value SW3 (at -6.222998 4.318) (layer B.SilkS))
    (pad 3 thru_hole circle (at 0 9.4) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad7)"))
    (pad 2 thru_hole circle (at 0 4.7) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 21 "Net-(SW3-Pad1)"))
  )
  (module "my library:Mini_Toggle_3pin" (layer F.Cu) (tedit 5D619F92)
    (at 109.22 62.992)
    (descr "mini toggle switch, 1/4 in., 0.185\" pin spacing, 0.73\" pin hole")
    (tags "M2011SS1W03, M2018SS1W03")
    (fp_text reference SW2 (at -6.265332 10.414) (layer F.SilkS))
    (fp_text value SW2 (at -6.011332 4.572) (layer B.SilkS))
    (pad 3 thru_hole circle (at 0 9.4) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 2 thru_hole circle (at 0 4.7) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 20 "Net-(SW2-Pad1)"))
  )
  (module "my library:Mini_Toggle_3pin" (layer F.Cu) (tedit 5D619F92)
    (at 83.82 62.992)
    (descr "mini toggle switch, 1/4 in., 0.185\" pin spacing, 0.73\" pin hole")
    (tags "M2011SS1W03, M2018SS1W03")
    (fp_text reference SW1 (at -5.926666 10.668) (layer F.SilkS))
    (fp_text value SW1 (at -6.053666 4.572) (layer B.SilkS))
    (pad 3 thru_hole circle (at 0 9.4) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (pad 2 thru_hole circle (at 0 4.7) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.048 3.048) (drill 1.8542) (layers *.Cu *.Mask)
      (net 19 "Net-(SW1-Pad1)"))
  )
  (gr_text "02-Sep-2019\n" (at 209.296 54.102) (layer B.SilkS))
  (gr_text Back (at 212.598 58.674) (layer B.SilkS))
  (gr_text Front (at 57.404 52.578) (layer F.SilkS))
  (gr_text 7 (at 177.8 61.468) (layer B.SilkS))
  (gr_text 6 (at 167.64 61.468) (layer B.SilkS))
  (gr_text 5 (at 154.686 61.468) (layer B.SilkS))
  (gr_text "Sec1\n\n\n" (at 89.154 56.134 -90) (layer B.SilkS))
  (gr_text "Sec2\n\n\n" (at 93.98 56.134 -90) (layer B.SilkS))
  (gr_text "Sec3\n\n\n" (at 91.44 56.134 -90) (layer B.SilkS))
  (gr_text "Sec4\n\n\n" (at 96.52 56.134 -90) (layer B.SilkS))
  (gr_text "Sec5\n\n" (at 100.584 56.134 -90) (layer B.SilkS))
  (gr_text "Sec6\n" (at 104.394 56.134 -90) (layer B.SilkS))
  (gr_text Sec7 (at 106.68 56.134 -90) (layer B.SilkS))
  (gr_text A (at 191.262 61.468) (layer B.SilkS))
  (gr_text 4 (at 147.828 61.468) (layer B.SilkS))
  (gr_text 3 (at 139.7 61.468) (layer B.SilkS))
  (gr_text 2 (at 127.762 61.468) (layer B.SilkS))
  (gr_text 1 (at 118.11 61.468) (layer B.SilkS))
  (gr_text 5V (at 65.786 56.134 -90) (layer B.SilkS))
  (gr_text GND (at 62.992 56.134 -90) (layer B.SilkS))
  (gr_text DOWN (at 88.9 56.134 -90) (layer B.SilkS))
  (gr_text UP (at 86.106 56.134 -90) (layer B.SilkS))
  (gr_text AUTO (at 83.82 56.134 -90) (layer B.SilkS))
  (gr_text SW4 (at 81.28 56.134 -90) (layer B.SilkS))
  (gr_text SW3 (at 78.74 56.134 -90) (layer B.SilkS))
  (gr_text SW2 (at 76.2 56.134 -90) (layer B.SilkS))
  (gr_text SW1 (at 73.66 56.134 -90) (layer B.SilkS))
  (gr_text "OFF\n" (at 71.12 56.134 -90) (layer B.SilkS))
  (gr_text ON (at 68.58 56.134 -90) (layer B.SilkS))
  (gr_text "Switches 1.0 \n" (at 209.55 52.07) (layer B.SilkS))
  (gr_line (start 53 75) (end 216 75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53 50) (end 53 75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53 50) (end 216 50) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 216 50) (end 216 75) (layer Edge.Cuts) (width 0.05))
  (zone (net 11) (net_name "Net-(J1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.646 50.292) (xy 215.646 74.676) (xy 53.34 74.676) (xy 53.34 50.292)
      )
    )
  )
)
