(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 34)
    (tracks 199)
    (zones 0)
    (modules 14)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.02)
    (via_min_drill 0.1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.01)
    (uvia_min_drill 0.05)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +BATT)
  (net 3 /RESET)
  (net 4 /SW_CLK)
  (net 5 /SW_DIO)
  (net 6 /P3_4)
  (net 7 /P3_1)
  (net 8 /P3_0)
  (net 9 /P2_7)
  (net 10 /P2_6)
  (net 11 /P2_5)
  (net 12 /P2_4)
  (net 13 /P2_3)
  (net 14 /P2_2)
  (net 15 /P0_0)
  (net 16 /P0_1)
  (net 17 /P0_2)
  (net 18 /P0_4)
  (net 19 /P0_5)
  (net 20 /P0_6)
  (net 21 /P1_0)
  (net 22 /P1_1)
  (net 23 /P1_2)
  (net 24 /P1_3)
  (net 25 "Net-(U1-Pad16)")
  (net 26 "Net-(U1-Pad17)")
  (net 27 "Net-(U1-Pad18)")
  (net 28 "Net-(C5-Pad2)")
  (net 29 "Net-(J1-Pad6)")
  (net 30 "Net-(J1-Pad7)")
  (net 31 "Net-(J1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
  )
  (net_class IO ""
    (clearance 0.1)
    (trace_width 0.15)
    (via_dia 0.4)
    (via_drill 0.2)
    (uvia_dia 0.1)
    (uvia_drill 0.05)
    (add_net /P0_0)
    (add_net /P0_1)
    (add_net /P0_2)
    (add_net /P0_4)
    (add_net /P0_5)
    (add_net /P0_6)
    (add_net /P1_0)
    (add_net /P1_1)
    (add_net /P1_2)
    (add_net /P1_3)
    (add_net /P2_2)
    (add_net /P2_3)
    (add_net /P2_4)
    (add_net /P2_5)
    (add_net /P2_6)
    (add_net /P2_7)
    (add_net /P3_0)
    (add_net /P3_1)
    (add_net /P3_4)
    (add_net /RESET)
    (add_net /SW_CLK)
    (add_net /SW_DIO)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net GND)
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 5EA8973E)
    (at 162.433 102.108)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J1 (at -2.54 -3.683) (layer F.SilkS))
    (fp_text value Conn_ARM_JTAG_SWD_10 (at 0 4.235) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 2 smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 /SW_DIO))
    (pad 3 smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 4 /SW_CLK))
    (pad 5 smd rect (at -1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at -1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 /RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PSoC4200D_Module (layer F.Cu) (tedit 5E979B78)
    (at 0 0)
    (fp_text reference REF** (at 0 12.7) (layer F.SilkS) hide)
    (fp_text value PSoC4200D_Module (at 0 -10.16) (layer F.Fab))
  )
  (module "PriceTec Docs:logo_front_silk" (layer B.Cu) (tedit 0)
    (at 167.259 101.473 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 164.578 108.204 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -1.284 -0.889 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 160.415 110.744 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -1.256 -0.889 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 165.114 110.744 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -1.256 -0.889 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 169.658 110.744 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -1.284 -0.889 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 174.23 110.744 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -1.284 -0.889) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +BATT))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 160.415 108.204 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -1.383 -0.889) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +BATT))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SSOP-28_5.3x10.2mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 171.196 103.886)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value CY8C4246PVI-DS402 (at 0 6.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /P1_0))
    (pad 2 smd rect (at -3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 /P1_1))
    (pad 3 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 /P1_2))
    (pad 4 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 /P1_3))
    (pad 5 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 /P2_2))
    (pad 6 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 /P2_3))
    (pad 7 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /P2_4))
    (pad 8 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /P2_5))
    (pad 9 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 /P2_6))
    (pad 10 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 /P2_7))
    (pad 11 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /P3_0))
    (pad 12 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /P3_1))
    (pad 13 smd rect (at -3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 /SW_DIO))
    (pad 14 smd rect (at -3.6 4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /SW_CLK))
    (pad 15 smd rect (at 3.6 4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 /P3_4))
    (pad 16 smd rect (at 3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /P0_0))
    (pad 20 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 /P0_1))
    (pad 21 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 /P0_2))
    (pad 22 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 /P0_4))
    (pad 23 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 /P0_5))
    (pad 24 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /P0_6))
    (pad 25 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 /RESET))
    (pad 26 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C5-Pad2)"))
    (pad 27 smd rect (at 3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 28 smd rect (at 3.6 -4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-28_5.3x10.2mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:01x06_Casellated (layer F.Cu) (tedit 5E97740B)
    (at 167.386 115.062 90)
    (fp_text reference J2 (at 1.27 8.382 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0 -8.89 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 0 6.35 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 3.81 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 1.27 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P3_4))
    (pad 3 thru_hole circle (at 0 -1.27 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P3_1))
    (pad 2 thru_hole circle (at 0 -3.81 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /P3_0))
    (pad 1 thru_hole circle (at 0 -6.35 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +BATT))
  )
  (module Connector_PinHeader_2.54mm:01x06_Casellated (layer F.Cu) (tedit 5E97740B)
    (at 155.956 104.902)
    (fp_text reference J3 (at 1.524 8.128) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0 -8.89) (layer F.Fab))
    (pad 6 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 /P2_7))
    (pad 5 thru_hole circle (at 0 3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 /P2_6))
    (pad 4 thru_hole circle (at 0 1.27) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 /P2_5))
    (pad 3 thru_hole circle (at 0 -1.27) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 /P2_4))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 /P2_3))
    (pad 1 thru_hole circle (at 0 -6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 /P2_2))
  )
  (module Connector_PinHeader_2.54mm:01x06_Casellated (layer F.Cu) (tedit 5E97740B)
    (at 178.816 104.902 180)
    (fp_text reference J4 (at 1.27 8.128) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0 -8.89) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -6.35 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 /P0_0))
    (pad 2 thru_hole circle (at 0 -3.81 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 /P0_1))
    (pad 3 thru_hole circle (at 0 -1.27 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 /P0_2))
    (pad 4 thru_hole circle (at 0 1.27 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 /P0_4))
    (pad 5 thru_hole circle (at 0 3.81 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 /P0_5))
    (pad 6 thru_hole circle (at 0 6.35 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 /P0_6))
  )
  (module Connector_PinHeader_2.54mm:01x06_Casellated (layer F.Cu) (tedit 5E97740B)
    (at 167.386 94.742 90)
    (fp_text reference J5 (at -1.27 -8.382 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0 -8.89 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -6.35 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +BATT))
    (pad 2 thru_hole circle (at 0 -3.81 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 /P1_0))
    (pad 3 thru_hole circle (at 0 -1.27 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 /P1_1))
    (pad 4 thru_hole circle (at 0 1.27 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 /P1_2))
    (pad 5 thru_hole circle (at 0 3.81 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 /P1_3))
    (pad 6 thru_hole circle (at 0 6.35 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_line (start 159.512 94.742) (end 175.26 94.742) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155.956 111.506) (end 155.956 98.298) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.639 115.062) (end 159.512 115.062) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 175.26 115.062) (end 159.639 115.062) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.816 98.298) (end 178.816 111.506) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 175.26 111.506) (end 175.26 115.062) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text VIN (at 161.036 113.284) (layer F.SilkS))
  (gr_text VIN (at 161.036 96.774) (layer F.SilkS))
  (gr_text P1.0 (at 163.576 96.774) (layer F.SilkS))
  (gr_text P1.1 (at 166.116 96.774) (layer F.SilkS))
  (gr_text P1.2 (at 168.656 96.774) (layer F.SilkS))
  (gr_text P1.3 (at 171.196 96.774) (layer F.SilkS))
  (gr_text GND (at 173.736 96.774) (layer F.SilkS))
  (gr_text P0.6 (at 177.038 98.552 90) (layer F.SilkS))
  (gr_text P0.5 (at 177.038 101.092 90) (layer F.SilkS))
  (gr_text P0.4 (at 177.038 103.632 90) (layer F.SilkS))
  (gr_text P0.2 (at 177.038 106.172 90) (layer F.SilkS))
  (gr_text P0.1 (at 177.038 108.712 90) (layer F.SilkS))
  (gr_text P0.0 (at 177.038 111.252 90) (layer F.SilkS))
  (gr_text P3.4 (at 168.656 113.284) (layer F.SilkS))
  (gr_text P3.1 (at 166.116 113.284) (layer F.SilkS))
  (gr_text P3.0 (at 163.576 113.284) (layer F.SilkS))
  (gr_text GND (at 173.736 113.284) (layer F.SilkS))
  (gr_text GND (at 171.196 113.284) (layer F.SilkS))
  (gr_text P2.7 (at 157.734 111.252 270) (layer F.SilkS))
  (gr_text P2.6 (at 157.734 108.712 270) (layer F.SilkS))
  (gr_text P2.5 (at 157.734 106.172 270) (layer F.SilkS))
  (gr_text P2.4 (at 157.734 103.632 270) (layer F.SilkS))
  (gr_text P2.3 (at 157.734 101.092 270) (layer F.SilkS))
  (gr_text P2.2 (at 157.734 98.552 270) (layer F.SilkS))
  (gr_arc (start 159.512 111.506) (end 155.956 111.506) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 175.26 98.298) (end 178.816 98.298) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 159.512 98.298) (end 159.512 94.742) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.575 94.742) (xy 179.197 94.742) (xy 178.943 115.697) (xy 155.702 115.316)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.829 94.488) (xy 178.689 94.488) (xy 178.816 116.078) (xy 155.702 115.824)
      )
    )
  )
)
