(kicad_pcb (version 3) (host pcbnew "(2013-07-07 BZR 4022)-stable")
  (general
    (links 27)
    (no_connects 0)
    (area 149.749999 130.799999 232.600001 147.800001)
    (thickness 1.6)
    (drawings 18)
    (tracks 53)
    (zones 0)
    (modules 27)
    (nets 17)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.25 1.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFBF)
    (pcbplotparams
      (layerselection 3178497)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /BATT_GREEN)
  (net 2 /BATT_RED)
  (net 3 /BATT_YELLOW)
  (net 4 /HOME)
  (net 5 /HOME_BLUE)
  (net 6 /HOME_RED)
  (net 7 /TV)
  (net 8 GND)
  (net 9 N-000001)
  (net 10 N-0000010)
  (net 11 N-0000016)
  (net 12 N-000002)
  (net 13 N-000003)
  (net 14 N-000007)
  (net 15 N-000008)
  (net 16 N-000009)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net /BATT_GREEN)
    (add_net /BATT_RED)
    (add_net /BATT_YELLOW)
    (add_net /HOME)
    (add_net /HOME_BLUE)
    (add_net /HOME_RED)
    (add_net /TV)
    (add_net GND)
    (add_net N-000001)
    (add_net N-0000010)
    (add_net N-0000016)
    (add_net N-000002)
    (add_net N-000003)
    (add_net N-000007)
    (add_net N-000008)
    (add_net N-000009)
  )
  (net_class Line1 ""
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module SM0805 (layer F.Cu) (tedit 59972D7D)
    (at 163.55 138.75 180)
    (attr smd)
    (fp_text reference R1 (at 0 -0.3175 180) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /HOME_RED)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 14 N-000007)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 59972D92)
    (at 163.55 140.75 180)
    (attr smd)
    (fp_text reference R2 (at 0 -0.3175 180) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /HOME_BLUE)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-0000010)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 59972D3E)
    (at 204.55 136.4 180)
    (attr smd)
    (fp_text reference R3 (at 0 -0.3175 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /BATT_RED)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 16 N-000009)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0805 (layer F.Cu) (tedit 59972D45)
    (at 204.55 138.4 180)
    (attr smd)
    (fp_text reference R4 (at 0 -0.3175 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /BATT_GREEN)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 15 N-000008)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 59972D89)
    (at 158.9 140.75 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference HOME_BLUE1 (at 0.025 -1.65 180) (layer F.SilkS) hide)
    (fp_text value LED (at 2.975 -0.075 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 10 N-0000010)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 8 GND)
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 599B4C78)
    (at 199.75 136.4 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference BATT_RED1 (at 3 0.95 180) (layer F.SilkS) hide)
    (fp_text value LED (at 3.05 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 16 N-000009)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 13 N-000003)
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 59972D77)
    (at 158.9 138.75 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference HOME_RED1 (at 0.225 1.35 180) (layer F.SilkS) hide)
    (fp_text value LED (at 2.925 -0.15 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 14 N-000007)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 8 GND)
    )
  )
  (module 210_mm_drillhole (layer F.Cu) (tedit 59972CA5)
    (at 169.85 138.3)
    (fp_text reference 210_mm_drillhole (at 0.25 -2.45) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0.1 2.8) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.1)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module 375_mm_drillhole (layer F.Cu) (tedit 59972CAF)
    (at 184.85 138.4)
    (fp_text reference 375_mm_drillhole (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0.2 3.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.75)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module 415_mm_drillhole (layer F.Cu) (tedit 59972EBA)
    (at 190.85 138.4)
    (fp_text reference 415_mm_drillhole (at 0.4 -4.35) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0.15 3.6) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.15)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module SM0805 (layer F.Cu) (tedit 599B4810)
    (at 204.55 140.4 180)
    (attr smd)
    (fp_text reference R5 (at 0 -0.3175 180) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /BATT_YELLOW)
    )
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397)
      (layers F.Cu F.Paste F.Mask)
      (net 12 N-000002)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 599B4753)
    (at 199.75 138.4 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference BATT_GREEN1 (at -0.2 0.8 180) (layer F.SilkS) hide)
    (fp_text value LED (at 3.05 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 15 N-000008)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 13 N-000003)
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 599B4596)
    (at 199.75 140.4 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference BATT_YELLOW1 (at 2.35 -1 180) (layer F.SilkS) hide)
    (fp_text value LED (at 3.05 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 12 N-000002)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 8 GND)
    )
  )
  (module 4mm_Tact_SW_SMD (layer F.Cu) (tedit 59A3A2E2)
    (at 158.9 134.2)
    (fp_text reference HOME (at 5 -0.05) (layer F.SilkS))
    (fp_text value SPST (at -0.35 1.45) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3 -1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /HOME)
    )
    (pad 1 smd rect (at 3 -1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /HOME)
    )
    (pad 2 smd rect (at -3 1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 8 GND)
    )
    (pad 2 smd rect (at 3 1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 8 GND)
    )
  )
  (module 4mm_Tact_SW_SMD (layer F.Cu) (tedit 59A3A2D9)
    (at 212.95 138.25)
    (fp_text reference TV (at 0 -3.55) (layer F.SilkS))
    (fp_text value SPST (at -0.2 0.45) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3 -1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /TV)
    )
    (pad 1 smd rect (at 3 -1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /TV)
    )
    (pad 2 smd rect (at -3 1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 8 GND)
    )
    (pad 2 smd rect (at 3 1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 8 GND)
    )
  )
  (module 4mm_Tact_SW_SMD (layer F.Cu) (tedit 59A3A2DC)
    (at 225.95 138.25)
    (fp_text reference POWER (at -0.15 -3.7) (layer F.SilkS))
    (fp_text value SPST (at 0.15 1.15) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3 -1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 11 N-0000016)
    )
    (pad 1 smd rect (at 3 -1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 11 N-0000016)
    )
    (pad 2 smd rect (at -3 1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000001)
    )
    (pad 2 smd rect (at 3 1.85) (size 1.25 1.25)
      (layers F.Cu F.Paste F.Mask)
      (net 9 N-000001)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 208.15 146.25)
    (fp_text reference P1 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 /HOME)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 214.15 146.25)
    (fp_text reference P2 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /HOME_RED)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 211.15 146.25)
    (fp_text reference P3 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 /HOME_BLUE)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 204.75 132.8)
    (fp_text reference P4 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 /BATT_GREEN)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 201.75 132.8)
    (fp_text reference P5 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 /BATT_RED)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 220.15 146.25)
    (fp_text reference P6 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /TV)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 229.9 146.25)
    (fp_text reference POWER1 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 N-0000016)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 226.9 146.25)
    (fp_text reference PGND1 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 N-000001)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 223.4 146.25)
    (fp_text reference GND1 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 GND)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 217.15 146.25)
    (fp_text reference P7 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 /BATT_YELLOW)
    )
  )
  (module 2mm_pad (layer F.Cu) (tedit 59A5D44C)
    (at 198.75 132.8)
    (fp_text reference GND2 (at 0 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.25)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 N-000003)
    )
  )
  (gr_text POWER (at 229.9 144.6) (layer F.SilkS))
  (gr_text "POWER\nGND" (at 226.9 143.9) (layer F.SilkS))
  (gr_text GND (at 223.4 144.55) (layer F.SilkS))
  (gr_text TV (at 220.1 144.55) (layer F.SilkS))
  (gr_text "BATT\nLED" (at 217.15 143.8) (layer F.SilkS))
  (gr_text "HOME \nLED 1\n" (at 211.2 143.8) (layer F.SilkS))
  (gr_text HOME (at 208.1 144.55) (layer F.SilkS))
  (gr_text "HOME \nLED 2\n" (at 214.15 143.8) (layer F.SilkS))
  (gr_text v2 (at 151.15 145.15) (layer F.SilkS))
  (gr_text "Wii U Button/LED board" (at 180.75 132.9) (layer F.SilkS))
  (gr_line (start 149.8 130.85) (end 149.8 146.35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.25 146.35) (end 149.8 146.35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.25 145.35) (end 200.25 146.35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 206.15 145.35) (end 200.25 145.35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 206.15 147.75) (end 206.15 145.35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.55 147.75) (end 206.15 147.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.55 130.85) (end 232.55 147.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.8 130.85) (end 232.55 130.85) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1905)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 232.55 147.75) (xy 149.8 147.75) (xy 149.8 130.85) (xy 232.55 130.85)
      )
    )
  )
)
