(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 0)
    (zones 0)
    (modules 6)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /Cathode)
  (net 2 /Anode)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Anode)
    (add_net /Cathode)
  )
  (module "My Libraries:CP_Elec_10x10.5-Modified_Silk" (layer F.Cu) (tedit 5F81DD19)
    (at 108.7374 70.4596 270)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C1 (at 6.04266 4.9657 180) (layer F.Cu))
    (fp_text value CP_Small (at 0 6.3 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 2 /Anode))
    (pad 2 smd roundrect (at 4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 /Cathode))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:CP_Elec_10x10.5-Modified_Silk" (layer F.Cu) (tedit 5F81DD19)
    (at 143.0274 70.485 270)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C4 (at 6.03758 4.99364 180) (layer F.Cu))
    (fp_text value CP_Small (at 0 6.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 2 /Anode))
    (pad 2 smd roundrect (at 4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 /Cathode))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:CP_Elec_10x10.5-Modified_Silk" (layer F.Cu) (tedit 5F81DD19)
    (at 131.5974 70.485 270)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C3 (at 6.06044 4.97586 180) (layer F.Cu))
    (fp_text value CP_Small (at 0 6.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 2 /Anode))
    (pad 2 smd roundrect (at 4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 /Cathode))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:CP_Elec_10x10.5-Modified_Silk" (layer F.Cu) (tedit 5F81DD19)
    (at 120.1674 70.485 270)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 6.01726 4.91236 180) (layer F.Cu))
    (fp_text value CP_Small (at 0 6.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 2 /Anode))
    (pad 2 smd roundrect (at 4.2 0 270) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 /Cathode))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:Slot-Conn_1x1" (layer F.Cu) (tedit 5F81C9AB)
    (at 151.4094 70.3675)
    (fp_text reference J2 (at -0.0254 -2.0828) (layer F.SilkS) hide)
    (fp_text value Cathode (at 0 2.2352) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 4.5 3) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 1 /Cathode))
  )
  (module "My Libraries:Slot-Conn_1x1" (layer F.Cu) (tedit 5F81C9AB)
    (at 100.4316 70.3675)
    (fp_text reference J1 (at -0.0254 -2.0828) (layer F.SilkS))
    (fp_text value Anode (at 0 2.2352) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 4.5 3) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 2 /Anode))
  )
  (gr_text "baldengineer.com\nAxial Polymer BAC Adapter\nrev1\n10x10.5" (at 125.920499 70.612) (layer B.Cu))
  (gr_text + (at 100.43922 72.62876 180) (layer B.SilkS))
  (gr_text + (at 100.4443 72.4916) (layer F.SilkS))
  (gr_text - (at 151.3586 72.64908 180) (layer B.SilkS))
  (gr_text - (at 151.3713 72.517) (layer F.SilkS))
  (gr_arc (start 149.9889 64.125381) (end 150.1139 64.12538) (angle -95.54806921) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.72446 64.12484) (end 101.72446 63.99984) (angle -95.54806921) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.72446 76.8751) (end 101.72446 77.0001) (angle 95.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 149.989 76.875) (end 149.989 77) (angle -95.54806921) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 150.876 73.914) (end 150.876 73.152) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 152.5778 73.0758) (end 152.5778 73.152) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 152.5778 67.6402) (end 152.654 67.6402) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 150.876 66.802) (end 150.114 66.802) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 99.3902 67.6402) (end 99.3902 67.564) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 99.3902 73.0758) (end 99.314 73.0758) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100.838 73.914) (end 101.6 73.914) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100.838 66.802) (end 100.838 67.564) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.72446 63.99984) (end 149.976814 64.000967) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.3902 73.152) (end 100.838 73.152) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.114 73.914) (end 150.113414 76.862915) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.5778 73.152) (end 150.876 73.152) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.654 67.6402) (end 152.654 73.0758) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.876 67.564) (end 152.5778 67.564) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.1139 64.12538) (end 150.114 66.802) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.6 73.914) (end 101.600035 76.863119) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.314 67.6402) (end 99.314 73.0758) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.838 67.564) (end 99.3902 67.564) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.600046 64.136925) (end 101.6 66.802) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.72446 77.0001) (end 149.989 77) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name /Anode) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.768) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 145.796 69.85) (xy 105.156 69.85) (xy 105.156 72.898) (xy 99.568 72.898) (xy 99.568 65.786)
        (xy 145.796 65.786)
      )
    )
  )
  (zone (net 1) (net_name /Cathode) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.768) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 152.4 75.184) (xy 106.172 75.184) (xy 106.172 70.866) (xy 146.812 70.866) (xy 146.812 68.072)
        (xy 152.4 68.072)
      )
    )
  )
)
