(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 412)
    (zones 0)
    (modules 106)
    (nets 45)
  )
  (page A4)
  (title_block
    (title "PS A Current DCCT Buffers")
    (date 10-11-2021)
    (rev v01)
    (comment 4 "Author: Sujana Uppalapati")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.762 0.508)
    (user_via 0.889 0.508)
    (user_via 1.016 0.508)
    (user_via 1.27 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.381)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.175 3.175)
    (pad_drill 3.175)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 GND)
  (net 4 +15V)
  (net 5 -15V)
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C8-Pad1)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "Net-(C9-Pad1)")
  (net 12 "Net-(C14-Pad2)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(C17-Pad1)")
  (net 15 "Net-(C18-Pad2)")
  (net 16 "Net-(C18-Pad1)")
  (net 17 "Net-(C21-Pad1)")
  (net 18 "Net-(C22-Pad2)")
  (net 19 "Net-(C22-Pad1)")
  (net 20 "Net-(J1-Pad5)")
  (net 21 "Net-(J1-Pad4)")
  (net 22 "Net-(J1-Pad2)")
  (net 23 "Net-(J1-Pad1)")
  (net 24 "Net-(R5-Pad2)")
  (net 25 "Net-(R5-Pad1)")
  (net 26 "Net-(R6-Pad1)")
  (net 27 "Net-(R7-Pad2)")
  (net 28 "Net-(R11-Pad1)")
  (net 29 "Net-(R11-Pad2)")
  (net 30 "Net-(R16-Pad1)")
  (net 31 "Net-(R16-Pad2)")
  (net 32 "Net-(R17-Pad1)")
  (net 33 "Net-(R18-Pad2)")
  (net 34 "Net-(R22-Pad2)")
  (net 35 "Net-(R22-Pad1)")
  (net 36 "Net-(R23-Pad1)")
  (net 37 "Net-(R24-Pad2)")
  (net 38 /Offset1)
  (net 39 /Offset2)
  (net 40 /Ref1)
  (net 41 /Ref2)
  (net 42 "Net-(U7-Pad6)")
  (net 43 "Net-(J2-Pad1)")
  (net 44 "Net-(J2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net +15V)
    (add_net -15V)
    (add_net /Offset1)
    (add_net /Offset2)
    (add_net /Ref1)
    (add_net /Ref2)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U7-Pad6)")
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 92.898905 68.409047)
    (fp_text reference TP1 (at -0.127 -2.032) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:Bourns_3296W" (layer F.Cu) (tedit 615EFFF3)
    (at 153.67 110.49 180)
    (fp_text reference RV25 (at 5.77088 3.62712 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(R23-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 /Offset1))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(R24-Pad2)"))
  )
  (module "KiCAD Library_SU:SOIC_W-16" (layer F.Cu) (tedit 615DE5F5)
    (at 156.21 90.17)
    (fp_text reference U5 (at -1.6129 -2.3368 90) (layer F.SilkS))
    (fp_text value OP270GSZ (at 4.572 1.8796) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C18-Pad2)"))
    (pad 2 smd rect (at 1.27 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 3 smd rect (at 2.54 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.81 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 5 smd rect (at 5.08 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 6.35 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C21-Pad1)"))
    (pad 7 smd rect (at 7.62 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C22-Pad2)"))
    (pad 10 smd rect (at 7.62 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R22-Pad2)"))
    (pad 11 smd rect (at 6.35 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 5.08 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 3.81 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 14 smd rect (at 2.54 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.27 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 0 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C18-Pad2)"))
    (pad 8 smd rect (at 8.89 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 8.89 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step
      (offset (xyz 3.81 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 179.187343 99.078585 180)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C25 (at 2.793463 1.790537) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 179.183144 94.538412 180)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C26 (at 2.8829 1.76022) (layer F.SilkS))
    (fp_text value 10uF (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 139.7 43.18)
    (fp_text reference TP4 (at 0.086052 -1.943587) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 133.271027 95.359991 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R17 (at 2.703114 1.823719) (layer F.SilkS))
    (fp_text value 470K (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 152.4 91.44 90)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R19 (at 4.852309 0.042644 180) (layer F.SilkS))
    (fp_text value 16.9K (at 1.25 3.5 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C18-Pad1)"))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 150.622 80.01)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R20 (at 0.352674 -1.821167 180) (layer F.SilkS))
    (fp_text value 4.22K (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C18-Pad2)"))
    (pad 1 smd rect (at 0 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 128.191027 89.009991 90)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R16 (at 4.907632 0.091517 180) (layer F.SilkS))
    (fp_text value 30K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_DIP_Thru:DIP08_Thru (layer F.Cu) (tedit 5EBB17A1)
    (at 133.1742 57.524336)
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (fp_text reference U1 (at -1.524 -2.286 -270 unlocked) (layer F.SilkS))
    (fp_text value "INA114(8-Pin)" (at 3.81 2.54) (layer F.Fab))
    (pad 8 thru_hole circle (at 0 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "Net-(R5-Pad2)"))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 +15V))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(R7-Pad2)"))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 /Ref1))
    (pad 4 thru_hole circle (at 7.62 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 -15V))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R6-Pad1)"))
  )
  (module ap_DIP_Thru:DIP08_Thru (layer F.Cu) (tedit 5EBB17A1)
    (at 133.271027 90.279991)
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (fp_text reference U4 (at -1.68402 -2.2733 -270 unlocked) (layer F.SilkS))
    (fp_text value "INA114(8-Pin)" (at 3.81 2.54) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R17-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "Net-(C14-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 -15V))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 /Ref2))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(R18-Pad2)"))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 +15V))
    (pad 8 thru_hole circle (at 0 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "Net-(R16-Pad2)"))
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 139.621027 76.309991)
    (fp_text reference TP10 (at -0.008017 -1.958251) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0.02794 2.286) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 135.7142 44.824336 180)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C2 (at 3.347779 1.799812) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 146.05 46.228 90)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R7 (at 4.84671 0.10325 180) (layer F.SilkS))
    (fp_text value 12.4K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 170.18 99.53149 90)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C22 (at 4.792561 -0.049347) (layer F.SilkS))
    (fp_text value 0.075uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C22-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 152.407613 96.396645 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C17 (at -1.760967 -0.011911) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 148.521758 88.40411 90)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C18 (at 4.750029 0.047138 180) (layer F.SilkS))
    (fp_text value 0.012uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C18-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 180.34 62.83452 180)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C13 (at 2.8956 1.7272) (layer F.SilkS))
    (fp_text value 10uF (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 180.34 66.62928 180)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C12 (at 2.794 1.778) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 160.02 96.52 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C20 (at -1.740863 -0.055286) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 162.56 96.52 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C21 (at -1.750915 0.062172) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 135.811027 76.309991 180)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C15 (at 2.702455 1.763063) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "KiCAD Library_SU:C_Electrolytic_SMD_EMVY101ARA101MKE0S" (layer F.Cu) (tedit 61647E1C)
    (at 123.19 127)
    (fp_text reference C32 (at -6.109305 -2.947279) (layer F.SilkS))
    (fp_text value "100uF Electrolytic" (at 0.381 13.589) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.2954 4.7752) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 9.144) (size 1.2954 4.7752) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
  )
  (module "KiCAD Library_SU:SOIC_W-16" (layer F.Cu) (tedit 615DE5F5)
    (at 156.21 58.42)
    (fp_text reference U2 (at -1.778 -2.286 90) (layer F.SilkS))
    (fp_text value OP270GSZ (at 4.572 1.8796) (layer F.Fab))
    (pad 9 smd rect (at 8.89 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 8.89 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 0 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 15 smd rect (at 1.27 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.54 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 3.81 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 12 smd rect (at 5.08 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 6.35 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 7.62 -10.16) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R11-Pad2)"))
    (pad 7 smd rect (at 7.62 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (pad 6 smd rect (at 6.35 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 5 smd rect (at 5.08 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.81 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 3 smd rect (at 2.54 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.27 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at 0 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step
      (offset (xyz 3.81 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "KiCAD Library_SU:C_Electrolytic_SMD_EMVY101ARA101MKE0S" (layer F.Cu) (tedit 61647E1C)
    (at 123.19 109.22)
    (fp_text reference C31 (at -6.1 -2.93) (layer F.SilkS))
    (fp_text value "100uF Electrolytic" (at 0.381 13.589) (layer F.Fab))
    (pad 2 smd rect (at 0 9.144) (size 1.2954 4.7752) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0) (size 1.2954 4.7752) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
  )
  (module ap_SOIC:SOIC-8 (layer F.Cu) (tedit 615F0EF6)
    (at 175.377343 90.188585)
    (fp_text reference U6 (at -1.4986 -2.159 90) (layer F.SilkS))
    (fp_text value BUF634A (at 2.2225 2.2225) (layer F.Fab))
    (pad 8 smd rect (at 0 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.27 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at 2.54 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C22-Pad2)"))
    (pad 5 smd rect (at 3.81 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.81 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 3 smd rect (at 2.54 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at 1.27 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (offset (xyz 1.905 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ap_SOIC:SOIC-8 (layer F.Cu) (tedit 615F0EF6)
    (at 165.1 120.65)
    (fp_text reference U7 (at -1.50114 -2.34696 90) (layer F.SilkS))
    (fp_text value REF200AU (at 2.2225 2.2225) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R23-Pad1)"))
    (pad 2 smd rect (at 1.27 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 3 smd rect (at 2.54 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.81 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 3.81 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.54 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U7-Pad6)"))
    (pad 7 smd rect (at 1.27 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R24-Pad2)"))
    (pad 8 smd rect (at 0 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (offset (xyz 1.905 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 180.34 125.73 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C28 (at -1.79324 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Pad_Hole:125_Hole_Iso (layer F.Cu) (tedit 62ACD5EE)
    (at 76.97216 35.56)
    (fp_text reference REF** (at 0.635 3.81) (layer F.SilkS) hide)
    (fp_text value 125_Hole_Iso (at 0.635 5.715) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -0.77216 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (module ap_Pad_Hole:125_Hole_Iso (layer F.Cu) (tedit 62ACD754)
    (at 79.73568 147.828)
    (fp_text reference REF** (at 0.635 3.81) (layer F.SilkS) hide)
    (fp_text value 125_Hole_Iso (at 0.635 5.715) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -3.53568 2.032) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (module ap_Pad_Hole:125_Hole_Iso (layer F.Cu) (tedit 62ACD632)
    (at 203.2 149.86)
    (fp_text reference REF** (at 0.635 3.81) (layer F.SilkS) hide)
    (fp_text value 125_Hole_Iso (at 0.635 5.715) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (module ap_Pad_Hole:125_Hole_Iso (layer F.Cu) (tedit 62ACD640)
    (at 198.12 35.56)
    (fp_text reference REF** (at 5.08 -2.54) (layer F.SilkS) hide)
    (fp_text value 125_Hole_Iso (at 0.635 5.715) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 5.08 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (module ap_PCB_Misc:Maglab_Logo (layer F.Cu) (tedit 5F3FD4DC)
    (at 172.72 152.4)
    (attr smd)
    (fp_text reference " **" (at 1.65862 -3.71856) (layer F.SilkS) hide)
    (fp_text value Maglab_Logo (at 2.62382 1.36652) (layer F.Fab) hide)
    (fp_text user NATIONAL (at 9.144 -4.2545) (layer F.SilkS))
    (fp_text user AGLAB (at 11.176 -1.5875) (layer F.SilkS))
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 109.22 52.07 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C1 (at -1.862708 0.027092 180) (layer F.SilkS))
    (fp_text value 2000pF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 140.7942 60.96 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C3 (at 3.16738 1.83642 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 152.4 63.5 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C4 (at -1.779281 0.050172) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 148.356771 55.376393 90)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C5 (at 4.817812 -0.025286) (layer F.SilkS))
    (fp_text value 0.012uF (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 160.02 44.45 90)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C6 (at 4.794032 -0.039133 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 160.02 63.5 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C7 (at -1.741188 0.025585) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 162.56 63.5 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C8 (at -1.745088 0.102223) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 169.642817 66.564876 90)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C9 (at 4.804189 0.043803) (layer F.SilkS))
    (fp_text value 0.075uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 177.8 48.26)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C10 (at 0.229777 -1.815765 -180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 3.048 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 177.8 44.45)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C11 (at 0.149616 -1.81751 -180) (layer F.SilkS))
    (fp_text value 10uF (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 109.598825 84.15142 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C14 (at -1.884253 0.054854 180) (layer F.SilkS))
    (fp_text value 2000pF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 140.891027 93.98 270)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C16 (at 2.792541 1.743947 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 160.02 76.2 90)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C19 (at 0.224 -1.84 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 176.676203 74.92561)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C23 (at 0.228 -1.798) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 3.048 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 176.647343 78.758585)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C24 (at 0.280241 -1.770827 -180) (layer F.SilkS))
    (fp_text value 10uF (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 161.789227 113.538 90)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C27 (at 4.879091 0.052978 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "KiCAD Library_SU:C_Tant_3024" (layer F.Cu) (tedit 615EFF39)
    (at 104.648 114.3 90)
    (fp_text reference C29 (at 4.347441 -0.065923 180) (layer F.SilkS))
    (fp_text value "47uF Tantalum" (at 0.127 8.1915 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 6.604 2.286) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 0 5.842 90) (size 6.604 2.286) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module "KiCAD Library_SU:C_Tant_3024" (layer F.Cu) (tedit 615EFF39)
    (at 110.49 130.81 270)
    (fp_text reference C30 (at -4.346899 5.935255 180) (layer F.SilkS))
    (fp_text value "47uF Tantalum" (at 0.127 8.1915 90) (layer F.Fab))
    (pad 2 smd rect (at 0 5.842 270) (size 6.604 2.286) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 1 smd rect (at 0 0 270) (size 6.604 2.286) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 134.62 109.22)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C33 (at 2.783826 1.833025) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 2 smd rect (at 3.048 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Cap_SMD:C_1206 (layer F.Cu) (tedit 5F3ADD4B)
    (at 138.415664 136.149177 180)
    (descr "Capacitor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference C34 (at 2.812 1.984) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 115.3942 63.874336 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D1 (at 2.03708 -2.02692 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 -15V))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 115.3942 52.205576 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D2 (at 1.99644 -2.06248 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +15V))
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 121.7442 52.205576 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D3 (at 2.09804 -2.05232 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +15V))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 121.7442 63.874336 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D4 (at 2.13868 -2.01676 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 -15V))
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 115.948825 95.58142 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D5 (at 1.8034 -2.15392 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 -15V))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(C14-Pad2)"))
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 115.948825 84.15142 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D6 (at 2.2098 -2.3368 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +15V))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(C14-Pad2)"))
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 122.298825 84.15142 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D7 (at 2.07264 -1.99898 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +15V))
  )
  (module "KiCAD Library_SU:D_300" (layer F.Cu) (tedit 615EFF71)
    (at 122.298825 95.58142 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags 300)
    (fp_text reference D8 (at 2.05486 -2.02438 90) (layer F.SilkS))
    (fp_text value FDH333 (at 3.81 2.286 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 -15V))
  )
  (module "KiCAD Library_SU:MCV_5Pin_1803455" (layer F.Cu) (tedit 615EFF57)
    (at 76.2 54.61 270)
    (fp_text reference J1 (at -3.556 3.556 270 unlocked) (layer F.SilkS))
    (fp_text value MCV_5Pin_1803455 (at 7.62 -5.08 90) (layer F.Fab))
    (pad 5 thru_hole roundrect (at 15.24 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(J1-Pad5)"))
    (pad 4 thru_hole roundrect (at 11.43 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(J1-Pad4)"))
    (pad 3 thru_hole roundrect (at 7.62 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 thru_hole roundrect (at 3.81 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(J1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_6-Pin_1803468.stp
      (offset (xyz -2.590799999999999 -3.4798 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Connector_Phoenix:MCV_3Pin_1803439 (layer F.Cu) (tedit 5F3AFEB9)
    (at 198.12 55.88 90)
    (fp_text reference J4 (at -3.81 3.81 90) (layer F.SilkS))
    (fp_text value MCV_3Pin_1803439 (at 3.81 6.35 90) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 7.62 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 thru_hole roundrect (at 3.81 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_3Pin_1803439.stp
      (offset (xyz 7.62 3.048 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module ap_Connector_Phoenix:MCV_3Pin_1803439 (layer F.Cu) (tedit 5F3AFEB9)
    (at 198.12 88.9 90)
    (fp_text reference J3 (at -4.064 4.064 90) (layer F.SilkS))
    (fp_text value MCV_3Pin_1803439 (at 3.81 6.35 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C22-Pad2)"))
    (pad 2 thru_hole roundrect (at 3.81 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 3 thru_hole roundrect (at 7.62 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_3Pin_1803439.stp
      (offset (xyz 7.62 3.048 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module ap_Connector_Phoenix:MCV_3Pin_1803439 (layer F.Cu) (tedit 5F3AFEB9)
    (at 76.2 123.19 270)
    (fp_text reference J2 (at -3.616 3.676 270 unlocked) (layer F.SilkS))
    (fp_text value MCV_3Pin_1803439 (at 3.81 6.35 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(J2-Pad1)"))
    (pad 2 thru_hole roundrect (at 3.81 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 3 thru_hole roundrect (at 7.62 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_3Pin_1803439.stp
      (offset (xyz 7.62 3.048 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module "KiCAD Library_SU:220uH_HDS124-221MTR" (layer F.Cu) (tedit 6164819F)
    (at 87.63 114.3 90)
    (fp_text reference L1 (at 7.856591 -1.172581) (layer F.SilkS))
    (fp_text value 220uH (at 0.254 13.97 90) (layer F.Fab))
    (pad 2 smd rect (at 0 10.16 90) (size 5.5118 3.0226) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 1 smd rect (at 0 0 90) (size 5.5118 3.0226) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J2-Pad1)"))
  )
  (module "KiCAD Library_SU:220uH_HDS124-221MTR" (layer F.Cu) (tedit 6164819F)
    (at 87.63 130.81 90)
    (fp_text reference L2 (at 7.929075 -1.008476) (layer F.SilkS))
    (fp_text value 220uH (at 0.254 13.97 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 5.5118 3.0226) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 0 10.16 90) (size 5.5118 3.0226) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 91.948 48.26 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R1 (at 3.302 1.778) (layer F.SilkS))
    (fp_text value 1k (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad1)"))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 92.71 58.42 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R2 (at 3.2766 1.8288) (layer F.SilkS))
    (fp_text value 1K (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 104.14 48.26 270)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R3 (at -1.907772 0.02326 180) (layer F.SilkS))
    (fp_text value 10K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 104.132526 58.154278 90)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R4 (at -1.732186 0.032511 180) (layer F.SilkS))
    (fp_text value 10K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 128.0942 56.254336 90)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R5 (at 4.843418 0.009185 180) (layer F.SilkS))
    (fp_text value 30K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 133.1742 60.96 270)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R6 (at 3.133455 1.831684 90) (layer F.SilkS))
    (fp_text value 470K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 152.4 58.42 90)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R8 (at 4.801558 0.007525 180) (layer F.SilkS))
    (fp_text value 16.9K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 150.622 48.26)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R9 (at -0.073454 -1.806488 -180) (layer F.SilkS))
    (fp_text value 4.22K (at 5.08 -2.032) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at 0 0) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 166.37 63.5 270)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R10 (at -1.713778 0.03951 180) (layer F.SilkS))
    (fp_text value 7.87K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 166.878 45.72 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R11 (at 2.54508 1.8288) (layer F.SilkS))
    (fp_text value 49.9 (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 91.722844 80.32267 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R12 (at 2.74092 1.812062 180) (layer F.SilkS))
    (fp_text value 1k (at -1.524 1.778) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 92.100256 90.50142 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R13 (at 2.7432 1.86436) (layer F.SilkS))
    (fp_text value 1K (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 104.518825 80.34142 270)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R14 (at -1.908894 -0.021465) (layer F.SilkS))
    (fp_text value 10K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 104.71312 87.419085 270)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R15 (at -1.741169 -0.071934 180) (layer F.SilkS))
    (fp_text value 10K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 146.05 77.978 90)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R18 (at 4.848779 -0.024998 180) (layer F.SilkS))
    (fp_text value 12.4K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 3.048 0 90) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 166.37 96.52 270)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R21 (at -1.750915 -0.0579 180) (layer F.SilkS))
    (fp_text value 7.87K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 166.852262 77.47 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R22 (at 2.7886 1.7924) (layer F.SilkS))
    (fp_text value 49.9 (at 1.778 3.7465) (layer F.Fab))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R22-Pad2)"))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 165.1 125.73 270)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R23 (at -1.884621 -0.003733) (layer F.SilkS))
    (fp_text value 1K (at 1.778 3.7465 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R23-Pad1)"))
    (pad 2 smd rect (at 3.048 0 270) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ap_Resistor_SMD:R_1206 (layer F.Cu) (tedit 5F3AF27A)
    (at 169.418 111.991921 180)
    (descr "Resistor SMD 1206 Package")
    (tags 1206)
    (attr smd)
    (fp_text reference R24 (at 2.78384 1.74752) (layer F.SilkS))
    (fp_text value 1K (at 1.778 3.7465) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 3.048 0 180) (size 1.7272 1.8288) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R24-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "KiCAD Library_SU:Bourns_3296W" (layer F.Cu) (tedit 615EFFF3)
    (at 153.67 120.65 180)
    (fp_text reference RV26 (at 5.877401 3.463829) (layer F.SilkS))
    (fp_text value 10K (at 2.54 3.81) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(R24-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 /Offset2))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(R23-Pad1)"))
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 76.2 48.26)
    (fp_text reference TP2 (at 0 -1.778) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 89.659868 63.001729)
    (fp_text reference TP3 (at 0 -1.778) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 153.67 44.45 180)
    (fp_text reference TP5 (at 0.762 1.778) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 163.83 41.91)
    (fp_text reference TP6 (at 0.0254 -1.81864) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 198.12 62.23)
    (fp_text reference TP7 (at 0.077624 -1.867808) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 88.696187 74.780045)
    (fp_text reference TP8 (at 0.041276 -1.810791 -180) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 76.2 80.01)
    (fp_text reference TP9 (at 0.002942 -1.848616) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 153.67 76.2)
    (fp_text reference TP11 (at -0.127 -1.77) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 1.25 -4) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C18-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 163.83 73.66)
    (fp_text reference TP12 (at -0.222 -1.746) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R22-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 198.12 95.25)
    (fp_text reference TP13 (at -0.045755 -1.855617) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 76.2 114.3)
    (fp_text reference TP14 (at -0.127 -1.778) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 76.2 137.16)
    (fp_text reference TP15 (at -0.127 -1.778) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 134.62 115.57)
    (fp_text reference TP16 (at -0.127 -2.032) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer F.Cu) (tedit 615DE2F7)
    (at 135.360904 130.321551)
    (fp_text reference TP17 (at -0.127 -2.032) (layer F.SilkS))
    (fp_text value TestPoint_S2761-46R (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "KiCAD Library_SU:D_400" (layer F.Cu) (tedit 615EFF7D)
    (at 97.79 48.26 270)
    (descr "Diode, Thru Hole, 400mil Spacing")
    (tags 400)
    (fp_text reference TVS1 (at 7.390854 2.666544 90) (layer F.SilkS))
    (fp_text value "P6KE39CA (33V)" (at 5.08 3.048 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module "KiCAD Library_SU:D_400" (layer F.Cu) (tedit 615EFF7D)
    (at 98.168825 80.34142 270)
    (descr "Diode, Thru Hole, 400mil Spacing")
    (tags 400)
    (fp_text reference TVS2 (at 7.308729 2.651153 90) (layer F.SilkS))
    (fp_text value "P6KE39CA (33V)" (at 5.08 3.048 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(C14-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
  )
  (module ap_SOIC:SOIC-8 (layer F.Cu) (tedit 615F0EF6)
    (at 176.53 58.42)
    (fp_text reference U3 (at -1.778 -2.286 90) (layer F.SilkS))
    (fp_text value BUF634A (at 2.2225 2.2225) (layer F.Fab))
    (pad 8 smd rect (at 0 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.27 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 6 smd rect (at 2.54 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (pad 5 smd rect (at 3.81 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.81 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 3 smd rect (at 2.54 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 1.27 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (offset (xyz 1.905 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ap_SOIC:SOIC-8 (layer F.Cu) (tedit 615F0EF6)
    (at 176.53 120.65)
    (fp_text reference U8 (at -1.618 -2.276 90) (layer F.SilkS))
    (fp_text value ADA4077-2 (at 2.2225 2.2225) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 40 /Ref1))
    (pad 2 smd rect (at 1.27 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 40 /Ref1))
    (pad 3 smd rect (at 2.54 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 38 /Offset1))
    (pad 4 smd rect (at 3.81 0) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 5 -15V))
    (pad 5 smd rect (at 3.81 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 39 /Offset2))
    (pad 6 smd rect (at 2.54 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 41 /Ref2))
    (pad 7 smd rect (at 1.27 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 41 /Ref2))
    (pad 8 smd rect (at 0 -5.715) (size 0.762 1.5748) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (offset (xyz 1.905 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text -15V (at 83.139196 130.610455) (layer F.SilkS))
  (gr_text COM (at 82.695164 127.0582) (layer F.SilkS))
  (gr_text +15V (at 82.985492 123.130226) (layer F.SilkS))
  (gr_text 1 (at 71.029783 120.979168 270) (layer F.SilkS))
  (gr_text Shield (at 190.938641 81.531259) (layer F.SilkS))
  (gr_text "Buff Holec" (at 189.23 55.88) (layer F.SilkS))
  (gr_text "Buff Holec" (at 189.171893 88.892706) (layer F.SilkS))
  (gr_text COM (at 191.634632 85.225367) (layer F.SilkS))
  (gr_text COM (at 191.534249 52.098892) (layer F.SilkS))
  (gr_text 1 (at 203.402614 91.061062 90) (layer F.SilkS))
  (gr_text 1 (at 203.494601 58.03516 -270) (layer F.SilkS))
  (gr_text "Holec -" (at 84.255882 69.983703) (layer F.SilkS))
  (gr_text "Holec +" (at 84.270277 66.197652) (layer F.SilkS))
  (gr_text COM (at 82.657967 62.354019) (layer F.SilkS))
  (gr_text "Holec -" (at 84.299068 58.337639) (layer F.SilkS))
  (gr_text "Holec +" (at 84.255882 54.666753) (layer F.SilkS))
  (gr_text 1 (at 70.757531 52.494385 -90) (layer F.SilkS))
  (gr_text Shield (at 190.865026 48.418169) (layer F.SilkS))
  (gr_line (start 66.04 27.94) (end 213.36 27.94) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.04 158.75) (end 213.36 158.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.04 27.94) (end 66.04 158.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.36 158.75) (end 213.36 27.94) (layer Edge.Cuts) (width 0.05))
  (gr_text "PS - Current DCCT buffers (v01)\nS Uppalapati 2022 " (at 155.448 150.368) (layer F.SilkS))
  (gr_text +/-10V (at 75.514822 73.425071) (layer F.SilkS))
  (gr_text +/-10V (at 198.771291 44.51599) (layer F.SilkS))
  (gr_text +/-10V (at 198.728221 77.605202) (layer F.SilkS))
  (gr_text "Buffered Holec Current \n(Even Cells)" (at 206.464991 52.125768 90) (layer F.SilkS))
  (gr_text "Buffered Holec Current \n(Odd Cells)" (at 206.568313 85.115246 90) (layer F.SilkS))
  (gr_text "DC Power Input" (at 69.850623 127.484881 -90) (layer F.SilkS))
  (gr_text "Holec Current" (at 69.903119 61.974154 -90) (layer F.SilkS))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.9 161.29) (xy 64.77 161.29) (xy 64.77 25.4) (xy 215.9 25.4)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 215.9 161.29) (xy 64.77 161.29) (xy 64.77 25.4) (xy 215.9 25.4)
      )
    )
  )
)
