(kicad_pcb (version 20171130) (host pcbnew "(5.1.0-0)")
  (general
    (thickness 1.6)
    (drawings 56)
    (tracks 710)
    (zones 0)
    (modules 28)
    (nets 65)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.762 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.65 1.65)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_7fffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 VDDA)
  (net 5 VDD)
  (net 6 OSC_IN)
  (net 7 OSC_OUT)
  (net 8 VIN)
  (net 9 "Net-(IC1-Pad4)")
  (net 10 PB10)
  (net 11 PB11)
  (net 12 PB0)
  (net 13 PB1)
  (net 14 PA0)
  (net 15 PA1)
  (net 16 PA2)
  (net 17 PA3)
  (net 18 PA4)
  (net 19 PA5)
  (net 20 PA6)
  (net 21 PA7)
  (net 22 PC5)
  (net 23 PC4)
  (net 24 PC3)
  (net 25 PC2)
  (net 26 PC1)
  (net 27 PC0)
  (net 28 PC15)
  (net 29 PC14)
  (net 30 PC13)
  (net 31 OTG_HS_DM)
  (net 32 OTG_HS_DP)
  (net 33 OTG_FS_DP)
  (net 34 "Net-(J3-Pad4)")
  (net 35 OTG_FS_DM)
  (net 36 PB3)
  (net 37 PB4)
  (net 38 PB5)
  (net 39 PB6)
  (net 40 PD2)
  (net 41 PC12)
  (net 42 PC11)
  (net 43 PC10)
  (net 44 PA15)
  (net 45 PA8)
  (net 46 PA9)
  (net 47 PA10)
  (net 48 PC9)
  (net 49 PC8)
  (net 50 PC7)
  (net 51 PC6)
  (net 52 PB12)
  (net 53 PB13)
  (net 54 "Net-(JP3-Pad1)")
  (net 55 BOOT0)
  (net 56 RESET_BTN)
  (net 57 PB9)
  (net 58 PB8)
  (net 59 SWCLK)
  (net 60 SWDIO)
  (net 61 "Net-(U2-Pad1)")
  (net 62 PB2)
  (net 63 "B7(BOOT)")
  (net 64 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "B7(BOOT)")
    (add_net BOOT0)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net OSC_IN)
    (add_net OSC_OUT)
    (add_net OTG_FS_DM)
    (add_net OTG_FS_DP)
    (add_net OTG_HS_DM)
    (add_net OTG_HS_DP)
    (add_net PA0)
    (add_net PA1)
    (add_net PA10)
    (add_net PA15)
    (add_net PA2)
    (add_net PA3)
    (add_net PA4)
    (add_net PA5)
    (add_net PA6)
    (add_net PA7)
    (add_net PA8)
    (add_net PA9)
    (add_net PB0)
    (add_net PB1)
    (add_net PB10)
    (add_net PB11)
    (add_net PB12)
    (add_net PB13)
    (add_net PB2)
    (add_net PB3)
    (add_net PB4)
    (add_net PB5)
    (add_net PB6)
    (add_net PB8)
    (add_net PB9)
    (add_net PC0)
    (add_net PC1)
    (add_net PC10)
    (add_net PC11)
    (add_net PC12)
    (add_net PC13)
    (add_net PC14)
    (add_net PC15)
    (add_net PC2)
    (add_net PC3)
    (add_net PC4)
    (add_net PC5)
    (add_net PC6)
    (add_net PC7)
    (add_net PC8)
    (add_net PC9)
    (add_net PD2)
    (add_net RESET_BTN)
    (add_net SWCLK)
    (add_net SWDIO)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VDD)
    (add_net VDDA)
    (add_net VIN)
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 57235F06)
    (at 91.4654 66.1162 90)
    (attr smd)
    (fp_text reference R2 (at 1.8796 0.0254 180) (layer F.SilkS))
    (fp_text value 1kΩ (at 0 0 90) (layer Cmts.User) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 30 PC13))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D1-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:LED-0603 (layer F.Cu) (tedit 57235EC0)
    (at 91.44 68.9864 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0.8128 1.4986 180) (layer F.SilkS))
    (fp_text value LED (at 0 -1.2065 90) (layer Cmts.User) hide)
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Package_QFP:LQFP-64_10x10mm_P0.5mm (layer F.Cu) (tedit 5C194D4E)
    (at 121.92 63.5)
    (descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (attr smd)
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value STM32F205RGTx (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 64 smd roundrect (at -3.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (pad 63 smd roundrect (at -3.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 62 smd roundrect (at -2.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 PB9))
    (pad 61 smd roundrect (at -2.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 PB8))
    (pad 60 smd roundrect (at -1.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 BOOT0))
    (pad 59 smd roundrect (at -1.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "B7(BOOT)"))
    (pad 58 smd roundrect (at -0.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 PB6))
    (pad 57 smd roundrect (at -0.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 PB5))
    (pad 56 smd roundrect (at 0.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 PB4))
    (pad 55 smd roundrect (at 0.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 PB3))
    (pad 54 smd roundrect (at 1.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 PD2))
    (pad 53 smd roundrect (at 1.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 PC12))
    (pad 52 smd roundrect (at 2.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PC11))
    (pad 51 smd roundrect (at 2.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 PC10))
    (pad 50 smd roundrect (at 3.25 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 PA15))
    (pad 49 smd roundrect (at 3.75 -5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 SWCLK))
    (pad 48 smd roundrect (at 5.675 -3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (pad 47 smd roundrect (at 5.675 -3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)"))
    (pad 46 smd roundrect (at 5.675 -2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 SWDIO))
    (pad 45 smd roundrect (at 5.675 -2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 OTG_FS_DP))
    (pad 44 smd roundrect (at 5.675 -1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 OTG_FS_DM))
    (pad 43 smd roundrect (at 5.675 -1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 PA10))
    (pad 42 smd roundrect (at 5.675 -0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PA9))
    (pad 41 smd roundrect (at 5.675 -0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 PA8))
    (pad 40 smd roundrect (at 5.675 0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 PC9))
    (pad 39 smd roundrect (at 5.675 0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 PC8))
    (pad 38 smd roundrect (at 5.675 1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 PC7))
    (pad 37 smd roundrect (at 5.675 1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 PC6))
    (pad 36 smd roundrect (at 5.675 2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 OTG_HS_DP))
    (pad 35 smd roundrect (at 5.675 2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 OTG_HS_DM))
    (pad 34 smd roundrect (at 5.675 3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 PB13))
    (pad 33 smd roundrect (at 5.675 3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 PB12))
    (pad 32 smd roundrect (at 3.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (pad 31 smd roundrect (at 3.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (pad 30 smd roundrect (at 2.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 PB11))
    (pad 29 smd roundrect (at 2.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 PB10))
    (pad 28 smd roundrect (at 1.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 PB2))
    (pad 27 smd roundrect (at 1.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 PB1))
    (pad 26 smd roundrect (at 0.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 PB0))
    (pad 25 smd roundrect (at 0.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 PC5))
    (pad 24 smd roundrect (at -0.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 PC4))
    (pad 23 smd roundrect (at -0.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 PA7))
    (pad 22 smd roundrect (at -1.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 PA6))
    (pad 21 smd roundrect (at -1.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 PA5))
    (pad 20 smd roundrect (at -2.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 PA4))
    (pad 19 smd roundrect (at -2.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (pad 18 smd roundrect (at -3.25 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 17 smd roundrect (at -3.75 5.675) (size 0.3 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 PA3))
    (pad 16 smd roundrect (at -5.675 3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 PA2))
    (pad 15 smd roundrect (at -5.675 3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 PA1))
    (pad 14 smd roundrect (at -5.675 2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 PA0))
    (pad 13 smd roundrect (at -5.675 2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDDA))
    (pad 12 smd roundrect (at -5.675 1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at -5.675 1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 PC3))
    (pad 10 smd roundrect (at -5.675 0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 PC2))
    (pad 9 smd roundrect (at -5.675 0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 PC1))
    (pad 8 smd roundrect (at -5.675 -0.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 PC0))
    (pad 7 smd roundrect (at -5.675 -0.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 RESET_BTN))
    (pad 6 smd roundrect (at -5.675 -1.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 OSC_OUT))
    (pad 5 smd roundrect (at -5.675 -1.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 OSC_IN))
    (pad 4 smd roundrect (at -5.675 -2.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 PC15))
    (pad 3 smd roundrect (at -5.675 -2.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 PC14))
    (pad 2 smd roundrect (at -5.675 -3.25) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 PC13))
    (pad 1 smd roundrect (at -5.675 -3.75) (size 1.55 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 128.6256 58.2422 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -2.4638 0.0254 90) (layer B.SilkS))
    (fp_text value 2.2µF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 125.6538 66.167 225)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.43 225) (layer B.SilkS))
    (fp_text value 2.2µF (at 0 -1.43 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module stm32_qfp64_breakout:MOLEX_104031-0811 (layer B.Cu) (tedit 5E27CBEB)
    (at 96.266 63.5 90)
    (fp_text reference J6 (at -2.545225 7.635735 90) (layer B.SilkS))
    (fp_text value Micro_SD_Card (at 5.092335 -7.002025 90) (layer B.Fab))
    (pad 8 smd rect (at -4.545 -5.2 90) (size 0.75 1.1) (layers B.Cu B.Paste B.Mask)
      (net 48 PC9))
    (pad 7 smd rect (at -3.495 -5.2 90) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 49 PC8))
    (pad 6 smd rect (at -2.395 -5.2 90) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.295 -5.2 90) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 41 PC12))
    (pad 4 smd rect (at -0.195 -5.2 90) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 5 VDD))
    (pad 3 smd rect (at 0.905 -5.2 90) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 40 PD2))
    (pad 2 smd rect (at 2.005 -5.2 90) (size 0.875 1.1) (layers B.Cu B.Paste B.Mask)
      (net 42 PC11))
    (pad 1 smd rect (at 3.105 -5.2 90) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 43 PC10))
    (pad 9 smd rect (at 5.74 0.95 90) (size 1.2 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 5.74 4.65 90) (size 1.2 1) (layers B.Cu B.Paste B.Mask)
      (net 39 PB6))
    (pad G3 smd rect (at -3.73 5.625 90) (size 1.9 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad G4 smd rect (at 2.24 5.625 90) (size 1.9 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad G2 smd rect (at -5.755 -4.85 90) (size 1.17 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad G1 smd rect (at 5.565 -5.075 90) (size 1.55 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module flabbergast:SOT-563 (layer F.Cu) (tedit 5723A697)
    (at 143.026556 63.222368 270)
    (attr smd)
    (fp_text reference IC1 (at 0 1.370756 270) (layer F.SilkS))
    (fp_text value NCV8170 (at 0 1.27 270) (layer Cmts.User))
    (pad 6 smd rect (at 0.9 -0.5 90) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 8 VIN))
    (pad 4 smd rect (at 0.9 0.5 90) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad4)"))
    (pad 2 smd rect (at -0.9 0 90) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.9 0.5 90) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 1 smd rect (at -0.9 -0.5 90) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 8 VIN))
    (pad 5 smd rect (at 0.9 0 90) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd_trans/tsot-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 90))
    )
  )
  (module flabbergast:USB_microB_2TH_OSHPARK (layer F.Cu) (tedit 5E24B42F)
    (at 149.86 63.5 90)
    (descr "USB microB 4pads THT")
    (tags "USB microB")
    (fp_text reference J3 (at 0 -1.397 90) (layer F.SilkS))
    (fp_text value USB_mini_micro_B (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "PCB edge" (at -0.05 1.45 90) (layer F.SilkS) hide)
    (pad "" smd rect (at 0.9 0 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -0.9 0 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 6 thru_hole circle (at -3.3 0 90) (size 1.65 1.65) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 smd rect (at -1.3 -3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 8 VIN) (clearance 0.1))
    (pad 2 smd rect (at -0.65 -3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 35 OTG_FS_DM) (clearance 0.1))
    (pad 3 smd rect (at 0 -3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 33 OTG_FS_DP) (clearance 0.1))
    (pad 4 smd rect (at 0.65 -3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J3-Pad4)") (clearance 0.1))
    (pad 5 smd rect (at 1.3 -3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (clearance 0.1))
    (pad 6 thru_hole circle (at 3.3 0 90) (size 1.65 1.65) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 144.526 61.2394)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.7686 0) (layer F.SilkS))
    (fp_text value 2.2µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.5192 57.4548 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 1.3462 -1.397 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:TACTILE-SWITCH-SMT-4x3 (layer F.Cu) (tedit 5723C817)
    (at 105.041089 61.545879 180)
    (attr smd)
    (fp_text reference S1 (at 0.012089 -0.023721) (layer F.SilkS))
    (fp_text value RESET (at -0.013311 2.363879) (layer F.SilkS))
    (pad 3 smd rect (at 1.9 0.8509 180) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.9 -0.8509 180) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 56 RESET_BTN))
    (pad 4 smd rect (at -1.9 0.85 180) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.9 -0.8509 180) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 56 RESET_BTN))
  )
  (module flabbergast:CRYSTAL-ABM3 (layer B.Cu) (tedit 5724557B)
    (at 110.509728 64.023731 270)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 0 180) (layer B.SilkS))
    (fp_text value "8MHz Xtal" (at 0 -3 270) (layer Dwgs.User))
    (pad 1 smd rect (at -2.05 0 270) (size 1.9 2.4) (layers B.Cu B.Paste B.Mask)
      (net 6 OSC_IN))
    (pad 2 smd rect (at 2.05 0 270) (size 1.9 2.4) (layers B.Cu B.Paste B.Mask)
      (net 7 OSC_OUT))
  )
  (module stm32_qfp64_breakout:M24_LOCK_NOSILK (layer F.Cu) (tedit 5E2625BF)
    (at 91.44 72.39)
    (attr virtual)
    (fp_text reference J1 (at 1.778 -2.032) (layer Cmts.User) hide)
    (fp_text value Conn_01x24 (at 1.778 2.032) (layer Cmts.User) hide)
    (pad 15 thru_hole circle (at 35.56 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 PA7))
    (pad 16 thru_hole circle (at 38.1 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 PC4))
    (pad 17 thru_hole circle (at 40.64 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 PC5))
    (pad 18 thru_hole circle (at 43.18 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 PB0))
    (pad 19 thru_hole circle (at 45.72 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 PB1))
    (pad 20 thru_hole circle (at 48.26 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 PB2))
    (pad 21 thru_hole circle (at 50.8 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 PB10))
    (pad 22 thru_hole circle (at 53.34 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 PB11))
    (pad 23 thru_hole circle (at 55.88 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 24 thru_hole circle (at 58.42 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 VDD))
    (pad 14 thru_hole circle (at 33.02 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 PA6))
    (pad 13 thru_hole circle (at 30.48 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 PA5))
    (pad 12 thru_hole circle (at 27.94 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 PA4))
    (pad 11 thru_hole circle (at 25.4 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 PA3))
    (pad 10 thru_hole circle (at 22.86 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 PA2))
    (pad 9 thru_hole circle (at 20.32 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 PA1))
    (pad 8 thru_hole circle (at 17.78 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 PA0))
    (pad 7 thru_hole circle (at 15.24 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 PC3))
    (pad 6 thru_hole circle (at 12.7 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 PC2))
    (pad 5 thru_hole circle (at 10.16 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 PC1))
    (pad 4 thru_hole circle (at 7.62 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 PC0))
    (pad 3 thru_hole circle (at 5.08 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 PC15))
    (pad 2 thru_hole circle (at 2.54 0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 PC14))
    (pad 1 thru_hole circle (at 0 -0.127) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 PC13))
  )
  (module stm32_qfp64_breakout:M24_LOCK_NOSILK (layer F.Cu) (tedit 5E2625BF)
    (at 149.86 54.61 180)
    (attr virtual)
    (fp_text reference J4 (at 1.778 -2.032 180) (layer Cmts.User) hide)
    (fp_text value Conn_01x24 (at 1.778 2.032 180) (layer Cmts.User) hide)
    (pad 15 thru_hole circle (at 35.56 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 PC10))
    (pad 16 thru_hole circle (at 38.1 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 PC11))
    (pad 17 thru_hole circle (at 40.64 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 PC12))
    (pad 18 thru_hole circle (at 43.18 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 PD2))
    (pad 19 thru_hole circle (at 45.72 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 PB3))
    (pad 20 thru_hole circle (at 48.26 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 PB4))
    (pad 21 thru_hole circle (at 50.8 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 PB5))
    (pad 22 thru_hole circle (at 53.34 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 PB6))
    (pad 23 thru_hole circle (at 55.88 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 PB8))
    (pad 24 thru_hole circle (at 58.42 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 PB9))
    (pad 14 thru_hole circle (at 33.02 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 PA15))
    (pad 13 thru_hole circle (at 30.48 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 SWCLK))
    (pad 12 thru_hole circle (at 27.94 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 SWDIO))
    (pad 11 thru_hole circle (at 25.4 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 PA10))
    (pad 10 thru_hole circle (at 22.86 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 PA9))
    (pad 9 thru_hole circle (at 20.32 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 PA8))
    (pad 8 thru_hole circle (at 17.78 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 PC9))
    (pad 7 thru_hole circle (at 15.24 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 PC8))
    (pad 6 thru_hole circle (at 12.7 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 PC7))
    (pad 5 thru_hole circle (at 10.16 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 PC6))
    (pad 4 thru_hole circle (at 7.62 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 OTG_HS_DP))
    (pad 3 thru_hole circle (at 5.08 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 OTG_HS_DM))
    (pad 2 thru_hole circle (at 2.54 0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 PB13))
    (pad 1 thru_hole circle (at 0 -0.127 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 PB12))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 139.7 59.69 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at -1.9558 -0.0508) (layer F.SilkS))
    (fp_text value SWD (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 SWCLK))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 SWDIO))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.576883 59.688489)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0.009317 -1.370089) (layer F.SilkS))
    (fp_text value 2.2µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 119.178753 67.054047 225)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 2.409471 -0.251447 225) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.43 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.776653 69.314647 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 2.377006 0.152664 45) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 107.5436 66.243301 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.583552 0 90) (layer B.SilkS))
    (fp_text value 18pF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 OSC_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 107.5944 62.433099 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.514472 0 270) (layer B.SilkS))
    (fp_text value 18pF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 OSC_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 127.0508 58.242099 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -2.463901 0.0254 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 111.2139 64.9581 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.3979 0.0381 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 112.7379 64.9581 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.4233 0.0127 90) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:TACTILE-SWITCH-SMT-4x3 (layer F.Cu) (tedit 5723C817)
    (at 104.8766 67.0306)
    (attr smd)
    (fp_text reference S2 (at 0 -0.127) (layer F.SilkS))
    (fp_text value BOOT0 (at 0 -2.3876 -180) (layer F.SilkS))
    (pad 3 smd rect (at 1.9 0.8509) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 2 smd rect (at 1.9 -0.8509) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 55 BOOT0))
    (pad 4 smd rect (at -1.9 0.85) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 1 smd rect (at -1.9 -0.8509) (size 1.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(JP3-Pad1)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 109.1692 67.0814 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 2.9464 0.127 270) (layer F.SilkS))
    (fp_text value BT0 (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 63 "B7(BOOT)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 54 "Net-(JP3-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 100.9396 64.262 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.0254 -1.3462 270) (layer F.SilkS))
    (fp_text value 10kΩ (at 3.4545 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 BOOT0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 134.62 67.31 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 1.9812 0.0254 180) (layer F.SilkS))
    (fp_text value USB_HS (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VIN))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 OTG_HS_DM))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 OTG_HS_DP))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 111.975799 67.2465)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at 0.190601 1.3843) (layer F.SilkS))
    (fp_text value "Ferrite Bead" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VDDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ryan@\nnuclearice.com" (at 96.6724 61.6458 45) (layer F.SilkS))
  (gr_text a8 (at 129.6162 56.8452 45) (layer F.SilkS))
  (gr_text a9 (at 127.127 56.8706 45) (layer F.SilkS))
  (gr_text b12 (at 149.7076 57.2008 45) (layer F.SilkS))
  (gr_text b13 (at 147.1168 57.2262 45) (layer F.SilkS))
  (gr_text d- (at 144.907 56.6674 45) (layer F.SilkS))
  (gr_text d+ (at 142.3162 56.6166 45) (layer F.SilkS))
  (gr_text c6 (at 139.6492 56.5658) (layer F.SilkS))
  (gr_text c7 (at 137.16 56.9214 45) (layer F.SilkS))
  (gr_text c8 (at 134.5438 56.8452 45) (layer F.SilkS))
  (gr_text c9 (at 132.08 56.8706 45) (layer F.SilkS))
  (gr_text a10 (at 124.8918 56.3626) (layer F.SilkS))
  (gr_text swcd (at 120.8786 56.388) (layer F.SilkS))
  (gr_text a15 (at 116.967 56.4388) (layer F.SilkS))
  (gr_text c10 (at 113.3094 57.0992 45) (layer F.SilkS))
  (gr_text c11 (at 111.2774 57.0738 45) (layer F.SilkS))
  (gr_text c12 (at 109.0422 57.1754 45) (layer F.SilkS))
  (gr_text d2 (at 106.8324 56.896 45) (layer F.SilkS))
  (gr_text b3 (at 104.2416 56.9468 45) (layer F.SilkS))
  (gr_text b4 (at 101.8286 56.8198 45) (layer F.SilkS))
  (gr_text b5 (at 99.1108 56.7944 45) (layer F.SilkS))
  (gr_text b6 (at 96.7994 56.7182 45) (layer F.SilkS))
  (gr_text b8 (at 93.9292 56.769 45) (layer F.SilkS))
  (gr_text b9 (at 91.4146 56.8198 45) (layer F.SilkS))
  (gr_text vdd (at 149.8346 70.2818) (layer F.SilkS))
  (gr_text gnd (at 147.701 69.596 45) (layer F.SilkS))
  (gr_text b11 (at 145.1102 70.4596) (layer F.SilkS))
  (gr_text b10 (at 142.7226 69.5706 45) (layer F.SilkS))
  (gr_text b2 (at 139.8778 70.231 45) (layer F.SilkS))
  (gr_text b1 (at 137.3886 70.2056 45) (layer F.SilkS))
  (gr_text b0 (at 134.8232 70.2564 45) (layer F.SilkS))
  (gr_text c5 (at 132.2832 70.2818 45) (layer F.SilkS))
  (gr_text c4 (at 128.651 70.5104 45) (layer F.SilkS))
  (gr_text a7 (at 126.1364 70.739 45) (layer F.SilkS))
  (gr_text a6 (at 124.3838 70.6374) (layer F.SilkS))
  (gr_text a5 (at 121.8692 70.5866) (layer F.SilkS))
  (gr_text a4 (at 120.015 70.612) (layer F.SilkS))
  (gr_text a3 (at 117.1194 70.1548 45) (layer F.SilkS))
  (gr_text a2 (at 114.2238 70.1294 45) (layer F.SilkS))
  (gr_text a1 (at 111.9632 70.2056 45) (layer F.SilkS))
  (gr_text a0 (at 109.4232 70.2564 45) (layer F.SilkS))
  (gr_text c3 (at 106.9086 70.231 45) (layer F.SilkS))
  (gr_text c2 (at 104.3432 70.231 45) (layer F.SilkS))
  (gr_text c1 (at 101.727 70.1802 45) (layer F.SilkS))
  (gr_text c0 (at 99.2632 70.104 45) (layer F.SilkS))
  (gr_text c15 (at 97.0534 69.8754 45) (layer F.SilkS))
  (gr_text "c14\n" (at 94.7928 70.0024 45) (layer F.SilkS))
  (gr_text c13 (at 92.8116 70.0024 45) (layer F.SilkS))
  (gr_arc (start 91.186 54.356) (end 91.186 53.34) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 91.186 72.644) (end 90.17 72.644) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 150.114 72.644) (end 150.114 73.66) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 150.114 54.356) (end 151.13 54.356) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 151.13 54.356) (end 151.13 72.644) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 150.114 73.66) (end 91.186 73.66) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 91.186 53.34) (end 150.114 53.34) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 90.17 72.644) (end 90.17 54.356) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.662 54.5719) (xy 151.13 54.71795) (xy 151.13 72.38365) (xy 89.662 72.4154)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.3048) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.7128 54.5719) (xy 151.1554 54.70525) (xy 151.1046 72.34555) (xy 89.662 72.39)
      )
    )
  )
)
