(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 157)
    (zones 0)
    (modules 20)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.95 0.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 /NIBIT)
  (net 7 /RESET)
  (net 8 /SER_DATA_OUT_H)
  (net 9 /SER_DATA_OUT_L)
  (net 10 /XMT_RCV_CLK_H)
  (net 11 /XMT_RCV_CLK_L)
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(R2-Pad1)")
  (net 14 "Net-(R4-Pad1)")
  (net 15 "Net-(R5-Pad1)")
  (net 16 "Net-(D4-Pad1)")
  (net 17 "Net-(D5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /NIBIT)
    (add_net /RESET)
    (add_net /SER_DATA_OUT_H)
    (add_net /SER_DATA_OUT_L)
    (add_net /XMT_RCV_CLK_H)
    (add_net /XMT_RCV_CLK_L)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 167.5 100.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value CC0603KRX7R8BB104 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 167.5 107.5)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 167.5 95)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 132.5 91)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RectangularConnector_Amphenol:95278-101A14LF (layer F.Cu) (tedit 5D54CF56)
    (at 149.86 87.05)
    (attr smd)
    (fp_text reference J2 (at -9.755 0 90) (layer F.SilkS))
    (fp_text value Amphenol_95278-101A14LF (at 0 0) (layer F.Fab))
    (fp_text user 1 (at -7.62 7.62) (layer F.SilkS))
    (fp_text user 2 (at -7.62 -7.62) (layer F.SilkS))
    (fp_text user 13 (at 7.62 7.62) (layer F.SilkS))
    (fp_text user 14 (at 7.62 -7.62) (layer F.SilkS))
    (pad 14 smd rect (at 7.62 -3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 11 /XMT_RCV_CLK_L))
    (pad 1 smd rect (at -7.62 3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 7.62 3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 10 /XMT_RCV_CLK_H))
    (pad 2 smd rect (at -7.62 -3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 12 smd rect (at 5.08 -3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.08 3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 5.08 3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -5.08 -3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.54 -3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 9 /SER_DATA_OUT_L))
    (pad 5 smd rect (at -2.54 3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 8 /SER_DATA_OUT_H))
    (pad 6 smd rect (at -2.54 -3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 7 /RESET))
    (pad 8 smd rect (at 0 -3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask)
      (net 6 /NIBIT))
    (pad 7 smd rect (at 0 3.23) (size 1.27 3.54) (layers F.Cu F.Paste F.Mask))
    (model ${KIPRJMOD}/s95278_y01_14_asm/95278_y01_14_asm.stp
      (offset (xyz -17.75 6 -10))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 162.5 107.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_US (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 162.5 95)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_US (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.5 91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value RC0603FR-07200RL (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D5599F8)
    (at 157.5 102.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 -3.4) (layer F.SilkS))
    (fp_text value LM358 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R2-Pad1)"))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R2-Pad1)"))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /XMT_RCV_CLK_L))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /XMT_RCV_CLK_H))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RectangularConnector_Samtec:CLT-107-02 locked (layer B.Cu) (tedit 5D52E69E)
    (at 150 114.9954 180)
    (fp_text reference J1 (at -8.25 0 270) (layer B.SilkS))
    (fp_text value Samtec_CLT-107-02 (at 0 0) (layer B.Fab))
    (fp_text user 1 (at 8.5 -1.5046) (layer B.SilkS))
    (fp_text user 2 (at 6.03 3.98) (layer B.SilkS))
    (fp_text user 14 (at -6 4) (layer B.SilkS))
    (fp_text user 13 (at -8.5 -1.6046) (layer B.SilkS))
    (pad 7 thru_hole circle (at 0 -1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /NIBIT))
    (pad 6 thru_hole circle (at 2 1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (pad 9 thru_hole circle (at -2 -1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /SER_DATA_OUT_H))
    (pad 5 thru_hole circle (at 2 -1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -2 1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /SER_DATA_OUT_L))
    (pad 4 thru_hole circle (at 4 1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -4 -1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 4 -1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -4 1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6 1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 13 thru_hole circle (at -6 -1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /XMT_RCV_CLK_H))
    (pad 1 thru_hole circle (at 6 -1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole circle (at -6 1.51 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /XMT_RCV_CLK_L))
    (pad "" thru_hole circle (at 5 0 180) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5 0 180) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/SAMTEC_CLT-107-01-F-D/CLT-107-01-F-D.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHoles_CapScrew:CapScrew_2-56 locked (layer F.Cu) (tedit 5D546CB3)
    (at 138.316 113.335)
    (fp_text reference MH1 (at -0.016 3.065) (layer F.SilkS))
    (fp_text value MH_CapScrew_2-56 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHoles_CapScrew:CapScrew_2-56 locked (layer F.Cu) (tedit 5D546CB3)
    (at 161.684 113.335)
    (fp_text reference MH2 (at 0.016 3.065) (layer F.SilkS))
    (fp_text value MH_CapScrew_2-56 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHoles_CapScrew:CapScrew_2-56 locked (layer F.Cu) (tedit 5D546CB3)
    (at 145.174 120.32)
    (fp_text reference MH3 (at -4.174 -0.32) (layer F.SilkS))
    (fp_text value MH_CapScrew_2-56 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHoles_CapScrew:CapScrew_2-56 locked (layer F.Cu) (tedit 5D546CB3)
    (at 154.826 120.32)
    (fp_text reference MH4 (at 4.174 -0.32) (layer F.SilkS))
    (fp_text value MH_CapScrew_2-56 (at 0 5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 132.5 104.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value CC0603KRX7R8BB104 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.5 95 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.5) (layer F.SilkS))
    (fp_text value R_US (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D4-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.5 107.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_US (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R5-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 142.5 102.5 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 0 -3.4) (layer F.SilkS))
    (fp_text value LM358 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R4-Pad1)"))
    (pad 3 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SER_DATA_OUT_H))
    (pad 4 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /SER_DATA_OUT_L))
    (pad 6 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R5-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R5-Pad1)"))
    (pad 8 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 132.5 95 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D4 (at 0 1.5) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 132.5 107.5 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "J2:1 = GND\nJ2:2 = 5V\nJ2:6 = RESET\nJ2:8 = NBIT\nJ2:9 = SER_DATA_OUT_H\nJ2:10 = SER_DATA_OUT_L\nJ2:13 = XMT_RCV_CLK_H\nJ2:14 = XMT_RCV_CLK_L" (at 165 100) (layer B.SilkS))
  (gr_text 13 (at 158.5 116.6) (layer F.SilkS))
  (gr_text 14 (at 156 111) (layer F.SilkS))
  (gr_text 2 (at 144 111) (layer F.SilkS))
  (gr_text 1 (at 141.5 116.5) (layer F.SilkS))
  (gr_text CLK_HIGH (at 167.3 109.3) (layer F.SilkS))
  (gr_text CLK_LOW (at 167.7 96.9) (layer F.SilkS))
  (gr_text "Desc: 1930 Breakout\nPart #: ZRT-2019-00001-A\nDate: 2019/08/15" (at 165 85) (layer B.SilkS))
  (gr_text POWER (at 133 88.1) (layer F.SilkS))
  (gr_text DATA_OUT_LOW (at 134.9 110.2) (layer F.SilkS))
  (gr_text DATA_OUT_HIGH (at 133.6 97.1) (layer F.SilkS))
  (gr_circle (center 150 100) (end 174 100) (layer Edge.Cuts) (width 0.3))
  (zone (net 1) (net_name +5V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150 77) (xy 158 78) (xy 162 80) (xy 166 83) (xy 170 88)
        (xy 172 92) (xy 173 98) (xy 173 100) (xy 173 103) (xy 172 108)
        (xy 170 112) (xy 166 117) (xy 162 120) (xy 158 122) (xy 150 123)
        (xy 142 122.1) (xy 138 120) (xy 134 117) (xy 130 112) (xy 128 108)
        (xy 127 103) (xy 127 98) (xy 128 92) (xy 130 88) (xy 134 83)
        (xy 138 80) (xy 142 78)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.893213 76.94491) (xy 157.893213 77.94491) (xy 161.893213 79.94491) (xy 165.893213 82.94491) (xy 169.893213 87.94491)
        (xy 171.893213 91.94491) (xy 172.893213 97.94491) (xy 172.893213 99.94491) (xy 172.893213 102.94491) (xy 171.893213 107.94491)
        (xy 169.893213 111.94491) (xy 165.893213 116.94491) (xy 161.893213 119.94491) (xy 157.893213 121.94491) (xy 149.893213 122.94491)
        (xy 141.893213 122.04491) (xy 137.893213 119.94491) (xy 133.893213 116.94491) (xy 129.893213 111.94491) (xy 127.893213 107.94491)
        (xy 126.893213 102.94491) (xy 126.893213 97.94491) (xy 127.893213 91.94491) (xy 129.893213 87.94491) (xy 133.893213 82.94491)
        (xy 137.893213 79.94491) (xy 141.893213 77.94491)
      )
    )
  )
)
