(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "Package_DIP:DIP-8_W8.89mm_SMDSocket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 106.68 88.9 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads")
    (attr smd)
    (fp_text reference "REF**" (at 0 -6.14) (layer "F.SilkS") hide)
    (fp_text value "DIP-8_W8.89mm_SMDSocket_LongPads" (at 0 6.14) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "GND" smd rect (at -4.445 3.81 180) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "RX" smd rect (at -4.445 -1.27 180) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "TS" smd rect (at -4.445 1.27 180) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "TX" smd rect (at -4.445 -3.81 180) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W8.89mm_SMDSocket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-10_W8.89mm_SMDSocket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 81.28 88.9)
    (descr "10-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads")
    (attr smd)
    (fp_text reference "REF**" (at 0 -7.41) (layer "F.SilkS") hide)
    (fp_text value "DIP-10_W8.89mm_SMDSocket_LongPads" (at 0 9.525) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "GND" smd rect (at -4.445 -5.08) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "RX" smd rect (at -4.445 2.54) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "TS" smd rect (at -4.445 0) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "TS" smd rect (at -4.445 -2.54) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "TX" smd rect (at -4.445 5.08) (size 3.1 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-10_W8.89mm_SMDSocket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 97.79 93.98) (end 95.885 95.885) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 93.345 83.82) (end 115.57 83.82) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 115.57 83.82) (end 115.57 93.98) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 91.44 81.915) (end 93.345 83.82) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 74.295 95.885) (end 74.295 81.915) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 115.57 93.98) (end 97.79 93.98) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 74.295 81.915) (end 91.44 81.915) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 95.885 95.885) (end 74.295 95.885) (layer "Edge.Cuts") (width 0.2))
  (gr_text "Black" (at 105.463795 92.413172) (layer "F.SilkS"))
  (gr_text "Brown" (at 83.185 86.36) (layer "F.SilkS"))
  (gr_text "Green\n" (at 105.394441 87.627777) (layer "F.SilkS"))
  (gr_text "Green\n" (at 83.185 88.9) (layer "F.SilkS"))
  (gr_text "Black" (at 83.185 83.82) (layer "F.SilkS"))
  (gr_text "Arsenio\nMenendez\nSerial\nAdapter\n" (at 94.615 88.9) (layer "F.SilkS"))
  (gr_text "Tab UP" (at 114.071933 88.915411 270) (layer "F.SilkS"))
  (gr_text "Yellow\n" (at 83.185 91.44) (layer "F.SilkS"))
  (gr_text "Yellow\n" (at 105.41 85.09) (layer "F.SilkS"))
  (gr_text "Red\n" (at 105.41 90.17) (layer "F.SilkS"))
  (gr_text "Orange\n" (at 83.185 93.98) (layer "F.SilkS"))
)
