(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 340)
    (zones 0)
    (modules 43)
    (nets 30)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 101.013 119.62)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +12V)
  (net 4 -12V)
  (net 5 "Net-(LOCK1-PadPOS1)")
  (net 6 "Net-(LOCK1-PadNEG1)")
  (net 7 "Net-(C8-Pad2)")
  (net 8 "Net-(R5-Pad2)")
  (net 9 "Net-(R4-Pad2)")
  (net 10 "Net-(C12-Pad2)")
  (net 11 "Net-(C12-Pad1)")
  (net 12 "Net-(IC2-Pad6)")
  (net 13 "Net-(C13-Pad1)")
  (net 14 "Net-(R7-Pad1)")
  (net 15 "Net-(LDR1-Pad2)")
  (net 16 "Net-(R6-Pad1)")
  (net 17 "Net-(C14-Pad1)")
  (net 18 "Net-(R6-Pad2)")
  (net 19 "Net-(CV-LVL1-Pad3)")
  (net 20 "Net-(FEEDBACK1-Pad1)")
  (net 21 "Net-(OUT1-PadP$1_TIP)")
  (net 22 "Net-(FORM1-PadCOM)")
  (net 23 "Net-(FILTER1-PadCOM)")
  (net 24 "Net-(C9-Pad1)")
  (net 25 "Net-(FEEDBACK1-Pad3)")
  (net 26 "Net-(R12-Pad2)")
  (net 27 "Net-(R12-Pad1)")
  (net 28 IN)
  (net 29 OUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net -12V)
    (add_net GND)
    (add_net IN)
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(CV-LVL1-Pad3)")
    (add_net "Net-(FEEDBACK1-Pad1)")
    (add_net "Net-(FEEDBACK1-Pad3)")
    (add_net "Net-(FILTER1-PadCOM)")
    (add_net "Net-(FORM1-PadCOM)")
    (add_net "Net-(IC2-Pad6)")
    (add_net "Net-(LDR1-Pad2)")
    (add_net "Net-(LOCK1-PadNEG1)")
    (add_net "Net-(LOCK1-PadPOS1)")
    (add_net "Net-(OUT1-PadP$1_TIP)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net OUT)
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 178.054 92.456 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_3314G_Vertical (layer Bottom) (tedit 5A81E1D7)
    (at 128.016 109.982 270)
    (descr "Potentiometer, vertical, Bourns 3314G, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer vertical Bourns 3314G")
    (attr smd)
    (fp_text reference RV1 (at 0 4.65 90) (layer B.SilkS))
    (fp_text value R_POT (at 0 -4.65 90) (layer B.Fab))
    (fp_text user %R (at 0 1.7 90) (layer B.Fab))
    (pad 3 smd rect (at -1.15 2.75 270) (size 1.3 1.3) (layers Bottom B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0 -2.75 270) (size 2 1.3) (layers Bottom B.Paste B.Mask)
      (net 27 "Net-(R12-Pad1)"))
    (pad 1 smd rect (at 1.15 2.75 270) (size 1.3 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314G_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 139.446 105.918 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 2.032 -2.37 90) (layer F.SilkS))
    (fp_text value 10k (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 126.492 96.012 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 4.572 0 180) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(FEEDBACK1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:PerkinElmer_VTL5C (layer Top) (tedit 5B86F5E5)
    (at 135.382 102.87 270)
    (descr "Axial Vactrol (http://www.qsl.net/wa1ion/vactrol/vactrol.pdf)")
    (tags vactrol)
    (fp_text reference LDR2 (at 4.826 5.842 90) (layer F.SilkS))
    (fp_text value VACTROL_4PIN (at 7.5 7.9 90) (layer F.Fab))
    (fp_text user %R (at 7.5 1.9 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 3.8 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "Net-(LDR1-Pad2)"))
    (pad 4 thru_hole circle (at 15 4.44 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask)
      (net 23 "Net-(FILTER1-PadCOM)"))
    (pad 3 thru_hole circle (at 15 -0.64 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/PerkinElmer_VTL5C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:PerkinElmer_VTL5C (layer Top) (tedit 5B86F5E5)
    (at 124.46 102.87 270)
    (descr "Axial Vactrol (http://www.qsl.net/wa1ion/vactrol/vactrol.pdf)")
    (tags vactrol)
    (fp_text reference LDR1 (at 4.318 5.842 90) (layer F.SilkS))
    (fp_text value VACTROL_4PIN (at 7.5 7.9 90) (layer F.Fab))
    (fp_text user %R (at 7.5 1.9 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 3.8 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "Net-(LDR1-Pad2)"))
    (pad 4 thru_hole circle (at 15 4.44 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 3 thru_hole circle (at 15 -0.64 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask)
      (net 24 "Net-(C9-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.15 1.15) (drill 0.55) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/PerkinElmer_VTL5C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer Bottom) (tedit 5A3D4994)
    (at 168.91 115.824 270)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference R7 (at -2.54 3.66 90) (layer B.SilkS))
    (fp_text value 20k (at -2.54 -3.67 90) (layer B.Fab))
    (fp_text user %R (at -3.175 -0.005 90) (layer B.Fab))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer Bottom) (tedit 5A02E8C5)
    (at 151.892 92.71 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at 4.064 -4.064) (layer B.SilkS))
    (fp_text value ATTINY85P (at 3.81 -9.95) (layer B.Fab))
    (fp_text user %R (at 3.81 -3.81) (layer B.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R5-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 OUT))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R12-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer Bottom) (tedit 5A02E8C5)
    (at 137.414 92.456 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference IC2 (at 3.556 -4.064) (layer B.SilkS))
    (fp_text value TL072P (at 3.81 -9.95) (layer B.Fab))
    (fp_text user %R (at 3.81 -3.81) (layer B.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -12V))
    (pad 7 thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(IC2-Pad6)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(FILTER1-PadCOM)"))
    (pad 6 thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(IC2-Pad6)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(FEEDBACK1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(FEEDBACK1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(FEEDBACK1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer Bottom) (tedit 5A3D4994)
    (at 152.654 105.634 180)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference R11 (at -2.54 3.66) (layer B.SilkS))
    (fp_text value 1M (at -2.54 -3.67) (layer B.Fab))
    (fp_text user %R (at -3.175 -0.005) (layer B.Fab))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(FILTER1-PadCOM)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer Bottom) (tedit 5A3D4994)
    (at 115.824 106.934 270)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference R10 (at -2.54 3.66 90) (layer B.SilkS))
    (fp_text value 1M (at -2.54 -3.67 90) (layer B.Fab))
    (fp_text user %R (at -3.175 -0.005 90) (layer B.Fab))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C9-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 107.95 108.458)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at -2.286 -0.254 90) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(IC2-Pad6)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(OUT1-PadP$1_TIP)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 165.811 104.999 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 100R (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 148.336 103.886 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 1.016 2.286) (layer F.SilkS))
    (fp_text value 22k (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 IN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 107.95 99.822)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -2.286 0.254 90) (layer F.SilkS))
    (fp_text value 10k (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(FORM1-PadCOM)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 142.494 105.918 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -0.508 2.286 90) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 OUT))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 179.324 115.159 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -2.3826 -0.0509 180) (layer F.SilkS))
    (fp_text value 22R (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(LOCK1-PadNEG1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -12V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 181.686 110.714)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 22R (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(LOCK1-PadPOS1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92 (layer Top) (tedit 5A279852)
    (at 170.875 94.85 90)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference IC1 (at 3.41 -3.997 180) (layer F.SilkS))
    (fp_text value 78Z05 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer Top) (tedit 5AE50EF0)
    (at 123.19 98.806 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C12 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 140.97 98.044 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C9 (at 0.762 2.032 90) (layer F.SilkS))
    (fp_text value CP (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer Top) (tedit 5AE50EF0)
    (at 119.888 93.726 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C8 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer Bottom) (tedit 5AE50EF0)
    (at 174.752 99.822)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 4.064 -2.286) (layer B.SilkS))
    (fp_text value CP (at 1.25 -3.75) (layer B.Fab))
    (fp_text user %R (at 1.25 0) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -12V))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer Bottom) (tedit 5AE50EF0)
    (at 177.292 105.664 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 3.81 -2.74) (layer B.SilkS))
    (fp_text value CP (at 1.25 -3.75) (layer B.Fab))
    (fp_text user %R (at 1.25 0) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 116.586 96.266 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C14 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 1.5n (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 175.514 110.236)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C13 (at 1.27 -2.286) (layer F.SilkS))
    (fp_text value 330p (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 141.046 94.742 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C11 (at 0.508 -2.1081 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -12V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 113.284 93.726 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C10 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 176.276 117.602 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 4.826 0 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 173.228 117.602 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 4.826 0.254 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 174.752 92.456 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 4.826 0.254 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 169.672 98.298)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 1.27 2.286 180) (layer F.SilkS))
    (fp_text value 330n (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module acid-casualty-v2:D-2.5 (layer Top) (tedit 0)
    (at 170.891 106.904 180)
    (descr <b>DIODE</b>)
    (fp_text reference D1 (at 2.4891 -0.5384 90) (layer F.SilkS))
    (fp_text value 1N4148 (at -1.651 2.413) (layer F.Fab))
    (pad C thru_hole circle (at -1.27 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 +12V) (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at 1.27 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module acid-casualty-v2:D-2.5 (layer Top) (tedit 0)
    (at 170.891 104.364)
    (descr <b>DIODE</b>)
    (fp_text reference D2 (at -2.4891 0.7924 90) (layer F.SilkS))
    (fp_text value 1N4148 (at -1.651 2.413) (layer F.Fab))
    (pad C thru_hole circle (at -1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at 1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 -12V) (solder_mask_margin 0.1016))
  )
  (module acid-casualty-v2:EURO_PWR_HEADER_LOCK (layer Bottom) (tedit 0)
    (at 187.401 104.999 180)
    (descr "Eurorack Modular Synth 5 x 2 power header, fat pads and offset pins for easier soldering")
    (fp_text reference LOCK1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value EURO_POWER_LOCK (at 0 0 180) (layer B.SilkS) hide)
    (fp_text user RED (at -6.909 1.621 -90) (layer B.SilkS))
    (fp_text user - (at -5.639 2.637 90) (layer B.SilkS))
    (fp_text user + (at 6.299 3.145 180) (layer B.SilkS))
    (fp_text user GND (at 2.235 2.512718 90) (layer B.SilkS))
    (fp_text user GND (at -0.305 2.637 90) (layer B.SilkS))
    (fp_text user GND (at -2.845 2.567284 90) (layer B.SilkS))
    (fp_text user POWER (at 7.569 1.875 -90) (layer B.SilkS))
    (pad POS1 thru_hole circle (at 5.08 1.397 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(LOCK1-PadPOS1)") (solder_mask_margin 0.1016))
    (pad GND5 thru_hole circle (at 2.54 1.143 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad GND3 thru_hole circle (at 0 1.397 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad GND1 thru_hole circle (at -2.54 1.143 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad NEG1 thru_hole circle (at -5.08 1.397 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(LOCK1-PadNEG1)") (solder_mask_margin 0.1016))
    (pad POS2 thru_hole circle (at 5.08 -1.143 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(LOCK1-PadPOS1)") (solder_mask_margin 0.1016))
    (pad GND6 thru_hole circle (at 2.54 -1.397 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad GND4 thru_hole circle (at 0 -1.143 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad GND2 thru_hole circle (at -2.54 -1.397 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad NEG2 thru_hole circle (at -5.08 -1.143 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(LOCK1-PadNEG1)") (solder_mask_margin 0.1016))
  )
  (module acid-casualty-v2:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 188.671 96.1086 270)
    (fp_text reference VCO_CV1 (at -3.1446 4.267) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 270) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +5V) (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(CV-LVL1-Pad3)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module acid-casualty-v2:9MM_SNAP-IN_POT (layer Top) (tedit 0)
    (at 162.001 97.3786 270)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference CV-LVL1 (at 1.9354 4.5211 90) (layer F.SilkS))
    (fp_text value B100k (at -3.81 3.81 90) (layer F.Fab))
    (pad CHASSIS1 thru_hole circle (at -4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad CHASSIS2 thru_hole circle (at 4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(CV-LVL1-Pad3)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 IN) (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module acid-casualty-v2:9MM_SNAP-IN_POT (layer Top) (tedit 0)
    (at 148.031 112.619 270)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference FEEDBACK1 (at 2.9514 4.5211 90) (layer F.SilkS))
    (fp_text value B1M (at -3.81 3.81 90) (layer F.Fab))
    (pad CHASSIS1 thru_hole circle (at -4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad CHASSIS2 thru_hole circle (at 4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(FEEDBACK1-Pad3)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(FEEDBACK1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(FEEDBACK1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module acid-casualty-v2:9MM_SNAP-IN_POT (layer Top) (tedit 0)
    (at 162.001 112.619 270)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference VCF-LVL1 (at 1.9354 4.2671 90) (layer F.SilkS))
    (fp_text value A100k (at -3.81 3.81 90) (layer F.Fab))
    (pad CHASSIS1 thru_hole circle (at -4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad CHASSIS2 thru_hole circle (at 4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(R7-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(LDR1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module acid-casualty-v2:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 188.671 113.889 270)
    (fp_text reference VCF_CV1 (at 3.967 4.013) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 270) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +12V) (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(R6-Pad1)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module acid-casualty-v2:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 108.661 114.524 90)
    (fp_text reference OUT1 (at 3.2716 -5.5371) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 90) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(OUT1-PadP$1_TIP)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module acid-casualty-v2:SUBMINI_TOGGLE (layer Top) (tedit 0)
    (at 107.391 95.4736)
    (descr "<b>Submini Toggle</b><p>\nThonk 108-0044-EVX")
    (fp_text reference FORM1 (at -4.521 1.5544 90) (layer F.SilkS))
    (fp_text value SUBMINI_SPDT (at 0 0) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.4224 1.4224) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad COM thru_hole circle (at 0 0 90) (size 1.4224 1.4224) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(FORM1-PadCOM)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.4224 1.4224) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V) (solder_mask_margin 0.1016))
  )
  (module acid-casualty-v2:SUBMINI_TOGGLE (layer Top) (tedit 0)
    (at 107.391 104.364)
    (descr "<b>Submini Toggle</b><p>\nThonk 108-0044-EVX")
    (fp_text reference FILTER1 (at -4.521 2.062 90) (layer F.SilkS))
    (fp_text value SUBMINI_SPDT (at 0 0) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.4224 1.4224) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C13-Pad1)") (solder_mask_margin 0.1016))
    (pad COM thru_hole circle (at 0 0 90) (size 1.4224 1.4224) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(FILTER1-PadCOM)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.4224 1.4224) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C14-Pad1)") (solder_mask_margin 0.1016))
  )
  (gr_text "Bad Trip 1.5" (at 128.778 114.808) (layer B.SilkS))
  (gr_line (start 103.0411 119.6036) (end 193.9611 119.6036) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 193.9611 117.6036) (end 193.9611 119.6036) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 195.9611 117.6036) (end 195.9611 92.4036) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 193.9611 92.4036) (end 195.9611 92.4036) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 193.9611 90.4036) (end 103.0411 90.4036) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.0411 92.4036) (end 103.0411 90.4036) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.0411 92.4036) (end 101.0411 117.6036) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.0411 117.6036) (end 101.0411 117.6036) (angle -90) (layer Edge.Cuts) (width 0.05))
)
