<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<board>
<plain>
<hole x="51.308484375" y="26.318040625" drill="27.999971875"/>
<hole x="25.908484375" y="47.400040625" drill="3.199971875"/>
<hole x="76.708484375" y="47.400040625" drill="3.199971875"/>
<hole x="76.708484375" y="5.236040625" drill="3.199971875"/>
<hole x="25.908484375" y="5.236040625" drill="3.199971875"/>
<wire x1="5" y1="0" x2="0" y2="5" width="0.254" layer="20" curve="-90"/>
<wire x1="0" y1="5" x2="0" y2="47.6361" width="0.254" layer="20"/>
<wire x1="0" y1="47.6361" x2="5" y2="52.6361" width="0.254" layer="20" curve="-90"/>
<wire x1="5" y1="52.6361" x2="11.0538" y2="52.6361" width="0.254" layer="20"/>
<wire x1="11.0538" y1="52.6361" x2="20.4432" y2="52.6361" width="0.254" layer="20" curve="81.671818"/>
<wire x1="20.4432" y1="52.6361" x2="82.1738" y2="52.6361" width="0.254" layer="20"/>
<wire x1="82.1738" y1="52.6361" x2="91.5632" y2="52.6361" width="0.254" layer="20" curve="81.671818"/>
<wire x1="91.5632" y1="52.6361" x2="97.617" y2="52.6361" width="0.254" layer="20"/>
<wire x1="97.617" y1="52.6361" x2="102.617" y2="47.6361" width="0.254" layer="20" curve="-90"/>
<wire x1="102.617" y1="47.6361" x2="102.617" y2="5" width="0.254" layer="20"/>
<wire x1="102.617" y1="5" x2="97.617" y2="0" width="0.254" layer="20" curve="-90"/>
<wire x1="97.617" y1="0" x2="91.5632" y2="0" width="0.254" layer="20"/>
<wire x1="91.5632" y1="0" x2="82.1738" y2="0" width="0.254" layer="20" curve="81.671818"/>
<wire x1="82.1738" y1="0" x2="20.4432" y2="0" width="0.254" layer="20"/>
<wire x1="20.4432" y1="0" x2="11.0538" y2="0" width="0.254" layer="20" curve="81.671818"/>
<wire x1="11.0538" y1="0" x2="5" y2="0" width="0.254" layer="20"/>
<wire x1="94.396" y1="30.625" x2="94.396" y2="17.625" width="0.254" layer="20"/>
<wire x1="94.396" y1="17.625" x2="97.496" y2="17.625" width="0.254" layer="20" curve="180"/>
<wire x1="97.496" y1="17.625" x2="97.496" y2="30.625" width="0.254" layer="20"/>
<wire x1="97.496" y1="30.625" x2="94.396" y2="30.625" width="0.254" layer="20" curve="180"/>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>AN</text>
<text>POWER</text>
<text>ON</text>
<text>OFF</text>
<text>CISTERN V1.1</text>
<text>CISTERN V1.1</text>
<text>antenna</text>
</plain>
<libraries>
<library name="TaylorSharpe Library">
<packages>
<package name="SWITCH_SPDT_PTH_11.6X4.0MM_LOCK">
<description>&lt;h3&gt;SPDT PTH Slide Switch - Locking Footprint&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the LOCK version of this package. This package has offset PTH pins, which help to hold the part in place while soldering.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/P040040c.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="KEYSTONE_PN108_NORIVETS">
<description>1/2AA Battery Holder Through-mount</description>
</package>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
<package name="0603_GENERIC">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805_GENERIC">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="SAMTEC_FTS-110-03-L-DV-DR_BACK">
</package>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="SCREWTERMINAL-2.54MM-3">
<description>&lt;h3&gt;Screw Terminal  2.54mm Pitch - 3 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="transistor-neu-to92">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO18">
<description>&lt;b&gt;TO 18&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SWITCH" library="TaylorSharpe Library" package="SWITCH_SPDT_PTH_11.6X4.0MM_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="TaylorSharpe Library" package="KEYSTONE_PN108_NORIVETS" value="PN108_BATTHOLDER_NORIVETSNO_RIVETS">
<attribute name="NAME"/>
</element>
<element name="B2" library="TaylorSharpe Library" package="KEYSTONE_PN108_NORIVETS" value="PN108_BATTHOLDER_NORIVETSNO_RIVETS">
<attribute name="NAME"/>
</element>
<element name="T1" library="transistor-neu-to92" package="TO18" value="2N2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WAKE_BUTTON" library="TaylorSharpe Library" package="TACTILE_SWITCH_PTH_6.0MM" value="MOM_SWITCH_B3F-1000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="TaylorSharpe Library" package="0603_GENERIC" value="39K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="TaylorSharpe Library" package="0805_GENERIC" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ENOCEAN" library="TaylorSharpe Library" package="SAMTEC_FTS-110-03-L-DV-DR_BACK" value="CONN_DROPPED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="TaylorSharpe Library" package="AXIAL-0.3" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="TaylorSharpe Library" package="AXIAL-0.3" value="130k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="TaylorSharpe Library" package="AXIAL-0.3" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="TaylorSharpe Library" package="CHIPLED_1206" value="1.7V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SONIC" library="TaylorSharpe Library" package="SCREWTERMINAL-2.54MM-3" value="SCREW_TERM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="B1" pad="2"/>
<contactref element="B2" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="ENOCEAN" pad="5"/>
<contactref element="R2" pad="P$1"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="B1" pad="1"/>
<contactref element="B2" pad="1"/>
<contactref element="SWITCH" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="SWITCH" pad="1"/>
<contactref element="ENOCEAN" pad="6"/>
<contactref element="SONIC" pad="2"/>
</signal>
<signal name="ADIO0">
<contactref element="ENOCEAN" pad="9"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="ADIO7">
<contactref element="ENOCEAN" pad="16"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="WAKE1">
<contactref element="WAKE_BUTTON" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="ENOCEAN" pad="3"/>
</signal>
<signal name="S_GND">
<contactref element="T1" pad="3"/>
<contactref element="SONIC" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="T1" pad="2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="S_AN">
<contactref element="R2" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="SONIC" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="WAKE_BUTTON" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="ENOCEAN" pad="1"/>
<contactref element="ENOCEAN" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="ENOCEAN" pad="13"/>
<contactref element="LED2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
