(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu17.04.1)
  (general
    (links 61)
    (no_connects 0)
    (area 30.060899 47.8028 103.986401 95.123)
    (thickness 1.6)
    (drawings 21)
    (tracks 227)
    (zones 0)
    (modules 15)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3302)
    (user_trace_width 0.3302)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad7)")
  (net 6 "Net-(U1-Pad10)")
  (net 7 "Net-(U1-Pad9)")
  (net 8 "Net-(U1-Pad8)")
  (net 9 "Net-(U1-Pad7)")
  (net 10 "Net-(J3-Pad3)")
  (net 11 "Net-(J3-Pad1)")
  (net 12 "Net-(J3-Pad2)")
  (net 13 "Net-(J3-Pad4)")
  (net 14 "Net-(J3-Pad9)")
  (net 15 "Net-(J5-Pad4)")
  (net 16 "Net-(J5-Pad3)")
  (net 17 "Net-(J5-Pad5)")
  (net 18 "Net-(J5-Pad6)")
  (net 19 GND)
  (net 20 +5V)
  (net 21 "Net-(J5-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.3302)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (net_class Power ""
    (clearance 0.1778)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +5V)
    (add_net GND)
  )
  (module teensy:Teensy2.0 (layer F.Cu) (tedit 581B9E8B)
    (at 87.2236 73.914 180)
    (descr 11)
    (fp_text reference U1 (at 0 -10.16 180) (layer F.SilkS))
    (fp_text value Teensy2.0 (at 0 10.16 180) (layer F.Fab))
    (pad 15 thru_hole circle (at 13.97 0 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
    (pad 1 thru_hole rect (at -13.97 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -11.43 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J5-Pad7)"))
    (pad 3 thru_hole circle (at -8.89 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J5-Pad3)"))
    (pad 4 thru_hole circle (at -6.35 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J5-Pad4)"))
    (pad 5 thru_hole circle (at -3.81 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -1.27 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J5-Pad5)"))
    (pad 7 thru_hole circle (at 1.27 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 3.81 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 6.35 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 8.89 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at 11.43 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at 13.97 7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 13.97 5.08 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 13.97 2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 16 thru_hole circle (at 13.97 -2.54 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 13.97 -5.08 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 13.97 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at 11.43 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at 8.89 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole circle (at 6.35 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole circle (at 3.81 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 1.27 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 24 thru_hole circle (at -1.27 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole circle (at -3.81 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole circle (at -6.35 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole circle (at -8.89 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J5-Pad6)"))
    (pad 28 thru_hole circle (at -11.43 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole circle (at -13.97 -7.62 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole circle (at -3.81 5.08 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole circle (at -3.81 -5.08 180) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module w_conn_mpt:mpt_0,5%2f7-2,54 (layer F.Cu) (tedit 0)
    (at 56.896 56.896)
    (descr "7-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 10.6807 -1.8415) (layer F.SilkS))
    (fp_text value "Phoenix MPT" (at -2.5273 -6.9215) (layer F.SilkS))
    (pad 4 thru_hole oval (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad4)"))
    (pad 1 thru_hole rect (at 7.62 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad3)"))
    (pad 5 thru_hole oval (at -2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
    (pad 6 thru_hole oval (at -5.08 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 7 thru_hole oval (at -7.62 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad7)"))
    (model walter/conn_mpt/mpt_0,5-7-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f7-2,54 (layer F.Cu) (tedit 0)
    (at 56.5404 91.4654 180)
    (descr "7-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J4 (at -10.7569 -2.1082 180) (layer F.SilkS))
    (fp_text value "Phoenix MPT" (at 1.6637 42.2656 180) (layer F.SilkS))
    (pad 4 thru_hole oval (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J3-Pad4)"))
    (pad 1 thru_hole rect (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J3-Pad3)"))
    (pad 5 thru_hole oval (at -2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 19 GND))
    (pad 6 thru_hole oval (at -5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 7 thru_hole oval (at -7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J3-Pad9)"))
    (model walter/conn_mpt/mpt_0,5-7-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 60.2869 78.3463 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at -3.3782 -0.0508 180) (layer F.SilkS))
    (fp_text value UA9637 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J3-Pad4)"))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad10)"))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad9)"))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 59.2364 69.458)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at 0.2377 4.3417) (layer F.SilkS))
    (fp_text value IC-Haus_iC-NV (at 0 4.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad8)"))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad7)"))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OLED_SPI_1:OLED_SPI_1.3 (layer F.Cu) (tedit 5A498E3E)
    (at 84.836 59.436)
    (fp_text reference J5 (at 0 -3.2) (layer F.SilkS))
    (fp_text value OLED (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole oval (at -7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 2 thru_hole oval (at -5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 3 thru_hole oval (at -2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J5-Pad7)"))
    (pad "" np_thru_hole circle (at -15.75 0.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 15.75 0.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -15.75 30) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 15.75 30) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 70.1929 71.4937 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.2966 -0.0127 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 67.8815 71.394 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.4471 -0.1016 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 65.4812 71.4829 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.4725 -0.1143 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 52.8193 65.913)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.2131 0.1016) (layer F.SilkS))
    (fp_text value R120 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 53.995 80.6577)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.2966 0.0381) (layer F.SilkS))
    (fp_text value R120 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J3-Pad4)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 54.082 76.0349 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.282 0 180) (layer F.SilkS))
    (fp_text value R120 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 65.4431 66.6115 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.0414 2.7559 180) (layer F.SilkS))
    (fp_text value R120 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RJ45_Wurth:RJ45 (layer F.Cu) (tedit 5A4ACEF2)
    (at 35.7632 63.5889 270)
    (descr "RJ45, shielded")
    (fp_text reference J2 (at 6.4389 -7.9756 270) (layer F.SilkS))
    (fp_text value RJ45 (at 0 -7.874 270) (layer F.SilkS))
    (pad 3 thru_hole circle (at 1.52146 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 3.55092 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.53746 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 0.508 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -0.508 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 6 thru_hole circle (at -1.52146 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -2.53746 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.55092 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 10 thru_hole circle (at -8.12038 -3.37312 270) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad7)"))
    (pad 9 thru_hole circle (at 8.12038 -3.37312 270) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.33984 0.05588 270) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu))
    (pad "" np_thru_hole circle (at 6.33984 0.05588 270) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu))
    (model walter/conn_pc/rj45-shield.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RJ45_Wurth:RJ45 (layer F.Cu) (tedit 5A4ACEF2)
    (at 35.7632 84.7979 270)
    (descr "RJ45, shielded")
    (fp_text reference J3 (at 6.3754 -8.7503 270) (layer F.SilkS))
    (fp_text value RJ45 (at 0 -7.874 270) (layer F.SilkS))
    (pad 3 thru_hole circle (at 1.52146 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad 1 thru_hole circle (at 3.55092 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 2.53746 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (pad 4 thru_hole circle (at 0.508 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -0.508 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 GND))
    (pad 6 thru_hole circle (at -1.52146 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -2.53746 -2.48412 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.55092 -4.26466 270) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 20 +5V))
    (pad 10 thru_hole circle (at -8.12038 -3.37312 270) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 8.12038 -3.37312 270) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad9)"))
    (pad "" np_thru_hole circle (at -6.33984 0.05588 270) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu))
    (pad "" np_thru_hole circle (at 6.33984 0.05588 270) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu))
    (model walter/conn_pc/rj45-shield.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Sin/Cos (at 58.8772 64.2112 180) (layer F.SilkS))
  (gr_text Incremental (at 54.0512 83.5914) (layer F.SilkS))
  (gr_text ~A (at 48.7934 86.9442) (layer F.SilkS))
  (gr_text A (at 51.4096 86.8553) (layer F.SilkS))
  (gr_text ~B (at 54.0512 86.8553) (layer F.SilkS))
  (gr_text B (at 56.6293 86.8553) (layer F.SilkS))
  (gr_text G (at 59.0423 86.8553) (layer F.SilkS))
  (gr_text 5 (at 61.6204 86.8553) (layer F.SilkS))
  (gr_text S (at 64.2366 86.7283 180) (layer F.SilkS))
  (gr_text S (at 49.2125 61.7093) (layer F.SilkS))
  (gr_text 5 (at 51.8287 61.5823 180) (layer F.SilkS))
  (gr_text G (at 54.4068 61.5823 180) (layer F.SilkS))
  (gr_text B (at 56.8198 61.5823 180) (layer F.SilkS))
  (gr_text ~B (at 59.3979 61.5823 180) (layer F.SilkS))
  (gr_text A (at 62.0395 61.5823 180) (layer F.SilkS))
  (gr_text ~A (at 64.6557 61.4934 180) (layer F.SilkS))
  (gr_line (start 103.25 53.5) (end 33.5 53.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 103.25 95) (end 103.25 53.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 33.5 95) (end 103.25 95) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 33.5 53.5) (end 33.5 95) (angle 90) (layer Edge.Cuts) (width 0.2))
)
