(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 42)
    (zones 0)
    (modules 7)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 4)
    (user_trace_width 6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module Connector_JST:JST_VH_S3P-VH_1x03_P3.96mm_Horizontal (layer F.Cu) (tedit 5B774B79)
    (at 116.84 119.38 180)
    (descr "JST VH series connector, S3P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST VH top entry")
    (fp_text reference J1 (at 3.96 -3.2 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 3.96 14.6 180) (layer F.Fab))
    (fp_text user %R (at 3.96 11.2 180) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.09259299999999999)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.96 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 7.92 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_VH_S3P-VH_1x03_P3.96mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 102.235 118.745)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 151.765 109.22)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module Connector_JST:JST_VH_S2P-VH_1x02_P3.96mm_Horizontal (layer F.Cu) (tedit 5B774B79)
    (at 149.86 120.015 90)
    (descr "JST VH series connector, S2P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST VH top entry")
    (fp_text reference J2 (at 1.98 -3.2 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 1.98 14.6 90) (layer F.Fab))
    (fp_text user %R (at 1.98 11.2 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.09259299999999999)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.96 0 90) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_VH_S2P-VH_1x02_P3.96mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_VH_S3P-VH_1x03_P3.96mm_Horizontal (layer F.Cu) (tedit 5B774B79)
    (at 130.81 119.38 180)
    (descr "JST VH series connector, S3P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST VH top entry")
    (fp_text reference J3 (at 3.96 -3.2 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 3.96 14.6 180) (layer F.Fab))
    (fp_text user %R (at 3.96 11.2 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.92 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 3.96 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.09259299999999999)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_VH_S3P-VH_1x03_P3.96mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_VH_S3P-VH_1x03_P3.96mm_Horizontal (layer F.Cu) (tedit 5B774B79)
    (at 144.78 119.38 180)
    (descr "JST VH series connector, S3P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST VH top entry")
    (fp_text reference J5 (at 3.96 -3.2 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 3.96 14.6 180) (layer F.Fab))
    (fp_text user %R (at 3.96 11.2 180) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.09259299999999999)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.96 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 7.92 0 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_VH_S3P-VH_1x03_P3.96mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 101.6 112.395 180)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 4.385 -2.27 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 4.385 7.35 180) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text - (at 103.632 107.315 270) (layer F.SilkS))
  (gr_text - (at 116.84 106.807 180) (layer F.SilkS))
  (gr_text - (at 130.81 106.807 180) (layer F.SilkS))
  (gr_text - (at 144.78 106.807 180) (layer F.SilkS))
  (gr_text + (at 136.906 106.68) (layer F.SilkS))
  (gr_text + (at 122.936 106.68) (layer F.SilkS))
  (gr_text + (at 108.966 106.68) (layer F.SilkS))
  (gr_text + (at 103.632 112.395) (layer F.SilkS))
  (gr_text - (at 155.829 122.555 90) (layer F.SilkS))
  (gr_text + (at 155.575 113.284) (layer F.SilkS))
  (gr_line (start 156.21 104.775) (end 156.21 123.19) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.79 104.775) (end 156.21 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.79 123.19) (end 97.79 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.21 123.19) (end 97.79 123.19) (layer Edge.Cuts) (width 0.05))
  (gr_text Controller (at 102.235 114.935) (layer F.SilkS))
  (gr_text Power (at 151.765 112.395) (layer F.SilkS))
  (gr_text "Raver Lights Distributer v1.0 Copyright Bryan Hughes 2019" (at 127 108.585) (layer B.SilkS))
  (gr_text "350 LEDs/7 amps max" (at 127 110.49) (layer B.SilkS))
)
