(kicad_pcb (version 20171130) (host pcbnew "(5.1.0-rc1-16-gc0a86d734)")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 1119)
    (zones 0)
    (modules 29)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.8)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 1.2 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 BIAS)
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(R1-Pad2)")
  (net 8 +24V)
  (net 9 /DRAIN)
  (net 10 /GATE)
  (net 11 "Net-(C2-Pad2)")
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net /DRAIN)
    (add_net /GATE)
    (add_net BIAS)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 86 161)
    (fp_text reference J5 (at 0 -2.54) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 8 +24V))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 0)
    (at 86 150)
    (fp_text reference J4 (at 0 -2.54) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 110 166.95 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.25 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 +24V))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_10x10 (layer F.Cu) (tedit 58AA9194)
    (at 117 165.5)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C7 (at 0 6.46) (layer F.SilkS))
    (fp_text value 470u (at 0 -6.46) (layer F.Fab))
    (fp_text user + (at -5.78 4.97) (layer F.SilkS))
    (fp_text user + (at -5.78 4.97) (layer F.SilkS))
    (fp_text user %R (at 0 6.46) (layer F.Fab))
    (pad 1 smd rect (at -4 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +24V))
    (pad 2 smd rect (at 4 0 180) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module classe:TerminalBlock_XINYA_Pitch5.00mm (layer F.Cu) (tedit 5CB6125D)
    (at 96 161 180)
    (descr "terminal block RND 205-00232, 2 pins, pitch 5.08mm, size 10.16x8.45mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00232_DB_EN.pdf")
    (tags "THT terminal block RND 205-00232 pitch 5.08mm size 10.16x8.45mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J3 (at 2.54 -11 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 2.54 5.11 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -11 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 +24V))
    (model ${KISYS3DMOD}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00232_Pitch5.08mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Bourns_3266Y (layer F.Cu) (tedit 58826B0B)
    (at 86.22 143.75 180)
    (descr "Spindle Trimmer Potentiometer, Bourns 3266Y, https://www.bourns.com/pdfs/3266.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3266Y")
    (fp_text reference RV1 (at -2.54 -3.41 180) (layer F.SilkS))
    (fp_text value R_POT (at -2.54 3.59 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 BIAS))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3266Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 86 163.65 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +24V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 595FCA25)
    (at 86 168.35 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 132.5 167.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer F.Cu) (tedit 0)
    (at 135.00126 155 270)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference J2 (at 0.508 9.652 270) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 10.89914 -9.6012) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 270) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.10032 0.7366 270) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 5.00126 270) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at -2.49936 5.00126 270) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module classe:FERROCORE_HPI0630-R33 (layer F.Cu) (tedit 5CB5F487)
    (at 120.8 155 180)
    (descr "Choke, SMD, 7.3x7.3mm 3.5mm height")
    (tags "Choke SMD")
    (attr smd)
    (fp_text reference L3 (at 0 -4.45 180) (layer F.SilkS))
    (fp_text value 330n (at 0 4.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.2 0 180) (size 2.3 3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 3.2 0 180) (size 2.3 3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_7.3x7.3_H3.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP_LargePads (layer F.Cu) (tedit 0)
    (at 77.49874 155 90)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference J1 (at 0.508 9.652 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 10.89914 -9.6012 180) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.10032 0.7366 90) (size 3.50012 7.00024) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at -2.49936 5.00126 90) (size 1.6002 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module classe:FERROCORE_DL22-10 (layer F.Cu) (tedit 5CB5FF41)
    (at 107.5 162.67 90)
    (fp_text reference L2 (at 0 3 90) (layer F.SilkS))
    (fp_text value 10u (at 0 -3 90) (layer F.Fab))
    (pad 1 smd rect (at -2.67 0 180) (size 3.05 1.02) (layers F.Cu F.Paste F.Mask)
      (net 8 +24V))
    (pad 2 smd rect (at 2.67 0) (size 3.05 1.02) (layers F.Cu F.Paste F.Mask)
      (net 9 /DRAIN))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 90.65 156 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -0.35 -2 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module classe:FERROCORE_HPI0630-R33 (layer F.Cu) (tedit 5CB5F487)
    (at 97 147.8 90)
    (descr "Choke, SMD, 7.3x7.3mm 3.5mm height")
    (tags "Choke SMD")
    (attr smd)
    (fp_text reference L1 (at -4.2 3 180) (layer F.SilkS))
    (fp_text value 330n (at 0 4.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.2 0 90) (size 2.3 3) (layers F.Cu F.Paste F.Mask)
      (net 10 /GATE))
    (pad 2 smd rect (at 3.2 0 90) (size 2.3 3) (layers F.Cu F.Paste F.Mask)
      (net 3 BIAS))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_7.3x7.3_H3.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 127 153.45 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.45 0 180) (layer F.SilkS))
    (fp_text value C (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 101 156.35 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /GATE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module classe:SMD_TO-220-3_Horizontal (layer F.Cu) (tedit 5CB61B13)
    (at 104.96 155)
    (descr "TO-220-3, Horizontal, RM 2.54mm")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference Q1 (at 2.54 -20.58) (layer F.SilkS))
    (fp_text value IRF520 (at 2.54 1.9) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.8 6) (layers F.Cu F.Paste F.Mask)
      (net 10 /GATE))
    (pad 2 smd oval (at 2.54 0) (size 1.8 6) (layers F.Cu F.Paste F.Mask)
      (net 9 /DRAIN))
    (pad 3 smd oval (at 5.08 0) (size 1.8 6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Horizontal.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 115 155.95 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.95 0 180) (layer F.SilkS))
    (fp_text value C (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 /DRAIN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 113 155.95 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value C (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 /DRAIN))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 102.05 160 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 /DRAIN))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 85.95 155 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value 3n3 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 90.65 154 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.35 2 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 92 148.95 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 2 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 BIAS))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 80 142.5 180)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 95.65 154 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.65 2 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /GATE))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 95.65 156 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0.65 -2 180) (layer F.SilkS))
    (fp_text value 27 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /GATE))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 80 167.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 132.5 142.5 180)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2 180) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 180) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_line (start 72 138) (end 100 138) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 70 147) (end 70 140) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113 140) (end 113 149) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141 138) (end 115 138) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143 147) (end 143 140) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 141 170) (end 141 172) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 72 170) (end 70 170) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 141 140) (end 141 138) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 70 147) (end 70 170) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141 172) (end 72 172) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143 147) (end 143 170) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 115 140) (end 113 140) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113 151) (end 113 149) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 112 151) (end 112 152) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103 152) (end 112 152) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103 151) (end 102 151) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102 140) (end 102 151) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100 140) (end 100 138) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 72 140) (end 70 140) (angle 90) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.8)
    (fill yes (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 143 138) (xy 70 138) (xy 70 172) (xy 143 172)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.8)
    (fill yes (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 143 138) (xy 70 138) (xy 70 172) (xy 143 172)
      )
    )
  )
)
