(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 34)
    (no_connects 0)
    (area 67.234999 60.884999 85.165001 91.515001)
    (thickness 1.6)
    (drawings 12)
    (tracks 125)
    (zones 0)
    (modules 6)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.95)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(IC1-Pad3)")
  (net 3 "Net-(IC1-Pad4)")
  (net 4 "Net-(IC1-Pad5)")
  (net 5 "Net-(IC1-Pad6)")
  (net 6 "Net-(IC1-Pad7)")
  (net 7 "Net-(IC1-Pad8)")
  (net 8 "Net-(IC1-Pad9)")
  (net 9 "Net-(IC1-Pad10)")
  (net 10 "Net-(IC1-Pad11)")
  (net 11 "Net-(IC1-Pad12)")
  (net 12 "Net-(IC1-Pad13)")
  (net 13 "Net-(IC1-Pad15)")
  (net 14 "Net-(IC1-Pad16)")
  (net 15 "Net-(IC1-Pad17)")
  (net 16 "Net-(IC1-Pad18)")
  (net 17 "Net-(IC1-Pad19)")
  (net 18 "Net-(IC1-Pad20)")
  (net 19 "Net-(IC1-Pad22)")
  (net 20 "Net-(IC1-Pad25)")
  (net 21 "Net-(IC1-Pad27)")
  (net 22 +5V)
  (net 23 "Net-(P1-Pad19)")
  (net 24 "Net-(P1-Pad22)")
  (net 25 "Net-(IC1-Pad2)")
  (net 26 "Net-(IC1-Pad21)")
  (net 27 "Net-(IC1-Pad23)")
  (net 28 "Net-(IC1-Pad24)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad22)")
  )
  (module Housings_DIP:DIP-24_W15.24mm (layer F.Cu) (tedit 57DC65B6)
    (at 68.58 62.23)
    (descr "24-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference P1 (at 2.54 2.54) (layer B.SilkS))
    (fp_text value CONN_02X12 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(IC1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(IC1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(IC1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(IC1-Pad15)"))
    (pad 14 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(IC1-Pad16)"))
    (pad 15 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(IC1-Pad17)"))
    (pad 16 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(IC1-Pad18)"))
    (pad 17 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(IC1-Pad19)"))
    (pad 18 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(IC1-Pad20)"))
    (pad 19 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P1-Pad19)"))
    (pad 20 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(IC1-Pad22)"))
    (pad 21 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(IC1-Pad27)"))
    (pad 22 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P1-Pad22)"))
    (pad 23 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(IC1-Pad25)"))
    (pad 24 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask F.SilkS)
      (net 22 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 -0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0.6 -0.55 -0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Housings_SOIC:SOIC-28_7.5x17.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 76.2 76.2)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0 10.16) (layer F.SilkS))
    (fp_text value FM16W08-SG (at 0 10.05) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at -4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at -4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at -4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at 4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad16)"))
    (pad 17 smd rect (at 4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad17)"))
    (pad 18 smd rect (at 4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad18)"))
    (pad 19 smd rect (at 4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad21)"))
    (pad 22 smd rect (at 4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (model Housings_SOIC.3dshapes/SOIC-28_7.5x17.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module jumper:SOLDER-JUMPER_2-WAY (layer F.Cu) (tedit 0)
    (at 72.39 64.516 90)
    (fp_text reference JP1 (at 2.54 -1.016 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad24)"))
  )
  (module jumper:SOLDER-JUMPER_2-WAY (layer F.Cu) (tedit 0)
    (at 74.93 64.516 90)
    (fp_text reference JP2 (at 2.54 -1.016 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad21)"))
  )
  (module jumper:SOLDER-JUMPER_2-WAY (layer F.Cu) (tedit 0)
    (at 77.47 64.516 90)
    (fp_text reference JP3 (at 2.54 1.016 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad23)"))
  )
  (module jumper:SOLDER-JUMPER_2-WAY (layer F.Cu) (tedit 0)
    (at 80.01 64.516 90)
    (fp_text reference JP4 (at 2.54 1.016 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad2)"))
  )
  (gr_text "Adapts an FM16W08 FeRAM IC to the pinout of\nan FM1208S for replacing the save memory in\na Sonic the Hedgehog 3 cartridge for the Sega\nGenesis / Mega Drive." (at 76.2 62.865 90) (layer B.SilkS))
  (gr_text "Sonic the Hedgehog 3\nFeRAM Adapter\n2016-09-16 CGH" (at 76.2 89.154) (layer F.SilkS))
  (gr_arc (start 67.945 90.805) (end 67.945 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 84.455 90.805) (end 85.09 90.805) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 84.455 61.595) (end 84.455 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 67.945 61.595) (end 67.31 61.595) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 76.2 60.96) (end 77.47 60.96) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.47 60.96) (end 84.455 60.96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.31 90.805) (end 67.31 61.595) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.455 91.44) (end 67.945 91.44) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 61.595) (end 85.09 90.805) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.945 60.96) (end 74.93 60.96) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.04 59.69) (xy 86.36 59.69) (xy 86.36 92.71) (xy 66.04 92.71)
      )
    )
  )
)
