(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Beetje 32U4 Blok")
    (date "2018-08-10")
    (rev "0.0")
    (company "www.MakersBox.us")
    (comment 1 "648.ken@gmail.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "/10")
  (net 2 "/01")
  (net 3 "/02")
  (net 4 "/04")
  (net 5 "/05")
  (net 6 "/06")
  (net 7 "/07")
  (net 8 "/08")
  (net 9 "/09")
  (net 10 "/11")
  (net 11 "/12")
  (net 12 "/13")
  (net 13 "/14")
  (net 14 "/15")
  (net 15 "/16")
  (net 16 "/17")
  (net 17 "/18")
  (net 18 "/19")
  (net 19 "/20")
  (net 20 "/03")
  (net 21 "/D2_SDA")
  (net 22 "GND")
  (net 23 "/D3_SCL")
  (net 24 "+5V")
  (net 25 "/A")
  (net 26 "Net-(R1-Pad1)")
  (net 27 "unconnected-(U1-Pad7)")
  (net 28 "/RESET")
  (footprint "footprints:MEC8-113-CARD_2" locked (layer "F.Cu")
    (tedit 637EA67F)
    (at 0 -0.1 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X0" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer "F.Fab"))
    (fp_line (start -1 47.5) (end -1 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 50.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start -1 7.5) (mid -0.707107 6.792893) (end 0 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 5.5) (mid 2.207107 6.207107) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 17 0) (mid 17.353553 0.146447) (end 17.5 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 21 50.5) (mid 20.707107 51.207107) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 18.5 6.5) (mid 17.792893 6.207107) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 9.4 6.5) (mid 8.692893 6.207107) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 0 51.5) (mid -0.707107 51.207107) (end -1 50.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 0.5) (mid 10.946447 0.146447) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 8.5 51.5) (mid 10 50) (end 11.5 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 5.5) (mid 10.507107 6.207107) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 0.5) (mid 2.646447 0.146447) (end 3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 20 6.5) (mid 20.707107 6.792893) (end 21 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 7.9 0) (mid 8.253553 0.146447) (end 8.4 0.5) (layer "Edge.Cuts") (width 0.12))
    (pad "1" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/RESET") (pinfunction "Pin_11") (pintype "passive+no_connect"))
    (pad "12" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/A") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "+5V") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/11") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/12") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/13") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/14") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/15") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/16") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/17") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/18") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/19") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/20") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/D3_SCL") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/D2_SDA") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND") (pinfunction "Pin_26") (pintype "passive"))
  )
  (footprint "footprints:DFN-8-1EP_3x2mm" (layer "F.Cu")
    (tedit 638826C0)
    (at 45 -18.5 180)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.55 180) (layer "F.SilkS") hide)
    (fp_text value "24LC32" (at 0.075 1.725 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "" smd rect locked (at 0.325 -0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.325 -0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.325 0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at 0.325 0.375 180) (size 0.5 0.6) (layers "F.Paste"))
    (pad "1" smd rect locked (at -1.45 -0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(R1-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "2" smd rect locked (at -1.45 -0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd rect locked (at -1.45 0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" smd rect locked (at -1.45 0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect locked (at 1.45 0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/D2_SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd rect locked (at 1.45 0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/D3_SCL") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd rect locked (at 1.45 -0.25 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(U1-Pad7)") (pinfunction "WP") (pintype "input+no_connect"))
    (pad "8" smd rect locked (at 1.45 -0.75 180) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd rect locked (at 0 0 180) (size 1.3 1.5) (layers "F.Cu" "F.Mask"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 48 -18.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.905 0 270) (layer "Dwgs.User"))
    (fp_text value "10K" (at 1.75 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/A") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_CLIK-Mate_502382-0970_1x09-1MP_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 27.5 -8.1 90)
    (descr "Molex CLIK-Mate series connector, 502382-0970 (http://www.molex.com/pdm_docs/sd/5023820270_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex CLIK-Mate side entry")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0.3 -1.6 90) (layer "F.SilkS") hide)
    (fp_text value "CLIK-MATE 9P" (at -2.1 3.6 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.77 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -5 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect locked (at -3.75 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.5 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect locked (at -1.25 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect locked (at 0 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect locked (at 1.25 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect locked (at 2.5 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd roundrect locked (at 3.75 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd roundrect locked (at 5 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "MP" smd roundrect locked (at -6.85 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect locked (at 6.85 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_CLIK-Mate_502382-0970_1x09-1MP_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_CLIK-Mate_502382-0470_1x04-1MP_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 44.75 -5 90)
    (descr "Molex CLIK-Mate series connector, 502382-0470 (http://www.molex.com/pdm_docs/sd/5023820270_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex CLIK-Mate side entry")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at -0.2 -2.3 90) (layer "F.SilkS") hide)
    (fp_text value "CLIK-MATE 4P" (at 1 3.75 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.77 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.875 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect locked (at -0.625 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.625 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect locked (at 1.875 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect locked (at -3.725 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect locked (at 3.725 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_CLIK-Mate_502382-0470_1x04-1MP_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_CLIK-Mate_502386-1270_1x12-1MP_P1.25mm_Horizontal" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 10.9 -9.925 -90)
    (descr "Molex CLIK-Mate series connector, 502386-1270 (http://www.molex.com/pdm_docs/sd/5023860270_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex CLIK-Mate top entry")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J4" (at 1.25 0.25 90) (layer "F.SilkS") hide)
    (fp_text value "CLIK-MATE 12P" (at 3.425 -3.4 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.22 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at 6.875 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 5.625 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 4.375 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 3.125 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at 1.875 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at 0.625 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect (at -0.625 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd roundrect (at -1.875 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd roundrect (at -3.125 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd roundrect (at -4.375 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd roundrect (at -5.625 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/11") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd roundrect (at -6.875 -1.85 270) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/12") (pinfunction "Pin_12") (pintype "passive"))
    (pad "MP" smd roundrect (at -8.725 1.35 270) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect (at 8.725 1.35 270) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_CLIK-Mate_502386-1270_1x12-1MP_P1.25mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_CLIK-Mate_502382-1070_1x10-1MP_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 19 -8.7 90)
    (descr "Molex CLIK-Mate series connector, 502382-1070 (http://www.molex.com/pdm_docs/sd/5023820270_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex CLIK-Mate side entry")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J5" (at 0 -4.7 90) (layer "F.Fab"))
    (fp_text value "CLIK-MATE 10P" (at -2.1 3.6 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.77 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.625 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -4.375 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -3.125 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at -1.875 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at -0.625 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at 0.625 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect (at 1.875 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd roundrect (at 3.125 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd roundrect (at 4.375 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd roundrect (at 5.625 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "MP" smd roundrect (at -7.475 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect (at 7.475 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_CLIK-Mate_502382-1070_1x10-1MP_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_CLIK-Mate_502382-0770_1x07-1MP_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 36.25 -6.9 90)
    (descr "Molex CLIK-Mate series connector, 502382-0770 (http://www.molex.com/pdm_docs/sd/5023820270_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex CLIK-Mate side entry")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at 0.1 -0.75 90) (layer "F.SilkS") hide)
    (fp_text value "CLIK-MATE 7P" (at -0.9 3.65 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.77 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.75 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -2.5 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -1.25 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 0 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at 1.25 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at 2.5 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect (at 3.75 1.95 90) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "MP" smd roundrect (at -5.6 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect (at 5.6 -1.4 90) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_CLIK-Mate_502382-0770_1x07-1MP_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "CLIK-Mate 12P 5023821271\nCLIK-Mate 10P 5023821071\nCLIK-Mate  9P 5023820971\nCLIK-Mate  7P 5023820771\nCLIK-Mate  4P 5023820471\n" (at 42 -11) (layer "B.SilkS"))
  (gr_text "Rev 0.0\nJan 2024" (at 49.75 -1.25) (layer "B.SilkS"))
  (gr_text "ken.olsen@agilityrobotics.com" (at 29 -1) (layer "B.SilkS"))
  (gr_text "Rapid Prototyping Card" (at 29 -3) (layer "B.SilkS"))
  (gr_text "CLIK-Mate 1.25mm" (at 30.75 -18.75) (layer "F.SilkS"))
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 51.5 -0.1) (xy 6.5 -0.1))
    (height -3.1)
    (gr_text "45.0000 mm" (at 29 1.85) (layer "F.SilkS"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 51.475 -21.1) (xy 51.475 0.9))
    (height -2.5)
    (gr_text "22.0000 mm" (at 52.825 -10.1 90) (layer "F.SilkS"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 45 -18) (xy 51.5 -18))
    (height -4.5)
    (gr_text "6.5000 mm" (at 48.25 -23.65) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 45 -18.5) (xy 45 -21))
    (height 10)
    (gr_text "2.5000 mm" (at 53.85 -19.75 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
)
