(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 54)
    (zones 0)
    (modules 7)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (user_trace_width 2.032)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.4572)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.889 0.508)
    (user_via 1.143 0.7112)
    (user_via 1.397 0.7112)
    (uvia_size 0.762)
    (uvia_drill 0.4572)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 0.889)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VBAT)
  (net 3 +4V)
  (net 4 /SDA)
  (net 5 /~RESET)
  (net 6 /~NMI)
  (net 7 /FOUT)
  (net 8 /SCL)
  (net 9 "Net-(JP1-Pad1)")
  (net 10 "Net-(JP2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.4572)
    (uvia_dia 0.762)
    (uvia_drill 0.4572)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net +4V)
    (add_net /FOUT)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VBAT)
    (add_net /~NMI)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(H1-Pad10)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad2)")
  )
  (module newRTC:RTC-DIP-Header locked (layer F.Cu) (tedit 5E245D6E)
    (at 111.76 60.96)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), sparse pins")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference H1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "RTC DIP Header" (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /SCL))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /FOUT))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /~NMI))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /~RESET))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VBAT))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +4V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5E2471AD)
    (at 115.951 68.453 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0.061 -1.27 90) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0.823 -0.889 90) (layer F.Fab))
    (fp_text user %R (at -1.082 -0.889 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.889) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBAT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 115.824 79.756 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP1 (at 0 2.54 unlocked) (layer F.SilkS) hide)
    (fp_text value "RTC NMI" (at 1.143 0) (layer F.Fab))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 6 /~NMI))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 119.38 72.268)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP2 (at 0 2.916 -270) (layer F.SilkS) hide)
    (fp_text value "RTC RESET" (at -0.127 3.424 -270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(JP2-Pad2)"))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 /~RESET))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 114.808 62.23 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.54 -0.127 270) (layer F.SilkS) hide)
    (fp_text value 3.3K (at -0.889 1.016 90) (layer F.Fab))
    (fp_text user %R (at 1.016 1.016 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +4V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 116.332 62.23 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.667 0 90) (layer F.SilkS) hide)
    (fp_text value 3.3K (at -0.889 -1.016 90) (layer F.Fab))
    (fp_text user %R (at 1.016 -1.016 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +4V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 115.316 74.168 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.254 0.635 90) (layer F.SilkS) hide)
    (fp_text value DS3232M (at 0.762 0 180) (layer F.Fab))
    (fp_text user %R (at -0.381 0.127 180) (layer F.Fab))
    (fp_text user "DS3232M RTC" (at 0.635 -3.81 270 unlocked) (layer F.SilkS))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VBAT))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(JP2-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +4V))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /FOUT))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Fo (at 113.411 63.5 270) (layer F.SilkS))
  (gr_text "Enab NMI" (at 115.57 81.661) (layer F.SilkS))
  (gr_text "Enab RES" (at 119.38 76.454 270) (layer F.SilkS))
  (gr_text NMI (at 113.411 66.04 270) (layer F.SilkS))
  (gr_text 4V (at 117.729 60.96 270) (layer F.SilkS))
  (gr_text TomCircuit (at 117.094 67.564 90) (layer B.SilkS))
  (gr_line (start 110.49 59.69) (end 110.49 82.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 59.69) (end 110.49 59.69) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 82.55) (end 120.65 59.69) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.49 82.55) (end 120.65 82.55) (layer Edge.Cuts) (width 0.05))
  (gr_text BAT (at 117.729 63.246 270) (layer F.SilkS))
  (gr_text SDA (at 117.729 66.167 270) (layer F.SilkS))
  (gr_text SCL (at 113.411 61.087 270) (layer F.SilkS))
  (gr_text "RTC7301  REFIT" (at 114.808 72.136 90) (layer B.SilkS))
  (gr_text 1/2020 (at 117.094 77.978 90) (layer B.SilkS))
)
