<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="22.53" y1="3.135" x2="22.53" y2="19.715" width="0" layer="20"/>
<wire x1="22.53" y1="19.715" x2="20.03" y2="22.215" width="0" layer="20" curve="90"/>
<wire x1="20.03" y1="22.215" x2="3.77" y2="22.215" width="0" layer="20"/>
<wire x1="3.77" y1="22.215" x2="1.27" y2="19.715" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="19.715" x2="1.27" y2="3.135" width="0" layer="20"/>
<wire x1="1.27" y1="3.135" x2="3.77" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="3.77" y1="0.635" x2="20.03" y2="0.635" width="0" layer="20"/>
<wire x1="20.03" y1="0.635" x2="22.53" y2="3.135" width="0" layer="20" curve="90"/>
<text>Bus Pirate v3</text>
<text>AVR ISP</text>
<text>&lt;Red&gt;</text>
<text>5V</text>
<text>3.3V</text>
<text>Avrrrinator Rev. A</text>
<text>Bus Pirate v3 ISP
adapter 
2014-2-18</text>
<text>PWR</text>
<text>open.konspyre.org/avra</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="PINSHRD_PTH_2X05B">
<description>2X5 Pin header with flipped shrouded case</description>
</package>
</packages>
</library>
<library name="bp_to_avr">
<description>Generated from &lt;b&gt;bp_to_avr.brd&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="ADAFRUIT_OSHWLOGO_TOP_0.2_NO_MASK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="J1" library="dp_devices" package="PINSHRD_PTH_2X05B" value="CON_HEADER_2X05-PTH+SHROUDED_B"/>
<element name="JP1" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="bp_to_avr" package="ADAFRUIT_OSHWLOGO_TOP_0.2_NO_MASK" value=""/>
</elements>
<signals>
<signal name="MISO">
<contactref element="ISP1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="PWRSEL">
<contactref element="ISP1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="ISP1" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="CS">
<contactref element="J1" pad="2"/>
<contactref element="ISP1" pad="5"/>
</signal>
<signal name="CLK">
<contactref element="J1" pad="4"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="VPU">
<contactref element="J1" pad="6"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="8"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="AUX">
<contactref element="J1" pad="5"/>
</signal>
<signal name="ADC">
<contactref element="J1" pad="7"/>
</signal>
<signal name="3V3">
<contactref element="J1" pad="9"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="ISP1" pad="6"/>
<contactref element="J1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
