<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="34.29" x2="0" y2="4.33604375" width="0" layer="20"/>
<wire x1="0" y1="4.33604375" x2="4.33604375" y2="0" width="0" layer="20" curve="90"/>
<wire x1="4.33604375" y1="0" x2="72.1148" y2="0" width="0" layer="20"/>
<wire x1="72.1148" y1="0" x2="75.87" y2="3.7552" width="0" layer="20" curve="90"/>
<wire x1="75.87" y1="3.7552" x2="75.87" y2="34.350921875" width="0" layer="20"/>
<wire x1="75.87" y1="34.350921875" x2="72.130921875" y2="38.09" width="0" layer="20" curve="90"/>
<wire x1="72.130921875" y1="38.09" x2="3.8" y2="38.09" width="0" layer="20"/>
<wire x1="3.8" y1="38.09" x2="0" y2="34.29" width="0" layer="20" curve="90"/>
<wire x1="30.52" y1="4.31" x2="45.68" y2="4.31" width="0.1524" layer="20"/>
<wire x1="45.68" y1="4.31" x2="45.68" y2="1.77" width="0.1524" layer="20"/>
<wire x1="45.68" y1="1.77" x2="30.52" y2="1.77" width="0.1524" layer="20"/>
<wire x1="30.52" y1="1.77" x2="30.52" y2="4.31" width="0.1524" layer="20"/>
<text>A</text>
<text>B</text>
<text>RESET</text>
<text>MODE</text>
<text>CODE@TACC Cybersecurity</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="jennie_badge">
<packages>
<package name="USB_MICRO_AB-SMD">
</package>
<package name="CR2032-HOLDER">
</package>
<package name="TQFP32-08-HD">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="APA102-5050">
<description>&lt;h3&gt;APA102C&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Size: 5.0 x 5.0 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf"&gt;APA102C&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH_SPST_SMD_A">
<description>&lt;h3&gt;SPDT Slide Switch - SMD&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SLIDE.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="J4" library="jennie_badge" package="USB_MICRO_AB-SMD" value=""/>
<element name="V1" library="jennie_badge" package="CR2032-HOLDER" value=""/>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="S1" library="SparkFun-Switches" package="SWITCH_SPST_SMD_A" value="">
<attribute name="PROD_ID" value="SWCH-10651"/>
<attribute name="SF_SKU" value="COM-10860"/>
</element>
<element name="U1" library="jennie_badge" package="TQFP32-08-HD" value=""/>
<element name="D1" library="jennie_badge" package="APA102-5050" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="jennie_badge" package="APA102-5050" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="jennie_badge" package="APA102-5050" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VBUS">
<contactref element="J4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="S1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="9"/>
<contactref element="D1" pad="P4"/>
<contactref element="D2" pad="P4"/>
<contactref element="D3" pad="P4"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="J4" pad="5"/>
<contactref element="V1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="GND"/>
<contactref element="D1" pad="P3"/>
<contactref element="D2" pad="P3"/>
<contactref element="D3" pad="P3"/>
</signal>
<signal name="VDDCORE">
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="RESETN">
<contactref element="J2" pad="6"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="SWDCLK">
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="SWDIO">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="SDA">
<contactref element="J2" pad="3"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="SCL">
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="13"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="11"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="CLK">
<contactref element="U1" pad="14"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="SS">
<contactref element="U1" pad="12"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="UART_TX">
<contactref element="J3" pad="2"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="UART_RX">
<contactref element="J3" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="VDD">
<contactref element="S1" pad="3"/>
<contactref element="V1" pad="1"/>
<contactref element="V1" pad="3"/>
</signal>
<signal name="SDI">
<contactref element="U1" pad="1"/>
<contactref element="D1" pad="P1"/>
</signal>
<signal name="CKI">
<contactref element="U1" pad="2"/>
<contactref element="D1" pad="P2"/>
</signal>
<signal name="CAPSENSE1">
<contactref element="U1" pad="5"/>
</signal>
<signal name="CAPSENSE2">
<contactref element="U1" pad="6"/>
</signal>
<signal name="CAPSENSE3">
<contactref element="U1" pad="7"/>
</signal>
<signal name="CAPSENSE4">
<contactref element="U1" pad="8"/>
</signal>
<signal name="D_N">
<contactref element="J4" pad="2"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="D_P">
<contactref element="J4" pad="3"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="CKI2">
<contactref element="D2" pad="P2"/>
<contactref element="D1" pad="P5"/>
</signal>
<signal name="SDI2">
<contactref element="D2" pad="P1"/>
<contactref element="D1" pad="P6"/>
</signal>
<signal name="CKI3">
<contactref element="D2" pad="P5"/>
<contactref element="D3" pad="P2"/>
</signal>
<signal name="SDI3">
<contactref element="D2" pad="P6"/>
<contactref element="D3" pad="P1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
