(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 240)
    (no_connects 0)
    (area 190.424999 25.324999 240.740001 50.875001)
    (thickness 1.6)
    (drawings 129)
    (tracks 932)
    (zones 0)
    (modules 135)
    (nets 102)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.635)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.635)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.3048)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C4-Pad2)")
  (net 9 "Net-(C5-Pad1)")
  (net 10 "Net-(C5-Pad2)")
  (net 11 "Net-(C6-Pad1)")
  (net 12 "Net-(C6-Pad2)")
  (net 13 "Net-(C7-Pad1)")
  (net 14 "Net-(C7-Pad2)")
  (net 15 "Net-(C8-Pad1)")
  (net 16 "Net-(C8-Pad2)")
  (net 17 GND)
  (net 18 VCC)
  (net 19 "Net-(Q1-Pad1)")
  (net 20 HT)
  (net 21 "Net-(Q10-Pad3)")
  (net 22 "Net-(Q11-Pad3)")
  (net 23 "Net-(Q12-Pad3)")
  (net 24 "Net-(Q13-Pad3)")
  (net 25 "Net-(Q14-Pad3)")
  (net 26 "Net-(Q15-Pad3)")
  (net 27 "Net-(Q16-Pad3)")
  (net 28 "Net-(Q9-Pad1)")
  (net 29 "Net-(Q10-Pad1)")
  (net 30 "Net-(Q11-Pad1)")
  (net 31 "Net-(Q12-Pad1)")
  (net 32 "Net-(Q13-Pad1)")
  (net 33 "Net-(Q14-Pad1)")
  (net 34 "Net-(Q15-Pad1)")
  (net 35 "Net-(Q16-Pad1)")
  (net 36 "Net-(Q17-Pad1)")
  (net 37 KO0)
  (net 38 "Net-(Q18-Pad1)")
  (net 39 KO1)
  (net 40 "Net-(Q19-Pad1)")
  (net 41 KO2)
  (net 42 "Net-(Q20-Pad1)")
  (net 43 KO3)
  (net 44 "Net-(Q21-Pad1)")
  (net 45 KO4)
  (net 46 "Net-(Q22-Pad1)")
  (net 47 KO5)
  (net 48 "Net-(Q23-Pad1)")
  (net 49 KO6)
  (net 50 "Net-(Q24-Pad1)")
  (net 51 KO7)
  (net 52 "Net-(R9-Pad2)")
  (net 53 "Net-(R10-Pad2)")
  (net 54 "Net-(R11-Pad2)")
  (net 55 "Net-(R12-Pad2)")
  (net 56 "Net-(R13-Pad2)")
  (net 57 "Net-(R14-Pad2)")
  (net 58 "Net-(R15-Pad2)")
  (net 59 "Net-(R16-Pad2)")
  (net 60 AI0)
  (net 61 AO0)
  (net 62 AI1)
  (net 63 AO1)
  (net 64 AI2)
  (net 65 AO2)
  (net 66 AI3)
  (net 67 AO3)
  (net 68 AI4)
  (net 69 AO4)
  (net 70 AI5)
  (net 71 AO5)
  (net 72 AI6)
  (net 73 AO6)
  (net 74 AI7)
  (net 75 AO7)
  (net 76 KI0)
  (net 77 KI1)
  (net 78 KI2)
  (net 79 KI3)
  (net 80 KI4)
  (net 81 KI5)
  (net 82 KI6)
  (net 83 KI7)
  (net 84 "Net-(J3-Pad1)")
  (net 85 "Net-(J3-Pad2)")
  (net 86 "Net-(J3-Pad3)")
  (net 87 "Net-(J3-Pad4)")
  (net 88 "Net-(J3-Pad5)")
  (net 89 "Net-(J3-Pad6)")
  (net 90 "Net-(J3-Pad7)")
  (net 91 "Net-(J3-Pad8)")
  (net 92 "Net-(J7-Pad1)")
  (net 93 "Net-(J7-Pad3)")
  (net 94 "Net-(J7-Pad5)")
  (net 95 "Net-(J7-Pad7)")
  (net 96 "Net-(J7-Pad2)")
  (net 97 "Net-(J7-Pad4)")
  (net 98 "Net-(J7-Pad6)")
  (net 99 "Net-(J7-Pad8)")
  (net 100 AS)
  (net 101 KS)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net AI0)
    (add_net AI1)
    (add_net AI2)
    (add_net AI3)
    (add_net AI4)
    (add_net AI5)
    (add_net AI6)
    (add_net AI7)
    (add_net AO0)
    (add_net AO1)
    (add_net AO2)
    (add_net AO3)
    (add_net AO4)
    (add_net AO5)
    (add_net AO6)
    (add_net AO7)
    (add_net AS)
    (add_net GND)
    (add_net HT)
    (add_net KI0)
    (add_net KI1)
    (add_net KI2)
    (add_net KI3)
    (add_net KI4)
    (add_net KI5)
    (add_net KI6)
    (add_net KI7)
    (add_net KO0)
    (add_net KO1)
    (add_net KO2)
    (add_net KO3)
    (add_net KO4)
    (add_net KO5)
    (add_net KO6)
    (add_net KO7)
    (add_net KS)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J7-Pad5)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(J7-Pad7)")
    (add_net "Net-(J7-Pad8)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q10-Pad1)")
    (add_net "Net-(Q10-Pad3)")
    (add_net "Net-(Q11-Pad1)")
    (add_net "Net-(Q11-Pad3)")
    (add_net "Net-(Q12-Pad1)")
    (add_net "Net-(Q12-Pad3)")
    (add_net "Net-(Q13-Pad1)")
    (add_net "Net-(Q13-Pad3)")
    (add_net "Net-(Q14-Pad1)")
    (add_net "Net-(Q14-Pad3)")
    (add_net "Net-(Q15-Pad1)")
    (add_net "Net-(Q15-Pad3)")
    (add_net "Net-(Q16-Pad1)")
    (add_net "Net-(Q16-Pad3)")
    (add_net "Net-(Q17-Pad1)")
    (add_net "Net-(Q18-Pad1)")
    (add_net "Net-(Q19-Pad1)")
    (add_net "Net-(Q20-Pad1)")
    (add_net "Net-(Q21-Pad1)")
    (add_net "Net-(Q22-Pad1)")
    (add_net "Net-(Q23-Pad1)")
    (add_net "Net-(Q24-Pad1)")
    (add_net "Net-(Q9-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net VCC)
  )
  (module TSSOP-20_4.4x6.5mm_Pitch0.65mm_handsoldering (layer F.Cu) (tedit 5A7AC463)
    (at 211.455 38.1)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65 handsoldering")
    (attr smd)
    (fp_text reference U9 (at 0.127 0) (layer F.SilkS))
    (fp_text value 74LS541 (at 0 4.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.25 -2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 100 AS))
    (pad 2 smd rect (at -3.25 -2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 84 "Net-(J3-Pad1)"))
    (pad 3 smd rect (at -3.25 -1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 85 "Net-(J3-Pad2)"))
    (pad 4 smd rect (at -3.25 -0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 86 "Net-(J3-Pad3)"))
    (pad 5 smd rect (at -3.25 -0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (pad 6 smd rect (at -3.25 0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 88 "Net-(J3-Pad5)"))
    (pad 7 smd rect (at -3.25 0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 89 "Net-(J3-Pad6)"))
    (pad 8 smd rect (at -3.25 1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 90 "Net-(J3-Pad7)"))
    (pad 9 smd rect (at -3.25 2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 91 "Net-(J3-Pad8)"))
    (pad 10 smd rect (at -3.25 2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 11 smd rect (at 3.25 2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 74 AI7))
    (pad 12 smd rect (at 3.25 2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 72 AI6))
    (pad 13 smd rect (at 3.25 1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 70 AI5))
    (pad 14 smd rect (at 3.25 0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 68 AI4))
    (pad 15 smd rect (at 3.25 0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 66 AI3))
    (pad 16 smd rect (at 3.25 -0.325) (size 2 0.4) (layers F.Cu F.Mask)
      (net 64 AI2))
    (pad 17 smd rect (at 3.25 -0.975) (size 2 0.4) (layers F.Cu F.Mask)
      (net 62 AI1))
    (pad 18 smd rect (at 3.25 -1.625) (size 2 0.4) (layers F.Cu F.Mask)
      (net 60 AI0))
    (pad 19 smd rect (at 3.25 -2.275) (size 2 0.4) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 20 smd rect (at 3.25 -2.925) (size 2 0.4) (layers F.Cu F.Mask)
      (net 18 VCC))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 207.518 45.974)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 214.376 47.752)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 214.376 46.736)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 214.376 45.72)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 214.376 42.672)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 219.964 38.1)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 214.63 32.766)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 214.63 31.242)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 214.63 27.686)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 209.55 31.75)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 208.026 29.718)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 203.2 30.226)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 203.2 31.242)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 203.2 32.258)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 198.12 38.1)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 209.042 45.974)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 209.804 45.212)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 208.28 45.212)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 203.454 42.926)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 203.454 43.942)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BE02)
    (at 218.267264 31.044356 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R17 (at -0.197644 0.426736 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 28 "Net-(Q9-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 60 AI0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 200.66 26.67)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J13 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 AS))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA5B)
    (at 225.887264 45.168304 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at 0.210304 0 90) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 59 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5A79BE50)
    (at 234.142264 31.044356 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1n (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5A79CAF1)
    (at 234.142264 31.006834 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1n (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5A79BE74)
    (at 234.142264 35.743356 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1n (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5A79CAF9)
    (at 234.142264 35.705834 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1n (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5A79BF34)
    (at 234.142264 40.45855 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1n (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5A79CAFF)
    (at 234.142264 40.469304 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1n (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5A79BF87)
    (at 234.142264 45.15755 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1n (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5A79CB09)
    (at 234.142264 45.168304 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1n (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5A79C032)
    (at 210.082 42.672)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 0) (layer F.SilkS))
    (fp_text value 100n (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5A79C996)
    (at 206.502 33.528 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0 0 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BE34)
    (at 228.427264 30.409356 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -0.172736 0 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79CA68)
    (at 228.427264 31.641834 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -0.426736 -0.108166 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 21 "Net-(Q10-Pad3)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BE86)
    (at 228.427264 35.108356 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -0.172736 0 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 22 "Net-(Q11-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79CAA5)
    (at 228.427264 36.340834 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -0.426736 0 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 23 "Net-(Q12-Pad3)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BF1E)
    (at 228.427264 39.82355 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 0 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 24 "Net-(Q13-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79CAB2)
    (at 228.427264 41.104304 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at -0.426736 0 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 25 "Net-(Q14-Pad3)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BF74)
    (at 228.427264 44.52255 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at 0 0 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 26 "Net-(Q15-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79CABC)
    (at 228.427264 45.803304 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at -0.426736 0.083304 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 27 "Net-(Q16-Pad3)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BE14)
    (at 220.807264 31.044356)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q9 (at -0.335264 0) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 28 "Net-(Q9-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79C9E7)
    (at 220.807264 31.006834)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q10 (at -0.335264 0) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 29 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 21 "Net-(Q10-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BEA9)
    (at 220.807264 35.743356)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q11 (at -0.589264 0) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 30 "Net-(Q11-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 22 "Net-(Q11-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79C9EE)
    (at 220.807264 35.705834)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q12 (at -0.335264 0) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 31 "Net-(Q12-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 23 "Net-(Q12-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BEF8)
    (at 220.807264 40.45855)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q13 (at -0.589264 0) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 32 "Net-(Q13-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 24 "Net-(Q13-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79CA00)
    (at 220.807264 40.469304)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q14 (at -0.335264 0) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 33 "Net-(Q14-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 25 "Net-(Q14-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BF54)
    (at 220.807264 45.15755)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q15 (at -0.635 0) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 34 "Net-(Q15-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 26 "Net-(Q15-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79CA09)
    (at 220.807264 45.168304)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q16 (at -0.335264 0) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 35 "Net-(Q16-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 27 "Net-(Q16-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BC2A)
    (at 197.185264 30.917356 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q17 (at -0.426736 0 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 36 "Net-(Q17-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 37 KO0))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79C928)
    (at 197.185264 30.88161 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q18 (at -0.635 0 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 38 "Net-(Q18-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 39 KO1))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BC5E)
    (at 197.185264 35.616356 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q19 (at -0.172736 0 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 40 "Net-(Q19-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 41 KO2))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79C947)
    (at 197.141142 35.604852 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q20 (at -0.635 0 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 42 "Net-(Q20-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 43 KO3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BDA8)
    (at 197.106148 40.541052 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q21 (at -0.251852 -0.098948 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 44 "Net-(Q21-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 45 KO4))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79C968)
    (at 197.139528 40.572712 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q22 (at -0.635 0 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 46 "Net-(Q22-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 47 KO5))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A79BDDB)
    (at 197.234398 45.40568 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q23 (at -0.377602 0 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 48 "Net-(Q23-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 49 KO6))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A79C982)
    (at 197.143136 45.398672 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q24 (at -0.635 0 180) (layer B.SilkS))
    (fp_text value Q_NPN_BEC (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 50 "Net-(Q24-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 51 KO7))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BE1E)
    (at 223.347264 31.044356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA14)
    (at 223.347264 31.006834 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 21 "Net-(Q10-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BEA0)
    (at 223.347264 35.743356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 22 "Net-(Q11-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA1C)
    (at 223.347264 35.705834 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 23 "Net-(Q12-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BF07)
    (at 223.347264 40.45855 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 24 "Net-(Q13-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA24)
    (at 223.347264 40.469304 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 25 "Net-(Q14-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BF5E)
    (at 223.347264 45.15755 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 26 "Net-(Q15-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA30)
    (at 223.347264 45.168304 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 27 "Net-(Q16-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BE2B)
    (at 225.887264 31.044356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 52 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA39)
    (at 225.887264 31.006834 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0.018834 0 90) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 53 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BE93)
    (at 225.887264 35.743356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0.070644 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 54 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA43)
    (at 225.887264 35.705834 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at 0.145834 0 90) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 55 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BF11)
    (at 225.887264 40.45855 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 0.18145 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 56 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CA51)
    (at 225.887264 40.469304 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at 0.083304 0 90) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 57 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BF68)
    (at 225.887264 45.15755 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 0.05445 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 58 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BE5B)
    (at 236.682264 31.044356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R18 (at 0.197644 -0.045736 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 61 AO0))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C9B4)
    (at 218.267264 31.006834 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R19 (at -0.018834 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 29 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 62 AI1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CB12)
    (at 236.682264 31.006834 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R20 (at 0.018834 0 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 63 AO1))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BEB7)
    (at 218.267264 35.743356 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R21 (at -0.070644 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 30 "Net-(Q11-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 64 AI2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BE66)
    (at 236.682264 35.743356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R22 (at 0.070644 0 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 65 AO2))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C9BD)
    (at 218.267264 35.705834 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R23 (at -0.145834 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 31 "Net-(Q12-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 66 AI3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CB1B)
    (at 236.682264 35.705834 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R24 (at 0.145834 0 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 67 AO3))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BEEC)
    (at 218.267264 40.45855 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R25 (at -0.18145 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 32 "Net-(Q13-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 68 AI4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BF3C)
    (at 236.682264 40.45855 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R26 (at 0.18145 0 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 69 AO4))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C9C6)
    (at 218.267264 40.469304 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R27 (at -0.083304 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 33 "Net-(Q14-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 70 AI5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CB25)
    (at 236.682264 40.469304 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R28 (at 0.083304 0 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 71 AO5))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BF4A)
    (at 218.267264 45.15755 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R29 (at -0.05445 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 34 "Net-(Q15-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 72 AI6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BF8F)
    (at 236.682264 45.15755 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R30 (at 0.05445 0 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 73 AO6))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C9DB)
    (at 218.267264 45.168304 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R31 (at 0.043696 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 35 "Net-(Q16-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 74 AI7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79CB2E)
    (at 236.682264 45.168304 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R32 (at -0.043696 0 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 75 AO7))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BC09)
    (at 194.645264 30.917356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R33 (at 0.070644 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 37 KO0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C91D)
    (at 194.645264 30.88161 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R34 (at 0.14761 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 39 KO1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BC4E)
    (at 194.645264 35.616356 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R35 (at 0.197644 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 41 KO2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C93B)
    (at 194.601142 35.604852 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R36 (at 0.044852 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 43 KO3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BD9C)
    (at 194.566148 40.541052 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R37 (at 0.098948 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 45 KO4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C95B)
    (at 194.599528 40.572712 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R38 (at 0.186712 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 47 KO5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BDD0)
    (at 194.694398 45.40568 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R39 (at 0.06032 0 270) (layer F.SilkS))
    (fp_text value 220K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 49 KO6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C989)
    (at 194.603136 45.398672 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R40 (at 0.186672 0 90) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 20 HT))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 51 KO7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BC3C)
    (at 199.725264 30.917356 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R41 (at -0.070644 -0.335264 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 36 "Net-(Q17-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 76 KI0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C931)
    (at 199.725264 30.88161 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R42 (at -0.14761 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 38 "Net-(Q18-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 77 KI1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BC79)
    (at 199.725264 35.616356 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R43 (at -0.197644 -0.335264 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 40 "Net-(Q19-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 78 KI2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C94E)
    (at 199.681142 35.604852 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R44 (at -0.044852 0.037142 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 42 "Net-(Q20-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 79 KI3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BDB9)
    (at 199.646148 40.541052 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R45 (at -0.098948 -0.510148 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 44 "Net-(Q21-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 80 KI4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C96F)
    (at 199.679528 40.572712 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R46 (at -0.186712 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 46 "Net-(Q22-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 81 KI5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A79BDE7)
    (at 199.774398 45.40568 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R47 (at -0.06032 -0.384398 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 48 "Net-(Q23-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 82 KI6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A79C978)
    (at 199.683136 45.398672 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R48 (at -0.186672 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 50 "Net-(Q24-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Mask)
      (net 83 KI7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-457 (layer F.Cu) (tedit 5A79BE47)
    (at 231.602264 31.044356 90)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U1 (at 0 0 90) (layer F.SilkS))
    (fp_text value DiodeArray (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at -1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 52 "Net-(R9-Pad2)"))
    (pad 6 smd rect (at 1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module footprints:SOT-457 (layer B.Cu) (tedit 5A79CACA)
    (at 231.602264 31.006834 270)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U2 (at 0 0 270) (layer B.SilkS))
    (fp_text value DiodeArray (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 21 "Net-(Q10-Pad3)"))
    (pad 3 smd rect (at -1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 53 "Net-(R10-Pad2)"))
    (pad 6 smd rect (at 1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 4 "Net-(C2-Pad2)"))
  )
  (module footprints:SOT-457 (layer F.Cu) (tedit 5A79BE7E)
    (at 231.602264 35.743356 90)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U3 (at 0 0 90) (layer F.SilkS))
    (fp_text value DiodeArray (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 22 "Net-(Q11-Pad3)"))
    (pad 3 smd rect (at -1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at 1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 54 "Net-(R11-Pad2)"))
    (pad 6 smd rect (at 1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 6 "Net-(C3-Pad2)"))
  )
  (module footprints:SOT-457 (layer B.Cu) (tedit 5A79CAD5)
    (at 231.602264 35.705834 270)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U4 (at 0 0 270) (layer B.SilkS))
    (fp_text value DiodeArray (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 23 "Net-(Q12-Pad3)"))
    (pad 3 smd rect (at -1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at 1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 55 "Net-(R12-Pad2)"))
    (pad 6 smd rect (at 1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 8 "Net-(C4-Pad2)"))
  )
  (module footprints:SOT-457 (layer F.Cu) (tedit 5A79BF2B)
    (at 231.602264 40.45855 90)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U5 (at 0 0 90) (layer F.SilkS))
    (fp_text value DiodeArray (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 24 "Net-(Q13-Pad3)"))
    (pad 3 smd rect (at -1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 4 smd rect (at 1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 56 "Net-(R13-Pad2)"))
    (pad 6 smd rect (at 1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 10 "Net-(C5-Pad2)"))
  )
  (module footprints:SOT-457 (layer B.Cu) (tedit 5A79CADE)
    (at 231.602264 40.469304 270)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U6 (at 0 0 270) (layer B.SilkS))
    (fp_text value DiodeArray (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 25 "Net-(Q14-Pad3)"))
    (pad 3 smd rect (at -1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 4 smd rect (at 1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 57 "Net-(R14-Pad2)"))
    (pad 6 smd rect (at 1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 12 "Net-(C6-Pad2)"))
  )
  (module footprints:SOT-457 (layer F.Cu) (tedit 5A79BF7D)
    (at 231.602264 45.15755 90)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U7 (at 0 0 90) (layer F.SilkS))
    (fp_text value DiodeArray (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 26 "Net-(Q15-Pad3)"))
    (pad 3 smd rect (at -1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 4 smd rect (at 1 0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 58 "Net-(R15-Pad2)"))
    (pad 6 smd rect (at 1 -0.95) (size 0.6 1) (layers F.Cu F.Mask)
      (net 14 "Net-(C7-Pad2)"))
  )
  (module footprints:SOT-457 (layer B.Cu) (tedit 5A79CAE8)
    (at 231.602264 45.168304 270)
    (descr "SOT-457 4 lead surface package")
    (tags SOT-457)
    (attr smd)
    (fp_text reference U8 (at 0 0 270) (layer B.SilkS))
    (fp_text value DiodeArray (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 27 "Net-(Q16-Pad3)"))
    (pad 3 smd rect (at -1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (pad 4 smd rect (at 1 -0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 59 "Net-(R16-Pad2)"))
    (pad 6 smd rect (at 1 0.95) (size 0.6 1) (layers B.Cu B.Mask)
      (net 16 "Net-(C8-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 217.17 26.67)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 217.17 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J4 (at 0 2.54) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 227.33 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J9 (at 0 2.54) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 227.33 26.67)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 198.12 26.67)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 198.12 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J12 (at 0 2.286) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 200.66 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J14 (at 0 2.286) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 KS))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_21x04_Pitch2.54mm_SMD_2sides (layer F.Cu) (tedit 5A78BB78)
    (at 239.395 38.1)
    (descr "surface-mounted pin header, 2x04, 2.54mm pitch, single row 2 sides")
    (tags "Surface mounted pin header SMD 2x04 2.54mm single row 2 sides")
    (attr smd)
    (fp_text reference J2 (at 2.413 -6.35) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 5.842) (layer F.Fab))
    (fp_text user %R (at -1.524 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0 -3.81) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 63 AO1))
    (pad 1 smd rect (at 0 -3.81) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 61 AO0))
    (pad 5 smd rect (at 0 1.27) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 69 AO4))
    (pad 6 smd rect (at 0 1.27) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 71 AO5))
    (pad 4 smd rect (at 0 -1.27) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 67 AO3))
    (pad 3 smd rect (at 0 -1.27) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 65 AO2))
    (pad 7 smd rect (at 0 3.81) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 73 AO6))
    (pad 8 smd rect (at 0 3.81) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 75 AO7))
  )
  (module footprints:Pin_Header_21x04_Pitch2.54mm_SMD_2sides (layer F.Cu) (tedit 5A78BB78)
    (at 191.77 38.1)
    (descr "surface-mounted pin header, 2x04, 2.54mm pitch, single row 2 sides")
    (tags "Surface mounted pin header SMD 2x04 2.54mm single row 2 sides")
    (attr smd)
    (fp_text reference J5 (at -2.794 -6.35) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 5.842) (layer F.Fab))
    (fp_text user %R (at -1.524 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0 -3.81) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 39 KO1))
    (pad 1 smd rect (at 0 -3.81) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 37 KO0))
    (pad 5 smd rect (at 0 1.27) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 45 KO4))
    (pad 6 smd rect (at 0 1.27) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 47 KO5))
    (pad 4 smd rect (at 0 -1.27) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 43 KO3))
    (pad 3 smd rect (at 0 -1.27) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 41 KO2))
    (pad 7 smd rect (at 0 3.81) (size 1.524 1.524) (layers F.Cu F.Mask)
      (net 49 KO6))
    (pad 8 smd rect (at 0 3.81) (size 1.524 1.524) (layers B.Cu B.Mask)
      (net 51 KO7))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 195.58 26.67)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J15 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 195.58 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J16 (at 0 2.286) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 HT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 219.71 26.67)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J17 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 219.71 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J18 (at 0 2.54) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_1x08_Pitch1.27mm_SMD (layer F.Cu) (tedit 5A79D3FD)
    (at 209.55 49.53 90)
    (descr "surface-mounted pin header, 1x08, 1.27mm pitch, single row")
    (tags "Surface mounted pin header SMD 1x08 1.27mm single row")
    (attr smd)
    (fp_text reference J3 (at -2.286 -6.858 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 6.35 90) (layer F.Fab))
    (fp_text user %R (at -1.27 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -5.08 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 84 "Net-(J3-Pad1)"))
    (pad 3 smd rect (at 0 -2.54 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 86 "Net-(J3-Pad3)"))
    (pad 5 smd rect (at 0 0 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 88 "Net-(J3-Pad5)"))
    (pad 7 smd rect (at 0 2.54 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 90 "Net-(J3-Pad7)"))
    (pad 2 smd rect (at 0 -3.81 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 85 "Net-(J3-Pad2)"))
    (pad 4 smd rect (at 0 -1.27 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (pad 6 smd rect (at 0 1.27 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 89 "Net-(J3-Pad6)"))
    (pad 8 smd rect (at 0 3.81 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 91 "Net-(J3-Pad8)"))
  )
  (module footprints:Pin_Header_1x08_Pitch1.27mm_SMD (layer F.Cu) (tedit 5A79D3C1)
    (at 209.55 26.67 90)
    (descr "surface-mounted pin header, 1x08, 1.27mm pitch, single row")
    (tags "Surface mounted pin header SMD 1x08 1.27mm single row")
    (attr smd)
    (fp_text reference J6 (at 2.286 -6.858 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 6.35 90) (layer F.Fab))
    (fp_text user %R (at -1.27 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -5.08 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 84 "Net-(J3-Pad1)"))
    (pad 3 smd rect (at 0 -2.54 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 86 "Net-(J3-Pad3)"))
    (pad 5 smd rect (at 0 0 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 88 "Net-(J3-Pad5)"))
    (pad 7 smd rect (at 0 2.54 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 90 "Net-(J3-Pad7)"))
    (pad 2 smd rect (at 0 -3.81 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 85 "Net-(J3-Pad2)"))
    (pad 4 smd rect (at 0 -1.27 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 87 "Net-(J3-Pad4)"))
    (pad 6 smd rect (at 0 1.27 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 89 "Net-(J3-Pad6)"))
    (pad 8 smd rect (at 0 3.81 90) (size 1.016 1.016) (layers F.Cu F.Mask)
      (net 91 "Net-(J3-Pad8)"))
  )
  (module footprints:Pin_Header_1x08_Pitch1.27mm_SMD (layer B.Cu) (tedit 5A79D476)
    (at 209.55 26.67 270)
    (descr "surface-mounted pin header, 1x08, 1.27mm pitch, single row")
    (tags "Surface mounted pin header SMD 1x08 1.27mm single row")
    (attr smd)
    (fp_text reference J7 (at -2.286 5.842 270) (layer B.SilkS))
    (fp_text value Conn_01x08 (at 0 -6.35 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -1.27 540) (layer B.Fab))
    (pad 1 smd rect (at 0 5.08 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 92 "Net-(J7-Pad1)"))
    (pad 3 smd rect (at 0 2.54 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 93 "Net-(J7-Pad3)"))
    (pad 5 smd rect (at 0 0 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 94 "Net-(J7-Pad5)"))
    (pad 7 smd rect (at 0 -2.54 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 95 "Net-(J7-Pad7)"))
    (pad 2 smd rect (at 0 3.81 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 96 "Net-(J7-Pad2)"))
    (pad 4 smd rect (at 0 1.27 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 97 "Net-(J7-Pad4)"))
    (pad 6 smd rect (at 0 -1.27 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 98 "Net-(J7-Pad6)"))
    (pad 8 smd rect (at 0 -3.81 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 99 "Net-(J7-Pad8)"))
  )
  (module footprints:Pin_Header_1x08_Pitch1.27mm_SMD (layer B.Cu) (tedit 5A79D46C)
    (at 209.55 49.53 270)
    (descr "surface-mounted pin header, 1x08, 1.27mm pitch, single row")
    (tags "Surface mounted pin header SMD 1x08 1.27mm single row")
    (attr smd)
    (fp_text reference J8 (at 2.286 5.842 270) (layer B.SilkS))
    (fp_text value Conn_01x08 (at 0 -6.35 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -1.27 540) (layer B.Fab))
    (pad 1 smd rect (at 0 5.08 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 92 "Net-(J7-Pad1)"))
    (pad 3 smd rect (at 0 2.54 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 93 "Net-(J7-Pad3)"))
    (pad 5 smd rect (at 0 0 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 94 "Net-(J7-Pad5)"))
    (pad 7 smd rect (at 0 -2.54 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 95 "Net-(J7-Pad7)"))
    (pad 2 smd rect (at 0 3.81 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 96 "Net-(J7-Pad2)"))
    (pad 4 smd rect (at 0 1.27 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 97 "Net-(J7-Pad4)"))
    (pad 6 smd rect (at 0 -1.27 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 98 "Net-(J7-Pad6)"))
    (pad 8 smd rect (at 0 -3.81 270) (size 1.016 1.016) (layers B.Cu B.Mask)
      (net 99 "Net-(J7-Pad8)"))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5A79B7D8)
    (at 192.405 27.305)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5A79B7EC)
    (at 238.76 27.305)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at -0.254 -2.921) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5A79B7E9)
    (at 238.76 48.895)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at -0.254 3.175) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5A79B7CF)
    (at 192.405 48.895)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0.127 2.921) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module footprints:via (layer F.Cu) (tedit 5A79D0C5)
    (at 203.454 44.958)
    (fp_text reference J19 (at 0 0.5) (layer Dwgs.User) hide)
    (fp_text value TEST_1P (at 0 -0.508) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 17 GND))
  )
  (module footprints:TSSOP-20_4.4x6.5mm_Pitch0.65mm_handsoldering (layer B.Cu) (tedit 5A7AC463)
    (at 206.375 38.1 180)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65 handsoldering")
    (attr smd)
    (fp_text reference U10 (at 0.127 0 180) (layer B.SilkS))
    (fp_text value 74LS541 (at 0 -4.3 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -3.25 2.925 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 101 KS))
    (pad 2 smd rect (at -3.25 2.275 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 92 "Net-(J7-Pad1)"))
    (pad 3 smd rect (at -3.25 1.625 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 96 "Net-(J7-Pad2)"))
    (pad 4 smd rect (at -3.25 0.975 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 93 "Net-(J7-Pad3)"))
    (pad 5 smd rect (at -3.25 0.325 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 97 "Net-(J7-Pad4)"))
    (pad 6 smd rect (at -3.25 -0.325 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 94 "Net-(J7-Pad5)"))
    (pad 7 smd rect (at -3.25 -0.975 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 98 "Net-(J7-Pad6)"))
    (pad 8 smd rect (at -3.25 -1.625 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 95 "Net-(J7-Pad7)"))
    (pad 9 smd rect (at -3.25 -2.275 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 99 "Net-(J7-Pad8)"))
    (pad 10 smd rect (at -3.25 -2.925 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 11 smd rect (at 3.25 -2.925 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 83 KI7))
    (pad 12 smd rect (at 3.25 -2.275 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 82 KI6))
    (pad 13 smd rect (at 3.25 -1.625 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 81 KI5))
    (pad 14 smd rect (at 3.25 -0.975 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 80 KI4))
    (pad 15 smd rect (at 3.25 -0.325 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 79 KI3))
    (pad 16 smd rect (at 3.25 0.325 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 78 KI2))
    (pad 17 smd rect (at 3.25 0.975 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 77 KI1))
    (pad 18 smd rect (at 3.25 1.625 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 76 KI0))
    (pad 19 smd rect (at 3.25 2.275 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 17 GND))
    (pad 20 smd rect (at 3.25 2.925 180) (size 2 0.4) (layers B.Cu B.Mask)
      (net 18 VCC))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Vcc (at 215.392 49.276 90) (layer B.SilkS))
  (gr_text Vcc (at 215.392 27.432 90) (layer F.SilkS))
  (gr_text Vcc (at 215.392 48.768 90) (layer F.SilkS))
  (gr_text Gnd (at 221.996 26.924) (layer F.SilkS))
  (gr_text Gnd (at 221.996 49.276) (layer F.SilkS))
  (gr_text hackaday.io/muth (at 216.154 38.1 90) (layer B.Mask))
  (gr_text driver (at 214.63 38.1 90) (layer B.Mask))
  (gr_text "ИГГ_ octal " (at 212.598 38.608 90) (layer B.SilkS))
  (gr_text "ИГГ_ octal " (at 202.184 37.338 90) (layer F.Mask))
  (gr_text hackaday.io/muth (at 205.994 37.846 90) (layer F.SilkS))
  (gr_text driver (at 204.216 37.592 90) (layer F.SilkS))
  (gr_text A6 (at 239.522 45.974 90) (layer F.SilkS))
  (gr_text A4 (at 239.522 43.942 90) (layer F.SilkS))
  (gr_text A2 (at 239.522 32.004 90) (layer F.SilkS))
  (gr_text A0 (at 239.522 29.972 90) (layer F.SilkS))
  (gr_text A7 (at 239.522 45.974 90) (layer B.SilkS))
  (gr_text A5 (at 239.522 43.942 90) (layer B.SilkS))
  (gr_text A3 (at 239.522 32.004 90) (layer B.SilkS))
  (gr_text A1 (at 239.522 29.972 90) (layer B.SilkS))
  (gr_text K1 (at 191.77 29.972 90) (layer B.SilkS))
  (gr_text K3 (at 191.77 32.004 90) (layer B.SilkS))
  (gr_text K5 (at 191.77 43.942 90) (layer B.SilkS))
  (gr_text K7 (at 191.77 45.974 90) (layer B.SilkS))
  (gr_text K6 (at 191.77 45.974 90) (layer F.SilkS))
  (gr_text K4 (at 191.77 43.942 90) (layer F.SilkS))
  (gr_text K0 (at 191.77 29.972 90) (layer F.SilkS))
  (gr_text K2 (at 191.77 32.004 90) (layer F.SilkS))
  (gr_text Gnd (at 221.996 49.276) (layer B.SilkS))
  (gr_text Gnd (at 221.996 26.924) (layer B.SilkS))
  (gr_text Vcc (at 215.392 26.924 90) (layer B.SilkS))
  (gr_text KS (at 207.264 44.196) (layer F.SilkS))
  (gr_text Gnd (at 204.978 44.196) (layer F.SilkS))
  (gr_text HV (at 202.438 44.196) (layer F.SilkS))
  (gr_text AS (at 207.01 31.75) (layer F.SilkS))
  (gr_text Gnd (at 204.724 31.75) (layer F.SilkS))
  (gr_text HV (at 202.184 31.75) (layer F.SilkS))
  (gr_text HV (at 225.044 26.924) (layer B.SilkS))
  (gr_text HV (at 225.044 49.276) (layer B.SilkS))
  (gr_text HV (at 225.044 49.276) (layer F.SilkS))
  (gr_text HV (at 225.044 26.924) (layer F.SilkS))
  (gr_text "CATHODE\n8 7 6 5 4 3 2 1" (at 208.788 47.752) (layer B.SilkS))
  (gr_text "8 7 6 5 4 3 2 1\nCATHODE" (at 208.788 28.702) (layer B.SilkS))
  (gr_text "ANODE\n1 2 3 4 5 6 7 8" (at 208.788 47.498) (layer F.SilkS))
  (gr_text "1 2 3 4 5 6 7 8\nANODE" (at 208.788 28.702) (layer F.SilkS))
  (gr_line (start 190.5 50.8) (end 190.5 25.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 240.665 50.8) (end 190.5 50.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 240.665 25.4) (end 240.665 50.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 25.4) (end 240.665 25.4) (layer Edge.Cuts) (width 0.15))
  (zone (net 20) (net_name HT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 194.31 26.416) (xy 194.31 26.67) (xy 194.31 28.448) (xy 193.802 28.956) (xy 193.802 47.498)
        (xy 194.31 48.006) (xy 194.31 49.276) (xy 194.31 49.784) (xy 196.85 49.784) (xy 196.85 48.006)
        (xy 197.104 47.752) (xy 197.104 28.702) (xy 196.85 28.448) (xy 196.85 26.416) (xy 194.818 26.416)
      )
    )
  )
  (zone (net 17) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 197.612 26.416) (xy 197.612 49.784) (xy 220.726 49.784) (xy 220.726 26.416)
      )
    )
  )
  (zone (net 20) (net_name HT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 220.98 29.21) (xy 220.98 46.99) (xy 223.774 49.784) (xy 228.6 49.784) (xy 228.6 47.244)
        (xy 228.6 28.702) (xy 228.6 26.416) (xy 223.774 26.416)
      )
    )
  )
  (zone (net 20) (net_name HT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 196.85 26.416) (xy 194.31 26.416) (xy 194.31 28.448) (xy 193.802 28.956) (xy 193.802 47.498)
        (xy 194.31 48.006) (xy 194.31 49.784) (xy 196.85 49.784) (xy 196.85 48.006) (xy 197.104 47.752)
        (xy 197.104 28.702) (xy 196.85 28.448)
      )
    )
  )
  (zone (net 17) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 197.358 26.416) (xy 197.358 49.784) (xy 220.472 49.784) (xy 220.472 27.686) (xy 220.472 26.416)
      )
    )
  )
  (zone (net 20) (net_name HT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 220.98 29.21) (xy 223.774 26.416) (xy 228.6 26.416) (xy 228.6 49.784) (xy 223.774 49.784)
        (xy 220.98 46.99)
      )
    )
  )
)
