(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 12)
    (no_connects 0)
    (area 142.672999 103.048999 151.713001 113.359001)
    (thickness 1.6)
    (drawings 14)
    (tracks 33)
    (zones 0)
    (modules 5)
    (nets 7)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.635)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.6858 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 0 0)
    (visible_elements 7FFCFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 /SDA)
  (net 4 /SCL)
  (net 5 "Net-(U1-Pad5)")
  (net 6 "Net-(U1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net VDD)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5C01C62E)
    (at 146.05 109.22 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5C01C615)
    (at 148.971 106.426)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 4.7k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5C01C60E)
    (at 148.971 104.902)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 4.7k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ms5607-breakout:MS5607-02BA (layer F.Cu) (tedit 5C01C607)
    (at 148.59 109.855)
    (fp_text reference U1 (at 0 3.4) (layer F.SilkS) hide)
    (fp_text value MS5607-02BA (at 0 -3.7) (layer F.Fab))
    (fp_text user RESERVED (at 0 0 90) (layer F.CrtYd))
    (pad 1 smd rect (at -1.1 -1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -1.1 -0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -1.1 0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.1 1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.1 1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 1.1 0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 1.1 -0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (pad 8 smd rect (at 1.1 -1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
  )
  (module ms5607-breakout:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5C01C7B4)
    (at 144.018 112.014 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 8.89 (width 0.3) (layer Dwgs.User)
    (gr_text "0.3500 in" (at 147.193 99.742) (layer Dwgs.User))
    (feature1 (pts (xy 151.638 103.124) (xy 151.638 98.392)))
    (feature2 (pts (xy 142.748 103.124) (xy 142.748 98.392)))
    (crossbar (pts (xy 142.748 101.092) (xy 151.638 101.092)))
    (arrow1a (pts (xy 151.638 101.092) (xy 150.511496 101.678421)))
    (arrow1b (pts (xy 151.638 101.092) (xy 150.511496 100.505579)))
    (arrow2a (pts (xy 142.748 101.092) (xy 143.874504 101.678421)))
    (arrow2b (pts (xy 142.748 101.092) (xy 143.874504 100.505579)))
  )
  (dimension 10.16 (width 0.3) (layer Dwgs.User)
    (gr_text "0.4000 in" (at 156.29 108.204 270) (layer Dwgs.User))
    (feature1 (pts (xy 152.146 113.284) (xy 157.64 113.284)))
    (feature2 (pts (xy 152.146 103.124) (xy 157.64 103.124)))
    (crossbar (pts (xy 154.94 103.124) (xy 154.94 113.284)))
    (arrow1a (pts (xy 154.94 113.284) (xy 154.353579 112.157496)))
    (arrow1b (pts (xy 154.94 113.284) (xy 155.526421 112.157496)))
    (arrow2a (pts (xy 154.94 103.124) (xy 154.353579 104.250504)))
    (arrow2b (pts (xy 154.94 103.124) (xy 155.526421 104.250504)))
  )
  (gr_line (start 142.748 112.268) (end 142.748 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.638 104.14) (end 151.638 112.268) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.622 113.284) (end 143.764 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.622 103.124) (end 143.764 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 150.622 112.268) (end 151.638 112.268) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.764 112.268) (end 143.764 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 150.622 104.14) (end 150.622 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.764 104.14) (end 142.748 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 147.828 112.014) (layer B.Mask))
  (gr_text VDD (at 147.828 109.474) (layer B.Mask))
  (gr_text SCL (at 147.828 106.934) (layer B.Mask))
  (gr_text SDA (at 147.828 104.394) (layer B.Mask))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.508)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 151.638 113.284) (xy 142.748 113.284) (xy 142.748 103.124) (xy 151.638 103.124) (xy 151.638 113.284)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.508)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 151.638 113.284) (xy 142.748 113.284) (xy 142.748 103.124) (xy 151.638 103.124) (xy 151.638 113.284)
      )
    )
  )
)
