(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~88~ubuntu18.04.1)
  (general
    (thickness 0.1016)
    (drawings 18)
    (tracks 27)
    (zones 0)
    (modules 2)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /SDA)
  (net 4 /SCL)
  (net 5 "Net-(U1-Pad7)")
  (net 6 "Net-(U1-Pad3)")
  (net 7 "Net-(U1-Pad2)")
  (net 8 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad7)")
    (add_net VCC)
  )
  (module SOIC8-EEPROM-MOD:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 6096C496)
    (at 25 23 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 -3.4 90) (layer F.SilkS) hide)
    (fp_text value 24LC00 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -3.1 -1.905 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(U1-Pad1)"))
    (pad 2 thru_hole roundrect (at -3.1 -0.635 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad2)"))
    (pad 3 thru_hole roundrect (at -3.1 0.635 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(U1-Pad3)"))
    (pad 4 thru_hole roundrect (at -3.1 1.905 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 thru_hole roundrect (at 3.1 1.905 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 /SDA))
    (pad 6 thru_hole roundrect (at 3.1 0.635 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 /SCL))
    (pad 7 thru_hole roundrect (at 3.1 -0.635 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U1-Pad7)"))
    (pad 8 thru_hole roundrect (at 3.1 -1.905 90) (size 0.7 0.6) (drill 0.254) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (offset (xyz 0 0 -0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "SM04B-SRSS-TB(LF)(SN):JST_SM04B-SRSS-TB(LF)(SN)" (layer F.Cu) (tedit 6096B8DD)
    (at 31 23 90)
    (fp_text reference J1 (at -0.545095 -1.767685 90) (layer F.SilkS) hide)
    (fp_text value "SM04B-SRSS-TB(LF)(SN)" (at 12.17039 5.74055 90) (layer F.Fab))
    (pad S2 smd rect (at 2.8 3.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S1 smd rect (at -2.8 3.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at 0.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (pad 4 smd rect (at 1.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (model "${KIPRJMOD}/kicad-library/SM04B-SRSS-TB(LF)(SN)/SM04B-SRSS-TB_LF__SN_.step"
      (offset (xyz 0 -0.5 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text "François Gervais\n28 mai 2021\nv1.0-3-gf25257a" (at 36.4 20.4) (layer B.SilkS))
  (gr_arc (start 27.85 20.6) (end 28 20.6) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 27.85 25.4) (end 27.85 25.55) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 22.15 25.4) (end 22 25.4) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 22.15 20.6) (end 22.15 20.45) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 36.2 19.1) (end 36.5 19.1) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 36.2 26.9) (end 36.2 27.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 21.3 26.9) (end 21 26.9) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 21.3 19.1) (end 21.3 18.8) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 27.85 20.45) (end 22.15 20.45) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 28 25.4) (end 28 20.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 22.15 25.55) (end 27.85 25.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 22 20.6) (end 22 25.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 21 26.9) (end 21 23) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 36.2 27.2) (end 21.3 27.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 36.5 19.1) (end 36.5 26.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 21.3 18.8) (end 36.2 18.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 21 23) (end 21 19.1) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 27.2) (xy 21 27.2) (xy 21 18.8) (xy 36.5 18.8)
      )
    )
  )
)
