(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 51)
    (no_connects 0)
    (area -9.284 -53.352701 34.149 53.352701)
    (thickness 1.6)
    (drawings 12)
    (tracks 62)
    (zones 0)
    (modules 25)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.0508)
    (uvia_drill 0.0254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J2-Pad3)")
  (net 5 "Net-(J3-Pad3)")
  (net 6 "Net-(J4-Pad3)")
  (net 7 "Net-(J5-Pad3)")
  (net 8 "Net-(J6-Pad3)")
  (net 9 "Net-(J7-Pad3)")
  (net 10 "Net-(J8-Pad3)")
  (net 11 "Net-(J9-Pad2)")
  (net 12 "Net-(J9-Pad3)")
  (net 13 "Net-(P1-Pad1)")
  (net 14 "Net-(P2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.0508)
    (uvia_drill 0.0254)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(J9-Pad3)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
  )
  (module nearness:Pin_1x5 (layer F.Cu) (tedit 59ACF3F7)
    (at 0 -42.2275 90)
    (fp_text reference P1 (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
  )
  (module nearness:Pin_1x5 (layer F.Cu) (tedit 59ACF3FA)
    (at 0 42.2275 90)
    (fp_text reference P2 (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(J9-Pad3)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 5A4878B8)
    (at -4.445 -39.0525 180)
    (fp_text reference R1 (at -2.8575 0 270) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.905 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 59AD355D)
    (at -4.445 -32.385 270)
    (fp_text reference R2 (at 0 -1.905 450) (layer B.SilkS))
    (fp_text value 1M67 (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P2-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 59AD3561)
    (at -4.445 -27.94 90)
    (fp_text reference R3 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value 103k (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 59AD35CC)
    (at -4.445 -20.32 270)
    (fp_text reference R4 (at 0 -1.905 270) (layer B.SilkS))
    (fp_text value 439k (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P2-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 58FF14BD)
    (at -4.445 -15.875 90)
    (fp_text reference R5 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value 113k (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J4-Pad3)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 59AD4203)
    (at -4.445 -8.255 270)
    (fp_text reference R6 (at 0 -1.905 270) (layer B.SilkS))
    (fp_text value 215k (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J4-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P2-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 58FF14BD)
    (at -4.445 -3.81 90)
    (fp_text reference R7 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value 141k (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J5-Pad3)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 59AD35B1)
    (at -4.445 3.81 270)
    (fp_text reference R8 (at 0 -1.905 270) (layer B.SilkS))
    (fp_text value 141k (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J5-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P2-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 58FF14BD)
    (at -4.445 8.255 90)
    (fp_text reference R9 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value 215k (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 59AD35B9)
    (at -4.445 15.875 270)
    (fp_text reference R10 (at 0 -1.905 270) (layer B.SilkS))
    (fp_text value 113k (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P2-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 58FF14BD)
    (at -4.445 20.32 90)
    (fp_text reference R11 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value 439k (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J7-Pad3)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 59AD35BE)
    (at -4.445 27.94 270)
    (fp_text reference R12 (at 0 -1.905 270) (layer B.SilkS))
    (fp_text value 103k (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J7-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P2-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 58FF14BD)
    (at -4.445 32.385 90)
    (fp_text reference R13 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value 1M67 (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J8-Pad3)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad1)"))
  )
  (module nearness:0805 (layer B.Cu) (tedit 5A4878C4)
    (at -4.445 39.0525)
    (fp_text reference R14 (at 2.8575 0 90) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.905) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J8-Pad3)"))
    (pad 2 smd rect (at 1 0) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(P2-Pad1)"))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DF4)
    (at 0 48.26 270)
    (fp_text reference J9 (at 0 8.255 270) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(J9-Pad2)"))
    (pad 3 thru_hole circle (at 0 -4.445 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(J9-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DF2)
    (at 0 36.195 90)
    (fp_text reference J8 (at 0 8.255 90) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -4.445 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(J8-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DEF)
    (at 0 24.13 90)
    (fp_text reference J7 (at 0 8.255 90) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -4.445 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(J7-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DEC)
    (at 0 12.065 90)
    (fp_text reference J6 (at 0 8.255 90) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -4.445 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(J6-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DE9)
    (at 0 0 90)
    (fp_text reference J5 (at 0 8.255 90) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -4.445 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(J5-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DE6)
    (at 0 -12.065 90)
    (fp_text reference J4 (at 0 8.255 90) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -4.445 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DE3)
    (at 0 -24.13 90)
    (fp_text reference J3 (at 0 8.255 90) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -4.445 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DE0)
    (at 0 -36.195 90)
    (fp_text reference J2 (at 0 8.255 90) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -4.445 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module nearness:PJ301M12 (layer F.Cu) (tedit 59AD1DDD)
    (at 0 -48.26 270)
    (fp_text reference J1 (at 0 8.255 270) (layer F.SilkS) hide)
    (fp_text value PJ301M12 (at 0 -6.985 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.715 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 3.175 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -4.445 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (gr_line (start -6.985 53.34) (end -6.985 -53.34) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 6.985 53.34) (end -6.985 53.34) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 6.985 -53.34) (end 6.985 53.34) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start -6.985 -53.34) (end 6.985 -53.34) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -6.477 -52.832) (xy 6.477 -52.832) (xy 6.477 52.832) (xy -6.477 52.832)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -6.477 -52.832) (xy 6.477 -52.832) (xy 6.477 52.832) (xy -6.477 52.832)
      )
    )
  )
)
