(kicad_pcb (version 20171130) (host pcbnew 5.1.12-84ad8e8a86~92~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 120)
    (tracks 59)
    (zones 0)
    (modules 9)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+5V)
  (net 2 /GND)
  (net 3 /D4)
  (net 4 /D3)
  (net 5 /D2)
  (net 6 /D1)
  (net 7 /RX)
  (net 8 /TX)
  (net 9 /+3.3V)
  (net 10 /D8)
  (net 11 /D7)
  (net 12 /D6)
  (net 13 /D5)
  (net 14 /D0)
  (net 15 /A0)
  (net 16 /RST)
  (net 17 "Net-(B1-PadHV4)")
  (net 18 "Net-(B1-PadHV3)")
  (net 19 "Net-(B1-PadHV2)")
  (net 20 "Net-(B1-PadHV1)")
  (net 21 "Net-(GB1-Pad4)")
  (net 22 "Net-(D1-PadK)")
  (net 23 "Net-(B1-PadLV4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3.3V)
    (add_net /+5V)
    (add_net /A0)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /GND)
    (add_net /RST)
    (add_net /RX)
    (add_net /TX)
    (add_net "Net-(B1-PadHV1)")
    (add_net "Net-(B1-PadHV2)")
    (add_net "Net-(B1-PadHV3)")
    (add_net "Net-(B1-PadHV4)")
    (add_net "Net-(B1-PadLV4)")
    (add_net "Net-(D1-PadK)")
    (add_net "Net-(GB1-Pad4)")
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 153.7 99.1 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab) hide)
    (fp_text user GB>D8 (at 0 1.6) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 10 /D8) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 23 "Net-(B1-PadLV4)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module D1_mini:D1_mini_Pin_Header (layer B.Cu) (tedit 5766B078)
    (at 170.41 96.15)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.11 2.45 180) (layer B.SilkS))
    (fp_text value CONN_01X08 (at 0 3.1 180) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 /+5V))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 /GND))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 /D4))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /D3))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 /D2))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 /D1))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 /RX))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 /TX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (offset (xyz 0 -8.889999866485596 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Aesthetics:gblinksmall (layer F.Cu) (tedit 0)
    (at 159 73.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Resistors:AXIAL-0.3 (layer F.Cu) (tedit 200000)
    (at 162 98.3)
    (descr AXIAL-0.3)
    (tags AXIAL-0.3)
    (attr virtual)
    (fp_text reference R1 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 1KOHM-HORIZ-1_4W-1% (at 0 1.397) (layer F.SilkS) hide)
    (pad P$2 thru_hole circle (at 3.81 0) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 22 "Net-(D1-PadK)") (solder_mask_margin 0.1016))
    (pad P$1 thru_hole circle (at -3.81 0) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 2 /GND) (solder_mask_margin 0.1016))
  )
  (module LED:LED_3MM (layer F.Cu) (tedit 200000)
    (at 168 101.9 180)
    (descr "LED 3MM PTH")
    (tags "LED 3MM PTH")
    (attr virtual)
    (fp_text reference D1 (at 0 -2.58826) (layer F.SilkS) hide)
    (fp_text value LED3MM (at 0 2.667) (layer F.SilkS) hide)
    (fp_text user LED (at -2.5 -2 180) (layer F.SilkS))
    (pad K thru_hole circle (at 1.27 0 180) (size 1.8796 1.8796) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "Net-(D1-PadK)") (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at -1.27 0 180) (size 1.8796 1.8796) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 "Net-(B1-PadHV4)") (solder_mask_margin 0.1016))
  )
  (module gb-link-socket:gb-link-socket (layer F.Cu) (tedit 574068B5)
    (at 158.8 108.3)
    (fp_text reference GB1 (at -6.8 -4.5) (layer F.SilkS) hide)
    (fp_text value gb-link-socket (at 0 -4) (layer F.Fab))
    (pad 1 connect rect (at -2 0) (size 1 5) (layers B.Cu B.Mask)
      (net 17 "Net-(B1-PadHV4)"))
    (pad 3 connect rect (at 0 0) (size 1 5) (layers B.Cu B.Mask)
      (net 20 "Net-(B1-PadHV1)"))
    (pad 5 connect rect (at 2 0) (size 1 5) (layers B.Cu B.Mask)
      (net 19 "Net-(B1-PadHV2)"))
    (pad 2 connect rect (at -2 0) (size 1 5) (layers F.Cu F.Mask)
      (net 18 "Net-(B1-PadHV3)"))
    (pad 6 connect rect (at 2 0) (size 1 5) (layers F.Cu F.Mask)
      (net 2 /GND))
    (pad 4 connect rect (at 0 0) (size 1 5) (layers F.Cu F.Mask)
      (net 21 "Net-(GB1-Pad4)"))
  )
  (module Boards:SPARKFUN_LOGIC_LEVEL_CONVERTER (layer F.Cu) (tedit 200000)
    (at 159.4 87.3)
    (descr "SPARKFUN LOGIC LEVEL CONVERTER")
    (tags "SPARKFUN LOGIC LEVEL CONVERTER")
    (attr virtual)
    (fp_text reference B1 (at 0 -6.985) (layer F.SilkS) hide)
    (fp_text value "LEVEL SHIFTER" (at 0 1 90) (layer F.SilkS))
    (fp_text user LV1 (at -2.54 -6.35) (layer F.SilkS))
    (fp_text user LV2 (at -2.54 -3.81) (layer F.SilkS))
    (fp_text user HV1 (at 2.54 -6.35) (layer F.SilkS))
    (fp_text user HV2 (at 2.413 -3.81) (layer F.SilkS))
    (fp_text user LV (at -2.921 -1.27) (layer F.SilkS))
    (fp_text user GND (at -2.286 1.27) (layer F.SilkS))
    (fp_text user LV3 (at -2.54 3.81) (layer F.SilkS))
    (fp_text user LV4 (at -2.54 6.35) (layer F.SilkS))
    (fp_text user HV (at 2.794 -1.27) (layer F.SilkS))
    (fp_text user GND (at 2.413 1.27) (layer F.SilkS))
    (fp_text user HV3 (at 2.54 3.81) (layer F.SilkS))
    (fp_text user HV4 (at 2.54 6.35) (layer F.SilkS))
    (pad GND1 thru_hole circle (at -5.08 1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /GND) (solder_mask_margin 0.1016))
    (pad GND2 thru_hole circle (at 5.08 1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /GND) (solder_mask_margin 0.1016))
    (pad HV thru_hole circle (at 5.08 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /+5V) (solder_mask_margin 0.1016))
    (pad HV1 thru_hole circle (at 5.08 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(B1-PadHV1)") (solder_mask_margin 0.1016))
    (pad HV2 thru_hole circle (at 5.08 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(B1-PadHV2)") (solder_mask_margin 0.1016))
    (pad HV3 thru_hole circle (at 5.08 3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(B1-PadHV3)") (solder_mask_margin 0.1016))
    (pad HV4 thru_hole circle (at 5.08 6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(B1-PadHV4)") (solder_mask_margin 0.1016))
    (pad LV thru_hole circle (at -5.08 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /+3.3V) (solder_mask_margin 0.1016))
    (pad LV1 thru_hole circle (at -5.08 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /D6) (solder_mask_margin 0.1016))
    (pad LV2 thru_hole circle (at -5.08 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /D5) (solder_mask_margin 0.1016))
    (pad LV3 thru_hole circle (at -5.08 3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /D7) (solder_mask_margin 0.1016))
    (pad LV4 thru_hole circle (at -5.08 6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(B1-PadLV4)") (solder_mask_margin 0.1016))
  )
  (module D1_mini:D1_mini_Pin_Header (layer B.Cu) (tedit 5766ABD3)
    (at 147.55 96.15)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.05 -20.15 180) (layer B.SilkS))
    (fp_text value CONN_01X08 (at 0 3.1 180) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 /+3.3V))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 /D8))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 /D7))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 /D6))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 /D5))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 /D0))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 /A0))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 /RST))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (offset (xyz 0 -8.889999866485596 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module D1_mini:OSHW (layer B.Cu) (tedit 5766B04E)
    (at 169 74.3 180)
    (descr OSHW)
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference "" (at 0.09906 4.38912) (layer B.SilkS) hide)
    (fp_text value OSHW (at 0 -5) (layer B.Fab) hide)
  )
  (gr_text "Optional\nON > GB\nconnected " (at 163.5 100.9) (layer F.SilkS))
  (gr_text "Solder jumper to\npull D8 high when\na GB is connected" (at 159.4 87.2 90) (layer B.SilkS))
  (gr_text "(optional)" (at 152.2 103.8) (layer B.SilkS))
  (gr_text "CL\nD5" (at 161.1 103.1) (layer B.SilkS))
  (gr_text "SI\nD6" (at 158.9 103.1) (layer B.SilkS))
  (gr_text "5V\nD8" (at 156.8 103.1) (layer B.SilkS))
  (gr_text "SO\nD7" (at 156.6 103.1) (layer F.SilkS))
  (gr_text "SD\n-" (at 158.8 103.1) (layer F.SilkS))
  (gr_text G (at 160.8 104) (layer F.SilkS))
  (gr_text "©2021 Jack Gaino\ngithub.com/iamjackg" (at 157.5 74.2) (layer B.SilkS))
  (gr_arc (start 161.5 111) (end 161.5 111.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 156.1 111) (end 155.6 111) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.6 111) (end 155.6 105) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162 111) (end 162 105) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.5 111.5) (end 156.1 111.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.53954 70.598266) (end 168.577453 70.627024) (layer Edge.Cuts) (width 0.1))
  (gr_text 3V3 (at 150.8 96.1) (layer F.SilkS))
  (gr_text D8 (at 150.1 93.6) (layer F.SilkS))
  (gr_text D7 (at 150.1 91) (layer F.SilkS))
  (gr_text D6 (at 150.1 88.6) (layer F.SilkS))
  (gr_text D5 (at 150.1 86.1) (layer F.SilkS))
  (gr_text D0 (at 150.1 83.5) (layer F.SilkS))
  (gr_text A0 (at 150.1 80.9) (layer F.SilkS))
  (gr_text Rst (at 150.5 78.3) (layer F.SilkS))
  (gr_text 5V (at 167.9 96.2) (layer F.SilkS))
  (gr_text G (at 168.4 93.7) (layer F.SilkS))
  (gr_text D4 (at 167.8 91.2) (layer F.SilkS))
  (gr_text D3 (at 167.8 88.6) (layer F.SilkS))
  (gr_text D2 (at 167.8 86) (layer F.SilkS))
  (gr_text D1 (at 167.8 83.4) (layer F.SilkS))
  (gr_text RX (at 167.8 81) (layer F.SilkS))
  (gr_text TX (at 168 78.4) (layer F.SilkS))
  (gr_text Rst (at 150.5 78.3) (layer B.SilkS))
  (gr_text A0 (at 150.1 80.9) (layer B.SilkS))
  (gr_text D0 (at 150.1 83.5) (layer B.SilkS))
  (gr_text D5 (at 150.1 86.1) (layer B.SilkS))
  (gr_text D6 (at 150.1 88.6) (layer B.SilkS))
  (gr_text D7 (at 150.1 91) (layer B.SilkS))
  (gr_text D8 (at 150.1 93.6) (layer B.SilkS))
  (gr_text 3V3 (at 150.8 96.1) (layer B.SilkS))
  (gr_text TX (at 168.1 78.4) (layer B.SilkS))
  (gr_text RX (at 167.9 81) (layer B.SilkS))
  (gr_text D1 (at 167.9 83.4) (layer B.SilkS))
  (gr_text D2 (at 167.9 86) (layer B.SilkS))
  (gr_text D3 (at 167.9 88.6) (layer B.SilkS))
  (gr_text D4 (at 167.9 91.2) (layer B.SilkS))
  (gr_text G (at 168.5 93.7) (layer B.SilkS))
  (gr_text 5V (at 168 96.2) (layer B.SilkS))
  (gr_line (start 148.13752 98.214181) (end 148.1 105) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.193974 97.253285) (end 148.13752 98.214181) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.218922 74.698193) (end 146.193974 97.253285) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.334518 73.805425) (end 146.218922 74.698193) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.562878 73.050387) (end 146.334518 73.805425) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.890405 72.41854) (end 146.562878 73.050387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.303497 71.895342) (end 146.890405 72.41854) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.788555 71.466257) (end 147.303497 71.895342) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.331982 71.116742) (end 147.788555 71.466257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.920176 70.832259) (end 148.331982 71.116742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.53954 70.598266) (end 148.920176 70.832259) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.17525 70.81269) (end 168.577453 70.627024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.71944 71.059623) (end 169.17525 70.81269) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.210512 71.367259) (end 169.71944 71.059623) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.648953 71.735048) (end 170.210512 71.367259) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.035253 72.162423) (end 170.648953 71.735048) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.369901 72.648833) (end 171.035253 72.162423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.653384 73.193714) (end 171.369901 72.648833) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.886195 73.796507) (end 171.653384 73.193714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.900193 104.966658) (end 171.886195 73.796507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162 105) (end 171.900193 104.966658) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.1 105) (end 155.6 105) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.7 112) (xy 146.4 112) (xy 146.4 76.6) (xy 171.7 76.6)
      )
    )
  )
)
