(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 71)
    (zones 0)
    (modules 14)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.4)
    (user_trace_width 1.6)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (user_via 0.4 0.254)
    (user_via 0.5 0.3)
    (user_via 0.6 0.4)
    (user_via 0.8 0.6)
    (user_via 1.1 0.8)
    (user_via 1.3 1)
    (user_via 1.5 1.2)
    (user_via 1.7 1.4)
    (user_via 1.9 1.6)
    (user_via 2.5 2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.12)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance_ratio -0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VSS)
  (net 2 "Net-(C1-Pad1)")
  (net 3 /VDD_int)
  (net 4 "Net-(C4-Pad1)")
  (net 5 /VDD)
  (net 6 /OUT)
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad4)")
  (net 10 "Net-(J1-Pad5)")
  (net 11 "Net-(J1-Pad6)")
  (net 12 "Net-(J2-Pad1)")
  (net 13 "Net-(J2-Pad2)")
  (net 14 "Net-(J2-Pad3)")
  (net 15 "Net-(J2-Pad4)")
  (net 16 "Net-(J2-Pad5)")
  (net 17 "Net-(J2-Pad6)")
  (net 18 "Net-(R1-Pad1)")
  (net 19 "Net-(R3-Pad2)")
  (net 20 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /OUT)
    (add_net /VDD)
    (add_net /VDD_int)
    (add_net /VSS)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad1)")
  )
  (module SquantorRcl:R_0805+0603 (layer F.Cu) (tedit 5DB204EF)
    (at 159.7 68.4 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.1 1.1 90) (layer F.SilkS))
    (fp_text value Rf (at 2.1 1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.775 0 180) (size 1.05 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -0.775 0 180) (size 1.05 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorCrystal:Crystal_3225_4 (layer F.Cu) (tedit 5D56AE32)
    (at 160.1 72.9 270)
    (descr "SMD crystal 3225 size")
    (tags "SMD 3225")
    (attr smd)
    (fp_text reference Y1 (at -1.4 -2.3 270) (layer F.SilkS))
    (fp_text value Any (at -0.3 -2.2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 3 smd rect (at 1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at -1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorIC:SOT363-hand locked (layer F.Cu) (tedit 5D56B004)
    (at 160.02 66.04 270)
    (descr "SOT363 Plastic surface-mounted package; 6 leads SC-88 NXP specification")
    (tags "SOT363-hand SC-88 NXP")
    (fp_text reference U1 (at -1.94 2.02) (layer F.SilkS))
    (fp_text value 74X1GX04 (at -1.94 1.62) (layer F.Fab))
    (pad 3 smd rect (at 0.75 1.05 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0 1.05 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -0.75 1.05 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad1)"))
    (pad 4 smd rect (at 0.75 -1.05 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R1-Pad1)"))
    (pad 5 smd rect (at 0 -1.05 270) (size 0.4 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VDD_int))
    (pad 6 smd rect (at -0.75 -1.05 270) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5D440136)
    (at 162 68.5 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -1.7 0.1 180) (layer F.SilkS))
    (fp_text value 100 (at -1.7 0.2) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5D440136)
    (at 160.7 70.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 2 0) (layer F.SilkS))
    (fp_text value Rs (at 2 0) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R1-Pad1)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorConnectors:Header-0254-1X07-H010 locked (layer B.Cu) (tedit 6044B6D8)
    (at 156.21 68.58 270)
    (descr "7pin 2.54mm header")
    (tags "pinheader 7pin 2.54")
    (attr virtual)
    (fp_text reference J2 (at -7.62 -2.286 270) (layer B.SilkS))
    (fp_text value Conn_01x07 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at -7.62 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 0 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 2.54 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VSS))
  )
  (module SquantorConnectors:Header-0254-1X07-H010 locked (layer B.Cu) (tedit 6044B6D8)
    (at 163.83 68.58 90)
    (descr "7pin 2.54mm header")
    (tags "pinheader 7pin 2.54")
    (attr virtual)
    (fp_text reference J1 (at -7.62 -2.032 270) (layer B.SilkS))
    (fp_text value Conn_01x07 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at -7.62 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 6 /OUT))
    (pad 2 thru_hole circle (at -5.08 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 0 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 2.54 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 5.08 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 5 /VDD))
  )
  (module SquantorRcl:L_0402 (layer F.Cu) (tedit 5D554A2D)
    (at 160 61.6 180)
    (descr "Inductor SMD 0402")
    (tags "Inductor 0402")
    (attr smd)
    (fp_text reference FB1 (at -0.1 1.1) (layer F.SilkS))
    (fp_text value 600 (at 0 1.1) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /VDD_int))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 5D442507)
    (at 160.6 76.2 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -2.2 -1.9 90) (layer F.SilkS))
    (fp_text value TBD (at -2.2 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 5D442507)
    (at 160 64.1 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -2 0) (layer F.SilkS))
    (fp_text value 100n (at -2 0) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /VDD_int))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 5D442507)
    (at 160 63 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -2 0.2) (layer F.SilkS))
    (fp_text value 1u (at -2 0.2) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /VDD_int))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 5D442507)
    (at 159.5 76.2 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at -2.2 1.7 90) (layer F.SilkS))
    (fp_text value TBD (at -2.2 1.7 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 160.02 69.596 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference N2 (at 0 0) (layer B.SilkS) hide)
    (fp_text value OHWLOGO (at 0.75 0) (layer B.Fab) hide)
  )
  (module SquantorLabels:Label_Generic (layer B.Cu) (tedit 5D8A7D4C)
    (at 159.385 74.93)
    (descr "Label for general purpose use")
    (tags Label)
    (attr smd)
    (fp_text reference N1 (at 0 -1.85) (layer B.Fab) hide)
    (fp_text value 20210315 (at 0.8 0.1) (layer B.SilkS))
  )
  (gr_text VDD (at 162.4 60.9 90) (layer F.SilkS))
  (gr_text OUT (at 162.5 76.2 90) (layer F.SilkS))
  (gr_text VSS (at 157.7 76.2 90) (layer F.SilkS))
  (gr_line (start 154.686 77.724) (end 154.686 59.436) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.354 77.724) (end 154.686 77.724) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.354 59.436) (end 165.354 77.724) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.686 59.436) (end 165.354 59.436) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name /VSS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 165.1 77.47) (xy 154.94 77.47) (xy 154.94 59.69) (xy 165.1 59.69)
      )
    )
  )
)
