(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 82)
    (no_connects 0)
    (area 47.772381 46.736666 120.183334 99.885)
    (thickness 1.6)
    (drawings 17)
    (tracks 258)
    (zones 0)
    (modules 47)
    (nets 42)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.18)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C7-Pad2)")
  (net 7 "Net-(J1-Pad3)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J1-Pad4)")
  (net 11 "Net-(R3-Pad2)")
  (net 12 "Net-(R4-Pad2)")
  (net 13 "Net-(R6-Pad2)")
  (net 14 "Net-(R7-Pad1)")
  (net 15 "Net-(R8-Pad1)")
  (net 16 "Net-(U2-Pad5)")
  (net 17 "Net-(U2-Pad6)")
  (net 18 "Net-(U2-Pad11)")
  (net 19 "Net-(U2-Pad13)")
  (net 20 "Net-(U2-Pad14)")
  (net 21 "Net-(U2-Pad15)")
  (net 22 "Net-(U2-Pad16)")
  (net 23 "Net-(U2-Pad21)")
  (net 24 "Net-(U2-Pad22)")
  (net 25 "Net-(U2-Pad23)")
  (net 26 "Net-(C6-Pad1)")
  (net 27 "Net-(C1-Pad2)")
  (net 28 VDD)
  (net 29 "Net-(J2-Pad1)")
  (net 30 "Net-(J2-Pad4)")
  (net 31 "Net-(J2-Pad5)")
  (net 32 "Net-(J2-Pad6)")
  (net 33 "Net-(R2-Pad1)")
  (net 34 "Net-(U1-Pad5)")
  (net 35 "Net-(U1-Pad7)")
  (net 36 "Net-(U1-Pad10)")
  (net 37 "Net-(U1-Pad14)")
  (net 38 "Net-(U1-Pad15)")
  (net 39 "Net-(R9-Pad2)")
  (net 40 "Net-(R12-Pad1)")
  (net 41 "Net-(U1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.18)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net VDD)
  )
  (module Amp:Screw (layer F.Cu) (tedit 59989110)
    (at 73.75 51.5)
    (fp_text reference Screw (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Screw (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Amp:Screw (layer F.Cu) (tedit 59988667)
    (at 51.5 73.75)
    (fp_text reference Screw (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Screw (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988C99)
    (at 67 54.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 5998839B)
    (at 66 68.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988399)
    (at 67.5 68.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 57C6481E)
    (at 60.75 54.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988362)
    (at 70 58.75 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -1.7 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988307)
    (at 63.5 65.25 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988C96)
    (at 71.5 54.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988367)
    (at 73.5 64.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 599883AE)
    (at 69 68.75 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_1206 (layer F.Cu) (tedit 599883BD)
    (at 70.75 69.75 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0 -1.75 270) (layer F.SilkS) hide)
    (fp_text value CP (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988365)
    (at 73.5 63 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:C_0402 (layer F.Cu) (tedit 59988317)
    (at 63.5 63.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 -1.7) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:SJ-3524-SMT-TR (layer F.Cu) (tedit 59988E84)
    (at 56.6 70.85 90)
    (fp_text reference J1 (at 0 -7.65 90) (layer F.SilkS) hide)
    (fp_text value JACK_TRS_4PINS (at 0 7.35 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -3.7 90) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -2 3.7 90) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 7.4 3.7 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at 11.3 -0.75 90) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad4)"))
    (pad "" np_thru_hole circle (at -0.9 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.1 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Amp:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5998890D)
    (at 51.75 51.75 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 VDD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 599883F8)
    (at 63 71 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 599889C1)
    (at 70 54.25 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 599883F6)
    (at 64.5 71 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 59988418)
    (at 66 71 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 5998841A)
    (at 67.5 71 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 599889AE)
    (at 68.5 54.25 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 59988C91)
    (at 68.5 56.5 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 59988C93)
    (at 67 56.5 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 599896DE)
    (at 54.25 53.75)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 59988C03)
    (at 70 56.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 59988C06)
    (at 71.5 56.5 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:R_0402 (layer F.Cu) (tedit 599896E2)
    (at 57 53.75)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 599893D3)
    (at 62 57.25)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -2.85) (layer F.SilkS) hide)
    (fp_text value PIC16F1503 (at 0 2.85) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C1-Pad2)"))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad1)"))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad4)"))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad5)"))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad5)"))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad7)"))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad1)"))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R8-Pad1)"))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad10)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-Pad5)"))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-Pad4)"))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad14)"))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad15)"))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Amp:QFN-28-LM49270 (layer F.Cu) (tedit 599893E0)
    (at 68.5 63.75)
    (attr smd)
    (fp_text reference U2 (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value LM49270 (at 0 4.1) (layer F.Fab))
    (pad 1 smd rect (at -2.45 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -2.45 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -2.45 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -2.45 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 5 smd rect (at -2.45 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -2.45 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -2.45 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C6-Pad1)"))
    (pad 8 smd rect (at -1.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 9 smd rect (at -1 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 10 smd rect (at -0.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 0.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 13 smd rect (at 1 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 1.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 2.45 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad15)"))
    (pad 16 smd rect (at 2.45 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 2.45 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 18 smd rect (at 2.45 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 2.45 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 20 smd rect (at 2.45 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 2.45 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 1.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 1 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad23)"))
    (pad 24 smd rect (at 0.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
    (pad 25 smd rect (at 0 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad1)"))
    (pad 26 smd rect (at -0.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R8-Pad1)"))
    (pad 27 smd rect (at -1 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad4)"))
    (pad 28 smd rect (at -1.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599889AC)
    (at 68.25 51)
    (fp_text reference W1 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R6-Pad2)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 59988481)
    (at 63.75 74.25)
    (fp_text reference W2 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad2)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 59988495)
    (at 66 74.25)
    (fp_text reference W3 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R4-Pad2)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599884BB)
    (at 71 74.25)
    (fp_text reference W4 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599884BD)
    (at 68.5 74.25)
    (fp_text reference W5 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599889C3)
    (at 70.5 51)
    (fp_text reference W6 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad1)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 59988539)
    (at 74.25 58.25)
    (fp_text reference W7 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad23)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 59988528)
    (at 74.25 60.5)
    (fp_text reference W8 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad22)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 59988514)
    (at 74.25 67)
    (fp_text reference W9 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad14)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 5998850F)
    (at 74.25 69.25)
    (fp_text reference W10 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad13)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 5982289D)
    (at 55.75 56)
    (fp_text reference W11 (at 0 2.5) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad4)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599888DC)
    (at 51 57.25)
    (fp_text reference W12 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad5)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599896D1)
    (at 57.25 56)
    (fp_text reference W13 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R12-Pad1)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599888B1)
    (at 51 55)
    (fp_text reference W14 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 28 VDD))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599896D6)
    (at 54.25 56)
    (fp_text reference W15 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R9-Pad2)"))
  )
  (module Amp:Pad (layer F.Cu) (tedit 599888C2)
    (at 51 59.5)
    (fp_text reference W16 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Amp:Screw (layer F.Cu) (tedit 59988667)
    (at 73.75 73.75)
    (fp_text reference Screw (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Screw (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 75.25 50) (end 50 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 75.25) (end 50 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.25 75.25) (end 50 75.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.25 50) (end 75.25 75.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text - (at 52.25 59.5) (layer F.SilkS))
  (gr_text + (at 52.25 55) (layer F.SilkS))
  (gr_text DN (at 70.5 52.5) (layer F.SilkS))
  (gr_text UP (at 68.25 52.5) (layer F.SilkS))
  (gr_text VOL (at 53 57.25) (layer F.SilkS))
  (gr_text L+ (at 72.75 58.25) (layer F.SilkS))
  (gr_text L- (at 72.75 60.5) (layer F.SilkS))
  (gr_text R- (at 72.75 67) (layer F.SilkS))
  (gr_text R+ (at 72.75 69.25) (layer F.SilkS))
  (gr_text V+ (at 71 72.75) (layer F.SilkS))
  (gr_text V- (at 68.5 72.75) (layer F.SilkS))
  (gr_text R (at 66 72.75) (layer F.SilkS))
  (gr_text L (at 63.75 72.75) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 75.25 75.25) (xy 50 75.25) (xy 50 50) (xy 75.25 50)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 75.25 75.25) (xy 50 75.25) (xy 50 50) (xy 75.25 50)
      )
    )
  )
)
