(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 171)
    (zones 0)
    (modules 31)
    (nets 25)
  )
  (page USLetter portrait)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.4064)
    (trace_clearance 0.1778)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (user_via 0.4064 0.254)
    (uvia_size 0.4064)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.1778)
    (aux_axis_origin 0 0)
    (grid_origin 25.4 25.4)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 +5V)
  (net 4 VCC)
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(D1-Pad1)")
  (net 8 USB_D+)
  (net 9 USB_D-)
  (net 10 VGA_VSYNCH)
  (net 11 VGA_HSYNCH)
  (net 12 "Net-(J3-Pad3)")
  (net 13 "Net-(J3-Pad2)")
  (net 14 "Net-(J3-Pad1)")
  (net 15 "Net-(J5-Pad3)")
  (net 16 SERIAL_TXD)
  (net 17 ICSP_PCC)
  (net 18 ICSP_PGD)
  (net 19 ICSP_MCLR)
  (net 20 "Net-(JP1-Pad1)")
  (net 21 "Net-(R2-Pad1)")
  (net 22 SERIAL_RXD)
  (net 23 VGA_VIDEO)
  (net 24 "Net-(R10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.254)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.4064)
    (uvia_drill 0.254)
    (diff_pair_width 0.1778)
    (diff_pair_gap 0.254)
    (add_net +5V)
    (add_net GND)
    (add_net ICSP_MCLR)
    (add_net ICSP_PCC)
    (add_net ICSP_PGD)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net SERIAL_RXD)
    (add_net SERIAL_TXD)
    (add_net USB_D+)
    (add_net USB_D-)
    (add_net VCC)
    (add_net VGA_HSYNCH)
    (add_net VGA_VIDEO)
    (add_net VGA_VSYNCH)
  )
  (module 0_LOCAL:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5F49B156)
    (at 93.345 51.435)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at 1.27 -3.81) (layer F.SilkS))
    (fp_text value MCP1700-3302E_TO92 (at 1.27 2.79) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -4.4) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6096) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6096) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 0.9 1.5) (drill 0.6096) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (model ${KIPRJMOD}/3d/TO-92_Inline.wrl
      (offset (xyz 0 0 -2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:LED_D5.0mm (layer F.Cu) (tedit 5F49B105)
    (at 95.885 59.055 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 3.81) (layer F.SilkS))
    (fp_text value Status (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 7 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KIPRJMOD}/3d/LED_D5.0mm.wrl
      (offset (xyz 0 0 -3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:DIP-28_W7.62mm_Socket placed (layer F.Cu) (tedit 5F444740)
    (at 66.04 44.196 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at 3.81 16.51 180) (layer F.SilkS))
    (fp_text value PIC32MX270F256B-I_SP (at 3.556 27.686 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 16.51 180) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 19 ICSP_MCLR))
    (pad 15 thru_hole circle (at 7.62 33.02 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 21 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 18 ICSP_PGD))
    (pad 16 thru_hole circle (at 7.62 30.48 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 17 ICSP_PCC))
    (pad 17 thru_hole circle (at 7.62 27.94 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 16 SERIAL_TXD))
    (pad 18 thru_hole circle (at 7.62 25.4 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 11 VGA_HSYNCH))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 22 SERIAL_RXD))
    (pad 19 thru_hole circle (at 7.62 22.86 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 7.62 20.32 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 7.62 17.78 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 8 USB_D+))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole circle (at 7.62 15.24 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 9 USB_D-))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 23 thru_hole circle (at 7.62 12.7 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 24 thru_hole circle (at 7.62 10.16 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 10 VGA_VSYNCH))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 7.62 7.62 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 11 VGA_HSYNCH))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 23 VGA_VIDEO))
    (pad 26 thru_hole circle (at 7.62 5.08 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 27 thru_hole circle (at 7.62 2.54 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 24 "Net-(R10-Pad1)"))
    (pad 28 thru_hole circle (at 7.62 0 90) (size 1.0922 1.0922) (drill 0.6858) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KIPRJMOD}/3d/DIP-28_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3d/DIP-28_W7.62mm.wrl
      (offset (xyz 0 0 4.0132))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5F443E2F)
    (at 58.42 40.64 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 5.715) (layer F.SilkS))
    (fp_text value Red (at 0 4.445) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad1)"))
    (model ${KIPRJMOD}/3d/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5F443E2F)
    (at 54.61 40.64 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 5.715) (layer F.SilkS))
    (fp_text value Green (at 0 4.445) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad2)"))
    (model ${KIPRJMOD}/3d/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5F443E2F)
    (at 50.8 40.64 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 5.715 180) (layer F.SilkS))
    (fp_text value Blue (at 0 4.445 180) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad3)"))
    (model ${KIPRJMOD}/3d/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:USB_A_Female_UE27AC54100 (layer F.Cu) (tedit 5F43BAC8)
    (at 81.915 53.34)
    (fp_text reference J1 (at 0 0 unlocked) (layer F.SilkS))
    (fp_text value USB (at 0 1.905 180) (layer F.SilkS))
    (fp_text user %R (at -0.025 0.975 180) (layer F.Fab))
    (pad 4 thru_hole circle (at 3.5 -2.71) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1 -2.71) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 USB_D+))
    (pad 2 thru_hole circle (at -1 -2.71) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 USB_D-))
    (pad 1 thru_hole roundrect (at -3.5 -2.71) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 3 +5V))
    (pad 5 thru_hole circle (at 6.57 0) (size 3.81 3.81) (drill 2.286) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -6.57 0) (size 3.81 3.81) (drill 2.286) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/3d/USB-A_female_horiz_thru.step
      (offset (xyz 0 3.47472 6.8326))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:ICD15S13E4GX00LF (layer F.Cu) (tedit 5F43A484)
    (at 53.34 52.07)
    (fp_text reference J3 (at 0 4.9276) (layer F.SilkS))
    (fp_text value VGA (at 0 6.5532) (layer F.SilkS))
    (pad S thru_hole circle (at 12.495 0) (size 5.08 5.08) (drill 3.048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S thru_hole circle (at -12.495 0) (size 5.08 5.08) (drill 3.048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at -4.83 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -2.54 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 VGA_VSYNCH))
    (pad 13 thru_hole circle (at -0.25 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 VGA_HSYNCH))
    (pad 12 thru_hole circle (at 2.04 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 4.33 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -3.685 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -1.395 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0.895 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 3.185 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 5.475 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -4.83 -2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -2.54 -2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -0.25 -2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 2.04 -2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad2)"))
    (pad 1 thru_hole roundrect (at 4.33 -2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 14 "Net-(J3-Pad1)"))
    (model ${KIPRJMOD}/3d/ICD15S13E4GX00LF.step
      (offset (xyz 0 -11.0236 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 180))
    )
  )
  (module 0_LOCAL:Symbol_Barrel_Polarity locked (layer F.Cu) (tedit 5F43ACB1)
    (at 111.125 59.055 90)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (fp_text reference REF** (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value Symbol_Barrel_Polarity (at 0 2 90) (layer F.Fab) hide)
    (fp_text user + (at 2.9972 -0.0254 90) (layer F.SilkS))
    (fp_text user - (at -2.9972 -0.0254 90) (layer F.SilkS))
  )
  (module 0_LOCAL:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5F438498)
    (at 60.96 29.21 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J7 (at 2.54 1.27) (layer F.SilkS))
    (fp_text value ICSP (at 2.54 6.35 180) (layer F.SilkS))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 19 ICSP_MCLR))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 ICSP_PGD))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 17 ICSP_PCC))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3d/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:Crystal_HC49-4H_Vertical (layer F.Cu) (tedit 5F4371F0)
    (at 43.815 43.18 90)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 2.44 0 90) (layer F.SilkS))
    (fp_text value 20MHz (at 2.44 3.525 90) (layer F.SilkS))
    (fp_text user %R (at 2.44 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3d/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:Barrel_Jack_5.5mmODx2.1mmID_PJ-102A (layer F.Cu) (tedit 5F436679)
    (at 104.14 52.705 180)
    (fp_text reference J4 (at 0 0) (layer F.SilkS))
    (fp_text value PJ-102A (at 0 5.8) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 0 -3 180) (size 2.6 2) (drill oval 1.6 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 3 180) (size 2.6 2) (drill oval 1.6 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 3 +5V))
    (pad 3 thru_hole roundrect (at -4.7 0 180) (size 2 2.6) (drill oval 1 1.6) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (model ${KIPRJMOD}/3d/CUI_DEVICES_PJ-102A.step
      (offset (xyz 0 10.668 6.4516))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module terminal:TE_3-641215-4 (layer F.Cu) (tedit 5F407B9F)
    (at 41.91 30.48 180)
    (fp_text reference J5 (at -3.81 -4.191 180) (layer F.SilkS))
    (fp_text value Serial (at -6.715 4.405 180) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -7.62 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad3)"))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 SERIAL_TXD))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (model ${KIPRJMOD}/3d/c-3-641215-4-z-3d.stp
      (offset (xyz -3.81 -0 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module terminal:TE_3-641215-2 (layer F.Cu) (tedit 5F407C9A)
    (at 104.775 30.48 180)
    (fp_text reference J6 (at -5.08 -0.508) (layer F.SilkS))
    (fp_text value "External 5V" (at -1.635 4.405) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 3 +5V))
    (model ${KIPRJMOD}/3d/c-3-641215-2-z-3d.stp
      (offset (xyz -1.27 0 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 107.95 36.83 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 1.8K (at 3.81 -2.54 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 36.83 38.862 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10K (at 3.81 -2.413 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 SERIAL_RXD))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 35.56 50.8 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 0) (layer F.SilkS))
    (fp_text value 100K (at 5.334 -2.54) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 SERIAL_RXD))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 58.42 44.45 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 0) (layer F.SilkS))
    (fp_text value 220 (at 3.81 -2.159) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(JP1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 VGA_VIDEO))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 104.14 36.83 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 4.064 2.37 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 36.83 28.448 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 ICSP_MCLR))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 114.3 28.956 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at -0.381 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 28.956 28.956 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 28.956 59.944 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 114.3 59.944 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 33.02 46.228 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 2.54 0) (layer F.SilkS))
    (fp_text value 27pF (at 2.286 2.286) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 33.02 41.529 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.5 0) (layer F.SilkS))
    (fp_text value 27pF (at 2.286 2.286) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 55.88 33.528 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 -2.54 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 33.02 36.83 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.286 2.413) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_Tantal_D5.0mm_P5.00mm placed (layer F.Cu) (tedit 5F407C40)
    (at 99.822 30.48 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 3.75) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_Tantal_D5.0mm_P5.00mm placed (layer F.Cu) (tedit 5F407C32)
    (at 91.44 30.48 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C2 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 3.75) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_Tantal_D5.0mm_P5.00mm placed (layer F.Cu) (tedit 5F407C25)
    (at 83.058 30.48 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 3.81) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 114.3 59.944) (end 114.3 63.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 114.3 28.956) (end 117.856 28.956) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 28.956 59.944) (end 25.4 59.944) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 28.956 28.956) (end 28.956 25.4) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text github.com/bkw777/Geoff_vt100 (at 115.8748 44.4246 90) (layer F.SilkS))
  (gr_text MCLR (at 60.96 33.02 90) (layer F.SilkS))
  (gr_text PCC (at 71.12 32.512 90) (layer F.SilkS))
  (gr_text PGD (at 68.58 32.512 90) (layer F.SilkS))
  (gr_text GND (at 66.04 32.512 90) (layer F.SilkS))
  (gr_text VCC (at 63.5 32.512 90) (layer F.SilkS))
  (gr_text 100ma (at 112.014 51.816 90) (layer F.SilkS))
  (gr_text 5vdc (at 110.744 52.705 90) (layer F.SilkS))
  (gr_line (start 25.4 28.956) (end 25.4 59.944) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.856 28.956) (end 117.856 59.944) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.3 63.5) (end 28.956 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 28.956 25.4) (end 114.3 25.4) (layer Edge.Cuts) (width 0.05))
  (gr_text VCC (at 50.165 26.67) (layer F.SilkS))
  (gr_text RX (at 46.99 26.67) (layer F.SilkS))
  (gr_text TX (at 44.45 26.67) (layer F.SilkS))
  (gr_text GND (at 41.275 26.67) (layer F.SilkS))
  (gr_text GND (at 107.315 26.67) (layer F.SilkS))
  (gr_text +5V (at 104.14 26.67) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 117.856 63.5) (xy 25.4 63.5) (xy 25.4 25.4) (xy 117.856 25.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 117.856 63.5) (xy 25.4 63.5) (xy 25.4 25.4) (xy 117.856 25.4)
      )
    )
  )
)
